(kicad_pcb
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(general
		(thickness 0.1)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting
			(front yes)
			(back yes)
		)
		(covering
			(front no)
			(back no)
		)
		(plugging
			(front no)
			(back no)
		)
		(capping no)
		(filling no)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12)
			(dashed_line_gap_ratio 3)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(footprint "ELFlex:TenNet_WireBank"
		(layer "F.Cu")
		(at 144.6 20)
		(property "Reference" "J6"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "127 mm CUT TERMINATION"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" smd rect
			(at 0 0.95)
			(size 3 1.2)
			(layers "F.Cu" "F.Mask")
			(net "V24_MOTOR2")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at 0 2.35)
			(size 3 1.2)
			(layers "F.Cu" "F.Mask")
			(net "GND")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at 0 3.4)
			(size 3 0.5)
			(layers "F.Cu" "F.Mask")
			(net "CAN_H")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at 0 4.099999)
			(size 3 0.5)
			(layers "F.Cu" "F.Mask")
			(net "CAN_L")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "5" smd rect
			(at 0 4.825)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT1_LED_PLUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "6" smd rect
			(at 0 5.575)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT1_LED_MINUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "7" smd rect
			(at 0 6.325)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT2_LED_PLUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "8" smd rect
			(at 0 7.075)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT2_LED_MINUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "9" smd rect
			(at 0 7.825)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT3_LED_PLUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "10" smd rect
			(at 0 8.575)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT3_LED_MINUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:TenNet_WireBank"
		(layer "F.Cu")
		(at 68.4 20)
		(property "Reference" "J3"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "50.8 mm CUT TERMINATION"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" smd rect
			(at 0 0.95)
			(size 3 1.2)
			(layers "F.Cu" "F.Mask")
			(net "V24_MOTOR2")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at 0 2.35)
			(size 3 1.2)
			(layers "F.Cu" "F.Mask")
			(net "GND")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at 0 3.4)
			(size 3 0.5)
			(layers "F.Cu" "F.Mask")
			(net "CAN_H")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at 0 4.099999)
			(size 3 0.5)
			(layers "F.Cu" "F.Mask")
			(net "CAN_L")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "5" smd rect
			(at 0 4.825)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT1_LED_PLUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "6" smd rect
			(at 0 5.575)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT1_LED_MINUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "7" smd rect
			(at 0 6.325)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT2_LED_PLUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "8" smd rect
			(at 0 7.075)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT2_LED_MINUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "9" smd rect
			(at 0 7.825)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT3_LED_PLUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "10" smd rect
			(at 0 8.575)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT3_LED_MINUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:TenNet_WireBank"
		(layer "F.Cu")
		(at 43 20)
		(property "Reference" "J2"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "25.4 mm CUT TERMINATION"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" smd rect
			(at 0 0.95)
			(size 3 1.2)
			(layers "F.Cu" "F.Mask")
			(net "V24_MOTOR2")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at 0 2.35)
			(size 3 1.2)
			(layers "F.Cu" "F.Mask")
			(net "GND")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at 0 3.4)
			(size 3 0.5)
			(layers "F.Cu" "F.Mask")
			(net "CAN_H")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at 0 4.099999)
			(size 3 0.5)
			(layers "F.Cu" "F.Mask")
			(net "CAN_L")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "5" smd rect
			(at 0 4.825)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT1_LED_PLUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "6" smd rect
			(at 0 5.575)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT1_LED_MINUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "7" smd rect
			(at 0 6.325)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT2_LED_PLUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "8" smd rect
			(at 0 7.075)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT2_LED_MINUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "9" smd rect
			(at 0 7.825)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT3_LED_PLUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "10" smd rect
			(at 0 8.575)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT3_LED_MINUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:TenNet_WireBank"
		(layer "F.Cu")
		(at 93.799999 20)
		(property "Reference" "J4"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "76.2 mm CUT TERMINATION"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" smd rect
			(at 0 0.95)
			(size 3 1.2)
			(layers "F.Cu" "F.Mask")
			(net "V24_MOTOR2")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at 0 2.35)
			(size 3 1.2)
			(layers "F.Cu" "F.Mask")
			(net "GND")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at 0 3.4)
			(size 3 0.5)
			(layers "F.Cu" "F.Mask")
			(net "CAN_H")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at 0 4.099999)
			(size 3 0.5)
			(layers "F.Cu" "F.Mask")
			(net "CAN_L")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "5" smd rect
			(at 0 4.825)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT1_LED_PLUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "6" smd rect
			(at 0 5.575)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT1_LED_MINUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "7" smd rect
			(at 0 6.325)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT2_LED_PLUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "8" smd rect
			(at 0 7.075)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT2_LED_MINUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "9" smd rect
			(at 0 7.825)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT3_LED_PLUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "10" smd rect
			(at 0 8.575)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT3_LED_MINUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:TenNet_WireBank"
		(layer "F.Cu")
		(at 119.199999 20)
		(property "Reference" "J5"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "101.6 mm CUT TERMINATION"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" smd rect
			(at 0 0.95)
			(size 3 1.2)
			(layers "F.Cu" "F.Mask")
			(net "V24_MOTOR2")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at 0 2.35)
			(size 3 1.2)
			(layers "F.Cu" "F.Mask")
			(net "GND")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at 0 3.4)
			(size 3 0.5)
			(layers "F.Cu" "F.Mask")
			(net "CAN_H")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at 0 4.099999)
			(size 3 0.5)
			(layers "F.Cu" "F.Mask")
			(net "CAN_L")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "5" smd rect
			(at 0 4.825)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT1_LED_PLUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "6" smd rect
			(at 0 5.575)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT1_LED_MINUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "7" smd rect
			(at 0 6.325)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT2_LED_PLUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "8" smd rect
			(at 0 7.075)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT2_LED_MINUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "9" smd rect
			(at 0 7.825)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT3_LED_PLUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "10" smd rect
			(at 0 8.575)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT3_LED_MINUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:TenNet_WireBank"
		(layer "F.Cu")
		(at 169.999999 20)
		(property "Reference" "J7"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "152.4 mm CUT TERMINATION"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" smd rect
			(at 0 0.95)
			(size 3 1.2)
			(layers "F.Cu" "F.Mask")
			(net "V24_MOTOR2")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at 0 2.35)
			(size 3 1.2)
			(layers "F.Cu" "F.Mask")
			(net "GND")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at 0 3.4)
			(size 3 0.5)
			(layers "F.Cu" "F.Mask")
			(net "CAN_H")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at 0 4.099999)
			(size 3 0.5)
			(layers "F.Cu" "F.Mask")
			(net "CAN_L")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "5" smd rect
			(at 0 4.825)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT1_LED_PLUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "6" smd rect
			(at 0 5.575)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT1_LED_MINUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "7" smd rect
			(at 0 6.325)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT2_LED_PLUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "8" smd rect
			(at 0 7.075)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT2_LED_MINUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "9" smd rect
			(at 0 7.825)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT3_LED_PLUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "10" smd rect
			(at 0 8.575)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT3_LED_MINUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:TenNet_WireBank"
		(layer "F.Cu")
		(at 23 20)
		(property "Reference" "J1"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "INPUT / KEEP THIS END"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" smd rect
			(at 0 0.95)
			(size 3 1.2)
			(layers "F.Cu" "F.Mask")
			(net "V24_MOTOR2")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at 0 2.35)
			(size 3 1.2)
			(layers "F.Cu" "F.Mask")
			(net "GND")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at 0 3.4)
			(size 3 0.5)
			(layers "F.Cu" "F.Mask")
			(net "CAN_H")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at 0 4.099999)
			(size 3 0.5)
			(layers "F.Cu" "F.Mask")
			(net "CAN_L")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "5" smd rect
			(at 0 4.825)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT1_LED_PLUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "6" smd rect
			(at 0 5.575)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT1_LED_MINUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "7" smd rect
			(at 0 6.325)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT2_LED_PLUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "8" smd rect
			(at 0 7.075)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT2_LED_MINUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "9" smd rect
			(at 0 7.825)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT3_LED_PLUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "10" smd rect
			(at 0 8.575)
			(size 3 0.55)
			(layers "F.Cu" "F.Mask")
			(net "SPOT3_LED_MINUS")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(gr_line
		(start 20 20)
		(end 172.4 20)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 20 29.2)
		(end 20 20)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.4 20)
		(end 172.4 29.2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.4 29.2)
		(end 20 29.2)
		(layer "Edge.Cuts")
	)
	(gr_text "25.4mm >"
		(at 36.4 24.6 0)
		(layer "F.SilkS")
	)
	(gr_text "50.8mm >"
		(at 61.8 24.6 0)
		(layer "F.SilkS")
	)
	(gr_text "76.2mm >"
		(at 87.2 24.6 0)
		(layer "F.SilkS")
	)
	(gr_text "101.6mm >"
		(at 112.6 24.6 0)
		(layer "F.SilkS")
	)
	(gr_text "127mm >"
		(at 138 24.6 0)
		(layer "F.SilkS")
	)
	(gr_text "152.4mm >"
		(at 163.4 24.6 0)
		(layer "F.SilkS")
	)
	(embedded_fonts no)
)
