(kicad_sch
  (version 20250114)
  (generator "engineered-lighting")
  (generator_version "0.2")
  (paper "A3")
  (title_block
    (title "Gimbal arm: stationary ten-net ribbon, QUOTE REVIEW")
    (date "2026-09-06")
    (rev "A draft")
    (company "Engineered Lighting")
    (comment 1 "ENGINEERING QUOTE REVIEW - see release status before fabrication"))
  (lib_symbols
    (symbol "Connector_Generic:Conn_01x10"
      (pin_names
        (offset 1.016)
        (hide yes))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "J"
        (at 0 12.7 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "Conn_01x10"
        (at 0 -15.24 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Generic connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "connector"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "Connector*:*_1x??_*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "Conn_01x10_1_1"
        (rectangle
          (start -1.27 11.43)
          (end 1.27 -13.97)
          (fill
            (type background)))
        (rectangle
          (start -1.27 10.287)
          (end 0 10.033)
          (fill
            (type none)))
        (rectangle
          (start -1.27 7.747)
          (end 0 7.493)
          (fill
            (type none)))
        (rectangle
          (start -1.27 5.207)
          (end 0 4.953)
          (fill
            (type none)))
        (rectangle
          (start -1.27 2.667)
          (end 0 2.413)
          (fill
            (type none)))
        (rectangle
          (start -1.27 0.127)
          (end 0 -0.127)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -2.413)
          (end 0 -2.667)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -4.953)
          (end 0 -5.207)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -7.493)
          (end 0 -7.747)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -10.033)
          (end 0 -10.287)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -12.573)
          (end 0 -12.827)
          (fill
            (type none)))
        (pin passive line
          (at -5.08 10.16 0)
          (length 3.81)
          (name "Pin_1")
          (number "1"))
        (pin passive line
          (at -5.08 7.62 0)
          (length 3.81)
          (name "Pin_2")
          (number "2"))
        (pin passive line
          (at -5.08 5.08 0)
          (length 3.81)
          (name "Pin_3")
          (number "3"))
        (pin passive line
          (at -5.08 2.54 0)
          (length 3.81)
          (name "Pin_4")
          (number "4"))
        (pin passive line
          (at -5.08 0 0)
          (length 3.81)
          (name "Pin_5")
          (number "5"))
        (pin passive line
          (at -5.08 -2.54 0)
          (length 3.81)
          (name "Pin_6")
          (number "6"))
        (pin passive line
          (at -5.08 -5.08 0)
          (length 3.81)
          (name "Pin_7")
          (number "7"))
        (pin passive line
          (at -5.08 -7.62 0)
          (length 3.81)
          (name "Pin_8")
          (number "8"))
        (pin passive line
          (at -5.08 -10.16 0)
          (length 3.81)
          (name "Pin_9")
          (number "9"))
        (pin passive line
          (at -5.08 -12.7 0)
          (length 3.81)
          (name "Pin_10")
          (number "10")))
      (embedded_fonts no)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x10")
    (at 74.93 80.01 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J1"
      (at 74.93 59.69 0.0))
    (property "Value" "INPUT / KEEP THIS END"
      (at 74.93 62.23 0.0))
    (property "Footprint" "ELFlex:TenNet_WireBank"
      (at 74.93 80.01 0.0)
      (hide yes))
    (instances
      (project "gimbal-static-v0.2"
        (path
          (reference "J1")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (pin "10"))
  (wire
    (pts
      (xy 69.85 69.85)
      (xy 58.42 69.85)))
  (global_label "V24_MOTOR2"
    (shape passive)
    (at 58.42 69.85 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 58.42 69.85 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 69.85 72.39)
      (xy 62.23 72.39)))
  (global_label "GND"
    (shape passive)
    (at 62.23 72.39 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 62.23 72.39 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 69.85 74.93)
      (xy 60.96 74.93)))
  (global_label "CAN_H"
    (shape passive)
    (at 60.96 74.93 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 60.96 74.93 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 69.85 77.47)
      (xy 60.96 77.47)))
  (global_label "CAN_L"
    (shape passive)
    (at 60.96 77.47 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 60.96 77.47 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 69.85 80.01)
      (xy 55.88 80.01)))
  (global_label "SPOT1_LED_PLUS"
    (shape passive)
    (at 55.88 80.01 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 55.88 80.01 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 69.85 82.55)
      (xy 55.88 82.55)))
  (global_label "SPOT1_LED_MINUS"
    (shape passive)
    (at 55.88 82.55 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 55.88 82.55 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 69.85 85.09)
      (xy 55.88 85.09)))
  (global_label "SPOT2_LED_PLUS"
    (shape passive)
    (at 55.88 85.09 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 55.88 85.09 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 69.85 87.63)
      (xy 55.88 87.63)))
  (global_label "SPOT2_LED_MINUS"
    (shape passive)
    (at 55.88 87.63 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 55.88 87.63 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 69.85 90.17)
      (xy 55.88 90.17)))
  (global_label "SPOT3_LED_PLUS"
    (shape passive)
    (at 55.88 90.17 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 55.88 90.17 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 69.85 92.71)
      (xy 55.88 92.71)))
  (global_label "SPOT3_LED_MINUS"
    (shape passive)
    (at 55.88 92.71 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 55.88 92.71 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x10")
    (at 170.18 80.01 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J2"
      (at 170.18 59.69 0.0))
    (property "Value" "25.4 mm CUT TERMINATION"
      (at 170.18 62.23 0.0))
    (property "Footprint" "ELFlex:TenNet_WireBank"
      (at 170.18 80.01 0.0)
      (hide yes))
    (instances
      (project "gimbal-static-v0.2"
        (path
          (reference "J2")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (pin "10"))
  (wire
    (pts
      (xy 165.1 69.85)
      (xy 153.67 69.85)))
  (global_label "V24_MOTOR2"
    (shape passive)
    (at 153.67 69.85 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 153.67 69.85 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 165.1 72.39)
      (xy 157.48 72.39)))
  (global_label "GND"
    (shape passive)
    (at 157.48 72.39 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 157.48 72.39 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 165.1 74.93)
      (xy 156.21 74.93)))
  (global_label "CAN_H"
    (shape passive)
    (at 156.21 74.93 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 156.21 74.93 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 165.1 77.47)
      (xy 156.21 77.47)))
  (global_label "CAN_L"
    (shape passive)
    (at 156.21 77.47 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 156.21 77.47 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 165.1 80.01)
      (xy 151.13 80.01)))
  (global_label "SPOT1_LED_PLUS"
    (shape passive)
    (at 151.13 80.01 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 151.13 80.01 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 165.1 82.55)
      (xy 151.13 82.55)))
  (global_label "SPOT1_LED_MINUS"
    (shape passive)
    (at 151.13 82.55 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 151.13 82.55 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 165.1 85.09)
      (xy 151.13 85.09)))
  (global_label "SPOT2_LED_PLUS"
    (shape passive)
    (at 151.13 85.09 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 151.13 85.09 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 165.1 87.63)
      (xy 151.13 87.63)))
  (global_label "SPOT2_LED_MINUS"
    (shape passive)
    (at 151.13 87.63 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 151.13 87.63 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 165.1 90.17)
      (xy 151.13 90.17)))
  (global_label "SPOT3_LED_PLUS"
    (shape passive)
    (at 151.13 90.17 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 151.13 90.17 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 165.1 92.71)
      (xy 151.13 92.71)))
  (global_label "SPOT3_LED_MINUS"
    (shape passive)
    (at 151.13 92.71 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 151.13 92.71 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x10")
    (at 265.43 80.01 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J3"
      (at 265.43 59.69 0.0))
    (property "Value" "50.8 mm CUT TERMINATION"
      (at 265.43 62.23 0.0))
    (property "Footprint" "ELFlex:TenNet_WireBank"
      (at 265.43 80.01 0.0)
      (hide yes))
    (instances
      (project "gimbal-static-v0.2"
        (path
          (reference "J3")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (pin "10"))
  (wire
    (pts
      (xy 260.35 69.85)
      (xy 248.92 69.85)))
  (global_label "V24_MOTOR2"
    (shape passive)
    (at 248.92 69.85 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 248.92 69.85 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 260.35 72.39)
      (xy 252.73 72.39)))
  (global_label "GND"
    (shape passive)
    (at 252.73 72.39 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 252.73 72.39 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 260.35 74.93)
      (xy 251.46 74.93)))
  (global_label "CAN_H"
    (shape passive)
    (at 251.46 74.93 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 251.46 74.93 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 260.35 77.47)
      (xy 251.46 77.47)))
  (global_label "CAN_L"
    (shape passive)
    (at 251.46 77.47 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 251.46 77.47 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 260.35 80.01)
      (xy 246.38 80.01)))
  (global_label "SPOT1_LED_PLUS"
    (shape passive)
    (at 246.38 80.01 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 246.38 80.01 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 260.35 82.55)
      (xy 246.38 82.55)))
  (global_label "SPOT1_LED_MINUS"
    (shape passive)
    (at 246.38 82.55 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 246.38 82.55 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 260.35 85.09)
      (xy 246.38 85.09)))
  (global_label "SPOT2_LED_PLUS"
    (shape passive)
    (at 246.38 85.09 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 246.38 85.09 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 260.35 87.63)
      (xy 246.38 87.63)))
  (global_label "SPOT2_LED_MINUS"
    (shape passive)
    (at 246.38 87.63 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 246.38 87.63 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 260.35 90.17)
      (xy 246.38 90.17)))
  (global_label "SPOT3_LED_PLUS"
    (shape passive)
    (at 246.38 90.17 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 246.38 90.17 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 260.35 92.71)
      (xy 246.38 92.71)))
  (global_label "SPOT3_LED_MINUS"
    (shape passive)
    (at 246.38 92.71 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 246.38 92.71 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x10")
    (at 359.41 80.01 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J4"
      (at 359.41 59.69 0.0))
    (property "Value" "76.2 mm CUT TERMINATION"
      (at 359.41 62.23 0.0))
    (property "Footprint" "ELFlex:TenNet_WireBank"
      (at 359.41 80.01 0.0)
      (hide yes))
    (instances
      (project "gimbal-static-v0.2"
        (path
          (reference "J4")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (pin "10"))
  (wire
    (pts
      (xy 354.33 69.85)
      (xy 342.9 69.85)))
  (global_label "V24_MOTOR2"
    (shape passive)
    (at 342.9 69.85 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 342.9 69.85 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 354.33 72.39)
      (xy 346.71 72.39)))
  (global_label "GND"
    (shape passive)
    (at 346.71 72.39 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 346.71 72.39 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 354.33 74.93)
      (xy 345.44 74.93)))
  (global_label "CAN_H"
    (shape passive)
    (at 345.44 74.93 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 345.44 74.93 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 354.33 77.47)
      (xy 345.44 77.47)))
  (global_label "CAN_L"
    (shape passive)
    (at 345.44 77.47 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 345.44 77.47 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 354.33 80.01)
      (xy 340.36 80.01)))
  (global_label "SPOT1_LED_PLUS"
    (shape passive)
    (at 340.36 80.01 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 340.36 80.01 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 354.33 82.55)
      (xy 340.36 82.55)))
  (global_label "SPOT1_LED_MINUS"
    (shape passive)
    (at 340.36 82.55 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 340.36 82.55 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 354.33 85.09)
      (xy 340.36 85.09)))
  (global_label "SPOT2_LED_PLUS"
    (shape passive)
    (at 340.36 85.09 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 340.36 85.09 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 354.33 87.63)
      (xy 340.36 87.63)))
  (global_label "SPOT2_LED_MINUS"
    (shape passive)
    (at 340.36 87.63 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 340.36 87.63 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 354.33 90.17)
      (xy 340.36 90.17)))
  (global_label "SPOT3_LED_PLUS"
    (shape passive)
    (at 340.36 90.17 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 340.36 90.17 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 354.33 92.71)
      (xy 340.36 92.71)))
  (global_label "SPOT3_LED_MINUS"
    (shape passive)
    (at 340.36 92.71 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 340.36 92.71 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x10")
    (at 74.93 180.34 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J5"
      (at 74.93 160.02 0.0))
    (property "Value" "101.6 mm CUT TERMINATION"
      (at 74.93 162.56 0.0))
    (property "Footprint" "ELFlex:TenNet_WireBank"
      (at 74.93 180.34 0.0)
      (hide yes))
    (instances
      (project "gimbal-static-v0.2"
        (path
          (reference "J5")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (pin "10"))
  (wire
    (pts
      (xy 69.85 170.18)
      (xy 58.42 170.18)))
  (global_label "V24_MOTOR2"
    (shape passive)
    (at 58.42 170.18 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 58.42 170.18 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 69.85 172.72)
      (xy 62.23 172.72)))
  (global_label "GND"
    (shape passive)
    (at 62.23 172.72 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 62.23 172.72 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 69.85 175.26)
      (xy 60.96 175.26)))
  (global_label "CAN_H"
    (shape passive)
    (at 60.96 175.26 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 60.96 175.26 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 69.85 177.8)
      (xy 60.96 177.8)))
  (global_label "CAN_L"
    (shape passive)
    (at 60.96 177.8 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 60.96 177.8 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 69.85 180.34)
      (xy 55.88 180.34)))
  (global_label "SPOT1_LED_PLUS"
    (shape passive)
    (at 55.88 180.34 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 55.88 180.34 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 69.85 182.88)
      (xy 55.88 182.88)))
  (global_label "SPOT1_LED_MINUS"
    (shape passive)
    (at 55.88 182.88 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 55.88 182.88 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 69.85 185.42)
      (xy 55.88 185.42)))
  (global_label "SPOT2_LED_PLUS"
    (shape passive)
    (at 55.88 185.42 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 55.88 185.42 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 69.85 187.96)
      (xy 55.88 187.96)))
  (global_label "SPOT2_LED_MINUS"
    (shape passive)
    (at 55.88 187.96 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 55.88 187.96 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 69.85 190.5)
      (xy 55.88 190.5)))
  (global_label "SPOT3_LED_PLUS"
    (shape passive)
    (at 55.88 190.5 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 55.88 190.5 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 69.85 193.04)
      (xy 55.88 193.04)))
  (global_label "SPOT3_LED_MINUS"
    (shape passive)
    (at 55.88 193.04 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 55.88 193.04 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x10")
    (at 170.18 180.34 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J6"
      (at 170.18 160.02 0.0))
    (property "Value" "127 mm CUT TERMINATION"
      (at 170.18 162.56 0.0))
    (property "Footprint" "ELFlex:TenNet_WireBank"
      (at 170.18 180.34 0.0)
      (hide yes))
    (instances
      (project "gimbal-static-v0.2"
        (path
          (reference "J6")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (pin "10"))
  (wire
    (pts
      (xy 165.1 170.18)
      (xy 153.67 170.18)))
  (global_label "V24_MOTOR2"
    (shape passive)
    (at 153.67 170.18 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 153.67 170.18 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 165.1 172.72)
      (xy 157.48 172.72)))
  (global_label "GND"
    (shape passive)
    (at 157.48 172.72 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 157.48 172.72 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 165.1 175.26)
      (xy 156.21 175.26)))
  (global_label "CAN_H"
    (shape passive)
    (at 156.21 175.26 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 156.21 175.26 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 165.1 177.8)
      (xy 156.21 177.8)))
  (global_label "CAN_L"
    (shape passive)
    (at 156.21 177.8 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 156.21 177.8 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 165.1 180.34)
      (xy 151.13 180.34)))
  (global_label "SPOT1_LED_PLUS"
    (shape passive)
    (at 151.13 180.34 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 151.13 180.34 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 165.1 182.88)
      (xy 151.13 182.88)))
  (global_label "SPOT1_LED_MINUS"
    (shape passive)
    (at 151.13 182.88 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 151.13 182.88 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 165.1 185.42)
      (xy 151.13 185.42)))
  (global_label "SPOT2_LED_PLUS"
    (shape passive)
    (at 151.13 185.42 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 151.13 185.42 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 165.1 187.96)
      (xy 151.13 187.96)))
  (global_label "SPOT2_LED_MINUS"
    (shape passive)
    (at 151.13 187.96 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 151.13 187.96 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 165.1 190.5)
      (xy 151.13 190.5)))
  (global_label "SPOT3_LED_PLUS"
    (shape passive)
    (at 151.13 190.5 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 151.13 190.5 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 165.1 193.04)
      (xy 151.13 193.04)))
  (global_label "SPOT3_LED_MINUS"
    (shape passive)
    (at 151.13 193.04 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 151.13 193.04 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x10")
    (at 265.43 180.34 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J7"
      (at 265.43 160.02 0.0))
    (property "Value" "152.4 mm CUT TERMINATION"
      (at 265.43 162.56 0.0))
    (property "Footprint" "ELFlex:TenNet_WireBank"
      (at 265.43 180.34 0.0)
      (hide yes))
    (instances
      (project "gimbal-static-v0.2"
        (path
          (reference "J7")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (pin "10"))
  (wire
    (pts
      (xy 260.35 170.18)
      (xy 248.92 170.18)))
  (global_label "V24_MOTOR2"
    (shape passive)
    (at 248.92 170.18 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 248.92 170.18 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 260.35 172.72)
      (xy 252.73 172.72)))
  (global_label "GND"
    (shape passive)
    (at 252.73 172.72 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 252.73 172.72 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 260.35 175.26)
      (xy 251.46 175.26)))
  (global_label "CAN_H"
    (shape passive)
    (at 251.46 175.26 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 251.46 175.26 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 260.35 177.8)
      (xy 251.46 177.8)))
  (global_label "CAN_L"
    (shape passive)
    (at 251.46 177.8 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 251.46 177.8 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 260.35 180.34)
      (xy 246.38 180.34)))
  (global_label "SPOT1_LED_PLUS"
    (shape passive)
    (at 246.38 180.34 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 246.38 180.34 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 260.35 182.88)
      (xy 246.38 182.88)))
  (global_label "SPOT1_LED_MINUS"
    (shape passive)
    (at 246.38 182.88 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 246.38 182.88 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 260.35 185.42)
      (xy 246.38 185.42)))
  (global_label "SPOT2_LED_PLUS"
    (shape passive)
    (at 246.38 185.42 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 246.38 185.42 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 260.35 187.96)
      (xy 246.38 187.96)))
  (global_label "SPOT2_LED_MINUS"
    (shape passive)
    (at 246.38 187.96 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 246.38 187.96 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 260.35 190.5)
      (xy 246.38 190.5)))
  (global_label "SPOT3_LED_PLUS"
    (shape passive)
    (at 246.38 190.5 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 246.38 190.5 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 260.35 193.04)
      (xy 246.38 193.04)))
  (global_label "SPOT3_LED_MINUS"
    (shape passive)
    (at 246.38 193.04 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 246.38 193.04 0.0)
      (hide yes)))
  (text "STATIC ARM INTERCONNECT. Joint motion uses ordinary end wires.\nRetain J1. Cut only at 25.4 / 50.8 / 76.2 / 101.6 / 127.0 / 152.4 mm marks.\nTen separate nets at every row. Motor return and three spotlight returns are not interchangeable.\nPhysical single copper layer: F.Cu only. KiCad B.Cu is an empty editor layer, not a fabricated copper layer."
    (at 30.0 235.0 0)))
