(kicad_pcb
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(general
		(thickness 0.15)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting
			(front yes)
			(back yes)
		)
		(covering
			(front no)
			(back no)
		)
		(plugging
			(front no)
			(back no)
		)
		(capping no)
		(filling no)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12)
			(dashed_line_gap_ratio 3)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(footprint "ELFlex:J32_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J32"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z3 S2 BOTTOM"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 286.924385 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z3_B12_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 288.956643 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z3_B12_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 294.545353 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z3_B12_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 296.577611 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z3_B12_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J21_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J21"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z2 S1 BOTTOM"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 218.889269 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z2_B12_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 220.921527 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z2_B12_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 226.510237 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z2_B12_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 228.542495 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z2_B12_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J62_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J62"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z6 S2 BOTTOM"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 123.640107 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z6_B12_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 125.672365 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z6_B12_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 131.261075 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z6_B12_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 133.293333 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z6_B12_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J41_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J41"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z4 S1 BOTTOM"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 1.176898 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z4_B12_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 3.209156 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z4_B12_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 8.797866 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z4_B12_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 10.830124 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z4_B12_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J31_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J31"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z3 S1 BOTTOM"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 273.317362 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z3_B12_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 275.34962 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z3_B12_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 280.93833 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z3_B12_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 282.970588 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z3_B12_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J44_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J44"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z4 S4 BOTTOM"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 41.997968 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z4_B34_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 44.030226 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z4_B34_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 49.618935 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z4_B34_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 51.651194 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z4_B34_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J61_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J61"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z6 S1 BOTTOM"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 110.033084 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z6_B12_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 112.065342 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z6_B12_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 117.654051 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z6_B12_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 119.686309 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z6_B12_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J64_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J64"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z6 S4 BOTTOM"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 150.854153 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z6_B34_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 152.886411 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z6_B34_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 158.475121 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z6_B34_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 160.507379 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z6_B34_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J43_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J43"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z4 S3 BOTTOM"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 28.390945 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z4_B34_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 30.423203 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z4_B34_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 36.011912 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z4_B34_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 38.04417 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z4_B34_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J51_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J51"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z5 S1 BOTTOM"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 55.604991 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z5_B12_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 57.637249 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z5_B12_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 63.225959 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z5_B12_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 65.258217 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z5_B12_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J23_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J23"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z2 S3 BOTTOM"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 246.103315 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z2_B34_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 248.135574 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z2_B34_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 253.724283 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z2_B34_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 255.756541 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z2_B34_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J42_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J42"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z4 S2 BOTTOM"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 14.783921 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z4_B12_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 16.816179 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z4_B12_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 22.404889 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z4_B12_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 24.437147 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z4_B12_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J33_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J33"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z3 S3 BOTTOM"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 300.531408 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z3_B34_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 302.563666 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z3_B34_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 308.152376 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z3_B34_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 310.184634 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z3_B34_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J34_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J34"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z3 S4 BOTTOM"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 314.138431 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z3_B34_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 316.170689 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z3_B34_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 321.759399 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z3_B34_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 323.791657 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z3_B34_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J22_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J22"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z2 S2 BOTTOM"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 232.496292 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z2_B12_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 234.52855 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z2_B12_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 240.11726 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z2_B12_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 242.149518 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z2_B12_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J54_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J54"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z5 S4 BOTTOM"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 96.42606 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z5_B34_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 98.458319 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z5_B34_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 104.047028 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z5_B34_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 106.079286 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z5_B34_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J63_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J63"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z6 S3 BOTTOM"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 137.24713 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z6_B34_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 139.279388 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z6_B34_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 144.868098 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z6_B34_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 146.900356 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z6_B34_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J24_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J24"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z2 S4 BOTTOM"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 259.710339 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z2_B34_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 261.742597 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z2_B34_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 267.331306 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z2_B34_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 269.363564 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z2_B34_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J13_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J13"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z1 S3 BOTTOM"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 191.675223 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z1_B34_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 193.707481 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z1_B34_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 199.29619 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z1_B34_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 201.328449 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z1_B34_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J52_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J52"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z5 S2 BOTTOM"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 69.212014 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z5_B12_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 71.244272 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z5_B12_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 76.832982 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z5_B12_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 78.86524 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z5_B12_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J53_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J53"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z5 S3 BOTTOM"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 82.819037 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z5_B34_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 84.851295 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z5_B34_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 90.440005 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z5_B34_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 92.472263 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z5_B34_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J14_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J14"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z1 S4 BOTTOM"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 205.282246 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z1_B34_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 207.314504 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z1_B34_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 212.903214 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z1_B34_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 214.935472 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z1_B34_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J11_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J11"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z1 S1 BOTTOM"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 164.461176 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z1_B12_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 166.493434 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z1_B12_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 172.082144 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z1_B12_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 174.114402 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z1_B12_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J12_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J12"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z1 S2 BOTTOM"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 178.0682 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z1_B12_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 180.100458 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z1_B12_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 185.689167 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z1_B12_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 187.721425 -0.799999)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z1_B12_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(gr_line
		(start 20 40.15)
		(end 20 46.25)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 20 40.15)
		(mid 20.043934 40.043934)
		(end 20.15 40)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 20.15 46.4)
		(mid 20.043934 46.356066)
		(end 20 46.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 20.15 46.4)
		(end 344.818556 46.4)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 20.326898 40)
		(end 20.15 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 20.476898 38.65)
		(end 20.476898 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 20.476898 38.65)
		(mid 20.520832 38.543933)
		(end 20.626898 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 20.476898 39.85)
		(mid 20.432964 39.956066)
		(end 20.326898 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 21.726898 38.5)
		(end 20.626898 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 21.726898 38.5)
		(mid 21.832965 38.543933)
		(end 21.876898 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 21.876898 39.85)
		(end 21.876898 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 22.026898 40)
		(mid 21.920832 39.956066)
		(end 21.876898 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 22.359156 40)
		(end 22.026898 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 22.509156 38.65)
		(end 22.509156 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 22.509156 38.65)
		(mid 22.553087 38.543918)
		(end 22.659156 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 22.509156 39.85)
		(mid 22.465222 39.956066)
		(end 22.359156 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 23.759156 38.5)
		(end 22.659156 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 23.759156 38.5)
		(mid 23.86525 38.543918)
		(end 23.909156 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 23.909156 39.85)
		(end 23.909156 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 24.059156 40)
		(mid 23.95309 39.956066)
		(end 23.909156 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 27.947866 40)
		(end 24.059156 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 28.097866 38.65)
		(end 28.097866 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 28.097866 38.65)
		(mid 28.141798 38.543922)
		(end 28.247866 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 28.097866 39.85)
		(mid 28.053932 39.956066)
		(end 27.947866 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 29.347866 38.5)
		(end 28.247866 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 29.347866 38.5)
		(mid 29.453954 38.543922)
		(end 29.497866 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 29.497866 39.85)
		(end 29.497866 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 29.647866 40)
		(mid 29.5418 39.956066)
		(end 29.497866 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 29.980124 40)
		(end 29.647866 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 30.130124 38.65)
		(end 30.130124 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 30.130124 38.65)
		(mid 30.174059 38.543942)
		(end 30.280124 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 30.130124 39.85)
		(mid 30.08619 39.956066)
		(end 29.980124 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 31.380124 38.5)
		(end 30.280124 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 31.380124 38.5)
		(mid 31.486175 38.543942)
		(end 31.530124 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 31.530124 39.85)
		(end 31.530124 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 31.680124 40)
		(mid 31.574058 39.956066)
		(end 31.530124 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 33.933921 40)
		(end 31.680124 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 34.083921 38.65)
		(end 34.083921 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 34.083921 38.65)
		(mid 34.127856 38.543941)
		(end 34.233921 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 34.083921 39.85)
		(mid 34.039987 39.956066)
		(end 33.933921 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 35.333921 38.5)
		(end 34.233921 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 35.333921 38.5)
		(mid 35.439973 38.543941)
		(end 35.483921 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 35.483921 39.85)
		(end 35.483921 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 35.633921 40)
		(mid 35.527855 39.956066)
		(end 35.483921 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 35.966179 40)
		(end 35.633921 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 36.116179 38.65)
		(end 36.116179 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 36.116179 38.65)
		(mid 36.160112 38.543927)
		(end 36.266179 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 36.116179 39.85)
		(mid 36.072245 39.956066)
		(end 35.966179 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 37.366179 38.5)
		(end 36.266179 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 37.366179 38.5)
		(mid 37.472259 38.543927)
		(end 37.516179 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 37.516179 39.85)
		(end 37.516179 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 37.666179 40)
		(mid 37.560113 39.956066)
		(end 37.516179 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 41.554889 40)
		(end 37.666179 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 41.704889 38.65)
		(end 41.704889 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 41.704889 38.65)
		(mid 41.748822 38.54393)
		(end 41.854889 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 41.704889 39.85)
		(mid 41.660955 39.956066)
		(end 41.554889 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 42.954889 38.5)
		(end 41.854889 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 42.954889 38.5)
		(mid 43.060962 38.54393)
		(end 43.104889 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 43.104889 39.85)
		(end 43.104889 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 43.254889 40)
		(mid 43.148823 39.956066)
		(end 43.104889 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 43.587147 40)
		(end 43.254889 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 43.737147 38.65)
		(end 43.737147 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 43.737147 38.65)
		(mid 43.781084 38.543951)
		(end 43.887147 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 43.737147 39.85)
		(mid 43.693213 39.956066)
		(end 43.587147 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 44.987147 38.5)
		(end 43.887147 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 44.987147 38.5)
		(mid 45.093183 38.543951)
		(end 45.137147 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 45.137147 39.85)
		(end 45.137147 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 45.287147 40)
		(mid 45.181081 39.956066)
		(end 45.137147 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 47.540945 40)
		(end 45.287147 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 47.690945 38.65)
		(end 47.690945 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 47.690945 38.65)
		(mid 47.734882 38.54395)
		(end 47.840945 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 47.690945 39.85)
		(mid 47.647011 39.956066)
		(end 47.540945 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 48.940945 38.5)
		(end 47.840945 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 48.940945 38.5)
		(mid 49.046982 38.54395)
		(end 49.090945 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 49.090945 39.85)
		(end 49.090945 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 49.240945 40)
		(mid 49.134879 39.956066)
		(end 49.090945 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 49.573203 40)
		(end 49.240945 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 49.723203 38.65)
		(end 49.723203 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 49.723203 38.65)
		(mid 49.767137 38.543935)
		(end 49.873203 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 49.723203 39.85)
		(mid 49.679269 39.956066)
		(end 49.573203 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 50.973203 38.5)
		(end 49.873203 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 50.973203 38.5)
		(mid 51.079267 38.543935)
		(end 51.123203 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 51.123203 39.85)
		(end 51.123203 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 51.273203 40)
		(mid 51.167137 39.956066)
		(end 51.123203 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 55.161912 40)
		(end 51.273203 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 55.311912 38.65)
		(end 55.311912 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 55.311912 38.65)
		(mid 55.355847 38.543938)
		(end 55.461912 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 55.311912 39.85)
		(mid 55.267978 39.956066)
		(end 55.161912 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 56.561912 38.5)
		(end 55.461912 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 56.561912 38.5)
		(mid 56.66797 38.543938)
		(end 56.711912 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 56.711912 39.85)
		(end 56.711912 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 56.861912 40)
		(mid 56.755846 39.956066)
		(end 56.711912 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 57.19417 40)
		(end 56.861912 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 57.34417 38.65)
		(end 57.34417 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 57.34417 38.65)
		(mid 57.388102 38.543923)
		(end 57.49417 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 57.34417 39.85)
		(mid 57.300236 39.956066)
		(end 57.19417 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 58.59417 38.5)
		(end 57.49417 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 58.59417 38.5)
		(mid 58.700255 38.543923)
		(end 58.74417 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 58.74417 39.85)
		(end 58.74417 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 58.89417 40)
		(mid 58.788104 39.956066)
		(end 58.74417 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 61.147968 40)
		(end 58.89417 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 61.297968 38.65)
		(end 61.297968 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 61.297968 38.65)
		(mid 61.3419 38.543923)
		(end 61.447968 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 61.297968 39.85)
		(mid 61.254034 39.956066)
		(end 61.147968 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 62.547968 38.5)
		(end 61.447968 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 62.547968 38.5)
		(mid 62.654055 38.543923)
		(end 62.697968 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 62.697968 39.85)
		(end 62.697968 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 62.847968 40)
		(mid 62.741902 39.956066)
		(end 62.697968 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 63.180226 40)
		(end 62.847968 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 63.330226 38.65)
		(end 63.330226 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 63.330226 38.65)
		(mid 63.374162 38.543943)
		(end 63.480226 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 63.330226 39.85)
		(mid 63.286292 39.956066)
		(end 63.180226 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 64.580226 38.5)
		(end 63.480226 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 64.580226 38.5)
		(mid 64.686275 38.543943)
		(end 64.730226 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 64.730226 39.85)
		(end 64.730226 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 64.880226 40)
		(mid 64.77416 39.956066)
		(end 64.730226 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 68.768935 40)
		(end 64.880226 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 68.918935 38.65)
		(end 68.918935 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 68.918935 38.65)
		(mid 68.962871 38.543946)
		(end 69.068935 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 68.918935 39.85)
		(mid 68.875001 39.956066)
		(end 68.768935 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 70.168935 38.5)
		(end 69.068935 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 70.168935 38.5)
		(mid 70.274978 38.543946)
		(end 70.318935 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 70.318935 39.85)
		(end 70.318935 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 70.468935 40)
		(mid 70.362869 39.956066)
		(end 70.318935 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 70.801194 40)
		(end 70.468935 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 70.951194 38.65)
		(end 70.951194 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 70.951194 38.65)
		(mid 70.995128 38.543932)
		(end 71.101194 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 70.951194 39.85)
		(mid 70.90726 39.956066)
		(end 70.801194 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 72.201194 38.5)
		(end 71.101194 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 72.201194 38.5)
		(mid 72.307264 38.543932)
		(end 72.351194 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 72.351194 39.85)
		(end 72.351194 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 72.501194 40)
		(mid 72.395128 39.956066)
		(end 72.351194 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 74.754991 40)
		(end 72.501194 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 74.904991 38.65)
		(end 74.904991 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 74.904991 38.65)
		(mid 74.948924 38.543931)
		(end 75.054991 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 74.904991 39.85)
		(mid 74.861057 39.956066)
		(end 74.754991 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 76.154991 38.5)
		(end 75.054991 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 76.154991 38.5)
		(mid 76.261063 38.543931)
		(end 76.304991 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 76.304991 39.85)
		(end 76.304991 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 76.454991 40)
		(mid 76.348925 39.956066)
		(end 76.304991 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 76.787249 40)
		(end 76.454991 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 76.937249 38.65)
		(end 76.937249 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 76.937249 38.65)
		(mid 76.981186 38.543951)
		(end 77.087249 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 76.937249 39.85)
		(mid 76.893315 39.956066)
		(end 76.787249 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 78.187249 38.5)
		(end 77.087249 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 78.187249 38.5)
		(mid 78.293348 38.543916)
		(end 78.337249 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 78.337249 39.85)
		(end 78.337249 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 78.487249 40)
		(mid 78.381183 39.956066)
		(end 78.337249 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.375959 40)
		(end 78.487249 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.525959 38.65)
		(end 82.525959 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 82.525959 38.65)
		(mid 82.56989 38.543919)
		(end 82.675959 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 82.525959 39.85)
		(mid 82.482025 39.956066)
		(end 82.375959 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 83.775959 38.5)
		(end 82.675959 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 83.775959 38.5)
		(mid 83.882052 38.543919)
		(end 83.925959 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 83.925959 39.85)
		(end 83.925959 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 84.075959 40)
		(mid 83.969893 39.956066)
		(end 83.925959 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 84.408217 40)
		(end 84.075959 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 84.558217 38.65)
		(end 84.558217 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 84.558217 38.65)
		(mid 84.602152 38.54394)
		(end 84.708217 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 84.558217 39.85)
		(mid 84.514283 39.956066)
		(end 84.408217 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 85.808217 38.5)
		(end 84.708217 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 85.808217 38.5)
		(mid 85.914272 38.54394)
		(end 85.958217 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 85.958217 39.85)
		(end 85.958217 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 86.108217 40)
		(mid 86.002151 39.956066)
		(end 85.958217 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 88.362014 40)
		(end 86.108217 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 88.512014 38.65)
		(end 88.512014 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 88.512014 38.65)
		(mid 88.555949 38.543939)
		(end 88.662014 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 88.512014 39.85)
		(mid 88.46808 39.956066)
		(end 88.362014 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 89.762014 38.5)
		(end 88.662014 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 89.762014 38.5)
		(mid 89.868071 38.543939)
		(end 89.912014 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 89.912014 39.85)
		(end 89.912014 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 90.062014 40)
		(mid 89.955948 39.956066)
		(end 89.912014 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 90.394272 40)
		(end 90.062014 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 90.544272 38.65)
		(end 90.544272 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 90.544272 38.65)
		(mid 90.588204 38.543924)
		(end 90.694272 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 90.544272 39.85)
		(mid 90.500338 39.956066)
		(end 90.394272 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 91.794272 38.5)
		(end 90.694272 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 91.794272 38.5)
		(mid 91.900356 38.543924)
		(end 91.944272 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 91.944272 39.85)
		(end 91.944272 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 92.094272 40)
		(mid 91.988206 39.956066)
		(end 91.944272 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 95.982982 40)
		(end 92.094272 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 96.132982 38.65)
		(end 96.132982 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 96.132982 38.65)
		(mid 96.176915 38.543928)
		(end 96.282982 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 96.132982 39.85)
		(mid 96.089048 39.956066)
		(end 95.982982 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.382982 38.5)
		(end 96.282982 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 97.382982 38.5)
		(mid 97.48906 38.543928)
		(end 97.532982 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.532982 39.85)
		(end 97.532982 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 97.682982 40)
		(mid 97.576916 39.956066)
		(end 97.532982 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.01524 40)
		(end 97.682982 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.16524 38.65)
		(end 98.16524 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 98.16524 38.65)
		(mid 98.209176 38.543948)
		(end 98.31524 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 98.16524 39.85)
		(mid 98.121306 39.956066)
		(end 98.01524 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 99.41524 38.5)
		(end 98.31524 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 99.41524 38.5)
		(mid 99.52128 38.543948)
		(end 99.56524 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 99.56524 39.85)
		(end 99.56524 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 99.71524 40)
		(mid 99.609174 39.956066)
		(end 99.56524 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 101.969037 40)
		(end 99.71524 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 102.119037 38.65)
		(end 102.119037 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 102.119037 38.65)
		(mid 102.162973 38.543947)
		(end 102.269037 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 102.119037 39.85)
		(mid 102.075103 39.956066)
		(end 101.969037 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 103.369037 38.5)
		(end 102.269037 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 103.369037 38.5)
		(mid 103.475079 38.543947)
		(end 103.519037 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 103.519037 39.85)
		(end 103.519037 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 103.669037 40)
		(mid 103.562971 39.956066)
		(end 103.519037 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 104.001295 40)
		(end 103.669037 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 104.151295 38.65)
		(end 104.151295 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 104.151295 38.65)
		(mid 104.195229 38.543932)
		(end 104.301295 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 104.151295 39.85)
		(mid 104.107361 39.956066)
		(end 104.001295 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 105.401295 38.5)
		(end 104.301295 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 105.401295 38.5)
		(mid 105.507364 38.543932)
		(end 105.551295 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 105.551295 39.85)
		(end 105.551295 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 105.701295 40)
		(mid 105.595229 39.956066)
		(end 105.551295 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 109.590005 40)
		(end 105.701295 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 109.740005 38.65)
		(end 109.740005 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 109.740005 38.65)
		(mid 109.783939 38.543936)
		(end 109.890005 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 109.740005 39.85)
		(mid 109.696071 39.956066)
		(end 109.590005 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 110.990005 38.5)
		(end 109.890005 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 110.990005 38.5)
		(mid 111.096068 38.543936)
		(end 111.140005 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.140005 39.85)
		(end 111.140005 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 111.290005 40)
		(mid 111.183939 39.956066)
		(end 111.140005 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.622263 40)
		(end 111.290005 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.772263 38.65)
		(end 111.772263 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 111.772263 38.65)
		(mid 111.816195 38.543921)
		(end 111.922263 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 111.772263 39.85)
		(mid 111.728329 39.956066)
		(end 111.622263 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 113.022263 38.5)
		(end 111.922263 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 113.022263 38.5)
		(mid 113.128353 38.543921)
		(end 113.172263 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 113.172263 39.85)
		(end 113.172263 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 113.322263 40)
		(mid 113.216197 39.956066)
		(end 113.172263 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 115.57606 40)
		(end 113.322263 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 115.72606 38.65)
		(end 115.72606 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 115.72606 38.65)
		(mid 115.769992 38.54392)
		(end 115.87606 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 115.72606 39.85)
		(mid 115.682126 39.956066)
		(end 115.57606 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 116.97606 38.5)
		(end 115.87606 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 116.97606 38.5)
		(mid 117.082152 38.54392)
		(end 117.12606 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 117.12606 39.85)
		(end 117.12606 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 117.27606 40)
		(mid 117.169994 39.956066)
		(end 117.12606 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 117.608319 40)
		(end 117.27606 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 117.758319 38.65)
		(end 117.758319 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 117.758319 38.65)
		(mid 117.802254 38.543941)
		(end 117.908319 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 117.758319 39.85)
		(mid 117.714385 39.956066)
		(end 117.608319 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 119.008319 38.5)
		(end 117.908319 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 119.008319 38.5)
		(mid 119.114373 38.543941)
		(end 119.158319 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 119.158319 39.85)
		(end 119.158319 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 119.308319 40)
		(mid 119.202253 39.956066)
		(end 119.158319 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.197028 40)
		(end 119.308319 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.347028 38.65)
		(end 123.347028 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 123.347028 38.65)
		(mid 123.390964 38.543944)
		(end 123.497028 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 123.347028 39.85)
		(mid 123.303094 39.956066)
		(end 123.197028 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 124.597028 38.5)
		(end 123.497028 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 124.597028 38.5)
		(mid 124.703076 38.543944)
		(end 124.747028 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 124.747028 39.85)
		(end 124.747028 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 124.897028 40)
		(mid 124.790962 39.956066)
		(end 124.747028 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 125.229286 40)
		(end 124.897028 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 125.379286 38.65)
		(end 125.379286 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 125.379286 38.65)
		(mid 125.423219 38.543929)
		(end 125.529286 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 125.379286 39.85)
		(mid 125.335352 39.956066)
		(end 125.229286 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 126.629286 38.5)
		(end 125.529286 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 126.629286 38.5)
		(mid 126.735361 38.543929)
		(end 126.779286 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 126.779286 39.85)
		(end 126.779286 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 126.929286 40)
		(mid 126.82322 39.956066)
		(end 126.779286 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 129.183084 40)
		(end 126.929286 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 129.333084 38.65)
		(end 129.333084 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 129.333084 38.65)
		(mid 129.377017 38.543928)
		(end 129.483084 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 129.333084 39.85)
		(mid 129.28915 39.956066)
		(end 129.183084 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 130.583084 38.5)
		(end 129.483084 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 130.583084 38.5)
		(mid 130.68916 38.543928)
		(end 130.733084 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 130.733084 39.85)
		(end 130.733084 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 130.883084 40)
		(mid 130.777018 39.956066)
		(end 130.733084 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 131.215342 40)
		(end 130.883084 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 131.365342 38.65)
		(end 131.365342 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 131.365342 38.65)
		(mid 131.409279 38.543949)
		(end 131.515342 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 131.365342 39.85)
		(mid 131.321408 39.956066)
		(end 131.215342 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 132.615342 38.5)
		(end 131.515342 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 132.615342 38.5)
		(mid 132.721381 38.543949)
		(end 132.765342 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 132.765342 39.85)
		(end 132.765342 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 132.915342 40)
		(mid 132.809276 39.956066)
		(end 132.765342 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 136.804051 40)
		(end 132.915342 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 136.954051 38.65)
		(end 136.954051 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 136.954051 38.65)
		(mid 136.997988 38.543952)
		(end 137.104051 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 136.954051 39.85)
		(mid 136.910117 39.956066)
		(end 136.804051 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.204051 38.5)
		(end 137.104051 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 138.204051 38.5)
		(mid 138.310149 38.543917)
		(end 138.354051 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.354051 39.85)
		(end 138.354051 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 138.504051 40)
		(mid 138.397985 39.956066)
		(end 138.354051 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.836309 40)
		(end 138.504051 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.986309 38.65)
		(end 138.986309 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 138.986309 38.65)
		(mid 139.030244 38.543937)
		(end 139.136309 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 138.986309 39.85)
		(mid 138.942375 39.956066)
		(end 138.836309 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 140.236309 38.5)
		(end 139.136309 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 140.236309 38.5)
		(mid 140.342369 38.543937)
		(end 140.386309 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 140.386309 39.85)
		(end 140.386309 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 140.536309 40)
		(mid 140.430243 39.956066)
		(end 140.386309 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.790107 40)
		(end 140.536309 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.940107 38.65)
		(end 142.940107 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 142.940107 38.65)
		(mid 142.984041 38.543936)
		(end 143.090107 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 142.940107 39.85)
		(mid 142.896173 39.956066)
		(end 142.790107 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.190107 38.5)
		(end 143.090107 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 144.190107 38.5)
		(mid 144.296168 38.543936)
		(end 144.340107 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.340107 39.85)
		(end 144.340107 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 144.490107 40)
		(mid 144.384041 39.956066)
		(end 144.340107 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.822365 40)
		(end 144.490107 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.972365 38.65)
		(end 144.972365 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 144.972365 38.65)
		(mid 145.016297 38.543922)
		(end 145.122365 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 144.972365 39.85)
		(mid 144.928431 39.956066)
		(end 144.822365 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 146.222365 38.5)
		(end 145.122365 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 146.222365 38.5)
		(mid 146.328454 38.543922)
		(end 146.372365 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 146.372365 39.85)
		(end 146.372365 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 146.522365 40)
		(mid 146.416299 39.956066)
		(end 146.372365 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150.411075 40)
		(end 146.522365 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150.561075 38.65)
		(end 150.561075 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 150.561075 38.65)
		(mid 150.605007 38.543925)
		(end 150.711075 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 150.561075 39.85)
		(mid 150.517141 39.956066)
		(end 150.411075 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 151.811075 38.5)
		(end 150.711075 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 151.811075 38.5)
		(mid 151.917157 38.543925)
		(end 151.961075 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 151.961075 39.85)
		(end 151.961075 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 152.111075 40)
		(mid 152.005009 39.956066)
		(end 151.961075 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 152.443333 40)
		(end 152.111075 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 152.593333 38.65)
		(end 152.593333 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 152.593333 38.65)
		(mid 152.637269 38.543946)
		(end 152.743333 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 152.593333 39.85)
		(mid 152.549399 39.956066)
		(end 152.443333 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.843333 38.5)
		(end 152.743333 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 153.843333 38.5)
		(mid 153.949378 38.543946)
		(end 153.993333 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.993333 39.85)
		(end 153.993333 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 154.143333 40)
		(mid 154.037267 39.956066)
		(end 153.993333 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 156.39713 40)
		(end 154.143333 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 156.54713 38.65)
		(end 156.54713 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 156.54713 38.65)
		(mid 156.591066 38.543945)
		(end 156.69713 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 156.54713 39.85)
		(mid 156.503196 39.956066)
		(end 156.39713 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.79713 38.5)
		(end 156.69713 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 157.79713 38.5)
		(mid 157.903177 38.543945)
		(end 157.94713 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.94713 39.85)
		(end 157.94713 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 158.09713 40)
		(mid 157.991064 39.956066)
		(end 157.94713 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.429388 40)
		(end 158.09713 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.579388 38.65)
		(end 158.579388 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 158.579388 38.65)
		(mid 158.623321 38.54393)
		(end 158.729388 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 158.579388 39.85)
		(mid 158.535454 39.956066)
		(end 158.429388 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 159.829388 38.5)
		(end 158.729388 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 159.829388 38.5)
		(mid 159.935462 38.54393)
		(end 159.979388 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 159.979388 39.85)
		(end 159.979388 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 160.129388 40)
		(mid 160.023322 39.956066)
		(end 159.979388 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 164.018098 40)
		(end 160.129388 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 164.168098 38.65)
		(end 164.168098 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 164.168098 38.65)
		(mid 164.212032 38.543933)
		(end 164.318098 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 164.168098 39.85)
		(mid 164.124164 39.956066)
		(end 164.018098 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 165.418098 38.5)
		(end 164.318098 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 165.418098 38.5)
		(mid 165.524165 38.543933)
		(end 165.568098 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 165.568098 39.85)
		(end 165.568098 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 165.718098 40)
		(mid 165.612032 39.956066)
		(end 165.568098 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 166.050356 40)
		(end 165.718098 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 166.200356 38.65)
		(end 166.200356 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 166.200356 38.65)
		(mid 166.244287 38.543918)
		(end 166.350356 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 166.200356 39.85)
		(mid 166.156422 39.956066)
		(end 166.050356 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.450356 38.5)
		(end 166.350356 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 167.450356 38.5)
		(mid 167.55645 38.543918)
		(end 167.600356 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.600356 39.85)
		(end 167.600356 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 167.750356 40)
		(mid 167.64429 39.956066)
		(end 167.600356 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.004153 40)
		(end 167.750356 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.154153 38.65)
		(end 170.154153 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 170.154153 38.65)
		(mid 170.198084 38.543917)
		(end 170.304153 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 170.154153 39.85)
		(mid 170.110219 39.956066)
		(end 170.004153 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 171.404153 38.5)
		(end 170.304153 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 171.404153 38.5)
		(mid 171.510249 38.543917)
		(end 171.554153 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 171.554153 39.85)
		(end 171.554153 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 171.704153 40)
		(mid 171.598087 39.956066)
		(end 171.554153 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.036411 40)
		(end 171.704153 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.186411 38.65)
		(end 172.186411 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 172.186411 38.65)
		(mid 172.230346 38.543938)
		(end 172.336411 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 172.186411 39.85)
		(mid 172.142477 39.956066)
		(end 172.036411 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.436411 38.5)
		(end 172.336411 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 173.436411 38.5)
		(mid 173.54247 38.543938)
		(end 173.586411 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.586411 39.85)
		(end 173.586411 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 173.736411 40)
		(mid 173.630345 39.956066)
		(end 173.586411 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.625121 40)
		(end 173.736411 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.775121 38.65)
		(end 177.775121 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 177.775121 38.65)
		(mid 177.819056 38.543941)
		(end 177.925121 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 177.775121 39.85)
		(mid 177.731187 39.956066)
		(end 177.625121 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 179.025121 38.5)
		(end 177.925121 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 179.025121 38.5)
		(mid 179.131173 38.543941)
		(end 179.175121 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 179.175121 39.85)
		(end 179.175121 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 179.325121 40)
		(mid 179.219055 39.956066)
		(end 179.175121 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 179.657379 40)
		(end 179.325121 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 179.807379 38.65)
		(end 179.807379 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 179.807379 38.65)
		(mid 179.851312 38.543927)
		(end 179.957379 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 179.807379 39.85)
		(mid 179.763445 39.956066)
		(end 179.657379 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 181.057379 38.5)
		(end 179.957379 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 181.057379 38.5)
		(mid 181.163459 38.543927)
		(end 181.207379 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 181.207379 39.85)
		(end 181.207379 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 181.357379 40)
		(mid 181.251313 39.956066)
		(end 181.207379 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 183.611176 40)
		(end 181.357379 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 183.761176 38.65)
		(end 183.761176 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 183.761176 38.65)
		(mid 183.805109 38.543925)
		(end 183.911176 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 183.761176 39.85)
		(mid 183.717242 39.956066)
		(end 183.611176 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.011176 38.5)
		(end 183.911176 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 185.011176 38.5)
		(mid 185.117258 38.543925)
		(end 185.161176 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.161176 39.85)
		(end 185.161176 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 185.311176 40)
		(mid 185.20511 39.956066)
		(end 185.161176 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.643434 40)
		(end 185.311176 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.793434 38.65)
		(end 185.793434 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 185.793434 38.65)
		(mid 185.83737 38.543946)
		(end 185.943434 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 185.793434 39.85)
		(mid 185.7495 39.956066)
		(end 185.643434 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 187.043434 38.5)
		(end 185.943434 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 187.043434 38.5)
		(mid 187.149478 38.543946)
		(end 187.193434 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 187.193434 39.85)
		(end 187.193434 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 187.343434 40)
		(mid 187.237368 39.956066)
		(end 187.193434 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 191.232144 40)
		(end 187.343434 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 191.382144 38.65)
		(end 191.382144 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 191.382144 38.65)
		(mid 191.426081 38.54395)
		(end 191.532144 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 191.382144 39.85)
		(mid 191.33821 39.956066)
		(end 191.232144 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.632144 38.5)
		(end 191.532144 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 192.632144 38.5)
		(mid 192.738182 38.54395)
		(end 192.782144 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.782144 39.85)
		(end 192.782144 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 192.932144 40)
		(mid 192.826078 39.956066)
		(end 192.782144 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 193.264402 40)
		(end 192.932144 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 193.414402 38.65)
		(end 193.414402 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 193.414402 38.65)
		(mid 193.458336 38.543935)
		(end 193.564402 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 193.414402 39.85)
		(mid 193.370468 39.956066)
		(end 193.264402 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 194.664402 38.5)
		(end 193.564402 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 194.664402 38.5)
		(mid 194.770467 38.543935)
		(end 194.814402 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 194.814402 39.85)
		(end 194.814402 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 194.964402 40)
		(mid 194.858336 39.956066)
		(end 194.814402 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 197.2182 40)
		(end 194.964402 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 197.3682 38.65)
		(end 197.3682 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 197.3682 38.65)
		(mid 197.412134 38.543934)
		(end 197.5182 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 197.3682 39.85)
		(mid 197.324266 39.956066)
		(end 197.2182 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.6182 38.5)
		(end 197.5182 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 198.6182 38.5)
		(mid 198.724266 38.543934)
		(end 198.7682 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.7682 39.85)
		(end 198.7682 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 198.9182 40)
		(mid 198.812134 39.956066)
		(end 198.7682 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.250458 40)
		(end 198.9182 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.400458 38.65)
		(end 199.400458 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 199.400458 38.65)
		(mid 199.444389 38.543919)
		(end 199.550458 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 199.400458 39.85)
		(mid 199.356524 39.956066)
		(end 199.250458 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 200.650458 38.5)
		(end 199.550458 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 200.650458 38.5)
		(mid 200.756551 38.543919)
		(end 200.800458 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 200.800458 39.85)
		(end 200.800458 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 200.950458 40)
		(mid 200.844392 39.956066)
		(end 200.800458 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 204.839167 40)
		(end 200.950458 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 204.989167 38.65)
		(end 204.989167 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 204.989167 38.65)
		(mid 205.033099 38.543922)
		(end 205.139167 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 204.989167 39.85)
		(mid 204.945233 39.956066)
		(end 204.839167 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 206.239167 38.5)
		(end 205.139167 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 206.239167 38.5)
		(mid 206.345254 38.543922)
		(end 206.389167 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 206.389167 39.85)
		(end 206.389167 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 206.539167 40)
		(mid 206.433101 39.956066)
		(end 206.389167 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 206.871425 40)
		(end 206.539167 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 207.021425 38.65)
		(end 207.021425 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 207.021425 38.65)
		(mid 207.06536 38.543943)
		(end 207.171425 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 207.021425 39.85)
		(mid 206.977491 39.956066)
		(end 206.871425 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 208.271425 38.5)
		(end 207.171425 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 208.271425 38.5)
		(mid 208.377475 38.543943)
		(end 208.421425 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 208.421425 39.85)
		(end 208.421425 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 208.571425 40)
		(mid 208.465359 39.956066)
		(end 208.421425 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 210.825223 40)
		(end 208.571425 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 210.975223 38.65)
		(end 210.975223 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 210.975223 38.65)
		(mid 211.019158 38.543942)
		(end 211.125223 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 210.975223 39.85)
		(mid 210.931289 39.956066)
		(end 210.825223 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 212.225223 38.5)
		(end 211.125223 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 212.225223 38.5)
		(mid 212.331274 38.543942)
		(end 212.375223 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 212.375223 39.85)
		(end 212.375223 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 212.525223 40)
		(mid 212.419157 39.956066)
		(end 212.375223 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 212.857481 40)
		(end 212.525223 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 213.007481 38.65)
		(end 213.007481 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 213.007481 38.65)
		(mid 213.051414 38.543927)
		(end 213.157481 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 213.007481 39.85)
		(mid 212.963547 39.956066)
		(end 212.857481 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.257481 38.5)
		(end 213.157481 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 214.257481 38.5)
		(mid 214.363559 38.543927)
		(end 214.407481 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.407481 39.85)
		(end 214.407481 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 214.557481 40)
		(mid 214.451415 39.956066)
		(end 214.407481 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 218.44619 40)
		(end 214.557481 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 218.59619 38.65)
		(end 218.59619 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 218.59619 38.65)
		(mid 218.640123 38.54393)
		(end 218.74619 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 218.59619 39.85)
		(mid 218.552256 39.956066)
		(end 218.44619 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 219.84619 38.5)
		(end 218.74619 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 219.84619 38.5)
		(mid 219.952262 38.54393)
		(end 219.99619 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 219.99619 39.85)
		(end 219.99619 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 220.14619 40)
		(mid 220.040124 39.956066)
		(end 219.99619 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 220.478449 40)
		(end 220.14619 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 220.628449 38.65)
		(end 220.628449 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 220.628449 38.65)
		(mid 220.672386 38.543951)
		(end 220.778449 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 220.628449 39.85)
		(mid 220.584515 39.956066)
		(end 220.478449 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 221.878449 38.5)
		(end 220.778449 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 221.878449 38.5)
		(mid 221.984548 38.543916)
		(end 222.028449 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 222.028449 39.85)
		(end 222.028449 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 222.178449 40)
		(mid 222.072383 39.956066)
		(end 222.028449 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 224.432246 40)
		(end 222.178449 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 224.582246 38.65)
		(end 224.582246 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 224.582246 38.65)
		(mid 224.626183 38.54395)
		(end 224.732246 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 224.582246 39.85)
		(mid 224.538312 39.956066)
		(end 224.432246 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 225.832246 38.5)
		(end 224.732246 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 225.832246 38.5)
		(mid 225.938282 38.54395)
		(end 225.982246 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 225.982246 39.85)
		(end 225.982246 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 226.132246 40)
		(mid 226.02618 39.956066)
		(end 225.982246 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 226.464504 40)
		(end 226.132246 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 226.614504 38.65)
		(end 226.614504 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 226.614504 38.65)
		(mid 226.658438 38.543935)
		(end 226.764504 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 226.614504 39.85)
		(mid 226.57057 39.956066)
		(end 226.464504 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 227.864504 38.5)
		(end 226.764504 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 227.864504 38.5)
		(mid 227.970567 38.543935)
		(end 228.014504 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 228.014504 39.85)
		(end 228.014504 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 228.164504 40)
		(mid 228.058438 39.956066)
		(end 228.014504 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 232.053214 40)
		(end 228.164504 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 232.203214 38.65)
		(end 232.203214 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 232.203214 38.65)
		(mid 232.247149 38.543939)
		(end 232.353214 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 232.203214 39.85)
		(mid 232.15928 39.956066)
		(end 232.053214 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 233.453214 38.5)
		(end 232.353214 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 233.453214 38.5)
		(mid 233.559271 38.543939)
		(end 233.603214 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 233.603214 39.85)
		(end 233.603214 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 233.753214 40)
		(mid 233.647148 39.956066)
		(end 233.603214 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 234.085472 40)
		(end 233.753214 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 234.235472 38.65)
		(end 234.235472 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 234.235472 38.65)
		(mid 234.279404 38.543924)
		(end 234.385472 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 234.235472 39.85)
		(mid 234.191538 39.956066)
		(end 234.085472 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 235.485472 38.5)
		(end 234.385472 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 235.485472 38.5)
		(mid 235.591556 38.543924)
		(end 235.635472 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 235.635472 39.85)
		(end 235.635472 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 235.785472 40)
		(mid 235.679406 39.956066)
		(end 235.635472 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 238.039269 40)
		(end 235.785472 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 238.189269 38.65)
		(end 238.189269 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 238.189269 38.65)
		(mid 238.233201 38.543923)
		(end 238.339269 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 238.189269 39.85)
		(mid 238.145335 39.956066)
		(end 238.039269 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 239.439269 38.5)
		(end 238.339269 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 239.439269 38.5)
		(mid 239.545355 38.543923)
		(end 239.589269 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 239.589269 39.85)
		(end 239.589269 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 239.739269 40)
		(mid 239.633203 39.956066)
		(end 239.589269 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 240.071527 40)
		(end 239.739269 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 240.221527 38.65)
		(end 240.221527 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 240.221527 38.65)
		(mid 240.265463 38.543944)
		(end 240.371527 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 240.221527 39.85)
		(mid 240.177593 39.956066)
		(end 240.071527 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 241.471527 38.5)
		(end 240.371527 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 241.471527 38.5)
		(mid 241.577576 38.543944)
		(end 241.621527 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 241.621527 39.85)
		(end 241.621527 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 241.771527 40)
		(mid 241.665461 39.956066)
		(end 241.621527 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 245.660237 40)
		(end 241.771527 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 245.810237 38.65)
		(end 245.810237 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 245.810237 38.65)
		(mid 245.854173 38.543947)
		(end 245.960237 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 245.810237 39.85)
		(mid 245.766303 39.956066)
		(end 245.660237 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 247.060237 38.5)
		(end 245.960237 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 247.060237 38.5)
		(mid 247.166279 38.543947)
		(end 247.210237 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 247.210237 39.85)
		(end 247.210237 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 247.360237 40)
		(mid 247.254171 39.956066)
		(end 247.210237 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 247.692495 40)
		(end 247.360237 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 247.842495 38.65)
		(end 247.842495 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 247.842495 38.65)
		(mid 247.886429 38.543932)
		(end 247.992495 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 247.842495 39.85)
		(mid 247.798561 39.956066)
		(end 247.692495 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 249.092495 38.5)
		(end 247.992495 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 249.092495 38.5)
		(mid 249.198564 38.543932)
		(end 249.242495 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 249.242495 39.85)
		(end 249.242495 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 249.392495 40)
		(mid 249.286429 39.956066)
		(end 249.242495 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 251.646292 40)
		(end 249.392495 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 251.796292 38.65)
		(end 251.796292 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 251.796292 38.65)
		(mid 251.840225 38.543931)
		(end 251.946292 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 251.796292 39.85)
		(mid 251.752358 39.956066)
		(end 251.646292 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 253.046292 38.5)
		(end 251.946292 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 253.046292 38.5)
		(mid 253.152363 38.543931)
		(end 253.196292 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 253.196292 39.85)
		(end 253.196292 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 253.346292 40)
		(mid 253.240226 39.956066)
		(end 253.196292 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 253.67855 40)
		(end 253.346292 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 253.82855 38.65)
		(end 253.82855 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 253.82855 38.65)
		(mid 253.872487 38.543952)
		(end 253.97855 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 253.82855 39.85)
		(mid 253.784616 39.956066)
		(end 253.67855 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 255.07855 38.5)
		(end 253.97855 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 255.07855 38.5)
		(mid 255.184648 38.543916)
		(end 255.22855 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 255.22855 39.85)
		(end 255.22855 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 255.37855 40)
		(mid 255.272484 39.956066)
		(end 255.22855 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 259.26726 40)
		(end 255.37855 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 259.41726 38.65)
		(end 259.41726 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 259.41726 38.65)
		(mid 259.461192 38.54392)
		(end 259.56726 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 259.41726 39.85)
		(mid 259.373326 39.956066)
		(end 259.26726 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 260.66726 38.5)
		(end 259.56726 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 260.66726 38.5)
		(mid 260.773352 38.54392)
		(end 260.81726 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 260.81726 39.85)
		(end 260.81726 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 260.96726 40)
		(mid 260.861194 39.956066)
		(end 260.81726 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 261.299518 40)
		(end 260.96726 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 261.449518 38.65)
		(end 261.449518 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 261.449518 38.65)
		(mid 261.493453 38.54394)
		(end 261.599518 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 261.449518 39.85)
		(mid 261.405584 39.956066)
		(end 261.299518 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 262.699518 38.5)
		(end 261.599518 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 262.699518 38.5)
		(mid 262.805572 38.54394)
		(end 262.849518 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 262.849518 39.85)
		(end 262.849518 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 262.999518 40)
		(mid 262.893452 39.956066)
		(end 262.849518 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 265.253315 40)
		(end 262.999518 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 265.403315 38.65)
		(end 265.403315 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 265.403315 38.65)
		(mid 265.44725 38.543939)
		(end 265.553315 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 265.403315 39.85)
		(mid 265.359381 39.956066)
		(end 265.253315 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 266.653315 38.5)
		(end 265.553315 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 266.653315 38.5)
		(mid 266.759371 38.543939)
		(end 266.803315 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 266.803315 39.85)
		(end 266.803315 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 266.953315 40)
		(mid 266.847249 39.956066)
		(end 266.803315 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 267.285574 40)
		(end 266.953315 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 267.435574 38.65)
		(end 267.435574 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 267.435574 38.65)
		(mid 267.479506 38.543925)
		(end 267.585574 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 267.435574 39.85)
		(mid 267.39164 39.956066)
		(end 267.285574 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 268.685574 38.5)
		(end 267.585574 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 268.685574 38.5)
		(mid 268.791657 38.543925)
		(end 268.835574 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 268.835574 39.85)
		(end 268.835574 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 268.985574 40)
		(mid 268.879507 39.956066)
		(end 268.835574 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 272.874283 40)
		(end 268.985574 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 273.024283 38.65)
		(end 273.024283 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 273.024283 38.65)
		(mid 273.068216 38.543928)
		(end 273.174283 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 273.024283 39.85)
		(mid 272.980349 39.956066)
		(end 272.874283 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 274.274283 38.5)
		(end 273.174283 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 274.274283 38.5)
		(mid 274.38036 38.543928)
		(end 274.424283 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 274.424283 39.85)
		(end 274.424283 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 274.574283 40)
		(mid 274.468217 39.956066)
		(end 274.424283 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 274.906541 40)
		(end 274.574283 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 275.056541 38.65)
		(end 275.056541 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 275.056541 38.65)
		(mid 275.100477 38.543948)
		(end 275.206541 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 275.056541 39.85)
		(mid 275.012607 39.956066)
		(end 274.906541 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 276.306541 38.5)
		(end 275.206541 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 276.306541 38.5)
		(mid 276.412581 38.543948)
		(end 276.456541 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 276.456541 39.85)
		(end 276.456541 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 276.606541 40)
		(mid 276.500475 39.956066)
		(end 276.456541 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 278.860339 40)
		(end 276.606541 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 279.010339 38.65)
		(end 279.010339 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 279.010339 38.65)
		(mid 279.054275 38.543948)
		(end 279.160339 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 279.010339 39.85)
		(mid 278.966405 39.956066)
		(end 278.860339 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 280.260339 38.5)
		(end 279.160339 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 280.260339 38.5)
		(mid 280.36638 38.543948)
		(end 280.410339 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 280.410339 39.85)
		(end 280.410339 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 280.560339 40)
		(mid 280.454273 39.956066)
		(end 280.410339 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 280.892597 40)
		(end 280.560339 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 281.042597 38.65)
		(end 281.042597 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 281.042597 38.65)
		(mid 281.086531 38.543933)
		(end 281.192597 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 281.042597 39.85)
		(mid 280.998663 39.956066)
		(end 280.892597 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 282.292597 38.5)
		(end 281.192597 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 282.292597 38.5)
		(mid 282.398665 38.543933)
		(end 282.442597 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 282.442597 39.85)
		(end 282.442597 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 282.592597 40)
		(mid 282.486531 39.956066)
		(end 282.442597 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 286.481306 40)
		(end 282.592597 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 286.631306 38.65)
		(end 286.631306 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 286.631306 38.65)
		(mid 286.67524 38.543936)
		(end 286.781306 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 286.631306 39.85)
		(mid 286.587372 39.956066)
		(end 286.481306 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 287.881306 38.5)
		(end 286.781306 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 287.881306 38.5)
		(mid 287.987368 38.543936)
		(end 288.031306 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 288.031306 39.85)
		(end 288.031306 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 288.181306 40)
		(mid 288.07524 39.956066)
		(end 288.031306 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 288.513564 40)
		(end 288.181306 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 288.663564 38.65)
		(end 288.663564 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 288.663564 38.65)
		(mid 288.707496 38.543921)
		(end 288.813564 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 288.663564 39.85)
		(mid 288.61963 39.956066)
		(end 288.513564 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 289.913564 38.5)
		(end 288.813564 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 289.913564 38.5)
		(mid 290.019653 38.543921)
		(end 290.063564 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 290.063564 39.85)
		(end 290.063564 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 290.213564 40)
		(mid 290.107498 39.956066)
		(end 290.063564 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 292.467362 40)
		(end 290.213564 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 292.617362 38.65)
		(end 292.617362 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 292.617362 38.65)
		(mid 292.661294 38.543921)
		(end 292.767362 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 292.617362 39.85)
		(mid 292.573428 39.956066)
		(end 292.467362 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 293.867362 38.5)
		(end 292.767362 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 293.867362 38.5)
		(mid 293.973453 38.543921)
		(end 294.017362 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 294.017362 39.85)
		(end 294.017362 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 294.167362 40)
		(mid 294.061296 39.956066)
		(end 294.017362 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 294.49962 40)
		(end 294.167362 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 294.64962 38.65)
		(end 294.64962 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 294.64962 38.65)
		(mid 294.693555 38.543941)
		(end 294.79962 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 294.64962 39.85)
		(mid 294.605686 39.956066)
		(end 294.49962 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 295.89962 38.5)
		(end 294.79962 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 295.89962 38.5)
		(mid 296.005673 38.543941)
		(end 296.04962 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 296.04962 39.85)
		(end 296.04962 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 296.19962 40)
		(mid 296.093554 39.956066)
		(end 296.04962 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 300.08833 40)
		(end 296.19962 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 300.23833 38.65)
		(end 300.23833 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 300.23833 38.65)
		(mid 300.282266 38.543945)
		(end 300.38833 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 300.23833 39.85)
		(mid 300.194396 39.956066)
		(end 300.08833 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 301.48833 38.5)
		(end 300.38833 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 301.48833 38.5)
		(mid 301.594377 38.543945)
		(end 301.63833 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 301.63833 39.85)
		(end 301.63833 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 301.78833 40)
		(mid 301.682264 39.956066)
		(end 301.63833 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 302.120588 40)
		(end 301.78833 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 302.270588 38.65)
		(end 302.270588 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 302.270588 38.65)
		(mid 302.314521 38.54393)
		(end 302.420588 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 302.270588 39.85)
		(mid 302.226654 39.956066)
		(end 302.120588 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 303.520588 38.5)
		(end 302.420588 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 303.520588 38.5)
		(mid 303.626662 38.54393)
		(end 303.670588 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 303.670588 39.85)
		(end 303.670588 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 303.820588 40)
		(mid 303.714522 39.956066)
		(end 303.670588 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 306.074385 40)
		(end 303.820588 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 306.224385 38.65)
		(end 306.224385 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 306.224385 38.65)
		(mid 306.268318 38.543929)
		(end 306.374385 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 306.224385 39.85)
		(mid 306.180451 39.956066)
		(end 306.074385 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 307.474385 38.5)
		(end 306.374385 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 307.474385 38.5)
		(mid 307.580461 38.543929)
		(end 307.624385 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 307.624385 39.85)
		(end 307.624385 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 307.774385 40)
		(mid 307.668319 39.956066)
		(end 307.624385 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 308.106643 40)
		(end 307.774385 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 308.256643 38.65)
		(end 308.256643 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 308.256643 38.65)
		(mid 308.30058 38.543949)
		(end 308.406643 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 308.256643 39.85)
		(mid 308.212709 39.956066)
		(end 308.106643 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 309.506643 38.5)
		(end 308.406643 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 309.506643 38.5)
		(mid 309.612681 38.543949)
		(end 309.656643 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 309.656643 39.85)
		(end 309.656643 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 309.806643 40)
		(mid 309.700577 39.956066)
		(end 309.656643 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 313.695353 40)
		(end 309.806643 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 313.845353 38.65)
		(end 313.845353 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 313.845353 38.65)
		(mid 313.889284 38.543917)
		(end 313.995353 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 313.845353 39.85)
		(mid 313.801419 39.956066)
		(end 313.695353 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 315.095353 38.5)
		(end 313.995353 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 315.095353 38.5)
		(mid 315.201449 38.543917)
		(end 315.245353 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 315.245353 39.85)
		(end 315.245353 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 315.395353 40)
		(mid 315.289287 39.956066)
		(end 315.245353 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 315.727611 40)
		(end 315.395353 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 315.877611 38.65)
		(end 315.877611 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 315.877611 38.65)
		(mid 315.921546 38.543938)
		(end 316.027611 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 315.877611 39.85)
		(mid 315.833677 39.956066)
		(end 315.727611 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 317.127611 38.5)
		(end 316.027611 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 317.127611 38.5)
		(mid 317.23367 38.543938)
		(end 317.277611 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 317.277611 39.85)
		(end 317.277611 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 317.427611 40)
		(mid 317.321545 39.956066)
		(end 317.277611 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 319.681408 40)
		(end 317.427611 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 319.831408 38.65)
		(end 319.831408 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 319.831408 38.65)
		(mid 319.875342 38.543937)
		(end 319.981408 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 319.831408 39.85)
		(mid 319.787474 39.956066)
		(end 319.681408 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 321.081408 38.5)
		(end 319.981408 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 321.081408 38.5)
		(mid 321.187469 38.543937)
		(end 321.231408 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 321.231408 39.85)
		(end 321.231408 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 321.381408 40)
		(mid 321.275342 39.956066)
		(end 321.231408 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 321.713666 40)
		(end 321.381408 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 321.863666 38.65)
		(end 321.863666 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 321.863666 38.65)
		(mid 321.907598 38.543922)
		(end 322.013666 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 321.863666 39.85)
		(mid 321.819732 39.956066)
		(end 321.713666 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 323.113666 38.5)
		(end 322.013666 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 323.113666 38.5)
		(mid 323.219754 38.543922)
		(end 323.263666 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 323.263666 39.85)
		(end 323.263666 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 323.413666 40)
		(mid 323.3076 39.956066)
		(end 323.263666 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 327.302376 40)
		(end 323.413666 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 327.452376 38.65)
		(end 327.452376 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 327.452376 38.65)
		(mid 327.496309 38.543925)
		(end 327.602376 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 327.452376 39.85)
		(mid 327.408442 39.956066)
		(end 327.302376 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 328.702376 38.5)
		(end 327.602376 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 328.702376 38.5)
		(mid 328.808458 38.543925)
		(end 328.852376 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 328.852376 39.85)
		(end 328.852376 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 329.002376 40)
		(mid 328.89631 39.956066)
		(end 328.852376 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 329.334634 40)
		(end 329.002376 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 329.484634 38.65)
		(end 329.484634 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 329.484634 38.65)
		(mid 329.52857 38.543946)
		(end 329.634634 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 329.484634 39.85)
		(mid 329.4407 39.956066)
		(end 329.334634 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 330.734634 38.5)
		(end 329.634634 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 330.734634 38.5)
		(mid 330.840678 38.543946)
		(end 330.884634 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 330.884634 39.85)
		(end 330.884634 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 331.034634 40)
		(mid 330.928568 39.956066)
		(end 330.884634 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 333.288431 40)
		(end 331.034634 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 333.438431 38.65)
		(end 333.438431 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 333.438431 38.65)
		(mid 333.482367 38.543945)
		(end 333.588431 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 333.438431 39.85)
		(mid 333.394497 39.956066)
		(end 333.288431 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 334.688431 38.5)
		(end 333.588431 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 334.688431 38.5)
		(mid 334.794477 38.543945)
		(end 334.838431 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 334.838431 39.85)
		(end 334.838431 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 334.988431 40)
		(mid 334.882365 39.956066)
		(end 334.838431 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 335.320689 40)
		(end 334.988431 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 335.470689 38.65)
		(end 335.470689 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 335.470689 38.65)
		(mid 335.514622 38.54393)
		(end 335.620689 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 335.470689 39.85)
		(mid 335.426755 39.956066)
		(end 335.320689 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 336.720689 38.5)
		(end 335.620689 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 336.720689 38.5)
		(mid 336.826762 38.54393)
		(end 336.870689 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 336.870689 39.85)
		(end 336.870689 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 337.020689 40)
		(mid 336.914623 39.956066)
		(end 336.870689 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 340.909399 40)
		(end 337.020689 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 341.059399 38.65)
		(end 341.059399 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 341.059399 38.65)
		(mid 341.103333 38.543934)
		(end 341.209399 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 341.059399 39.85)
		(mid 341.015465 39.956066)
		(end 340.909399 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 342.309399 38.5)
		(end 341.209399 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 342.309399 38.5)
		(mid 342.415466 38.543934)
		(end 342.459399 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 342.459399 39.85)
		(end 342.459399 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 342.609399 40)
		(mid 342.503333 39.956066)
		(end 342.459399 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 342.941657 40)
		(end 342.609399 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 343.091657 38.65)
		(end 343.091657 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 343.091657 38.65)
		(mid 343.135588 38.543919)
		(end 343.241657 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 343.091657 39.85)
		(mid 343.047723 39.956066)
		(end 342.941657 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 344.341657 38.5)
		(end 343.241657 38.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 344.341657 38.5)
		(mid 344.447751 38.543919)
		(end 344.491657 38.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 344.491657 39.85)
		(end 344.491657 38.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 344.641657 40)
		(mid 344.535591 39.956066)
		(end 344.491657 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 344.818556 40)
		(end 344.641657 40)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 344.818556 40)
		(mid 344.92465 40.043918)
		(end 344.968556 40.15)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 344.968556 46.25)
		(mid 344.924619 46.35605)
		(end 344.818556 46.4)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 344.968556 46.25)
		(end 344.968556 40.15)
		(layer "Edge.Cuts")
	)
	(gr_text "+ W   N C"
		(at 26.003511 40.65 0)
		(layer "F.SilkS")
	)
	(gr_text "Z4S1"
		(at 26.003511 41.9 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 39.610534 40.65 0)
		(layer "F.SilkS")
	)
	(gr_text "Z4S2"
		(at 39.610534 41.9 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 53.217557 40.65 0)
		(layer "F.SilkS")
	)
	(gr_text "Z4S3"
		(at 53.217557 41.9 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 66.824581 40.65 0)
		(layer "F.SilkS")
	)
	(gr_text "Z4S4"
		(at 66.824581 41.9 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 80.431604 40.65 0)
		(layer "F.SilkS")
	)
	(gr_text "Z5S1"
		(at 80.431604 41.9 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 94.038627 40.65 0)
		(layer "F.SilkS")
	)
	(gr_text "Z5S2"
		(at 94.038627 41.9 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 107.64565 40.65 0)
		(layer "F.SilkS")
	)
	(gr_text "Z5S3"
		(at 107.64565 41.9 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 121.252673 40.65 0)
		(layer "F.SilkS")
	)
	(gr_text "Z5S4"
		(at 121.252673 41.9 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 134.859697 40.65 0)
		(layer "F.SilkS")
	)
	(gr_text "Z6S1"
		(at 134.859697 41.9 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 148.46672 40.65 0)
		(layer "F.SilkS")
	)
	(gr_text "Z6S2"
		(at 148.46672 41.9 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 162.073743 40.65 0)
		(layer "F.SilkS")
	)
	(gr_text "Z6S3"
		(at 162.073743 41.9 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 175.680766 40.65 0)
		(layer "F.SilkS")
	)
	(gr_text "Z6S4"
		(at 175.680766 41.9 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 189.287789 40.65 0)
		(layer "F.SilkS")
	)
	(gr_text "Z1S1"
		(at 189.287789 41.9 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 202.894812 40.65 0)
		(layer "F.SilkS")
	)
	(gr_text "Z1S2"
		(at 202.894812 41.9 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 216.501836 40.65 0)
		(layer "F.SilkS")
	)
	(gr_text "Z1S3"
		(at 216.501836 41.9 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 230.108859 40.65 0)
		(layer "F.SilkS")
	)
	(gr_text "Z1S4"
		(at 230.108859 41.9 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 243.715882 40.65 0)
		(layer "F.SilkS")
	)
	(gr_text "Z2S1"
		(at 243.715882 41.9 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 257.322905 40.65 0)
		(layer "F.SilkS")
	)
	(gr_text "Z2S2"
		(at 257.322905 41.9 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 270.929928 40.65 0)
		(layer "F.SilkS")
	)
	(gr_text "Z2S3"
		(at 270.929928 41.9 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 284.536952 40.65 0)
		(layer "F.SilkS")
	)
	(gr_text "Z2S4"
		(at 284.536952 41.9 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 298.143975 40.65 0)
		(layer "F.SilkS")
	)
	(gr_text "Z3S1"
		(at 298.143975 41.9 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 311.750998 40.65 0)
		(layer "F.SilkS")
	)
	(gr_text "Z3S2"
		(at 311.750998 41.9 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 325.358021 40.65 0)
		(layer "F.SilkS")
	)
	(gr_text "Z3S3"
		(at 325.358021 41.9 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 338.965044 40.65 0)
		(layer "F.SilkS")
	)
	(gr_text "Z3S4"
		(at 338.965044 41.9 0)
		(layer "F.SilkS")
	)
	(embedded_fonts no)
)
