(kicad_sch
  (version 20250114)
  (generator "engineered-lighting")
  (generator_version "0.2")
  (paper "A2")
  (title_block
    (title "led-lower-v0.2 / passive interconnect")
    (date "2026-09-06")
    (rev "0.2 QUOTE REVIEW")
    (company "Engineered Lighting")
    (comment 1 "ENGINEERING DRAFT - see release status before fabrication"))
  (lib_symbols
    (symbol "Connector_Generic:Conn_01x04"
      (pin_names
        (offset 1.016)
        (hide yes))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "J"
        (at 0 5.08 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "Conn_01x04"
        (at 0 -7.62 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "connector"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "Connector*:*_1x??_*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "Conn_01x04_1_1"
        (rectangle
          (start -1.27 3.81)
          (end 1.27 -6.35)
          (fill
            (type background)))
        (rectangle
          (start -1.27 2.667)
          (end 0 2.413)
          (fill
            (type none)))
        (rectangle
          (start -1.27 0.127)
          (end 0 -0.127)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -2.413)
          (end 0 -2.667)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -4.953)
          (end 0 -5.207)
          (fill
            (type none)))
        (pin passive line
          (at -5.08 2.54 0)
          (length 3.81)
          (name "Pin_1")
          (number "1"))
        (pin passive line
          (at -5.08 0 0)
          (length 3.81)
          (name "Pin_2")
          (number "2"))
        (pin passive line
          (at -5.08 -2.54 0)
          (length 3.81)
          (name "Pin_3")
          (number "3"))
        (pin passive line
          (at -5.08 -5.08 0)
          (length 3.81)
          (name "Pin_4")
          (number "4")))
      (embedded_fonts no)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 90.17 48.26 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J11"
      (at 90.17 35.56 0.0))
    (property "Value" "Z1 S1 BOTTOM"
      (at 90.17 38.1 0.0))
    (property "Footprint" "ELFlex:J11_Solder4"
      (at 90.17 48.26 0.0)
      (hide yes))
    (instances
      (project "led-lower-v0.2"
        (path
          (reference "J11")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 85.09 45.72)
      (xy 73.66 45.72)))
  (global_label "Z1_B12_24V"
    (shape passive)
    (at 73.66 45.72 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 73.66 45.72 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 48.26)
      (xy 74.93 48.26)))
  (global_label "Z1_B12_W"
    (shape passive)
    (at 74.93 48.26 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 48.26 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 50.8)
      (xy 74.93 50.8)))
  (global_label "Z1_B12_N"
    (shape passive)
    (at 74.93 50.8 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 50.8 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 53.34)
      (xy 74.93 53.34)))
  (global_label "Z1_B12_C"
    (shape passive)
    (at 74.93 53.34 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 53.34 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 189.23 48.26 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J12"
      (at 189.23 35.56 0.0))
    (property "Value" "Z1 S2 BOTTOM"
      (at 189.23 38.1 0.0))
    (property "Footprint" "ELFlex:J12_Solder4"
      (at 189.23 48.26 0.0)
      (hide yes))
    (instances
      (project "led-lower-v0.2"
        (path
          (reference "J12")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 184.15 45.72)
      (xy 172.72 45.72)))
  (global_label "Z1_B12_24V"
    (shape passive)
    (at 172.72 45.72 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 172.72 45.72 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 184.15 48.26)
      (xy 173.99 48.26)))
  (global_label "Z1_B12_W"
    (shape passive)
    (at 173.99 48.26 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 173.99 48.26 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 184.15 50.8)
      (xy 173.99 50.8)))
  (global_label "Z1_B12_N"
    (shape passive)
    (at 173.99 50.8 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 173.99 50.8 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 184.15 53.34)
      (xy 173.99 53.34)))
  (global_label "Z1_B12_C"
    (shape passive)
    (at 173.99 53.34 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 173.99 53.34 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 288.29 48.26 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J13"
      (at 288.29 35.56 0.0))
    (property "Value" "Z1 S3 BOTTOM"
      (at 288.29 38.1 0.0))
    (property "Footprint" "ELFlex:J13_Solder4"
      (at 288.29 48.26 0.0)
      (hide yes))
    (instances
      (project "led-lower-v0.2"
        (path
          (reference "J13")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 283.21 45.72)
      (xy 271.78 45.72)))
  (global_label "Z1_B34_24V"
    (shape passive)
    (at 271.78 45.72 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 271.78 45.72 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 283.21 48.26)
      (xy 273.05 48.26)))
  (global_label "Z1_B34_W"
    (shape passive)
    (at 273.05 48.26 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 273.05 48.26 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 283.21 50.8)
      (xy 273.05 50.8)))
  (global_label "Z1_B34_N"
    (shape passive)
    (at 273.05 50.8 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 273.05 50.8 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 283.21 53.34)
      (xy 273.05 53.34)))
  (global_label "Z1_B34_C"
    (shape passive)
    (at 273.05 53.34 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 273.05 53.34 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 387.35 48.26 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J14"
      (at 387.35 35.56 0.0))
    (property "Value" "Z1 S4 BOTTOM"
      (at 387.35 38.1 0.0))
    (property "Footprint" "ELFlex:J14_Solder4"
      (at 387.35 48.26 0.0)
      (hide yes))
    (instances
      (project "led-lower-v0.2"
        (path
          (reference "J14")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 382.27 45.72)
      (xy 370.84 45.72)))
  (global_label "Z1_B34_24V"
    (shape passive)
    (at 370.84 45.72 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 370.84 45.72 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 382.27 48.26)
      (xy 372.11 48.26)))
  (global_label "Z1_B34_W"
    (shape passive)
    (at 372.11 48.26 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 372.11 48.26 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 382.27 50.8)
      (xy 372.11 50.8)))
  (global_label "Z1_B34_N"
    (shape passive)
    (at 372.11 50.8 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 372.11 50.8 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 382.27 53.34)
      (xy 372.11 53.34)))
  (global_label "Z1_B34_C"
    (shape passive)
    (at 372.11 53.34 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 372.11 53.34 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 90.17 96.52 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J21"
      (at 90.17 83.82 0.0))
    (property "Value" "Z2 S1 BOTTOM"
      (at 90.17 86.36 0.0))
    (property "Footprint" "ELFlex:J21_Solder4"
      (at 90.17 96.52 0.0)
      (hide yes))
    (instances
      (project "led-lower-v0.2"
        (path
          (reference "J21")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 85.09 93.98)
      (xy 73.66 93.98)))
  (global_label "Z2_B12_24V"
    (shape passive)
    (at 73.66 93.98 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 73.66 93.98 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 96.52)
      (xy 74.93 96.52)))
  (global_label "Z2_B12_W"
    (shape passive)
    (at 74.93 96.52 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 96.52 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 99.06)
      (xy 74.93 99.06)))
  (global_label "Z2_B12_N"
    (shape passive)
    (at 74.93 99.06 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 99.06 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 101.6)
      (xy 74.93 101.6)))
  (global_label "Z2_B12_C"
    (shape passive)
    (at 74.93 101.6 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 101.6 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 189.23 96.52 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J22"
      (at 189.23 83.82 0.0))
    (property "Value" "Z2 S2 BOTTOM"
      (at 189.23 86.36 0.0))
    (property "Footprint" "ELFlex:J22_Solder4"
      (at 189.23 96.52 0.0)
      (hide yes))
    (instances
      (project "led-lower-v0.2"
        (path
          (reference "J22")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 184.15 93.98)
      (xy 172.72 93.98)))
  (global_label "Z2_B12_24V"
    (shape passive)
    (at 172.72 93.98 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 172.72 93.98 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 184.15 96.52)
      (xy 173.99 96.52)))
  (global_label "Z2_B12_W"
    (shape passive)
    (at 173.99 96.52 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 173.99 96.52 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 184.15 99.06)
      (xy 173.99 99.06)))
  (global_label "Z2_B12_N"
    (shape passive)
    (at 173.99 99.06 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 173.99 99.06 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 184.15 101.6)
      (xy 173.99 101.6)))
  (global_label "Z2_B12_C"
    (shape passive)
    (at 173.99 101.6 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 173.99 101.6 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 288.29 96.52 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J23"
      (at 288.29 83.82 0.0))
    (property "Value" "Z2 S3 BOTTOM"
      (at 288.29 86.36 0.0))
    (property "Footprint" "ELFlex:J23_Solder4"
      (at 288.29 96.52 0.0)
      (hide yes))
    (instances
      (project "led-lower-v0.2"
        (path
          (reference "J23")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 283.21 93.98)
      (xy 271.78 93.98)))
  (global_label "Z2_B34_24V"
    (shape passive)
    (at 271.78 93.98 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 271.78 93.98 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 283.21 96.52)
      (xy 273.05 96.52)))
  (global_label "Z2_B34_W"
    (shape passive)
    (at 273.05 96.52 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 273.05 96.52 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 283.21 99.06)
      (xy 273.05 99.06)))
  (global_label "Z2_B34_N"
    (shape passive)
    (at 273.05 99.06 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 273.05 99.06 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 283.21 101.6)
      (xy 273.05 101.6)))
  (global_label "Z2_B34_C"
    (shape passive)
    (at 273.05 101.6 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 273.05 101.6 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 387.35 96.52 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J24"
      (at 387.35 83.82 0.0))
    (property "Value" "Z2 S4 BOTTOM"
      (at 387.35 86.36 0.0))
    (property "Footprint" "ELFlex:J24_Solder4"
      (at 387.35 96.52 0.0)
      (hide yes))
    (instances
      (project "led-lower-v0.2"
        (path
          (reference "J24")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 382.27 93.98)
      (xy 370.84 93.98)))
  (global_label "Z2_B34_24V"
    (shape passive)
    (at 370.84 93.98 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 370.84 93.98 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 382.27 96.52)
      (xy 372.11 96.52)))
  (global_label "Z2_B34_W"
    (shape passive)
    (at 372.11 96.52 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 372.11 96.52 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 382.27 99.06)
      (xy 372.11 99.06)))
  (global_label "Z2_B34_N"
    (shape passive)
    (at 372.11 99.06 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 372.11 99.06 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 382.27 101.6)
      (xy 372.11 101.6)))
  (global_label "Z2_B34_C"
    (shape passive)
    (at 372.11 101.6 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 372.11 101.6 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 90.17 146.05 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J31"
      (at 90.17 133.35 0.0))
    (property "Value" "Z3 S1 BOTTOM"
      (at 90.17 135.89 0.0))
    (property "Footprint" "ELFlex:J31_Solder4"
      (at 90.17 146.05 0.0)
      (hide yes))
    (instances
      (project "led-lower-v0.2"
        (path
          (reference "J31")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 85.09 143.51)
      (xy 73.66 143.51)))
  (global_label "Z3_B12_24V"
    (shape passive)
    (at 73.66 143.51 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 73.66 143.51 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 146.05)
      (xy 74.93 146.05)))
  (global_label "Z3_B12_W"
    (shape passive)
    (at 74.93 146.05 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 146.05 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 148.59)
      (xy 74.93 148.59)))
  (global_label "Z3_B12_N"
    (shape passive)
    (at 74.93 148.59 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 148.59 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 151.13)
      (xy 74.93 151.13)))
  (global_label "Z3_B12_C"
    (shape passive)
    (at 74.93 151.13 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 151.13 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 189.23 146.05 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J32"
      (at 189.23 133.35 0.0))
    (property "Value" "Z3 S2 BOTTOM"
      (at 189.23 135.89 0.0))
    (property "Footprint" "ELFlex:J32_Solder4"
      (at 189.23 146.05 0.0)
      (hide yes))
    (instances
      (project "led-lower-v0.2"
        (path
          (reference "J32")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 184.15 143.51)
      (xy 172.72 143.51)))
  (global_label "Z3_B12_24V"
    (shape passive)
    (at 172.72 143.51 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 172.72 143.51 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 184.15 146.05)
      (xy 173.99 146.05)))
  (global_label "Z3_B12_W"
    (shape passive)
    (at 173.99 146.05 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 173.99 146.05 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 184.15 148.59)
      (xy 173.99 148.59)))
  (global_label "Z3_B12_N"
    (shape passive)
    (at 173.99 148.59 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 173.99 148.59 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 184.15 151.13)
      (xy 173.99 151.13)))
  (global_label "Z3_B12_C"
    (shape passive)
    (at 173.99 151.13 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 173.99 151.13 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 288.29 146.05 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J33"
      (at 288.29 133.35 0.0))
    (property "Value" "Z3 S3 BOTTOM"
      (at 288.29 135.89 0.0))
    (property "Footprint" "ELFlex:J33_Solder4"
      (at 288.29 146.05 0.0)
      (hide yes))
    (instances
      (project "led-lower-v0.2"
        (path
          (reference "J33")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 283.21 143.51)
      (xy 271.78 143.51)))
  (global_label "Z3_B34_24V"
    (shape passive)
    (at 271.78 143.51 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 271.78 143.51 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 283.21 146.05)
      (xy 273.05 146.05)))
  (global_label "Z3_B34_W"
    (shape passive)
    (at 273.05 146.05 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 273.05 146.05 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 283.21 148.59)
      (xy 273.05 148.59)))
  (global_label "Z3_B34_N"
    (shape passive)
    (at 273.05 148.59 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 273.05 148.59 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 283.21 151.13)
      (xy 273.05 151.13)))
  (global_label "Z3_B34_C"
    (shape passive)
    (at 273.05 151.13 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 273.05 151.13 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 387.35 146.05 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J34"
      (at 387.35 133.35 0.0))
    (property "Value" "Z3 S4 BOTTOM"
      (at 387.35 135.89 0.0))
    (property "Footprint" "ELFlex:J34_Solder4"
      (at 387.35 146.05 0.0)
      (hide yes))
    (instances
      (project "led-lower-v0.2"
        (path
          (reference "J34")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 382.27 143.51)
      (xy 370.84 143.51)))
  (global_label "Z3_B34_24V"
    (shape passive)
    (at 370.84 143.51 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 370.84 143.51 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 382.27 146.05)
      (xy 372.11 146.05)))
  (global_label "Z3_B34_W"
    (shape passive)
    (at 372.11 146.05 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 372.11 146.05 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 382.27 148.59)
      (xy 372.11 148.59)))
  (global_label "Z3_B34_N"
    (shape passive)
    (at 372.11 148.59 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 372.11 148.59 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 382.27 151.13)
      (xy 372.11 151.13)))
  (global_label "Z3_B34_C"
    (shape passive)
    (at 372.11 151.13 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 372.11 151.13 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 90.17 195.58 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J41"
      (at 90.17 182.88 0.0))
    (property "Value" "Z4 S1 BOTTOM"
      (at 90.17 185.42 0.0))
    (property "Footprint" "ELFlex:J41_Solder4"
      (at 90.17 195.58 0.0)
      (hide yes))
    (instances
      (project "led-lower-v0.2"
        (path
          (reference "J41")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 85.09 193.04)
      (xy 73.66 193.04)))
  (global_label "Z4_B12_24V"
    (shape passive)
    (at 73.66 193.04 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 73.66 193.04 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 195.58)
      (xy 74.93 195.58)))
  (global_label "Z4_B12_W"
    (shape passive)
    (at 74.93 195.58 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 195.58 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 198.12)
      (xy 74.93 198.12)))
  (global_label "Z4_B12_N"
    (shape passive)
    (at 74.93 198.12 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 198.12 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 200.66)
      (xy 74.93 200.66)))
  (global_label "Z4_B12_C"
    (shape passive)
    (at 74.93 200.66 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 200.66 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 189.23 195.58 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J42"
      (at 189.23 182.88 0.0))
    (property "Value" "Z4 S2 BOTTOM"
      (at 189.23 185.42 0.0))
    (property "Footprint" "ELFlex:J42_Solder4"
      (at 189.23 195.58 0.0)
      (hide yes))
    (instances
      (project "led-lower-v0.2"
        (path
          (reference "J42")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 184.15 193.04)
      (xy 172.72 193.04)))
  (global_label "Z4_B12_24V"
    (shape passive)
    (at 172.72 193.04 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 172.72 193.04 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 184.15 195.58)
      (xy 173.99 195.58)))
  (global_label "Z4_B12_W"
    (shape passive)
    (at 173.99 195.58 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 173.99 195.58 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 184.15 198.12)
      (xy 173.99 198.12)))
  (global_label "Z4_B12_N"
    (shape passive)
    (at 173.99 198.12 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 173.99 198.12 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 184.15 200.66)
      (xy 173.99 200.66)))
  (global_label "Z4_B12_C"
    (shape passive)
    (at 173.99 200.66 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 173.99 200.66 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 288.29 195.58 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J43"
      (at 288.29 182.88 0.0))
    (property "Value" "Z4 S3 BOTTOM"
      (at 288.29 185.42 0.0))
    (property "Footprint" "ELFlex:J43_Solder4"
      (at 288.29 195.58 0.0)
      (hide yes))
    (instances
      (project "led-lower-v0.2"
        (path
          (reference "J43")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 283.21 193.04)
      (xy 271.78 193.04)))
  (global_label "Z4_B34_24V"
    (shape passive)
    (at 271.78 193.04 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 271.78 193.04 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 283.21 195.58)
      (xy 273.05 195.58)))
  (global_label "Z4_B34_W"
    (shape passive)
    (at 273.05 195.58 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 273.05 195.58 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 283.21 198.12)
      (xy 273.05 198.12)))
  (global_label "Z4_B34_N"
    (shape passive)
    (at 273.05 198.12 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 273.05 198.12 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 283.21 200.66)
      (xy 273.05 200.66)))
  (global_label "Z4_B34_C"
    (shape passive)
    (at 273.05 200.66 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 273.05 200.66 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 387.35 195.58 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J44"
      (at 387.35 182.88 0.0))
    (property "Value" "Z4 S4 BOTTOM"
      (at 387.35 185.42 0.0))
    (property "Footprint" "ELFlex:J44_Solder4"
      (at 387.35 195.58 0.0)
      (hide yes))
    (instances
      (project "led-lower-v0.2"
        (path
          (reference "J44")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 382.27 193.04)
      (xy 370.84 193.04)))
  (global_label "Z4_B34_24V"
    (shape passive)
    (at 370.84 193.04 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 370.84 193.04 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 382.27 195.58)
      (xy 372.11 195.58)))
  (global_label "Z4_B34_W"
    (shape passive)
    (at 372.11 195.58 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 372.11 195.58 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 382.27 198.12)
      (xy 372.11 198.12)))
  (global_label "Z4_B34_N"
    (shape passive)
    (at 372.11 198.12 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 372.11 198.12 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 382.27 200.66)
      (xy 372.11 200.66)))
  (global_label "Z4_B34_C"
    (shape passive)
    (at 372.11 200.66 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 372.11 200.66 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 90.17 243.84 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J51"
      (at 90.17 231.14 0.0))
    (property "Value" "Z5 S1 BOTTOM"
      (at 90.17 233.68 0.0))
    (property "Footprint" "ELFlex:J51_Solder4"
      (at 90.17 243.84 0.0)
      (hide yes))
    (instances
      (project "led-lower-v0.2"
        (path
          (reference "J51")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 85.09 241.3)
      (xy 73.66 241.3)))
  (global_label "Z5_B12_24V"
    (shape passive)
    (at 73.66 241.3 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 73.66 241.3 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 243.84)
      (xy 74.93 243.84)))
  (global_label "Z5_B12_W"
    (shape passive)
    (at 74.93 243.84 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 243.84 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 246.38)
      (xy 74.93 246.38)))
  (global_label "Z5_B12_N"
    (shape passive)
    (at 74.93 246.38 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 246.38 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 248.92)
      (xy 74.93 248.92)))
  (global_label "Z5_B12_C"
    (shape passive)
    (at 74.93 248.92 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 248.92 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 189.23 243.84 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J52"
      (at 189.23 231.14 0.0))
    (property "Value" "Z5 S2 BOTTOM"
      (at 189.23 233.68 0.0))
    (property "Footprint" "ELFlex:J52_Solder4"
      (at 189.23 243.84 0.0)
      (hide yes))
    (instances
      (project "led-lower-v0.2"
        (path
          (reference "J52")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 184.15 241.3)
      (xy 172.72 241.3)))
  (global_label "Z5_B12_24V"
    (shape passive)
    (at 172.72 241.3 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 172.72 241.3 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 184.15 243.84)
      (xy 173.99 243.84)))
  (global_label "Z5_B12_W"
    (shape passive)
    (at 173.99 243.84 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 173.99 243.84 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 184.15 246.38)
      (xy 173.99 246.38)))
  (global_label "Z5_B12_N"
    (shape passive)
    (at 173.99 246.38 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 173.99 246.38 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 184.15 248.92)
      (xy 173.99 248.92)))
  (global_label "Z5_B12_C"
    (shape passive)
    (at 173.99 248.92 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 173.99 248.92 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 288.29 243.84 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J53"
      (at 288.29 231.14 0.0))
    (property "Value" "Z5 S3 BOTTOM"
      (at 288.29 233.68 0.0))
    (property "Footprint" "ELFlex:J53_Solder4"
      (at 288.29 243.84 0.0)
      (hide yes))
    (instances
      (project "led-lower-v0.2"
        (path
          (reference "J53")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 283.21 241.3)
      (xy 271.78 241.3)))
  (global_label "Z5_B34_24V"
    (shape passive)
    (at 271.78 241.3 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 271.78 241.3 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 283.21 243.84)
      (xy 273.05 243.84)))
  (global_label "Z5_B34_W"
    (shape passive)
    (at 273.05 243.84 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 273.05 243.84 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 283.21 246.38)
      (xy 273.05 246.38)))
  (global_label "Z5_B34_N"
    (shape passive)
    (at 273.05 246.38 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 273.05 246.38 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 283.21 248.92)
      (xy 273.05 248.92)))
  (global_label "Z5_B34_C"
    (shape passive)
    (at 273.05 248.92 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 273.05 248.92 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 387.35 243.84 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J54"
      (at 387.35 231.14 0.0))
    (property "Value" "Z5 S4 BOTTOM"
      (at 387.35 233.68 0.0))
    (property "Footprint" "ELFlex:J54_Solder4"
      (at 387.35 243.84 0.0)
      (hide yes))
    (instances
      (project "led-lower-v0.2"
        (path
          (reference "J54")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 382.27 241.3)
      (xy 370.84 241.3)))
  (global_label "Z5_B34_24V"
    (shape passive)
    (at 370.84 241.3 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 370.84 241.3 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 382.27 243.84)
      (xy 372.11 243.84)))
  (global_label "Z5_B34_W"
    (shape passive)
    (at 372.11 243.84 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 372.11 243.84 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 382.27 246.38)
      (xy 372.11 246.38)))
  (global_label "Z5_B34_N"
    (shape passive)
    (at 372.11 246.38 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 372.11 246.38 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 382.27 248.92)
      (xy 372.11 248.92)))
  (global_label "Z5_B34_C"
    (shape passive)
    (at 372.11 248.92 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 372.11 248.92 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 90.17 293.37 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J61"
      (at 90.17 280.67 0.0))
    (property "Value" "Z6 S1 BOTTOM"
      (at 90.17 283.21 0.0))
    (property "Footprint" "ELFlex:J61_Solder4"
      (at 90.17 293.37 0.0)
      (hide yes))
    (instances
      (project "led-lower-v0.2"
        (path
          (reference "J61")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 85.09 290.83)
      (xy 73.66 290.83)))
  (global_label "Z6_B12_24V"
    (shape passive)
    (at 73.66 290.83 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 73.66 290.83 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 293.37)
      (xy 74.93 293.37)))
  (global_label "Z6_B12_W"
    (shape passive)
    (at 74.93 293.37 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 293.37 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 295.91)
      (xy 74.93 295.91)))
  (global_label "Z6_B12_N"
    (shape passive)
    (at 74.93 295.91 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 295.91 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 298.45)
      (xy 74.93 298.45)))
  (global_label "Z6_B12_C"
    (shape passive)
    (at 74.93 298.45 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 298.45 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 189.23 293.37 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J62"
      (at 189.23 280.67 0.0))
    (property "Value" "Z6 S2 BOTTOM"
      (at 189.23 283.21 0.0))
    (property "Footprint" "ELFlex:J62_Solder4"
      (at 189.23 293.37 0.0)
      (hide yes))
    (instances
      (project "led-lower-v0.2"
        (path
          (reference "J62")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 184.15 290.83)
      (xy 172.72 290.83)))
  (global_label "Z6_B12_24V"
    (shape passive)
    (at 172.72 290.83 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 172.72 290.83 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 184.15 293.37)
      (xy 173.99 293.37)))
  (global_label "Z6_B12_W"
    (shape passive)
    (at 173.99 293.37 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 173.99 293.37 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 184.15 295.91)
      (xy 173.99 295.91)))
  (global_label "Z6_B12_N"
    (shape passive)
    (at 173.99 295.91 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 173.99 295.91 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 184.15 298.45)
      (xy 173.99 298.45)))
  (global_label "Z6_B12_C"
    (shape passive)
    (at 173.99 298.45 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 173.99 298.45 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 288.29 293.37 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J63"
      (at 288.29 280.67 0.0))
    (property "Value" "Z6 S3 BOTTOM"
      (at 288.29 283.21 0.0))
    (property "Footprint" "ELFlex:J63_Solder4"
      (at 288.29 293.37 0.0)
      (hide yes))
    (instances
      (project "led-lower-v0.2"
        (path
          (reference "J63")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 283.21 290.83)
      (xy 271.78 290.83)))
  (global_label "Z6_B34_24V"
    (shape passive)
    (at 271.78 290.83 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 271.78 290.83 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 283.21 293.37)
      (xy 273.05 293.37)))
  (global_label "Z6_B34_W"
    (shape passive)
    (at 273.05 293.37 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 273.05 293.37 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 283.21 295.91)
      (xy 273.05 295.91)))
  (global_label "Z6_B34_N"
    (shape passive)
    (at 273.05 295.91 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 273.05 295.91 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 283.21 298.45)
      (xy 273.05 298.45)))
  (global_label "Z6_B34_C"
    (shape passive)
    (at 273.05 298.45 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 273.05 298.45 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 387.35 293.37 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J64"
      (at 387.35 280.67 0.0))
    (property "Value" "Z6 S4 BOTTOM"
      (at 387.35 283.21 0.0))
    (property "Footprint" "ELFlex:J64_Solder4"
      (at 387.35 293.37 0.0)
      (hide yes))
    (instances
      (project "led-lower-v0.2"
        (path
          (reference "J64")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 382.27 290.83)
      (xy 370.84 290.83)))
  (global_label "Z6_B34_24V"
    (shape passive)
    (at 370.84 290.83 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 370.84 290.83 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 382.27 293.37)
      (xy 372.11 293.37)))
  (global_label "Z6_B34_W"
    (shape passive)
    (at 372.11 293.37 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 372.11 293.37 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 382.27 295.91)
      (xy 372.11 295.91)))
  (global_label "Z6_B34_N"
    (shape passive)
    (at 372.11 295.91 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 372.11 295.91 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 382.27 298.45)
      (xy 372.11 298.45)))
  (global_label "Z6_B34_C"
    (shape passive)
    (at 372.11 298.45 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 372.11 298.45 0.0)
      (hide yes)))
  (text "Passive copper only. Pin 1=+24V, 2=W, 3=N, 4=C in the OUTSIDE installed view.\nSeparate net names denote isolation ON THIS FLEX, joined by LED-strip through rails only after assembly.\nUpper unused end pads have explicit no-connects: they are isolated probe/solder lands, not missing routes.\nNo zone boundary bridges; no commoning of the six fused +24V supplies. See wiring matrix and assembly instructions."
    (at 30.0 355.0 0)))
