(footprint "J100_FPC30_BottomContacts"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "J100"
		(at 0 0 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(property "Value" "30-contact FPC tail / Molex 2005280300"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
	(duplicate_pad_numbers_are_jumpers no)
	(pad "1" smd rect
		(at -14.5 1.75)
		(size 0.55 3.5)
		(layers "B.Cu" "B.Mask")
		(solder_mask_margin 0)
		(thermal_bridge_angle 45)
	)
	(pad "2" smd rect
		(at -13.5 1.75)
		(size 0.55 3.5)
		(layers "B.Cu" "B.Mask")
		(solder_mask_margin 0)
		(thermal_bridge_angle 45)
	)
	(pad "3" smd rect
		(at -12.5 1.75)
		(size 0.55 3.5)
		(layers "B.Cu" "B.Mask")
		(solder_mask_margin 0)
		(thermal_bridge_angle 45)
	)
	(pad "4" smd rect
		(at -11.5 1.75)
		(size 0.55 3.5)
		(layers "B.Cu" "B.Mask")
		(solder_mask_margin 0)
		(thermal_bridge_angle 45)
	)
	(pad "5" smd rect
		(at -10.5 1.75)
		(size 0.55 3.5)
		(layers "B.Cu" "B.Mask")
		(solder_mask_margin 0)
		(thermal_bridge_angle 45)
	)
	(pad "6" smd rect
		(at -9.5 1.75)
		(size 0.55 3.5)
		(layers "B.Cu" "B.Mask")
		(solder_mask_margin 0)
		(thermal_bridge_angle 45)
	)
	(pad "7" smd rect
		(at -8.5 1.75)
		(size 0.55 3.5)
		(layers "B.Cu" "B.Mask")
		(solder_mask_margin 0)
		(thermal_bridge_angle 45)
	)
	(pad "8" smd rect
		(at -7.5 1.75)
		(size 0.55 3.5)
		(layers "B.Cu" "B.Mask")
		(solder_mask_margin 0)
		(thermal_bridge_angle 45)
	)
	(pad "9" smd rect
		(at -6.5 1.75)
		(size 0.55 3.5)
		(layers "B.Cu" "B.Mask")
		(solder_mask_margin 0)
		(thermal_bridge_angle 45)
	)
	(pad "10" smd rect
		(at -5.5 1.75)
		(size 0.55 3.5)
		(layers "B.Cu" "B.Mask")
		(solder_mask_margin 0)
		(thermal_bridge_angle 45)
	)
	(pad "11" smd rect
		(at -4.5 1.75)
		(size 0.55 3.5)
		(layers "B.Cu" "B.Mask")
		(solder_mask_margin 0)
		(thermal_bridge_angle 45)
	)
	(pad "12" smd rect
		(at -3.5 1.75)
		(size 0.55 3.5)
		(layers "B.Cu" "B.Mask")
		(solder_mask_margin 0)
		(thermal_bridge_angle 45)
	)
	(pad "13" smd rect
		(at -2.5 1.75)
		(size 0.55 3.5)
		(layers "B.Cu" "B.Mask")
		(solder_mask_margin 0)
		(thermal_bridge_angle 45)
	)
	(pad "14" smd rect
		(at -1.5 1.75)
		(size 0.55 3.5)
		(layers "B.Cu" "B.Mask")
		(solder_mask_margin 0)
		(thermal_bridge_angle 45)
	)
	(pad "15" smd rect
		(at -0.5 1.75)
		(size 0.55 3.5)
		(layers "B.Cu" "B.Mask")
		(solder_mask_margin 0)
		(thermal_bridge_angle 45)
	)
	(pad "16" smd rect
		(at 0.5 1.75)
		(size 0.55 3.5)
		(layers "B.Cu" "B.Mask")
		(solder_mask_margin 0)
		(thermal_bridge_angle 45)
	)
	(pad "17" smd rect
		(at 1.5 1.75)
		(size 0.55 3.5)
		(layers "B.Cu" "B.Mask")
		(solder_mask_margin 0)
		(thermal_bridge_angle 45)
	)
	(pad "18" smd rect
		(at 2.5 1.75)
		(size 0.55 3.5)
		(layers "B.Cu" "B.Mask")
		(solder_mask_margin 0)
		(thermal_bridge_angle 45)
	)
	(pad "19" smd rect
		(at 3.5 1.75)
		(size 0.55 3.5)
		(layers "B.Cu" "B.Mask")
		(solder_mask_margin 0)
		(thermal_bridge_angle 45)
	)
	(pad "20" smd rect
		(at 4.5 1.75)
		(size 0.55 3.5)
		(layers "B.Cu" "B.Mask")
		(solder_mask_margin 0)
		(thermal_bridge_angle 45)
	)
	(pad "21" smd rect
		(at 5.5 1.75)
		(size 0.55 3.5)
		(layers "B.Cu" "B.Mask")
		(solder_mask_margin 0)
		(thermal_bridge_angle 45)
	)
	(pad "22" smd rect
		(at 6.5 1.75)
		(size 0.55 3.5)
		(layers "B.Cu" "B.Mask")
		(solder_mask_margin 0)
		(thermal_bridge_angle 45)
	)
	(pad "23" smd rect
		(at 7.5 1.75)
		(size 0.55 3.5)
		(layers "B.Cu" "B.Mask")
		(solder_mask_margin 0)
		(thermal_bridge_angle 45)
	)
	(pad "24" smd rect
		(at 8.5 1.75)
		(size 0.55 3.5)
		(layers "B.Cu" "B.Mask")
		(solder_mask_margin 0)
		(thermal_bridge_angle 45)
	)
	(pad "25" smd rect
		(at 9.5 1.75)
		(size 0.55 3.5)
		(layers "B.Cu" "B.Mask")
		(solder_mask_margin 0)
		(thermal_bridge_angle 45)
	)
	(pad "26" smd rect
		(at 10.5 1.75)
		(size 0.55 3.5)
		(layers "B.Cu" "B.Mask")
		(solder_mask_margin 0)
		(thermal_bridge_angle 45)
	)
	(pad "27" smd rect
		(at 11.5 1.75)
		(size 0.55 3.5)
		(layers "B.Cu" "B.Mask")
		(solder_mask_margin 0)
		(thermal_bridge_angle 45)
	)
	(pad "28" smd rect
		(at 12.5 1.75)
		(size 0.55 3.5)
		(layers "B.Cu" "B.Mask")
		(solder_mask_margin 0)
		(thermal_bridge_angle 45)
	)
	(pad "29" smd rect
		(at 13.5 1.75)
		(size 0.55 3.5)
		(layers "B.Cu" "B.Mask")
		(solder_mask_margin 0)
		(thermal_bridge_angle 45)
	)
	(pad "30" smd rect
		(at 14.5 1.75)
		(size 0.55 3.5)
		(layers "B.Cu" "B.Mask")
		(solder_mask_margin 0)
		(thermal_bridge_angle 45)
	)
	(embedded_fonts no)
)
