(footprint "J63_Solder4"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "J63"
		(at 0 0 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(property "Value" "Z6 S3 TOP"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_bom)
	(duplicate_pad_numbers_are_jumpers no)
	(pad "1" thru_hole roundrect
		(at 137.24713 7.2)
		(size 0.9 1)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.15)
		(solder_mask_margin -0.05)
		(thermal_bridge_angle 45)
	)
	(pad "2" thru_hole roundrect
		(at 139.279388 7.2)
		(size 0.9 1)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.15)
		(solder_mask_margin -0.05)
		(thermal_bridge_angle 45)
	)
	(pad "3" thru_hole roundrect
		(at 144.868098 7.2)
		(size 0.9 1)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.15)
		(solder_mask_margin -0.05)
		(thermal_bridge_angle 45)
	)
	(pad "4" thru_hole roundrect
		(at 146.900356 7.2)
		(size 0.9 1)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.15)
		(solder_mask_margin -0.05)
		(thermal_bridge_angle 45)
	)
	(embedded_fonts no)
)
