(kicad_pcb
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(general
		(thickness 0.15)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting
			(front yes)
			(back yes)
		)
		(covering
			(front no)
			(back no)
		)
		(plugging
			(front no)
			(back no)
		)
		(capping no)
		(filling no)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12)
			(dashed_line_gap_ratio 3)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(footprint "ELFlex:J43_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J43"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z4 S3 TOP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 28.390945 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z4_T23_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 30.423203 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z4_T23_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 36.011912 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z4_T23_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 38.04417 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z4_T23_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J64_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J64"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z6 S4 TOP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 150.854153 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "ZONE6_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 152.886411 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "ZONE6_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 158.475121 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "ZONE6_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 160.507379 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "ZONE6_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J41_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J41"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z4 S1 TOP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 1.176898 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "unconnected-(J41-Pin_1-Pad1)")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 3.209156 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "unconnected-(J41-Pin_2-Pad2)")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 8.797866 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "unconnected-(J41-Pin_3-Pad3)")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 10.830124 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "unconnected-(J41-Pin_4-Pad4)")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J12_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J12"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z1 S2 TOP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 178.0682 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z1_T23_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 180.100458 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z1_T23_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 185.689167 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z1_T23_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 187.721425 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z1_T23_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J14_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J14"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z1 S4 TOP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 205.282246 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "unconnected-(J14-Pin_1-Pad1)")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 207.314504 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "unconnected-(J14-Pin_2-Pad2)")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 212.903214 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "unconnected-(J14-Pin_3-Pad3)")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 214.935472 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "unconnected-(J14-Pin_4-Pad4)")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J21_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J21"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z2 S1 TOP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 218.889269 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "ZONE2_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 220.921527 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "ZONE2_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 226.510237 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "ZONE2_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 228.542495 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "ZONE2_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J51_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J51"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z5 S1 TOP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 55.604991 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "unconnected-(J51-Pin_1-Pad1)")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 57.637249 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "unconnected-(J51-Pin_2-Pad2)")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 63.225959 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "unconnected-(J51-Pin_3-Pad3)")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 65.258217 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "unconnected-(J51-Pin_4-Pad4)")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J52_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J52"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z5 S2 TOP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 69.212014 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z5_T23_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 71.244272 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z5_T23_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 76.832982 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z5_T23_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 78.86524 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z5_T23_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J11_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J11"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z1 S1 TOP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 164.461176 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "ZONE1_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 166.493434 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "ZONE1_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 172.082144 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "ZONE1_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 174.114402 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "ZONE1_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J54_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J54"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z5 S4 TOP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 96.42606 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "ZONE5_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 98.458319 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "ZONE5_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 104.047028 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "ZONE5_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 106.079286 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "ZONE5_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J42_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J42"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z4 S2 TOP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 14.783921 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z4_T23_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 16.816179 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z4_T23_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 22.404889 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z4_T23_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 24.437147 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z4_T23_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J100_FPC30_BottomContacts"
		(layer "F.Cu")
		(at 182.484278 5)
		(property "Reference" "J100"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "30-contact FPC tail / Molex 2005280300"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" smd rect
			(at -14.5 1.75)
			(size 0.55 3.5)
			(layers "B.Cu" "B.Mask")
			(net "ZONE4_24V")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at -13.5 1.75)
			(size 0.55 3.5)
			(layers "B.Cu" "B.Mask")
			(net "ZONE4_24V")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at -12.5 1.75)
			(size 0.55 3.5)
			(layers "B.Cu" "B.Mask")
			(net "ZONE4_W")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at -11.5 1.75)
			(size 0.55 3.5)
			(layers "B.Cu" "B.Mask")
			(net "ZONE4_N")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "5" smd rect
			(at -10.5 1.75)
			(size 0.55 3.5)
			(layers "B.Cu" "B.Mask")
			(net "ZONE4_C")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "6" smd rect
			(at -9.5 1.75)
			(size 0.55 3.5)
			(layers "B.Cu" "B.Mask")
			(net "ZONE5_24V")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "7" smd rect
			(at -8.5 1.75)
			(size 0.55 3.5)
			(layers "B.Cu" "B.Mask")
			(net "ZONE5_24V")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "8" smd rect
			(at -7.5 1.75)
			(size 0.55 3.5)
			(layers "B.Cu" "B.Mask")
			(net "ZONE5_W")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "9" smd rect
			(at -6.5 1.75)
			(size 0.55 3.5)
			(layers "B.Cu" "B.Mask")
			(net "ZONE5_N")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "10" smd rect
			(at -5.5 1.75)
			(size 0.55 3.5)
			(layers "B.Cu" "B.Mask")
			(net "ZONE5_C")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "11" smd rect
			(at -4.5 1.75)
			(size 0.55 3.5)
			(layers "B.Cu" "B.Mask")
			(net "ZONE6_24V")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "12" smd rect
			(at -3.5 1.75)
			(size 0.55 3.5)
			(layers "B.Cu" "B.Mask")
			(net "ZONE6_24V")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "13" smd rect
			(at -2.5 1.75)
			(size 0.55 3.5)
			(layers "B.Cu" "B.Mask")
			(net "ZONE6_W")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "14" smd rect
			(at -1.5 1.75)
			(size 0.55 3.5)
			(layers "B.Cu" "B.Mask")
			(net "ZONE6_N")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "15" smd rect
			(at -0.5 1.75)
			(size 0.55 3.5)
			(layers "B.Cu" "B.Mask")
			(net "ZONE6_C")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "16" smd rect
			(at 0.5 1.75)
			(size 0.55 3.5)
			(layers "B.Cu" "B.Mask")
			(net "ZONE1_24V")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "17" smd rect
			(at 1.5 1.75)
			(size 0.55 3.5)
			(layers "B.Cu" "B.Mask")
			(net "ZONE1_24V")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "18" smd rect
			(at 2.5 1.75)
			(size 0.55 3.5)
			(layers "B.Cu" "B.Mask")
			(net "ZONE1_W")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "19" smd rect
			(at 3.5 1.75)
			(size 0.55 3.5)
			(layers "B.Cu" "B.Mask")
			(net "ZONE1_N")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "20" smd rect
			(at 4.5 1.75)
			(size 0.55 3.5)
			(layers "B.Cu" "B.Mask")
			(net "ZONE1_C")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "21" smd rect
			(at 5.5 1.75)
			(size 0.55 3.5)
			(layers "B.Cu" "B.Mask")
			(net "ZONE2_24V")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "22" smd rect
			(at 6.5 1.75)
			(size 0.55 3.5)
			(layers "B.Cu" "B.Mask")
			(net "ZONE2_24V")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "23" smd rect
			(at 7.5 1.75)
			(size 0.55 3.5)
			(layers "B.Cu" "B.Mask")
			(net "ZONE2_W")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "24" smd rect
			(at 8.5 1.75)
			(size 0.55 3.5)
			(layers "B.Cu" "B.Mask")
			(net "ZONE2_N")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "25" smd rect
			(at 9.5 1.75)
			(size 0.55 3.5)
			(layers "B.Cu" "B.Mask")
			(net "ZONE2_C")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "26" smd rect
			(at 10.5 1.75)
			(size 0.55 3.5)
			(layers "B.Cu" "B.Mask")
			(net "ZONE3_24V")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "27" smd rect
			(at 11.5 1.75)
			(size 0.55 3.5)
			(layers "B.Cu" "B.Mask")
			(net "ZONE3_24V")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "28" smd rect
			(at 12.5 1.75)
			(size 0.55 3.5)
			(layers "B.Cu" "B.Mask")
			(net "ZONE3_W")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "29" smd rect
			(at 13.5 1.75)
			(size 0.55 3.5)
			(layers "B.Cu" "B.Mask")
			(net "ZONE3_N")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "30" smd rect
			(at 14.5 1.75)
			(size 0.55 3.5)
			(layers "B.Cu" "B.Mask")
			(net "ZONE3_C")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J22_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J22"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z2 S2 TOP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 232.496292 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z2_T23_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 234.52855 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z2_T23_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 240.11726 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z2_T23_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 242.149518 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z2_T23_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J34_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J34"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z3 S4 TOP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 314.138431 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "unconnected-(J34-Pin_1-Pad1)")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 316.170689 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "unconnected-(J34-Pin_2-Pad2)")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 321.759399 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "unconnected-(J34-Pin_3-Pad3)")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 323.791657 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "unconnected-(J34-Pin_4-Pad4)")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J44_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J44"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z4 S4 TOP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 41.997968 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "ZONE4_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 44.030226 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "ZONE4_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 49.618935 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "ZONE4_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 51.651194 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "ZONE4_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J32_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J32"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z3 S2 TOP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 286.924385 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z3_T23_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 288.956643 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z3_T23_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 294.545353 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z3_T23_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 296.577611 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z3_T23_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J53_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J53"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z5 S3 TOP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 82.819037 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z5_T23_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 84.851295 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z5_T23_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 90.440005 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z5_T23_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 92.472263 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z5_T23_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J23_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J23"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z2 S3 TOP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 246.103315 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z2_T23_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 248.135574 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z2_T23_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 253.724283 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z2_T23_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 255.756541 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z2_T23_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J62_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J62"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z6 S2 TOP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 123.640107 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z6_T23_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 125.672365 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z6_T23_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 131.261075 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z6_T23_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 133.293333 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z6_T23_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J24_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J24"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z2 S4 TOP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 259.710339 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "unconnected-(J24-Pin_1-Pad1)")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 261.742597 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "unconnected-(J24-Pin_2-Pad2)")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 267.331306 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "unconnected-(J24-Pin_3-Pad3)")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 269.363564 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "unconnected-(J24-Pin_4-Pad4)")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J63_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J63"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z6 S3 TOP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 137.24713 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z6_T23_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 139.279388 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z6_T23_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 144.868098 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z6_T23_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 146.900356 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z6_T23_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J33_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J33"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z3 S3 TOP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 300.531408 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z3_T23_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 302.563666 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z3_T23_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 308.152376 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z3_T23_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 310.184634 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z3_T23_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J13_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J13"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z1 S3 TOP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 191.675223 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z1_T23_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 193.707481 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z1_T23_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 199.29619 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z1_T23_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 201.328449 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "Z1_T23_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J31_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J31"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z3 S1 TOP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 273.317362 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "ZONE3_24V")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 275.34962 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "ZONE3_W")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 280.93833 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "ZONE3_N")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 282.970588 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "ZONE3_C")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "ELFlex:J61_Solder4"
		(layer "F.Cu")
		(at 20 40)
		(property "Reference" "J61"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z6 S1 TOP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole roundrect
			(at 110.033084 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "unconnected-(J61-Pin_1-Pad1)")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 112.065342 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "unconnected-(J61-Pin_2-Pad2)")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 117.654051 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "unconnected-(J61-Pin_3-Pad3)")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 119.686309 7.2)
			(size 0.9 1)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net "unconnected-(J61-Pin_4-Pad4)")
			(solder_mask_margin -0.05)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(gr_arc
		(start 20 40.15)
		(mid 20.043933 40.043933)
		(end 20.15 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 20 46.25)
		(end 20 40.15)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 20.15 40)
		(end 163.084278 40)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 20.15 46.4)
		(mid 20.043933 46.356066)
		(end 20 46.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 20.326898 46.4)
		(end 20.15 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 20.326898 46.4)
		(mid 20.432965 46.443933)
		(end 20.476898 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 20.476898 47.75)
		(end 20.476898 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 20.626898 47.9)
		(mid 20.520832 47.856066)
		(end 20.476898 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 21.726898 47.9)
		(end 20.626898 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 21.876898 46.55)
		(end 21.876898 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 21.876898 46.55)
		(mid 21.920832 46.443933)
		(end 22.026898 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 21.876898 47.75)
		(mid 21.832964 47.856066)
		(end 21.726898 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 22.359156 46.4)
		(end 22.026898 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 22.359156 46.4)
		(mid 22.46525 46.443918)
		(end 22.509156 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 22.509156 47.75)
		(end 22.509156 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 22.659156 47.9)
		(mid 22.55309 47.856066)
		(end 22.509156 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 23.759156 47.9)
		(end 22.659156 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 23.909156 46.55)
		(end 23.909156 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 23.909156 46.55)
		(mid 23.953087 46.443918)
		(end 24.059156 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 23.909156 47.75)
		(mid 23.865222 47.856066)
		(end 23.759156 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 27.947866 46.4)
		(end 24.059156 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 27.947866 46.4)
		(mid 28.053954 46.443922)
		(end 28.097866 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 28.097866 47.75)
		(end 28.097866 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 28.247866 47.9)
		(mid 28.1418 47.856066)
		(end 28.097866 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 29.347866 47.9)
		(end 28.247866 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 29.497866 46.55)
		(end 29.497866 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 29.497866 46.55)
		(mid 29.541798 46.443922)
		(end 29.647866 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 29.497866 47.75)
		(mid 29.453932 47.856066)
		(end 29.347866 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 29.980124 46.4)
		(end 29.647866 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 29.980124 46.4)
		(mid 30.086175 46.443942)
		(end 30.130124 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 30.130124 47.75)
		(end 30.130124 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 30.280124 47.9)
		(mid 30.174058 47.856066)
		(end 30.130124 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 31.380124 47.9)
		(end 30.280124 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 31.530124 46.55)
		(end 31.530124 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 31.530124 46.55)
		(mid 31.574059 46.443942)
		(end 31.680124 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 31.530124 47.75)
		(mid 31.48619 47.856066)
		(end 31.380124 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 33.933921 46.4)
		(end 31.680124 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 33.933921 46.4)
		(mid 34.039973 46.443941)
		(end 34.083921 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 34.083921 47.75)
		(end 34.083921 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 34.233921 47.9)
		(mid 34.127855 47.856066)
		(end 34.083921 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 35.333921 47.9)
		(end 34.233921 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 35.483921 46.55)
		(end 35.483921 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 35.483921 46.55)
		(mid 35.527856 46.443941)
		(end 35.633921 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 35.483921 47.75)
		(mid 35.439987 47.856066)
		(end 35.333921 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 35.966179 46.4)
		(end 35.633921 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 35.966179 46.4)
		(mid 36.072259 46.443927)
		(end 36.116179 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 36.116179 47.75)
		(end 36.116179 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 36.266179 47.9)
		(mid 36.160113 47.856066)
		(end 36.116179 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 37.366179 47.9)
		(end 36.266179 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 37.516179 46.55)
		(end 37.516179 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 37.516179 46.55)
		(mid 37.560112 46.443927)
		(end 37.666179 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 37.516179 47.75)
		(mid 37.472245 47.856066)
		(end 37.366179 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 41.554889 46.4)
		(end 37.666179 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 41.554889 46.4)
		(mid 41.660962 46.44393)
		(end 41.704889 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 41.704889 47.75)
		(end 41.704889 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 41.854889 47.9)
		(mid 41.748823 47.856066)
		(end 41.704889 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 42.954889 47.9)
		(end 41.854889 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 43.104889 46.55)
		(end 43.104889 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 43.104889 46.55)
		(mid 43.148822 46.44393)
		(end 43.254889 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 43.104889 47.75)
		(mid 43.060955 47.856066)
		(end 42.954889 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 43.587147 46.4)
		(end 43.254889 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 43.587147 46.4)
		(mid 43.693183 46.443951)
		(end 43.737147 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 43.737147 47.75)
		(end 43.737147 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 43.887147 47.9)
		(mid 43.781081 47.856066)
		(end 43.737147 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 44.987147 47.9)
		(end 43.887147 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 45.137147 46.55)
		(end 45.137147 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 45.137147 46.55)
		(mid 45.181084 46.443951)
		(end 45.287147 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 45.137147 47.75)
		(mid 45.093213 47.856066)
		(end 44.987147 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 47.540945 46.4)
		(end 45.287147 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 47.540945 46.4)
		(mid 47.646982 46.44395)
		(end 47.690945 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 47.690945 47.75)
		(end 47.690945 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 47.840945 47.9)
		(mid 47.734879 47.856066)
		(end 47.690945 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 48.940945 47.9)
		(end 47.840945 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 49.090945 46.55)
		(end 49.090945 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 49.090945 46.55)
		(mid 49.134882 46.44395)
		(end 49.240945 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 49.090945 47.75)
		(mid 49.047011 47.856066)
		(end 48.940945 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 49.573203 46.4)
		(end 49.240945 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 49.573203 46.4)
		(mid 49.679267 46.443935)
		(end 49.723203 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 49.723203 47.75)
		(end 49.723203 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 49.873203 47.9)
		(mid 49.767137 47.856066)
		(end 49.723203 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 50.973203 47.9)
		(end 49.873203 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 51.123203 46.55)
		(end 51.123203 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 51.123203 46.55)
		(mid 51.167137 46.443935)
		(end 51.273203 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 51.123203 47.75)
		(mid 51.079269 47.856066)
		(end 50.973203 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 55.161912 46.4)
		(end 51.273203 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 55.161912 46.4)
		(mid 55.26797 46.443938)
		(end 55.311912 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 55.311912 47.75)
		(end 55.311912 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 55.461912 47.9)
		(mid 55.355846 47.856066)
		(end 55.311912 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 56.561912 47.9)
		(end 55.461912 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 56.711912 46.55)
		(end 56.711912 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 56.711912 46.55)
		(mid 56.755847 46.443938)
		(end 56.861912 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 56.711912 47.75)
		(mid 56.667978 47.856066)
		(end 56.561912 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 57.19417 46.4)
		(end 56.861912 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 57.19417 46.4)
		(mid 57.300255 46.443923)
		(end 57.34417 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 57.34417 47.75)
		(end 57.34417 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 57.49417 47.9)
		(mid 57.388104 47.856066)
		(end 57.34417 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 58.59417 47.9)
		(end 57.49417 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 58.74417 46.55)
		(end 58.74417 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 58.74417 46.55)
		(mid 58.788102 46.443923)
		(end 58.89417 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 58.74417 47.75)
		(mid 58.700236 47.856066)
		(end 58.59417 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 61.147968 46.4)
		(end 58.89417 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 61.147968 46.4)
		(mid 61.254055 46.443923)
		(end 61.297968 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 61.297968 47.75)
		(end 61.297968 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 61.447968 47.9)
		(mid 61.341902 47.856066)
		(end 61.297968 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 62.547968 47.9)
		(end 61.447968 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 62.697968 46.55)
		(end 62.697968 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 62.697968 46.55)
		(mid 62.7419 46.443923)
		(end 62.847968 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 62.697968 47.75)
		(mid 62.654034 47.856066)
		(end 62.547968 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 63.180226 46.4)
		(end 62.847968 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 63.180226 46.4)
		(mid 63.286275 46.443943)
		(end 63.330226 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 63.330226 47.75)
		(end 63.330226 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 63.480226 47.9)
		(mid 63.37416 47.856066)
		(end 63.330226 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 64.580226 47.9)
		(end 63.480226 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 64.730226 46.55)
		(end 64.730226 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 64.730226 46.55)
		(mid 64.774162 46.443943)
		(end 64.880226 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 64.730226 47.75)
		(mid 64.686292 47.856066)
		(end 64.580226 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 68.768935 46.4)
		(end 64.880226 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 68.768935 46.4)
		(mid 68.874978 46.443946)
		(end 68.918935 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 68.918935 47.75)
		(end 68.918935 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 69.068935 47.9)
		(mid 68.962869 47.856066)
		(end 68.918935 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 70.168935 47.9)
		(end 69.068935 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 70.318935 46.55)
		(end 70.318935 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 70.318935 46.55)
		(mid 70.362871 46.443946)
		(end 70.468935 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 70.318935 47.75)
		(mid 70.275001 47.856066)
		(end 70.168935 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 70.801194 46.4)
		(end 70.468935 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 70.801194 46.4)
		(mid 70.907264 46.443932)
		(end 70.951194 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 70.951194 47.75)
		(end 70.951194 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 71.101194 47.9)
		(mid 70.995128 47.856066)
		(end 70.951194 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 72.201194 47.9)
		(end 71.101194 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 72.351194 46.55)
		(end 72.351194 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 72.351194 46.55)
		(mid 72.395128 46.443932)
		(end 72.501194 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 72.351194 47.75)
		(mid 72.30726 47.856066)
		(end 72.201194 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 74.754991 46.4)
		(end 72.501194 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 74.754991 46.4)
		(mid 74.861063 46.443931)
		(end 74.904991 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 74.904991 47.75)
		(end 74.904991 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 75.054991 47.9)
		(mid 74.948925 47.856066)
		(end 74.904991 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 76.154991 47.9)
		(end 75.054991 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 76.304991 46.55)
		(end 76.304991 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 76.304991 46.55)
		(mid 76.348924 46.443931)
		(end 76.454991 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 76.304991 47.75)
		(mid 76.261057 47.856066)
		(end 76.154991 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 76.787249 46.4)
		(end 76.454991 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 76.787249 46.4)
		(mid 76.893348 46.443916)
		(end 76.937249 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 76.937249 47.75)
		(end 76.937249 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 77.087249 47.9)
		(mid 76.981183 47.856066)
		(end 76.937249 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 78.187249 47.9)
		(end 77.087249 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 78.337249 46.55)
		(end 78.337249 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 78.337249 46.55)
		(mid 78.381186 46.443951)
		(end 78.487249 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 78.337249 47.75)
		(mid 78.293315 47.856066)
		(end 78.187249 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.375959 46.4)
		(end 78.487249 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 82.375959 46.4)
		(mid 82.482052 46.443919)
		(end 82.525959 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.525959 47.75)
		(end 82.525959 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 82.675959 47.9)
		(mid 82.569893 47.856066)
		(end 82.525959 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 83.775959 47.9)
		(end 82.675959 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 83.925959 46.55)
		(end 83.925959 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 83.925959 46.55)
		(mid 83.96989 46.443919)
		(end 84.075959 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 83.925959 47.75)
		(mid 83.882025 47.856066)
		(end 83.775959 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 84.408217 46.4)
		(end 84.075959 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 84.408217 46.4)
		(mid 84.514272 46.44394)
		(end 84.558217 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 84.558217 47.75)
		(end 84.558217 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 84.708217 47.9)
		(mid 84.602151 47.856066)
		(end 84.558217 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 85.808217 47.9)
		(end 84.708217 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 85.958217 46.55)
		(end 85.958217 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 85.958217 46.55)
		(mid 86.002152 46.44394)
		(end 86.108217 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 85.958217 47.75)
		(mid 85.914283 47.856066)
		(end 85.808217 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 88.362014 46.4)
		(end 86.108217 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 88.362014 46.4)
		(mid 88.468071 46.443939)
		(end 88.512014 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 88.512014 47.75)
		(end 88.512014 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 88.662014 47.9)
		(mid 88.555948 47.856066)
		(end 88.512014 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 89.762014 47.9)
		(end 88.662014 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 89.912014 46.55)
		(end 89.912014 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 89.912014 46.55)
		(mid 89.955949 46.443939)
		(end 90.062014 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 89.912014 47.75)
		(mid 89.86808 47.856066)
		(end 89.762014 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 90.394272 46.4)
		(end 90.062014 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 90.394272 46.4)
		(mid 90.500356 46.443924)
		(end 90.544272 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 90.544272 47.75)
		(end 90.544272 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 90.694272 47.9)
		(mid 90.588206 47.856066)
		(end 90.544272 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 91.794272 47.9)
		(end 90.694272 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 91.944272 46.55)
		(end 91.944272 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 91.944272 46.55)
		(mid 91.988204 46.443924)
		(end 92.094272 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 91.944272 47.75)
		(mid 91.900338 47.856066)
		(end 91.794272 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 95.982982 46.4)
		(end 92.094272 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 95.982982 46.4)
		(mid 96.08906 46.443928)
		(end 96.132982 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 96.132982 47.75)
		(end 96.132982 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 96.282982 47.9)
		(mid 96.176916 47.856066)
		(end 96.132982 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.382982 47.9)
		(end 96.282982 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.532982 46.55)
		(end 97.532982 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 97.532982 46.55)
		(mid 97.576915 46.443928)
		(end 97.682982 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 97.532982 47.75)
		(mid 97.489048 47.856066)
		(end 97.382982 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.01524 46.4)
		(end 97.682982 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 98.01524 46.4)
		(mid 98.12128 46.443948)
		(end 98.16524 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.16524 47.75)
		(end 98.16524 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 98.31524 47.9)
		(mid 98.209174 47.856066)
		(end 98.16524 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 99.41524 47.9)
		(end 98.31524 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 99.56524 46.55)
		(end 99.56524 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 99.56524 46.55)
		(mid 99.609176 46.443948)
		(end 99.71524 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 99.56524 47.75)
		(mid 99.521306 47.856066)
		(end 99.41524 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 101.969037 46.4)
		(end 99.71524 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 101.969037 46.4)
		(mid 102.075079 46.443947)
		(end 102.119037 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 102.119037 47.75)
		(end 102.119037 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 102.269037 47.9)
		(mid 102.162971 47.856066)
		(end 102.119037 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 103.369037 47.9)
		(end 102.269037 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 103.519037 46.55)
		(end 103.519037 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 103.519037 46.55)
		(mid 103.562973 46.443947)
		(end 103.669037 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 103.519037 47.75)
		(mid 103.475103 47.856066)
		(end 103.369037 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 104.001295 46.4)
		(end 103.669037 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 104.001295 46.4)
		(mid 104.107364 46.443932)
		(end 104.151295 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 104.151295 47.75)
		(end 104.151295 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 104.301295 47.9)
		(mid 104.195229 47.856066)
		(end 104.151295 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 105.401295 47.9)
		(end 104.301295 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 105.551295 46.55)
		(end 105.551295 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 105.551295 46.55)
		(mid 105.595229 46.443932)
		(end 105.701295 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 105.551295 47.75)
		(mid 105.507361 47.856066)
		(end 105.401295 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 109.590005 46.4)
		(end 105.701295 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 109.590005 46.4)
		(mid 109.696068 46.443936)
		(end 109.740005 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 109.740005 47.75)
		(end 109.740005 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 109.890005 47.9)
		(mid 109.783939 47.856066)
		(end 109.740005 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 110.990005 47.9)
		(end 109.890005 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.140005 46.55)
		(end 111.140005 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 111.140005 46.55)
		(mid 111.183939 46.443936)
		(end 111.290005 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 111.140005 47.75)
		(mid 111.096071 47.856066)
		(end 110.990005 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.622263 46.4)
		(end 111.290005 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 111.622263 46.4)
		(mid 111.728353 46.443921)
		(end 111.772263 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.772263 47.75)
		(end 111.772263 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 111.922263 47.9)
		(mid 111.816197 47.856066)
		(end 111.772263 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 113.022263 47.9)
		(end 111.922263 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 113.172263 46.55)
		(end 113.172263 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 113.172263 46.55)
		(mid 113.216195 46.443921)
		(end 113.322263 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 113.172263 47.75)
		(mid 113.128329 47.856066)
		(end 113.022263 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 115.57606 46.4)
		(end 113.322263 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 115.57606 46.4)
		(mid 115.682152 46.44392)
		(end 115.72606 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 115.72606 47.75)
		(end 115.72606 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 115.87606 47.9)
		(mid 115.769994 47.856066)
		(end 115.72606 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 116.97606 47.9)
		(end 115.87606 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 117.12606 46.55)
		(end 117.12606 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 117.12606 46.55)
		(mid 117.169992 46.44392)
		(end 117.27606 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 117.12606 47.75)
		(mid 117.082126 47.856066)
		(end 116.97606 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 117.608319 46.4)
		(end 117.27606 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 117.608319 46.4)
		(mid 117.714373 46.443941)
		(end 117.758319 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 117.758319 47.75)
		(end 117.758319 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 117.908319 47.9)
		(mid 117.802253 47.856066)
		(end 117.758319 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 119.008319 47.9)
		(end 117.908319 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 119.158319 46.55)
		(end 119.158319 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 119.158319 46.55)
		(mid 119.202254 46.443941)
		(end 119.308319 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 119.158319 47.75)
		(mid 119.114385 47.856066)
		(end 119.008319 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.197028 46.4)
		(end 119.308319 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 123.197028 46.4)
		(mid 123.303076 46.443944)
		(end 123.347028 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.347028 47.75)
		(end 123.347028 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 123.497028 47.9)
		(mid 123.390962 47.856066)
		(end 123.347028 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 124.597028 47.9)
		(end 123.497028 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 124.747028 46.55)
		(end 124.747028 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 124.747028 46.55)
		(mid 124.790964 46.443944)
		(end 124.897028 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 124.747028 47.75)
		(mid 124.703094 47.856066)
		(end 124.597028 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 125.229286 46.4)
		(end 124.897028 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 125.229286 46.4)
		(mid 125.335361 46.443929)
		(end 125.379286 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 125.379286 47.75)
		(end 125.379286 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 125.529286 47.9)
		(mid 125.42322 47.856066)
		(end 125.379286 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 126.629286 47.9)
		(end 125.529286 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 126.779286 46.55)
		(end 126.779286 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 126.779286 46.55)
		(mid 126.823219 46.443929)
		(end 126.929286 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 126.779286 47.75)
		(mid 126.735352 47.856066)
		(end 126.629286 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 129.183084 46.4)
		(end 126.929286 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 129.183084 46.4)
		(mid 129.28916 46.443928)
		(end 129.333084 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 129.333084 47.75)
		(end 129.333084 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 129.483084 47.9)
		(mid 129.377018 47.856066)
		(end 129.333084 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 130.583084 47.9)
		(end 129.483084 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 130.733084 46.55)
		(end 130.733084 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 130.733084 46.55)
		(mid 130.777017 46.443928)
		(end 130.883084 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 130.733084 47.75)
		(mid 130.68915 47.856066)
		(end 130.583084 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 131.215342 46.4)
		(end 130.883084 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 131.215342 46.4)
		(mid 131.321381 46.443949)
		(end 131.365342 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 131.365342 47.75)
		(end 131.365342 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 131.515342 47.9)
		(mid 131.409276 47.856066)
		(end 131.365342 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 132.615342 47.9)
		(end 131.515342 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 132.765342 46.55)
		(end 132.765342 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 132.765342 46.55)
		(mid 132.809279 46.443949)
		(end 132.915342 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 132.765342 47.75)
		(mid 132.721408 47.856066)
		(end 132.615342 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 136.804051 46.4)
		(end 132.915342 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 136.804051 46.4)
		(mid 136.910149 46.443917)
		(end 136.954051 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 136.954051 47.75)
		(end 136.954051 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 137.104051 47.9)
		(mid 136.997985 47.856066)
		(end 136.954051 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.204051 47.9)
		(end 137.104051 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.354051 46.55)
		(end 138.354051 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 138.354051 46.55)
		(mid 138.397988 46.443952)
		(end 138.504051 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 138.354051 47.75)
		(mid 138.310117 47.856066)
		(end 138.204051 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.836309 46.4)
		(end 138.504051 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 138.836309 46.4)
		(mid 138.942369 46.443937)
		(end 138.986309 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.986309 47.75)
		(end 138.986309 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 139.136309 47.9)
		(mid 139.030243 47.856066)
		(end 138.986309 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 140.236309 47.9)
		(end 139.136309 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 140.386309 46.55)
		(end 140.386309 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 140.386309 46.55)
		(mid 140.430244 46.443937)
		(end 140.536309 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 140.386309 47.75)
		(mid 140.342375 47.856066)
		(end 140.236309 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.790107 46.4)
		(end 140.536309 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 142.790107 46.4)
		(mid 142.896168 46.443936)
		(end 142.940107 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.940107 47.75)
		(end 142.940107 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 143.090107 47.9)
		(mid 142.984041 47.856066)
		(end 142.940107 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.190107 47.9)
		(end 143.090107 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.340107 46.55)
		(end 144.340107 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 144.340107 46.55)
		(mid 144.384041 46.443936)
		(end 144.490107 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 144.340107 47.75)
		(mid 144.296173 47.856066)
		(end 144.190107 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.822365 46.4)
		(end 144.490107 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 144.822365 46.4)
		(mid 144.928454 46.443922)
		(end 144.972365 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.972365 47.75)
		(end 144.972365 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 145.122365 47.9)
		(mid 145.016299 47.856066)
		(end 144.972365 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 146.222365 47.9)
		(end 145.122365 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 146.372365 46.55)
		(end 146.372365 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 146.372365 46.55)
		(mid 146.416297 46.443922)
		(end 146.522365 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 146.372365 47.75)
		(mid 146.328431 47.856066)
		(end 146.222365 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150.411075 46.4)
		(end 146.522365 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 150.411075 46.4)
		(mid 150.517157 46.443925)
		(end 150.561075 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150.561075 47.75)
		(end 150.561075 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 150.711075 47.9)
		(mid 150.605009 47.856066)
		(end 150.561075 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 151.811075 47.9)
		(end 150.711075 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 151.961075 46.55)
		(end 151.961075 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 151.961075 46.55)
		(mid 152.005007 46.443925)
		(end 152.111075 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 151.961075 47.75)
		(mid 151.917141 47.856066)
		(end 151.811075 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 152.443333 46.4)
		(end 152.111075 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 152.443333 46.4)
		(mid 152.549378 46.443946)
		(end 152.593333 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 152.593333 47.75)
		(end 152.593333 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 152.743333 47.9)
		(mid 152.637267 47.856066)
		(end 152.593333 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.843333 47.9)
		(end 152.743333 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.993333 46.55)
		(end 153.993333 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 153.993333 46.55)
		(mid 154.037269 46.443946)
		(end 154.143333 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 153.993333 47.75)
		(mid 153.949399 47.856066)
		(end 153.843333 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 156.39713 46.4)
		(end 154.143333 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 156.39713 46.4)
		(mid 156.503177 46.443945)
		(end 156.54713 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 156.54713 47.75)
		(end 156.54713 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 156.69713 47.9)
		(mid 156.591064 47.856066)
		(end 156.54713 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.79713 47.9)
		(end 156.69713 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.94713 46.55)
		(end 157.94713 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 157.94713 46.55)
		(mid 157.991066 46.443945)
		(end 158.09713 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 157.94713 47.75)
		(mid 157.903196 47.856066)
		(end 157.79713 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.429388 46.4)
		(end 158.09713 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 158.429388 46.4)
		(mid 158.535462 46.44393)
		(end 158.579388 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.579388 47.75)
		(end 158.579388 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 158.729388 47.9)
		(mid 158.623322 47.856066)
		(end 158.579388 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 159.829388 47.9)
		(end 158.729388 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 159.979388 46.55)
		(end 159.979388 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 159.979388 46.55)
		(mid 160.023321 46.44393)
		(end 160.129388 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 159.979388 47.75)
		(mid 159.935454 47.856066)
		(end 159.829388 47.9)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 163.234278 33.123105)
		(mid 163.24177 33.000922)
		(end 163.264135 32.88057)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 163.234278 35)
		(end 163.234278 33.123105)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 163.234278 39.85)
		(mid 163.190343 39.956058)
		(end 163.084278 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 163.234278 39.85)
		(end 163.234278 35)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 163.264135 32.88057)
		(end 166.95442 18.119429)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 164.018098 46.4)
		(end 160.129388 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 164.018098 46.4)
		(mid 164.124165 46.443933)
		(end 164.168098 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 164.168098 47.75)
		(end 164.168098 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 164.318098 47.9)
		(mid 164.212032 47.856066)
		(end 164.168098 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 165.418098 47.9)
		(end 164.318098 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 165.568098 46.55)
		(end 165.568098 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 165.568098 46.55)
		(mid 165.612032 46.443933)
		(end 165.718098 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 165.568098 47.75)
		(mid 165.524164 47.856066)
		(end 165.418098 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 166.050356 46.4)
		(end 165.718098 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 166.050356 46.4)
		(mid 166.15645 46.443918)
		(end 166.200356 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 166.200356 47.75)
		(end 166.200356 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 166.350356 47.9)
		(mid 166.24429 47.856066)
		(end 166.200356 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 166.984278 5.3)
		(mid 167.072146 5.087867)
		(end 167.284278 5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 166.984278 17.876894)
		(mid 166.976787 17.999077)
		(end 166.95442 18.119429)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 166.984278 17.876894)
		(end 166.984278 5.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.284278 5)
		(end 197.684278 5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.450356 47.9)
		(end 166.350356 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.600356 46.55)
		(end 167.600356 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 167.600356 46.55)
		(mid 167.644287 46.443918)
		(end 167.750356 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 167.600356 47.75)
		(mid 167.556422 47.856066)
		(end 167.450356 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.004153 46.4)
		(end 167.750356 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 170.004153 46.4)
		(mid 170.110249 46.443917)
		(end 170.154153 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.154153 47.75)
		(end 170.154153 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 170.304153 47.9)
		(mid 170.198087 47.856066)
		(end 170.154153 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 171.404153 47.9)
		(end 170.304153 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 171.554153 46.55)
		(end 171.554153 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 171.554153 46.55)
		(mid 171.598084 46.443917)
		(end 171.704153 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 171.554153 47.75)
		(mid 171.510219 47.856066)
		(end 171.404153 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.036411 46.4)
		(end 171.704153 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 172.036411 46.4)
		(mid 172.14247 46.443938)
		(end 172.186411 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.186411 47.75)
		(end 172.186411 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 172.336411 47.9)
		(mid 172.230345 47.856066)
		(end 172.186411 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.436411 47.9)
		(end 172.336411 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.586411 46.55)
		(end 173.586411 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 173.586411 46.55)
		(mid 173.630346 46.443938)
		(end 173.736411 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 173.586411 47.75)
		(mid 173.542477 47.856066)
		(end 173.436411 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.625121 46.4)
		(end 173.736411 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 177.625121 46.4)
		(mid 177.731173 46.443941)
		(end 177.775121 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.775121 47.75)
		(end 177.775121 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 177.925121 47.9)
		(mid 177.819055 47.856066)
		(end 177.775121 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 179.025121 47.9)
		(end 177.925121 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 179.175121 46.55)
		(end 179.175121 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 179.175121 46.55)
		(mid 179.219056 46.443941)
		(end 179.325121 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 179.175121 47.75)
		(mid 179.131187 47.856066)
		(end 179.025121 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 179.657379 46.4)
		(end 179.325121 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 179.657379 46.4)
		(mid 179.763459 46.443927)
		(end 179.807379 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 179.807379 47.75)
		(end 179.807379 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 179.957379 47.9)
		(mid 179.851313 47.856066)
		(end 179.807379 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 181.057379 47.9)
		(end 179.957379 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 181.207379 46.55)
		(end 181.207379 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 181.207379 46.55)
		(mid 181.251312 46.443927)
		(end 181.357379 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 181.207379 47.75)
		(mid 181.163445 47.856066)
		(end 181.057379 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 183.611176 46.4)
		(end 181.357379 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 183.611176 46.4)
		(mid 183.717258 46.443925)
		(end 183.761176 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 183.761176 47.75)
		(end 183.761176 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 183.911176 47.9)
		(mid 183.80511 47.856066)
		(end 183.761176 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.011176 47.9)
		(end 183.911176 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.161176 46.55)
		(end 185.161176 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 185.161176 46.55)
		(mid 185.205109 46.443925)
		(end 185.311176 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 185.161176 47.75)
		(mid 185.117242 47.856066)
		(end 185.011176 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.643434 46.4)
		(end 185.311176 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 185.643434 46.4)
		(mid 185.749478 46.443946)
		(end 185.793434 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.793434 47.75)
		(end 185.793434 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 185.943434 47.9)
		(mid 185.837368 47.856066)
		(end 185.793434 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 187.043434 47.9)
		(end 185.943434 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 187.193434 46.55)
		(end 187.193434 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 187.193434 46.55)
		(mid 187.23737 46.443946)
		(end 187.343434 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 187.193434 47.75)
		(mid 187.1495 47.856066)
		(end 187.043434 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 191.232144 46.4)
		(end 187.343434 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 191.232144 46.4)
		(mid 191.338182 46.44395)
		(end 191.382144 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 191.382144 47.75)
		(end 191.382144 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 191.532144 47.9)
		(mid 191.426078 47.856066)
		(end 191.382144 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.632144 47.9)
		(end 191.532144 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.782144 46.55)
		(end 192.782144 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 192.782144 46.55)
		(mid 192.826081 46.44395)
		(end 192.932144 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 192.782144 47.75)
		(mid 192.73821 47.856066)
		(end 192.632144 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 193.264402 46.4)
		(end 192.932144 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 193.264402 46.4)
		(mid 193.370467 46.443935)
		(end 193.414402 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 193.414402 47.75)
		(end 193.414402 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 193.564402 47.9)
		(mid 193.458336 47.856066)
		(end 193.414402 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 194.664402 47.9)
		(end 193.564402 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 194.814402 46.55)
		(end 194.814402 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 194.814402 46.55)
		(mid 194.858336 46.443935)
		(end 194.964402 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 194.814402 47.75)
		(mid 194.770468 47.856066)
		(end 194.664402 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 197.2182 46.4)
		(end 194.964402 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 197.2182 46.4)
		(mid 197.324266 46.443934)
		(end 197.3682 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 197.3682 47.75)
		(end 197.3682 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 197.5182 47.9)
		(mid 197.412134 47.856066)
		(end 197.3682 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 197.684278 5)
		(mid 197.89641 5.087867)
		(end 197.984278 5.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 197.984278 5.3)
		(end 197.984278 17.876894)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 198.014135 18.119429)
		(mid 197.991769 17.999077)
		(end 197.984278 17.876894)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.014135 18.119429)
		(end 201.70442 32.88057)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.6182 47.9)
		(end 197.5182 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.7682 46.55)
		(end 198.7682 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 198.7682 46.55)
		(mid 198.812134 46.443934)
		(end 198.9182 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 198.7682 47.75)
		(mid 198.724266 47.856066)
		(end 198.6182 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.250458 46.4)
		(end 198.9182 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 199.250458 46.4)
		(mid 199.356551 46.443919)
		(end 199.400458 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.400458 47.75)
		(end 199.400458 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 199.550458 47.9)
		(mid 199.444392 47.856066)
		(end 199.400458 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 200.650458 47.9)
		(end 199.550458 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 200.800458 46.55)
		(end 200.800458 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 200.800458 46.55)
		(mid 200.844389 46.443919)
		(end 200.950458 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 200.800458 47.75)
		(mid 200.756524 47.856066)
		(end 200.650458 47.9)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 201.70442 32.88057)
		(mid 201.726785 33.000922)
		(end 201.734278 33.123105)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 201.734278 33.123105)
		(end 201.734278 35)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 201.734278 35)
		(end 201.734278 39.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 201.884278 40)
		(mid 201.778226 39.956058)
		(end 201.734278 39.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 201.884278 40)
		(end 344.818556 40)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 204.839167 46.4)
		(end 200.950458 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 204.839167 46.4)
		(mid 204.945254 46.443922)
		(end 204.989167 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 204.989167 47.75)
		(end 204.989167 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 205.139167 47.9)
		(mid 205.033101 47.856066)
		(end 204.989167 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 206.239167 47.9)
		(end 205.139167 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 206.389167 46.55)
		(end 206.389167 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 206.389167 46.55)
		(mid 206.433099 46.443922)
		(end 206.539167 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 206.389167 47.75)
		(mid 206.345233 47.856066)
		(end 206.239167 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 206.871425 46.4)
		(end 206.539167 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 206.871425 46.4)
		(mid 206.977475 46.443943)
		(end 207.021425 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 207.021425 47.75)
		(end 207.021425 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 207.171425 47.9)
		(mid 207.065359 47.856066)
		(end 207.021425 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 208.271425 47.9)
		(end 207.171425 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 208.421425 46.55)
		(end 208.421425 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 208.421425 46.55)
		(mid 208.46536 46.443943)
		(end 208.571425 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 208.421425 47.75)
		(mid 208.377491 47.856066)
		(end 208.271425 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 210.825223 46.4)
		(end 208.571425 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 210.825223 46.4)
		(mid 210.931274 46.443942)
		(end 210.975223 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 210.975223 47.75)
		(end 210.975223 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 211.125223 47.9)
		(mid 211.019157 47.856066)
		(end 210.975223 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 212.225223 47.9)
		(end 211.125223 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 212.375223 46.55)
		(end 212.375223 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 212.375223 46.55)
		(mid 212.419158 46.443942)
		(end 212.525223 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 212.375223 47.75)
		(mid 212.331289 47.856066)
		(end 212.225223 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 212.857481 46.4)
		(end 212.525223 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 212.857481 46.4)
		(mid 212.963559 46.443927)
		(end 213.007481 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 213.007481 47.75)
		(end 213.007481 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 213.157481 47.9)
		(mid 213.051415 47.856066)
		(end 213.007481 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.257481 47.9)
		(end 213.157481 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.407481 46.55)
		(end 214.407481 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 214.407481 46.55)
		(mid 214.451414 46.443927)
		(end 214.557481 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 214.407481 47.75)
		(mid 214.363547 47.856066)
		(end 214.257481 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 218.44619 46.4)
		(end 214.557481 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 218.44619 46.4)
		(mid 218.552262 46.44393)
		(end 218.59619 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 218.59619 47.75)
		(end 218.59619 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 218.74619 47.9)
		(mid 218.640124 47.856066)
		(end 218.59619 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 219.84619 47.9)
		(end 218.74619 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 219.99619 46.55)
		(end 219.99619 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 219.99619 46.55)
		(mid 220.040123 46.44393)
		(end 220.14619 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 219.99619 47.75)
		(mid 219.952256 47.856066)
		(end 219.84619 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 220.478449 46.4)
		(end 220.14619 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 220.478449 46.4)
		(mid 220.584548 46.443916)
		(end 220.628449 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 220.628449 47.75)
		(end 220.628449 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 220.778449 47.9)
		(mid 220.672383 47.856066)
		(end 220.628449 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 221.878449 47.9)
		(end 220.778449 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 222.028449 46.55)
		(end 222.028449 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 222.028449 46.55)
		(mid 222.072386 46.443951)
		(end 222.178449 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 222.028449 47.75)
		(mid 221.984515 47.856066)
		(end 221.878449 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 224.432246 46.4)
		(end 222.178449 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 224.432246 46.4)
		(mid 224.538282 46.44395)
		(end 224.582246 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 224.582246 47.75)
		(end 224.582246 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 224.732246 47.9)
		(mid 224.62618 47.856066)
		(end 224.582246 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 225.832246 47.9)
		(end 224.732246 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 225.982246 46.55)
		(end 225.982246 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 225.982246 46.55)
		(mid 226.026183 46.44395)
		(end 226.132246 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 225.982246 47.75)
		(mid 225.938312 47.856066)
		(end 225.832246 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 226.464504 46.4)
		(end 226.132246 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 226.464504 46.4)
		(mid 226.570567 46.443935)
		(end 226.614504 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 226.614504 47.75)
		(end 226.614504 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 226.764504 47.9)
		(mid 226.658438 47.856066)
		(end 226.614504 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 227.864504 47.9)
		(end 226.764504 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 228.014504 46.55)
		(end 228.014504 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 228.014504 46.55)
		(mid 228.058438 46.443935)
		(end 228.164504 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 228.014504 47.75)
		(mid 227.97057 47.856066)
		(end 227.864504 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 232.053214 46.4)
		(end 228.164504 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 232.053214 46.4)
		(mid 232.159271 46.443939)
		(end 232.203214 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 232.203214 47.75)
		(end 232.203214 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 232.353214 47.9)
		(mid 232.247148 47.856066)
		(end 232.203214 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 233.453214 47.9)
		(end 232.353214 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 233.603214 46.55)
		(end 233.603214 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 233.603214 46.55)
		(mid 233.647149 46.443939)
		(end 233.753214 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 233.603214 47.75)
		(mid 233.55928 47.856066)
		(end 233.453214 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 234.085472 46.4)
		(end 233.753214 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 234.085472 46.4)
		(mid 234.191556 46.443924)
		(end 234.235472 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 234.235472 47.75)
		(end 234.235472 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 234.385472 47.9)
		(mid 234.279406 47.856066)
		(end 234.235472 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 235.485472 47.9)
		(end 234.385472 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 235.635472 46.55)
		(end 235.635472 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 235.635472 46.55)
		(mid 235.679404 46.443924)
		(end 235.785472 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 235.635472 47.75)
		(mid 235.591538 47.856066)
		(end 235.485472 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 238.039269 46.4)
		(end 235.785472 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 238.039269 46.4)
		(mid 238.145355 46.443923)
		(end 238.189269 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 238.189269 47.75)
		(end 238.189269 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 238.339269 47.9)
		(mid 238.233203 47.856066)
		(end 238.189269 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 239.439269 47.9)
		(end 238.339269 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 239.589269 46.55)
		(end 239.589269 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 239.589269 46.55)
		(mid 239.633201 46.443923)
		(end 239.739269 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 239.589269 47.75)
		(mid 239.545335 47.856066)
		(end 239.439269 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 240.071527 46.4)
		(end 239.739269 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 240.071527 46.4)
		(mid 240.177576 46.443944)
		(end 240.221527 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 240.221527 47.75)
		(end 240.221527 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 240.371527 47.9)
		(mid 240.265461 47.856066)
		(end 240.221527 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 241.471527 47.9)
		(end 240.371527 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 241.621527 46.55)
		(end 241.621527 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 241.621527 46.55)
		(mid 241.665463 46.443944)
		(end 241.771527 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 241.621527 47.75)
		(mid 241.577593 47.856066)
		(end 241.471527 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 245.660237 46.4)
		(end 241.771527 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 245.660237 46.4)
		(mid 245.766279 46.443947)
		(end 245.810237 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 245.810237 47.75)
		(end 245.810237 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 245.960237 47.9)
		(mid 245.854171 47.856066)
		(end 245.810237 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 247.060237 47.9)
		(end 245.960237 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 247.210237 46.55)
		(end 247.210237 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 247.210237 46.55)
		(mid 247.254173 46.443947)
		(end 247.360237 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 247.210237 47.75)
		(mid 247.166303 47.856066)
		(end 247.060237 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 247.692495 46.4)
		(end 247.360237 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 247.692495 46.4)
		(mid 247.798564 46.443932)
		(end 247.842495 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 247.842495 47.75)
		(end 247.842495 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 247.992495 47.9)
		(mid 247.886429 47.856066)
		(end 247.842495 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 249.092495 47.9)
		(end 247.992495 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 249.242495 46.55)
		(end 249.242495 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 249.242495 46.55)
		(mid 249.286429 46.443932)
		(end 249.392495 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 249.242495 47.75)
		(mid 249.198561 47.856066)
		(end 249.092495 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 251.646292 46.4)
		(end 249.392495 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 251.646292 46.4)
		(mid 251.752363 46.443931)
		(end 251.796292 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 251.796292 47.75)
		(end 251.796292 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 251.946292 47.9)
		(mid 251.840226 47.856066)
		(end 251.796292 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 253.046292 47.9)
		(end 251.946292 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 253.196292 46.55)
		(end 253.196292 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 253.196292 46.55)
		(mid 253.240225 46.443931)
		(end 253.346292 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 253.196292 47.75)
		(mid 253.152358 47.856066)
		(end 253.046292 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 253.67855 46.4)
		(end 253.346292 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 253.67855 46.4)
		(mid 253.784648 46.443916)
		(end 253.82855 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 253.82855 47.75)
		(end 253.82855 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 253.97855 47.9)
		(mid 253.872484 47.856066)
		(end 253.82855 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 255.07855 47.9)
		(end 253.97855 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 255.22855 46.55)
		(end 255.22855 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 255.22855 46.55)
		(mid 255.272487 46.443952)
		(end 255.37855 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 255.22855 47.75)
		(mid 255.184616 47.856066)
		(end 255.07855 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 259.26726 46.4)
		(end 255.37855 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 259.26726 46.4)
		(mid 259.373352 46.44392)
		(end 259.41726 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 259.41726 47.75)
		(end 259.41726 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 259.56726 47.9)
		(mid 259.461194 47.856066)
		(end 259.41726 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 260.66726 47.9)
		(end 259.56726 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 260.81726 46.55)
		(end 260.81726 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 260.81726 46.55)
		(mid 260.861192 46.44392)
		(end 260.96726 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 260.81726 47.75)
		(mid 260.773326 47.856066)
		(end 260.66726 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 261.299518 46.4)
		(end 260.96726 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 261.299518 46.4)
		(mid 261.405572 46.44394)
		(end 261.449518 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 261.449518 47.75)
		(end 261.449518 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 261.599518 47.9)
		(mid 261.493452 47.856066)
		(end 261.449518 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 262.699518 47.9)
		(end 261.599518 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 262.849518 46.55)
		(end 262.849518 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 262.849518 46.55)
		(mid 262.893453 46.44394)
		(end 262.999518 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 262.849518 47.75)
		(mid 262.805584 47.856066)
		(end 262.699518 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 265.253315 46.4)
		(end 262.999518 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 265.253315 46.4)
		(mid 265.359371 46.443939)
		(end 265.403315 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 265.403315 47.75)
		(end 265.403315 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 265.553315 47.9)
		(mid 265.447249 47.856066)
		(end 265.403315 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 266.653315 47.9)
		(end 265.553315 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 266.803315 46.55)
		(end 266.803315 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 266.803315 46.55)
		(mid 266.84725 46.443939)
		(end 266.953315 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 266.803315 47.75)
		(mid 266.759381 47.856066)
		(end 266.653315 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 267.285574 46.4)
		(end 266.953315 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 267.285574 46.4)
		(mid 267.391657 46.443925)
		(end 267.435574 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 267.435574 47.75)
		(end 267.435574 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 267.585574 47.9)
		(mid 267.479507 47.856066)
		(end 267.435574 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 268.685574 47.9)
		(end 267.585574 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 268.835574 46.55)
		(end 268.835574 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 268.835574 46.55)
		(mid 268.879506 46.443925)
		(end 268.985574 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 268.835574 47.75)
		(mid 268.79164 47.856066)
		(end 268.685574 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 272.874283 46.4)
		(end 268.985574 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 272.874283 46.4)
		(mid 272.98036 46.443928)
		(end 273.024283 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 273.024283 47.75)
		(end 273.024283 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 273.174283 47.9)
		(mid 273.068217 47.856066)
		(end 273.024283 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 274.274283 47.9)
		(end 273.174283 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 274.424283 46.55)
		(end 274.424283 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 274.424283 46.55)
		(mid 274.468216 46.443928)
		(end 274.574283 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 274.424283 47.75)
		(mid 274.380349 47.856066)
		(end 274.274283 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 274.906541 46.4)
		(end 274.574283 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 274.906541 46.4)
		(mid 275.012581 46.443948)
		(end 275.056541 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 275.056541 47.75)
		(end 275.056541 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 275.206541 47.9)
		(mid 275.100475 47.856066)
		(end 275.056541 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 276.306541 47.9)
		(end 275.206541 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 276.456541 46.55)
		(end 276.456541 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 276.456541 46.55)
		(mid 276.500477 46.443948)
		(end 276.606541 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 276.456541 47.75)
		(mid 276.412607 47.856066)
		(end 276.306541 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 278.860339 46.4)
		(end 276.606541 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 278.860339 46.4)
		(mid 278.96638 46.443948)
		(end 279.010339 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 279.010339 47.75)
		(end 279.010339 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 279.160339 47.9)
		(mid 279.054273 47.856066)
		(end 279.010339 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 280.260339 47.9)
		(end 279.160339 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 280.410339 46.55)
		(end 280.410339 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 280.410339 46.55)
		(mid 280.454275 46.443948)
		(end 280.560339 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 280.410339 47.75)
		(mid 280.366405 47.856066)
		(end 280.260339 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 280.892597 46.4)
		(end 280.560339 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 280.892597 46.4)
		(mid 280.998665 46.443933)
		(end 281.042597 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 281.042597 47.75)
		(end 281.042597 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 281.192597 47.9)
		(mid 281.086531 47.856066)
		(end 281.042597 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 282.292597 47.9)
		(end 281.192597 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 282.442597 46.55)
		(end 282.442597 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 282.442597 46.55)
		(mid 282.486531 46.443933)
		(end 282.592597 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 282.442597 47.75)
		(mid 282.398663 47.856066)
		(end 282.292597 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 286.481306 46.4)
		(end 282.592597 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 286.481306 46.4)
		(mid 286.587368 46.443936)
		(end 286.631306 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 286.631306 47.75)
		(end 286.631306 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 286.781306 47.9)
		(mid 286.67524 47.856066)
		(end 286.631306 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 287.881306 47.9)
		(end 286.781306 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 288.031306 46.55)
		(end 288.031306 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 288.031306 46.55)
		(mid 288.07524 46.443936)
		(end 288.181306 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 288.031306 47.75)
		(mid 287.987372 47.856066)
		(end 287.881306 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 288.513564 46.4)
		(end 288.181306 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 288.513564 46.4)
		(mid 288.619653 46.443921)
		(end 288.663564 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 288.663564 47.75)
		(end 288.663564 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 288.813564 47.9)
		(mid 288.707498 47.856066)
		(end 288.663564 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 289.913564 47.9)
		(end 288.813564 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 290.063564 46.55)
		(end 290.063564 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 290.063564 46.55)
		(mid 290.107496 46.443921)
		(end 290.213564 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 290.063564 47.75)
		(mid 290.01963 47.856066)
		(end 289.913564 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 292.467362 46.4)
		(end 290.213564 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 292.467362 46.4)
		(mid 292.573453 46.443921)
		(end 292.617362 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 292.617362 47.75)
		(end 292.617362 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 292.767362 47.9)
		(mid 292.661296 47.856066)
		(end 292.617362 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 293.867362 47.9)
		(end 292.767362 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 294.017362 46.55)
		(end 294.017362 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 294.017362 46.55)
		(mid 294.061294 46.443921)
		(end 294.167362 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 294.017362 47.75)
		(mid 293.973428 47.856066)
		(end 293.867362 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 294.49962 46.4)
		(end 294.167362 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 294.49962 46.4)
		(mid 294.605673 46.443941)
		(end 294.64962 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 294.64962 47.75)
		(end 294.64962 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 294.79962 47.9)
		(mid 294.693554 47.856066)
		(end 294.64962 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 295.89962 47.9)
		(end 294.79962 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 296.04962 46.55)
		(end 296.04962 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 296.04962 46.55)
		(mid 296.093555 46.443941)
		(end 296.19962 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 296.04962 47.75)
		(mid 296.005686 47.856066)
		(end 295.89962 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 300.08833 46.4)
		(end 296.19962 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 300.08833 46.4)
		(mid 300.194377 46.443945)
		(end 300.23833 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 300.23833 47.75)
		(end 300.23833 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 300.38833 47.9)
		(mid 300.282264 47.856066)
		(end 300.23833 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 301.48833 47.9)
		(end 300.38833 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 301.63833 46.55)
		(end 301.63833 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 301.63833 46.55)
		(mid 301.682266 46.443945)
		(end 301.78833 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 301.63833 47.75)
		(mid 301.594396 47.856066)
		(end 301.48833 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 302.120588 46.4)
		(end 301.78833 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 302.120588 46.4)
		(mid 302.226662 46.44393)
		(end 302.270588 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 302.270588 47.75)
		(end 302.270588 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 302.420588 47.9)
		(mid 302.314522 47.856066)
		(end 302.270588 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 303.520588 47.9)
		(end 302.420588 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 303.670588 46.55)
		(end 303.670588 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 303.670588 46.55)
		(mid 303.714521 46.44393)
		(end 303.820588 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 303.670588 47.75)
		(mid 303.626654 47.856066)
		(end 303.520588 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 306.074385 46.4)
		(end 303.820588 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 306.074385 46.4)
		(mid 306.180461 46.443929)
		(end 306.224385 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 306.224385 47.75)
		(end 306.224385 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 306.374385 47.9)
		(mid 306.268319 47.856066)
		(end 306.224385 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 307.474385 47.9)
		(end 306.374385 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 307.624385 46.55)
		(end 307.624385 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 307.624385 46.55)
		(mid 307.668318 46.443929)
		(end 307.774385 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 307.624385 47.75)
		(mid 307.580451 47.856066)
		(end 307.474385 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 308.106643 46.4)
		(end 307.774385 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 308.106643 46.4)
		(mid 308.212681 46.443949)
		(end 308.256643 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 308.256643 47.75)
		(end 308.256643 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 308.406643 47.9)
		(mid 308.300577 47.856066)
		(end 308.256643 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 309.506643 47.9)
		(end 308.406643 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 309.656643 46.55)
		(end 309.656643 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 309.656643 46.55)
		(mid 309.70058 46.443949)
		(end 309.806643 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 309.656643 47.75)
		(mid 309.612709 47.856066)
		(end 309.506643 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 313.695353 46.4)
		(end 309.806643 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 313.695353 46.4)
		(mid 313.801449 46.443917)
		(end 313.845353 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 313.845353 47.75)
		(end 313.845353 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 313.995353 47.9)
		(mid 313.889287 47.856066)
		(end 313.845353 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 315.095353 47.9)
		(end 313.995353 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 315.245353 46.55)
		(end 315.245353 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 315.245353 46.55)
		(mid 315.289284 46.443917)
		(end 315.395353 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 315.245353 47.75)
		(mid 315.201419 47.856066)
		(end 315.095353 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 315.727611 46.4)
		(end 315.395353 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 315.727611 46.4)
		(mid 315.83367 46.443938)
		(end 315.877611 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 315.877611 47.75)
		(end 315.877611 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 316.027611 47.9)
		(mid 315.921545 47.856066)
		(end 315.877611 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 317.127611 47.9)
		(end 316.027611 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 317.277611 46.55)
		(end 317.277611 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 317.277611 46.55)
		(mid 317.321546 46.443938)
		(end 317.427611 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 317.277611 47.75)
		(mid 317.233677 47.856066)
		(end 317.127611 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 319.681408 46.4)
		(end 317.427611 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 319.681408 46.4)
		(mid 319.787469 46.443937)
		(end 319.831408 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 319.831408 47.75)
		(end 319.831408 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 319.981408 47.9)
		(mid 319.875342 47.856066)
		(end 319.831408 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 321.081408 47.9)
		(end 319.981408 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 321.231408 46.55)
		(end 321.231408 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 321.231408 46.55)
		(mid 321.275342 46.443937)
		(end 321.381408 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 321.231408 47.75)
		(mid 321.187474 47.856066)
		(end 321.081408 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 321.713666 46.4)
		(end 321.381408 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 321.713666 46.4)
		(mid 321.819754 46.443922)
		(end 321.863666 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 321.863666 47.75)
		(end 321.863666 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 322.013666 47.9)
		(mid 321.9076 47.856066)
		(end 321.863666 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 323.113666 47.9)
		(end 322.013666 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 323.263666 46.55)
		(end 323.263666 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 323.263666 46.55)
		(mid 323.307598 46.443922)
		(end 323.413666 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 323.263666 47.75)
		(mid 323.219732 47.856066)
		(end 323.113666 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 327.302376 46.4)
		(end 323.413666 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 327.302376 46.4)
		(mid 327.408458 46.443925)
		(end 327.452376 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 327.452376 47.75)
		(end 327.452376 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 327.602376 47.9)
		(mid 327.49631 47.856066)
		(end 327.452376 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 328.702376 47.9)
		(end 327.602376 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 328.852376 46.55)
		(end 328.852376 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 328.852376 46.55)
		(mid 328.896309 46.443925)
		(end 329.002376 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 328.852376 47.75)
		(mid 328.808442 47.856066)
		(end 328.702376 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 329.334634 46.4)
		(end 329.002376 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 329.334634 46.4)
		(mid 329.440678 46.443946)
		(end 329.484634 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 329.484634 47.75)
		(end 329.484634 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 329.634634 47.9)
		(mid 329.528568 47.856066)
		(end 329.484634 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 330.734634 47.9)
		(end 329.634634 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 330.884634 46.55)
		(end 330.884634 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 330.884634 46.55)
		(mid 330.92857 46.443946)
		(end 331.034634 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 330.884634 47.75)
		(mid 330.8407 47.856066)
		(end 330.734634 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 333.288431 46.4)
		(end 331.034634 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 333.288431 46.4)
		(mid 333.394477 46.443945)
		(end 333.438431 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 333.438431 47.75)
		(end 333.438431 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 333.588431 47.9)
		(mid 333.482365 47.856066)
		(end 333.438431 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 334.688431 47.9)
		(end 333.588431 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 334.838431 46.55)
		(end 334.838431 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 334.838431 46.55)
		(mid 334.882367 46.443945)
		(end 334.988431 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 334.838431 47.75)
		(mid 334.794497 47.856066)
		(end 334.688431 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 335.320689 46.4)
		(end 334.988431 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 335.320689 46.4)
		(mid 335.426762 46.44393)
		(end 335.470689 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 335.470689 47.75)
		(end 335.470689 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 335.620689 47.9)
		(mid 335.514623 47.856066)
		(end 335.470689 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 336.720689 47.9)
		(end 335.620689 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 336.870689 46.55)
		(end 336.870689 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 336.870689 46.55)
		(mid 336.914622 46.44393)
		(end 337.020689 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 336.870689 47.75)
		(mid 336.826755 47.856066)
		(end 336.720689 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 340.909399 46.4)
		(end 337.020689 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 340.909399 46.4)
		(mid 341.015466 46.443934)
		(end 341.059399 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 341.059399 47.75)
		(end 341.059399 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 341.209399 47.9)
		(mid 341.103333 47.856066)
		(end 341.059399 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 342.309399 47.9)
		(end 341.209399 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 342.459399 46.55)
		(end 342.459399 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 342.459399 46.55)
		(mid 342.503333 46.443934)
		(end 342.609399 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 342.459399 47.75)
		(mid 342.415465 47.856066)
		(end 342.309399 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 342.941657 46.4)
		(end 342.609399 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 342.941657 46.4)
		(mid 343.047751 46.443919)
		(end 343.091657 46.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 343.091657 47.75)
		(end 343.091657 46.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 343.241657 47.9)
		(mid 343.135591 47.856066)
		(end 343.091657 47.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 344.341657 47.9)
		(end 343.241657 47.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 344.491657 46.55)
		(end 344.491657 47.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 344.491657 46.55)
		(mid 344.535588 46.443919)
		(end 344.641657 46.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 344.491657 47.75)
		(mid 344.447723 47.856066)
		(end 344.341657 47.9)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 344.818556 40)
		(mid 344.924622 40.043933)
		(end 344.968556 40.15)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 344.818556 46.4)
		(end 344.641657 46.4)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 344.968556 40.15)
		(end 344.968556 46.25)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 344.968556 46.25)
		(mid 344.924622 46.356066)
		(end 344.818556 46.4)
		(layer "Edge.Cuts")
	)
	(gr_text "Z4S1"
		(at 26.003511 44.5 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 26.003511 45.75 0)
		(layer "F.SilkS")
	)
	(gr_text "Z4S2"
		(at 39.610534 44.5 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 39.610534 45.75 0)
		(layer "F.SilkS")
	)
	(gr_text "Z4S3"
		(at 53.217557 44.5 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 53.217557 45.75 0)
		(layer "F.SilkS")
	)
	(gr_text "Z4S4"
		(at 66.824581 44.5 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 66.824581 45.75 0)
		(layer "F.SilkS")
	)
	(gr_text "Z5S1"
		(at 80.431604 44.5 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 80.431604 45.75 0)
		(layer "F.SilkS")
	)
	(gr_text "Z5S2"
		(at 94.038627 44.5 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 94.038627 45.75 0)
		(layer "F.SilkS")
	)
	(gr_text "Z5S3"
		(at 107.64565 44.5 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 107.64565 45.75 0)
		(layer "F.SilkS")
	)
	(gr_text "Z5S4"
		(at 121.252673 44.5 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 121.252673 45.75 0)
		(layer "F.SilkS")
	)
	(gr_text "Z6S1"
		(at 134.859697 44.5 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 134.859697 45.75 0)
		(layer "F.SilkS")
	)
	(gr_text "Z6S2"
		(at 148.46672 44.5 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 148.46672 45.75 0)
		(layer "F.SilkS")
	)
	(gr_text "Z6S3"
		(at 162.073743 44.5 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 162.073743 45.75 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 167.984278 12.3 0)
		(layer "F.SilkS")
	)
	(gr_text "Z6S4"
		(at 175.680766 44.5 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 175.680766 45.75 0)
		(layer "F.SilkS")
	)
	(gr_text "FPC TOP / GOLD ON BACK"
		(at 182.484278 19 0)
		(layer "F.SilkS")
	)
	(gr_text "LIGHT UPPER v0.3"
		(at 182.484278 21 0)
		(layer "F.SilkS")
	)
	(gr_text "Z1S1"
		(at 189.287789 44.5 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 189.287789 45.75 0)
		(layer "F.SilkS")
	)
	(gr_text "30"
		(at 196.984278 12.3 0)
		(layer "F.SilkS")
	)
	(gr_text "Z1S2"
		(at 202.894812 44.5 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 202.894812 45.75 0)
		(layer "F.SilkS")
	)
	(gr_text "Z1S3"
		(at 216.501836 44.5 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 216.501836 45.75 0)
		(layer "F.SilkS")
	)
	(gr_text "Z1S4"
		(at 230.108859 44.5 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 230.108859 45.75 0)
		(layer "F.SilkS")
	)
	(gr_text "Z2S1"
		(at 243.715882 44.5 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 243.715882 45.75 0)
		(layer "F.SilkS")
	)
	(gr_text "Z2S2"
		(at 257.322905 44.5 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 257.322905 45.75 0)
		(layer "F.SilkS")
	)
	(gr_text "Z2S3"
		(at 270.929928 44.5 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 270.929928 45.75 0)
		(layer "F.SilkS")
	)
	(gr_text "Z2S4"
		(at 284.536952 44.5 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 284.536952 45.75 0)
		(layer "F.SilkS")
	)
	(gr_text "Z3S1"
		(at 298.143975 44.5 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 298.143975 45.75 0)
		(layer "F.SilkS")
	)
	(gr_text "Z3S2"
		(at 311.750998 44.5 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 311.750998 45.75 0)
		(layer "F.SilkS")
	)
	(gr_text "Z3S3"
		(at 325.358021 44.5 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 325.358021 45.75 0)
		(layer "F.SilkS")
	)
	(gr_text "Z3S4"
		(at 338.965044 44.5 0)
		(layer "F.SilkS")
	)
	(gr_text "+ W   N C"
		(at 338.965044 45.75 0)
		(layer "F.SilkS")
	)
	(embedded_fonts no)
)
