(kicad_sch
  (version 20250114)
  (generator "engineered-lighting")
  (generator_version "0.2")
  (paper "A3")
  (title_block
    (title "Can")
    (date "2026-09-06")
    (rev "A draft")
    (company "Engineered Lighting")
    (comment 1 "ENGINEERING DRAFT - see release status before fabrication"))
  (lib_symbols
    (symbol "EL:TCAN1042HGV"
      (pin_names
        (offset 0.8))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (property "Reference" "U"
        (at 0 11.43 0))
      (property "Value" "TCAN1042HGV"
        (at 0 -11.43 0))
      (symbol "TCAN1042HGV_0_1"
        (rectangle
          (start -12.7 8.89)
          (end 12.7 -8.89)
          (fill
            (type background))))
      (symbol "TCAN1042HGV_1_1"
        (pin input line
          (at -17.78 6.3500000000000005 0)
          (length 5.08)
          (name "TXD")
          (number "1"))
        (pin power_in line
          (at -17.78 3.8100000000000005 0)
          (length 5.08)
          (name "GND")
          (number "2"))
        (pin power_in line
          (at -17.78 1.2700000000000005 0)
          (length 5.08)
          (name "VCC")
          (number "3"))
        (pin output line
          (at -17.78 -1.2699999999999996 0)
          (length 5.08)
          (name "RXD")
          (number "4"))
        (pin power_in line
          (at -17.78 -3.8099999999999996 0)
          (length 5.08)
          (name "VIO")
          (number "5"))
        (pin input line
          (at -17.78 -6.349999999999999 0)
          (length 5.08)
          (name "STB")
          (number "8"))
        (pin bidirectional line
          (at 17.78 6.3500000000000005 180)
          (length 5.08)
          (name "CANL")
          (number "6"))
        (pin bidirectional line
          (at 17.78 3.8100000000000005 180)
          (length 5.08)
          (name "CANH")
          (number "7"))))
    (symbol "Device:R"
      (pin_numbers
        (hide yes))
      (pin_names
        (offset 0))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "R"
        (at 2.032 0 90)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "R"
        (at 0 0 90)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" ""
        (at -1.778 0 90)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Resistor"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "R res resistor"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "R_*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "R_0_1"
        (rectangle
          (start -1.016 -2.54)
          (end 1.016 2.54)
          (fill
            (type none))))
      (symbol "R_1_1"
        (pin passive line
          (at 0 3.81 270)
          (length 1.27)
          (name "")
          (number "1"))
        (pin passive line
          (at 0 -3.81 90)
          (length 1.27)
          (name "")
          (number "2")))
      (embedded_fonts no))
    (symbol "Device:C"
      (pin_numbers
        (hide yes))
      (pin_names
        (offset 0.254))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "C"
        (at 0.635 2.54 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "C"
        (at 0.635 -2.54 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" ""
        (at 0.9652 -3.81 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Unpolarized capacitor"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "cap capacitor"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "C_*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762))
          (fill
            (type none)))
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762))
          (fill
            (type none))))
      (symbol "C_1_1"
        (pin passive line
          (at 0 3.81 270)
          (length 2.794)
          (name "")
          (number "1"))
        (pin passive line
          (at 0 -3.81 90)
          (length 2.794)
          (name "")
          (number "2")))
      (embedded_fonts no))
    (symbol "Power_Protection:NUP2105L"
      (pin_names
        (hide yes))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "D"
        (at 5.715 2.54 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "NUP2105L"
        (at 5.715 0.635 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" "Package_TO_SOT_SMD:SOT-23"
        (at 5.715 -1.27 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" "https://www.onsemi.com/pub_link/Collateral/NUP2105L-D.PDF"
        (at 3.175 3.175 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Dual Line CAN Bus Protector, 24Vrwm"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "can esd protection suppression transient"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "SOT?23*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "NUP2105L_0_0"
        (pin passive line
          (at 0 -5.08 90)
          (length 2.54)
          (name "A")
          (number "3")))
      (symbol "NUP2105L_0_1"
        (rectangle
          (start -4.445 2.54)
          (end 4.445 -2.54)
          (fill
            (type background)))
        (polyline
          (pts
            (xy -3.81 1.27)
            (xy -3.175 0.635)
            (xy -1.905 0.635)
            (xy -1.27 0))
          (fill
            (type none)))
        (polyline
          (pts
            (xy -2.54 2.54)
            (xy -2.54 0.635))
          (fill
            (type none)))
        (polyline
          (pts
            (xy -2.54 0.635)
            (xy -2.54 -1.27)
            (xy 2.54 -1.27)
            (xy 2.54 0.635))
          (fill
            (type none)))
        (polyline
          (pts
            (xy -2.54 0.635)
            (xy -1.905 -0.635)
            (xy -3.175 -0.635)
            (xy -2.54 0.635))
          (fill
            (type none)))
        (polyline
          (pts
            (xy -2.54 0.635)
            (xy -3.175 1.905)
            (xy -1.905 1.905)
            (xy -2.54 0.635)
            (xy -2.54 1.27))
          (fill
            (type none)))
        (polyline
          (pts
            (xy 0 -1.27)
            (xy 0 -2.54))
          (fill
            (type none)))
        (polyline
          (pts
            (xy 1.27 1.27)
            (xy 1.905 0.635)
            (xy 2.54 0.635)
            (xy 3.175 0.635)
            (xy 3.81 0))
          (fill
            (type none)))
        (polyline
          (pts
            (xy 2.54 2.54)
            (xy 2.54 0.635))
          (fill
            (type none)))
        (polyline
          (pts
            (xy 2.54 0.635)
            (xy 1.905 -0.635)
            (xy 3.175 -0.635)
            (xy 2.54 0.635))
          (fill
            (type none)))
        (polyline
          (pts
            (xy 2.54 0.635)
            (xy 3.175 1.905)
            (xy 1.905 1.905)
            (xy 2.54 0.635))
          (fill
            (type none))))
      (symbol "NUP2105L_1_1"
        (pin passive line
          (at -2.54 5.08 270)
          (length 2.54)
          (name "K")
          (number "1"))
        (pin passive line
          (at 2.54 5.08 270)
          (length 2.54)
          (name "K")
          (number "2")))
      (embedded_fonts no))
    (symbol "Jumper:SolderJumper_2_Open"
      (pin_numbers
        (hide yes))
      (pin_names
        (offset 0)
        (hide yes))
      (exclude_from_sim no)
      (in_bom no)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "JP"
        (at 0 2.032 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "SolderJumper_2_Open"
        (at 0 -2.54 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" ""
        (at 0 -7.62 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Solder Jumper, 2-pole, open"
        (at 0 -5.08 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "solder jumper SPST"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "SolderJumper*Open*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "SolderJumper_2_Open_0_1"
        (polyline
          (pts
            (xy -0.254 1.016)
            (xy -0.254 -1.016))
          (fill
            (type none)))
        (arc
          (start -0.254 -1.016)
          (mid -1.2656 0)
          (end -0.254 1.016)
          (fill
            (type outline)))
        (arc
          (start 0.254 1.016)
          (mid 1.2656 0)
          (end 0.254 -1.016)
          (fill
            (type outline)))
        (polyline
          (pts
            (xy 0.254 1.016)
            (xy 0.254 -1.016))
          (fill
            (type none))))
      (symbol "SolderJumper_2_Open_1_1"
        (pin passive line
          (at -5.08 0 0)
          (length 3.81)
          (name "A")
          (number "1"))
        (pin passive line
          (at 5.08 0 180)
          (length 3.81)
          (name "B")
          (number "2")))
      (embedded_fonts no))
    (symbol "Connector_Generic:Conn_01x04"
      (pin_names
        (offset 1.016)
        (hide yes))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "J"
        (at 0 5.08 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "Conn_01x04"
        (at 0 -7.62 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "connector"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "Connector*:*_1x??_*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "Conn_01x04_1_1"
        (rectangle
          (start -1.27 3.81)
          (end 1.27 -6.35)
          (fill
            (type background)))
        (rectangle
          (start -1.27 2.667)
          (end 0 2.413)
          (fill
            (type none)))
        (rectangle
          (start -1.27 0.127)
          (end 0 -0.127)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -2.413)
          (end 0 -2.667)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -4.953)
          (end 0 -5.207)
          (fill
            (type none)))
        (pin passive line
          (at -5.08 2.54 0)
          (length 3.81)
          (name "Pin_1")
          (number "1"))
        (pin passive line
          (at -5.08 0 0)
          (length 3.81)
          (name "Pin_2")
          (number "2"))
        (pin passive line
          (at -5.08 -2.54 0)
          (length 3.81)
          (name "Pin_3")
          (number "3"))
        (pin passive line
          (at -5.08 -5.08 0)
          (length 3.81)
          (name "Pin_4")
          (number "4")))
      (embedded_fonts no)))
  (symbol
    (lib_id "EL:TCAN1042HGV")
    (at 83.82 91.44 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "U4"
      (at 104.14 74.93 0.0))
    (property "Value" "TCAN1042HGVDRQ1"
      (at 104.14 77.47 0.0))
    (property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
      (at 83.82 91.44 0.0)
      (hide yes))
    (property "MPN" "TCAN1042HGVDRQ1"
      (at 83.82 91.44 0.0)
      (hide yes))
    (property "Manufacturer" "Texas Instruments"
      (at 83.82 91.44 0.0)
      (hide yes))
    (property "Datasheet" "https://www.ti.com/lit/gpn/tcan1042hgv-q1"
      (at 83.82 91.44 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "U4")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "8")
    (pin "6")
    (pin "7"))
  (wire
    (pts
      (xy 66.04 85.09)
      (xy 57.15 85.09)))
  (global_label "CAN_TX"
    (shape passive)
    (at 57.15 85.09 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 57.15 85.09 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 66.04 87.63)
      (xy 58.42 87.63)))
  (global_label "GND"
    (shape passive)
    (at 58.42 87.63 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 58.42 87.63 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 66.04 90.17)
      (xy 58.42 90.17)))
  (global_label "+5V"
    (shape passive)
    (at 58.42 90.17 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 58.42 90.17 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 66.04 92.71)
      (xy 57.15 92.71)))
  (global_label "CAN_RX"
    (shape passive)
    (at 57.15 92.71 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 57.15 92.71 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 66.04 95.25)
      (xy 58.42 95.25)))
  (global_label "+3V3"
    (shape passive)
    (at 58.42 95.25 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 58.42 95.25 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 66.04 97.79)
      (xy 55.88 97.79)))
  (global_label "CAN_STB"
    (shape passive)
    (at 55.88 97.79 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 55.88 97.79 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 101.6 85.09)
      (xy 110.49 85.09)))
  (global_label "CAN_L"
    (shape passive)
    (at 110.49 85.09 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 110.49 85.09 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 101.6 87.63)
      (xy 110.49 87.63)))
  (global_label "CAN_H"
    (shape passive)
    (at 110.49 87.63 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 110.49 87.63 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 43.18 157.48 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R20"
      (at 48.26 156.21 0.0))
    (property "Value" "10k"
      (at 48.26 158.75 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 43.18 157.48 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-0710KL"
      (at 43.18 157.48 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 43.18 157.48 0.0)
      (hide yes))
    (property "Datasheet" ""
      (at 43.18 157.48 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R20")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 43.18 153.67)
      (xy 43.18 144.78)))
  (global_label "CAN_TX"
    (shape passive)
    (at 43.18 144.78 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 43.18 144.78 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 43.18 161.29)
      (xy 43.18 168.91)))
  (global_label "+3V3"
    (shape passive)
    (at 43.18 168.91 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 43.18 168.91 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 111.76 157.48 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R21"
      (at 116.84 156.21 0.0))
    (property "Value" "10k"
      (at 116.84 158.75 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 111.76 157.48 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-0710KL"
      (at 111.76 157.48 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 111.76 157.48 0.0)
      (hide yes))
    (property "Datasheet" ""
      (at 111.76 157.48 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R21")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 111.76 153.67)
      (xy 111.76 143.51)))
  (global_label "CAN_STB"
    (shape passive)
    (at 111.76 143.51 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 111.76 143.51 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 111.76 161.29)
      (xy 111.76 168.91)))
  (global_label "GND"
    (shape passive)
    (at 111.76 168.91 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 111.76 168.91 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:C")
    (at 180.34 60.96 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C20"
      (at 185.42 59.69 0.0))
    (property "Value" "100n"
      (at 185.42 62.23 0.0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
      (at 180.34 60.96 0.0)
      (hide yes))
    (property "MPN" "GRM188R72A104KA35D"
      (at 180.34 60.96 0.0)
      (hide yes))
    (property "Manufacturer" "Murata"
      (at 180.34 60.96 0.0)
      (hide yes))
    (property "Datasheet" ""
      (at 180.34 60.96 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C20")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 180.34 57.15)
      (xy 180.34 49.53)))
  (global_label "+5V"
    (shape passive)
    (at 180.34 49.53 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 180.34 49.53 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 180.34 64.77)
      (xy 180.34 72.39)))
  (global_label "GND"
    (shape passive)
    (at 180.34 72.39 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 180.34 72.39 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:C")
    (at 236.22 60.96 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C21"
      (at 241.3 59.69 0.0))
    (property "Value" "100n"
      (at 241.3 62.23 0.0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
      (at 236.22 60.96 0.0)
      (hide yes))
    (property "MPN" "GRM188R72A104KA35D"
      (at 236.22 60.96 0.0)
      (hide yes))
    (property "Manufacturer" "Murata"
      (at 236.22 60.96 0.0)
      (hide yes))
    (property "Datasheet" ""
      (at 236.22 60.96 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C21")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 236.22 57.15)
      (xy 236.22 49.53)))
  (global_label "+3V3"
    (shape passive)
    (at 236.22 49.53 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 236.22 49.53 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 236.22 64.77)
      (xy 236.22 72.39)))
  (global_label "GND"
    (shape passive)
    (at 236.22 72.39 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 236.22 72.39 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:C")
    (at 292.1 60.96 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C22"
      (at 297.18 59.69 0.0))
    (property "Value" "1u"
      (at 297.18 62.23 0.0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
      (at 292.1 60.96 0.0)
      (hide yes))
    (property "MPN" "C1608X7R1E105K080AB"
      (at 292.1 60.96 0.0)
      (hide yes))
    (property "Manufacturer" "TDK"
      (at 292.1 60.96 0.0)
      (hide yes))
    (property "Datasheet" ""
      (at 292.1 60.96 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C22")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 292.1 57.15)
      (xy 292.1 49.53)))
  (global_label "+5V"
    (shape passive)
    (at 292.1 49.53 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 292.1 49.53 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 292.1 64.77)
      (xy 292.1 72.39)))
  (global_label "GND"
    (shape passive)
    (at 292.1 72.39 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 292.1 72.39 0.0)
      (hide yes)))
  (symbol
    (lib_id "Power_Protection:NUP2105L")
    (at 231.14 147.32 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "U16"
      (at 238.125 134.62 0.0))
    (property "Value" "NUP2105LT1G"
      (at 238.125 137.16 0.0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23"
      (at 231.14 147.32 0.0)
      (hide yes))
    (property "MPN" "NUP2105LT1G"
      (at 231.14 147.32 0.0)
      (hide yes))
    (property "Manufacturer" "onsemi"
      (at 231.14 147.32 0.0)
      (hide yes))
    (property "Datasheet" "https://www.onsemi.com/products/discrete-power-modules/esd-protection-diodes/nup2105l"
      (at 231.14 147.32 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "U16")
          (unit 1))))
    (pin "3")
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 231.14 152.4)
      (xy 231.14 160.02)))
  (global_label "GND"
    (shape passive)
    (at 231.14 160.02 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 231.14 160.02 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 228.6 142.24)
      (xy 228.6 133.35)))
  (global_label "CAN_H"
    (shape passive)
    (at 228.6 133.35 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 228.6 133.35 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 233.68 142.24)
      (xy 233.68 133.35)))
  (global_label "CAN_L"
    (shape passive)
    (at 233.68 133.35 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 233.68 133.35 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 289.56 147.32 90)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R22"
      (at 289.56 138.684 90.0))
    (property "Value" "120"
      (at 289.56 141.224 90.0))
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric"
      (at 289.56 147.32 0.0)
      (hide yes))
    (property "MPN" "RC0805FR-07120RL"
      (at 289.56 147.32 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 289.56 147.32 0.0)
      (hide yes))
    (property "Datasheet" ""
      (at 289.56 147.32 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R22")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 285.75 147.32)
      (xy 276.86 147.32)))
  (global_label "CAN_H"
    (shape passive)
    (at 276.86 147.32 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 276.86 147.32 0.0)
      (hide yes)))
  (symbol
    (lib_id "Jumper:SolderJumper_2_Open")
    (at 350.52 147.32 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "JP1"
      (at 350.52 139.7 0.0))
    (property "Value" "CAN TERMINATION"
      (at 350.52 142.24 0.0))
    (property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
      (at 350.52 147.32 0.0)
      (hide yes))
    (property "MPN" ""
      (at 350.52 147.32 0.0)
      (hide yes))
    (property "Manufacturer" ""
      (at 350.52 147.32 0.0)
      (hide yes))
    (property "Datasheet" ""
      (at 350.52 147.32 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "JP1")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 355.6 147.32)
      (xy 364.49 147.32)))
  (global_label "CAN_L"
    (shape passive)
    (at 364.49 147.32 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 364.49 147.32 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 279.4 228.6 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "J12"
      (at 279.4 215.9 0.0))
    (property "Value" "MOTOR 1"
      (at 279.4 218.44 0.0))
    (property "Footprint" "ELF:JST_PA_BM04B_PASS_TFT_1x04_P2mm_Vertical"
      (at 279.4 228.6 0.0)
      (hide yes))
    (property "MPN" "BM04B-PASS-TFT(LF)(SN)"
      (at 279.4 228.6 0.0)
      (hide yes))
    (property "Manufacturer" "JST"
      (at 279.4 228.6 0.0)
      (hide yes))
    (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/ePA-F.pdf"
      (at 279.4 228.6 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "J12")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 274.32 226.06)
      (xy 262.89 226.06)))
  (global_label "V24_MOTOR1"
    (shape passive)
    (at 262.89 226.06 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 262.89 226.06 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 274.32 228.6)
      (xy 266.7 228.6)))
  (global_label "GND"
    (shape passive)
    (at 266.7 228.6 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 266.7 228.6 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 274.32 231.14)
      (xy 265.43 231.14)))
  (global_label "CAN_H"
    (shape passive)
    (at 265.43 231.14 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 265.43 231.14 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 274.32 233.68)
      (xy 265.43 233.68)))
  (global_label "CAN_L"
    (shape passive)
    (at 265.43 233.68 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 265.43 233.68 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 365.76 228.6 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "J13"
      (at 365.76 215.9 0.0))
    (property "Value" "MOTOR 2"
      (at 365.76 218.44 0.0))
    (property "Footprint" "ELF:JST_PA_BM04B_PASS_TFT_1x04_P2mm_Vertical"
      (at 365.76 228.6 0.0)
      (hide yes))
    (property "MPN" "BM04B-PASS-TFT(LF)(SN)"
      (at 365.76 228.6 0.0)
      (hide yes))
    (property "Manufacturer" "JST"
      (at 365.76 228.6 0.0)
      (hide yes))
    (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/ePA-F.pdf"
      (at 365.76 228.6 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "J13")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 360.68 226.06)
      (xy 349.25 226.06)))
  (global_label "V24_MOTOR2"
    (shape passive)
    (at 349.25 226.06 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 349.25 226.06 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 360.68 228.6)
      (xy 353.06 228.6)))
  (global_label "GND"
    (shape passive)
    (at 353.06 228.6 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 353.06 228.6 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 360.68 231.14)
      (xy 351.79 231.14)))
  (global_label "CAN_H"
    (shape passive)
    (at 351.79 231.14 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 351.79 231.14 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 360.68 233.68)
      (xy 351.79 233.68)))
  (global_label "CAN_L"
    (shape passive)
    (at 351.79 233.68 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 351.79 233.68 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 293.37 147.32)
      (xy 345.44 147.32)))
  (global_label "CAN_TERM"
    (shape passive)
    (at 345.44 147.32 0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 345.44 147.32 0.0)
      (hide yes)))
  (text "CAN"
    (at 20.32 15.24 0))
  (text "CAN: 5V transceiver supply / 3.3V logic interface.\nExactly two endpoint terminations; close JP1 only if this controller is an endpoint."
    (at 20.32 27.94 0))
  (text "Motor connector: 1 = fused +24V, 2 = GND, 3 = CANH, 4 = CANL.\nUnit-specific motor harness polarity must be verified before connection."
    (at 20.32 195.58 0))
  (embedded_fonts no))