(kicad_pcb
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(4 "In1.Cu" signal)
		(6 "In2.Cu" signal)
		(8 "In3.Cu" signal)
		(10 "In4.Cu" signal)
		(12 "In5.Cu" signal)
		(14 "In6.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting
			(front yes)
			(back yes)
		)
		(covering
			(front no)
			(back no)
		)
		(plugging
			(front no)
			(back no)
		)
		(capping no)
		(filling no)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12)
			(dashed_line_gap_ratio 3)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 90 96)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R108"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "220"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07220RL"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_08")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_08")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fuse:Fuse_Littelfuse-NANO2-451_453"
		(locked yes)
		(layer "F.Cu")
		(at 77 79.5 90)
		(descr "Littelfuse NANO2 https://www.littelfuse.com/~/media/electronics/datasheets/fuses/littelfuse_fuse_451_453_datasheet.pdf.pdf")
		(tags "Fuse Nano2")
		(property "Reference" "F4"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Value" "0.75A ambient zone fuse"
			(at 0 2.7 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.littelfuse.com/assetdocs/fuse-451-and-453-datasheet?assetguid=533cd5cc-956c-4243-867f-6ab5a62f6ba1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0451.750MRL"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Littelfuse"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.455 0 90)
			(size 1.96 3.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "V24_BUS")
		)
		(pad "2" smd rect
			(at 2.455 0 90)
			(size 1.96 3.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE1_24V")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Fuse.3dshapes/Fuse_Littelfuse-NANO2-451_453.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fuse:Fuse_Littelfuse-NANO2-451_453"
		(locked yes)
		(layer "F.Cu")
		(at 96.5 115.5)
		(descr "Littelfuse NANO2 https://www.littelfuse.com/~/media/electronics/datasheets/fuses/littelfuse_fuse_451_453_datasheet.pdf.pdf")
		(tags "Fuse Nano2")
		(property "Reference" "F2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Value" "1A motor branch fuse"
			(at 0 2.7 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.littelfuse.com/assetdocs/fuse-451-and-453-datasheet?assetguid=533cd5cc-956c-4243-867f-6ab5a62f6ba1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0451001.MRL"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Littelfuse"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.455 0)
			(size 1.96 3.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "V24_BUS")
		)
		(pad "2" smd rect
			(at 2.455 0)
			(size 1.96 3.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "V24_MOTOR1")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Fuse.3dshapes/Fuse_Littelfuse-NANO2-451_453.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ELF:Molex_2005280300_30P_Central_LED"
		(layer "F.Cu")
		(at 70 99.4 -90)
		(descr "Molex 1.00mm Pitch Easy-On Front Flip, Right-Angle, Bottom Contact FFC/FPC, 200528-0300, 30 Circuits (https://www.molex.com/pdm_docs/sd/2005280300_sd.pdf)")
		(tags "connector Molex  horizontal")
		(property "Reference" "J2"
			(at 0 -2.61 270)
			(layer "F.Fab")
		)
		(property "Value" "2005280300 / 6-ZONE FLEX"
			(at 0 5.39 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.molex.com/en-us/products/part-detail/2005280300"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "connector/Molex"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "2005280300"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Molex"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.39 270)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -14.5 -0.91 270)
			(size 0.4 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE4_24V")
		)
		(pad "2" smd rect
			(at -13.5 -0.91 270)
			(size 0.4 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE4_24V")
		)
		(pad "3" smd rect
			(at -12.5 -0.91 270)
			(size 0.4 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE4_W")
		)
		(pad "4" smd rect
			(at -11.5 -0.91 270)
			(size 0.4 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE4_N")
		)
		(pad "5" smd rect
			(at -10.5 -0.91 270)
			(size 0.4 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE4_C")
		)
		(pad "6" smd rect
			(at -9.5 -0.91 270)
			(size 0.4 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE5_24V")
		)
		(pad "7" smd rect
			(at -8.5 -0.91 270)
			(size 0.4 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE5_24V")
		)
		(pad "8" smd rect
			(at -7.5 -0.91 270)
			(size 0.4 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE5_W")
		)
		(pad "9" smd rect
			(at -6.5 -0.91 270)
			(size 0.4 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE5_N")
		)
		(pad "10" smd rect
			(at -5.5 -0.91 270)
			(size 0.4 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE5_C")
		)
		(pad "11" smd rect
			(at -4.5 -0.91 270)
			(size 0.4 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE6_24V")
		)
		(pad "12" smd rect
			(at -3.5 -0.91 270)
			(size 0.4 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE6_24V")
		)
		(pad "13" smd rect
			(at -2.5 -0.91 270)
			(size 0.4 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE6_W")
		)
		(pad "14" smd rect
			(at -1.5 -0.91 270)
			(size 0.4 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE6_N")
		)
		(pad "15" smd rect
			(at -0.5 -0.91 270)
			(size 0.4 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE6_C")
		)
		(pad "16" smd rect
			(at 0.5 -0.91 270)
			(size 0.4 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE1_24V")
		)
		(pad "17" smd rect
			(at 1.5 -0.91 270)
			(size 0.4 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE1_24V")
		)
		(pad "18" smd rect
			(at 2.5 -0.91 270)
			(size 0.4 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE1_W")
		)
		(pad "19" smd rect
			(at 3.5 -0.91 270)
			(size 0.4 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE1_N")
		)
		(pad "20" smd rect
			(at 4.5 -0.91 270)
			(size 0.4 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE1_C")
		)
		(pad "21" smd rect
			(at 5.5 -0.91 270)
			(size 0.4 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE2_24V")
		)
		(pad "22" smd rect
			(at 6.5 -0.91 270)
			(size 0.4 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE2_24V")
		)
		(pad "23" smd rect
			(at 7.5 -0.91 270)
			(size 0.4 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE2_W")
		)
		(pad "24" smd rect
			(at 8.5 -0.91 270)
			(size 0.4 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE2_N")
		)
		(pad "25" smd rect
			(at 9.5 -0.91 270)
			(size 0.4 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE2_C")
		)
		(pad "26" smd rect
			(at 10.5 -0.91 270)
			(size 0.4 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE3_24V")
		)
		(pad "27" smd rect
			(at 11.5 -0.91 270)
			(size 0.4 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE3_24V")
		)
		(pad "28" smd rect
			(at 12.5 -0.91 270)
			(size 0.4 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE3_W")
		)
		(pad "29" smd rect
			(at 13.5 -0.91 270)
			(size 0.4 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE3_N")
		)
		(pad "30" smd rect
			(at 14.5 -0.91 270)
			(size 0.4 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE3_C")
		)
		(pad "MP" smd rect
			(at -17.3 1.79 270)
			(size 2 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "MP" smd rect
			(at 17.3 1.79 270)
			(size 2 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_FFC-FPC.3dshapes/Molex_200528-0300_1x30-1MP_P1.00mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 125 105.5 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R117"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "220"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07220RL"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_17")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_17")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-523"
		(locked yes)
		(layer "F.Cu")
		(at 115 91 90)
		(descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
		(tags "Diode SOD523")
		(property "Reference" "D30"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "TPD1E10B06DYAR"
			(at 0 1.4 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tpd1e10b06.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "TPD1E10B06DYAR"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -1.3 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7 0 270)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_VBUS")
		)
		(pad "2" smd roundrect
			(at 0.7 0 270)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-523.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(locked yes)
		(layer "F.Cu")
		(at 121.916283 98.082571 5)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236)")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q120"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "AO3422"
			(at 0 2.4 5)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.aosmd.com/res/data_sheets/AO3422.pdf"
			(at 0 0 5)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 5)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 5)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "AO3422"
			(at 0 0 5)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Alpha & Omega Semiconductor"
			(at 0 0 5)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 95)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 5)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_20")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.949998 5)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at 0.937504 0 5)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "ZONE7_N")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_USB:USB_C_Receptacle_GCT_USB4105-xx-A_16P_TopMnt_Horizontal"
		(locked yes)
		(layer "F.Cu")
		(at 100 134.425)
		(descr "USB 2.0 Type C Receptacle, GCT, 16P, top mounted, horizontal, 5A: https://gct.co/files/drawings/usb4105.pdf")
		(tags "USB C Type-C Receptacle SMD USB 2.0 16P 16C USB4105-15-A USB4105-15-A-060 USB4105-15-A-120 USB4105-GF-A USB4105-GF-A-060 USB4105-GF-A-120")
		(property "Reference" "J14"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Value" "USB DATA /24V REQUIRED"
			(at 0 5 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "USB4105-GF-A"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "GCT"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "PCB Edge"
			(at 0 3.1 0)
			(unlocked yes)
			(layer "Dwgs.User")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -2.89 -2.605)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2.89 -2.605)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
		)
		(pad "A1" smd roundrect
			(at -3.2 -3.68)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "A4" smd roundrect
			(at -2.4 -3.68)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_VBUS")
		)
		(pad "A5" smd roundrect
			(at -1.25 -3.68)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_CC1")
		)
		(pad "A6" smd roundrect
			(at -0.25 -3.68)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_DP_HOST")
		)
		(pad "A7" smd roundrect
			(at 0.25 -3.68)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_DM_HOST")
		)
		(pad "A8" smd roundrect
			(at 1.25 -3.68)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "unconnected-(J14-SBU1-PadA8)")
		)
		(pad "A9" smd roundrect
			(at 2.4 -3.68)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_VBUS")
		)
		(pad "A12" smd roundrect
			(at 3.2 -3.68)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "B1" smd roundrect
			(at 3.2 -3.68)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "B4" smd roundrect
			(at 2.4 -3.68)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_VBUS")
		)
		(pad "B5" smd roundrect
			(at 1.75 -3.68)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_CC2")
		)
		(pad "B6" smd roundrect
			(at 0.75 -3.68)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_DP_HOST")
		)
		(pad "B7" smd roundrect
			(at -0.75 -3.68)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_DM_HOST")
		)
		(pad "B8" smd roundrect
			(at -1.75 -3.68)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "unconnected-(J14-SBU2-PadB8)")
		)
		(pad "B9" smd roundrect
			(at -2.4 -3.68)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_VBUS")
		)
		(pad "B12" smd roundrect
			(at -3.2 -3.68)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "SH" thru_hole oval
			(at -4.32 -3.105)
			(size 1 2.1)
			(drill oval 0.6 1.7)
			(property pad_prop_mechanical)
			(layers "*.Cu" "*.Mask" "F.Paste")
			(remove_unused_layers no)
			(net "GND")
		)
		(pad "SH" thru_hole oval
			(at -4.32 1.075)
			(size 1 1.8)
			(drill oval 0.6 1.4)
			(property pad_prop_mechanical)
			(layers "*.Cu" "*.Mask" "F.Paste")
			(remove_unused_layers no)
			(net "GND")
		)
		(pad "SH" thru_hole oval
			(at 4.32 -3.105)
			(size 1 2.1)
			(drill oval 0.6 1.7)
			(property pad_prop_mechanical)
			(layers "*.Cu" "*.Mask" "F.Paste")
			(remove_unused_layers no)
			(net "GND")
		)
		(pad "SH" thru_hole oval
			(at 4.32 1.075)
			(size 1 1.8)
			(drill oval 0.6 1.4)
			(property pad_prop_mechanical)
			(layers "*.Cu" "*.Mask" "F.Paste")
			(remove_unused_layers no)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_GCT_USB4105-xx-A_16P_TopMnt_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 82 76)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R8"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "2.2k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-072K2L"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "I2C_SCL")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 93 95.5 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R110"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "220"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07220RL"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_10")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_10")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_SPST_TL3305A"
		(locked yes)
		(layer "F.Cu")
		(at 113 80 -90)
		(descr "https://www.e-switch.com/system/asset/product_line/data_sheet/213/TL3305.pdf")
		(tags "TL3305 Series Tact Switch")
		(property "Reference" "S2"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(property "Value" "BOOT"
			(at 0 3.2 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "TL3305AF160QG"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "E-Switch"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.6 -1.5 270)
			(size 1.6 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "BOOT_GPIO9")
		)
		(pad "1" smd rect
			(at 3.6 -1.5 270)
			(size 1.6 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "BOOT_GPIO9")
		)
		(pad "2" smd rect
			(at -3.6 1.5 270)
			(size 1.6 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "2" smd rect
			(at 3.6 1.5 270)
			(size 1.6 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_TL3305A.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ELF:Enclosure_F1"
		(locked yes)
		(layer "F.Cu")
		(at 90.55 123.75 90)
		(descr "Littelfuse NANO2 https://www.littelfuse.com/~/media/electronics/datasheets/fuses/littelfuse_fuse_451_453_datasheet.pdf.pdf")
		(tags "Fuse Nano2")
		(property "Reference" "F1"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Value" "6.3A backup fuse"
			(at 0 2.7 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.littelfuse.com/assetdocs/fuse-451-and-453-datasheet?assetguid=533cd5cc-956c-4243-867f-6ab5a62f6ba1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "045106.3MRL"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Littelfuse"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.455 0 90)
			(size 1.96 3.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "VIN24_RAW")
		)
		(pad "2" smd rect
			(at 2.455 0 90)
			(size 1.96 3.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "VIN24_FUSED")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Fuse.3dshapes/Fuse_Littelfuse-NANO2-451_453.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(locked yes)
		(layer "F.Cu")
		(at 90 129.5 90)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP1"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Value" "CAN TERMINATION"
			(at 0 1.9 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" smd custom
			(at -0.65 0 90)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net "CAN_TERM")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 90)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net "CAN_L")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(locked yes)
		(layer "F.Cu")
		(at 88.75 69.4)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP13"
			(at 0 -1.448 0)
			(layer "F.Fab")
		)
		(property "Value" "GPIO4 STRAP"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "PCB FEATURE"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "PCB"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net "GPIO4_STRAP")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 126.5 93.5 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R120"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "220"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07220RL"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_20")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_20")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(locked yes)
		(layer "F.Cu")
		(at 119.5 118 90)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236)")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q115"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "AO3422"
			(at 0 2.4 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.aosmd.com/res/data_sheets/AO3422.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "AO3422"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Alpha & Omega Semiconductor"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_15")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "ZONE5_C")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(locked yes)
		(layer "F.Cu")
		(at 77.5 86)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236)")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q103"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "AO3422"
			(at 0 2.4 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.aosmd.com/res/data_sheets/AO3422.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "AO3422"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Alpha & Omega Semiconductor"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_03")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at 0.9375 0)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "ZONE1_C")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
		(locked yes)
		(layer "F.Cu")
		(at 130.36131 85.84229 115)
		(descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf)")
		(tags "connector JST SH horizontal")
		(property "Reference" "J15"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "UART DEBUG"
			(at 0 3.98 115)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 115)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 115)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "connector/SMD_single_row_plus_mounting_pad"
			(at 0 0 115)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "SM04B-SRSS-TB(LF)(SN)"
			(at 0 0 115)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "JST"
			(at 0 0 115)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 115)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 -2 115)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(pad "2" smd roundrect
			(at -0.5 -1.999999 115)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at 0.5 -2 115)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "UART_TX")
		)
		(pad "4" smd roundrect
			(at 1.5 -2 115)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "UART_RX")
		)
		(pad "MP" smd roundrect
			(at -2.8 1.875 115)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
		)
		(pad "MP" smd roundrect
			(at 2.8 1.875 115)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 88 74)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R6"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "10k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-0710KL"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PCA_OE")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ELF:TestPoint_Pad_D1mm_NoComponentCourtyard"
		(layer "F.Cu")
		(at 89 127.7)
		(property "Reference" "TP2"
			(at 0 -1.2 0)
			(layer "F.Fab")
		)
		(property "Value" "VIN24_RAW"
			(at 0 1.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd exclude_from_pos_files exclude_from_bom dnp)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net "VIN24_RAW")
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(locked yes)
		(layer "F.Cu")
		(at 121.250368 105.694019 -15)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236)")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q117"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "AO3422"
			(at 0 2.4 165)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.aosmd.com/res/data_sheets/AO3422.pdf"
			(at 0 0 165)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 165)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 165)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "AO3422"
			(at 0 0 165)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Alpha & Omega Semiconductor"
			(at 0 0 165)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 75)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 345)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_17")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 345)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 345)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "ZONE6_N")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(locked yes)
		(layer "F.Cu")
		(at 103.5 122.5)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236)")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q30"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "MMBT3904"
			(at 0 2.4 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "MMBT3904-7-F"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Diodes Incorporated"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_SENSE_BASE")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at 0.9375 0)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_PRESENT_N")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 94 89.5)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C514"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "100nF 100V X7R"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.murata.com/products/productdetail?partno=GRM188R72A104KA35%23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "GRM188R72A104KA35D"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Murata"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(locked yes)
		(layer "F.Cu")
		(at 85.045921 93.026799 155)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236)")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q101"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "AO3422"
			(at 0 2.4 155)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.aosmd.com/res/data_sheets/AO3422.pdf"
			(at 0 0 155)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 155)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 155)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "AO3422"
			(at 0 0 155)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Alpha & Omega Semiconductor"
			(at 0 0 155)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 65)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 155)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_01")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 155)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at 0.937501 0 155)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "ZONE1_W")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 88.5 84.5 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-0710KL"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "BOOT_GPIO9")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 73.75 101.25)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R106"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "220"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07220RL"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_06")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_06")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 79.5 102)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R104"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "220"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07220RL"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_04")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_04")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(locked yes)
		(layer "F.Cu")
		(at 122 78.5)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP7"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "LIGHT_ENABLE_SAFE"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom dnp)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net "LIGHT_ENABLE_SAFE")
		)
		(embedded_fonts no)
	)
	(footprint "Fuse:Fuse_Littelfuse-NANO2-451_453"
		(locked yes)
		(layer "F.Cu")
		(at 123 91 90)
		(descr "Littelfuse NANO2 https://www.littelfuse.com/~/media/electronics/datasheets/fuses/littelfuse_fuse_451_453_datasheet.pdf.pdf")
		(tags "Fuse Nano2")
		(property "Reference" "F10"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Value" "0.75A ambient zone fuse"
			(at 0 2.7 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.littelfuse.com/assetdocs/fuse-451-and-453-datasheet?assetguid=533cd5cc-956c-4243-867f-6ab5a62f6ba1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0451.750MRL"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Littelfuse"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.455 0 90)
			(size 1.96 3.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "V24_BUS")
		)
		(pad "2" smd rect
			(at 2.455 0 90)
			(size 1.96 3.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE7_24V")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Fuse.3dshapes/Fuse_Littelfuse-NANO2-451_453.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 106 109)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R212"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Value" "100k"
			(at 0 1.43 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07100KL"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_12")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_SPST_TL3305A"
		(locked yes)
		(layer "F.Cu")
		(at 109 92)
		(descr "https://www.e-switch.com/system/asset/product_line/data_sheet/213/TL3305.pdf")
		(tags "TL3305 Series Tact Switch")
		(property "Reference" "S1"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "RESET"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "TL3305AF160QG"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "E-Switch"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.6 -1.5)
			(size 1.6 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "MCU_EN")
		)
		(pad "1" smd rect
			(at 3.6 -1.5)
			(size 1.6 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "MCU_EN")
		)
		(pad "2" smd rect
			(at -3.6 1.5)
			(size 1.6 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "2" smd rect
			(at 3.6 1.5)
			(size 1.6 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_TL3305A.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(locked yes)
		(layer "F.Cu")
		(at 83.562787 98.561928 175)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236)")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q104"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "AO3422"
			(at 0 2.4 175)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.aosmd.com/res/data_sheets/AO3422.pdf"
			(at 0 0 175)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 175)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 175)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "AO3422"
			(at 0 0 175)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Alpha & Omega Semiconductor"
			(at 0 0 175)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 85)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.949998 175)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_04")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 175)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at 0.937504 0 175)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "ZONE2_W")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ELF:Enclosure_J16"
		(locked yes)
		(layer "F.Cu")
		(at 113.8 126.699999 -90)
		(descr "Molex Pico-Lock series connector, 205338-0002 (https://www.molex.com/pdm_docs/sd/2053380002_sd.pdf)")
		(tags "connector Molex Pico-Lock horizontal")
		(property "Reference" "J16"
			(at 0 0 290)
			(layer "F.Fab")
		)
		(property "Value" "BRAKE / BUS"
			(at 0 5.37 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "connector/SMD_single_row_plus_mounting_pad"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "2053380002"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Molex"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0.37 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 -3.359999 270)
			(size 1.1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.227273)
			(net "V24_BUS")
		)
		(pad "2" smd roundrect
			(at 0.999999 -3.36 270)
			(size 1.1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.227273)
			(net "GND")
		)
		(pad "MP" smd roundrect
			(at -3.895 2.635 270)
			(size 1.35 2.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.185185)
		)
		(pad "MP" smd roundrect
			(at 3.895 2.635 270)
			(size 1.35 2.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.185185)
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Pico-Lock_205338-0002_1x02-1MP_P2.00mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(locked yes)
		(layer "F.Cu")
		(at 86.5 109)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236)")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q110"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "AO3422"
			(at 0 2.4 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.aosmd.com/res/data_sheets/AO3422.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "AO3422"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Alpha & Omega Semiconductor"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_10")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at 0.9375 0)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "ZONE4_W")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(locked yes)
		(layer "F.Cu")
		(at 111 70.69)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP15"
			(at 0 -1.448 0)
			(layer "F.Fab")
		)
		(property "Value" "GPIO15 STRAP"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "PCB FEATURE"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "PCB"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net "GPIO15_STRAP")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 113 113)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R113"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "220"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07220RL"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_13")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_13")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(locked yes)
		(layer "F.Cu")
		(at 127 97.5)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236)")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q121"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "AO3422"
			(at 0 2.4 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.aosmd.com/res/data_sheets/AO3422.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "AO3422"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Alpha & Omega Semiconductor"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_21")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at 0.9375 0)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "ZONE7_C")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 109 110.5)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R21"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "10k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-0710KL"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "CAN_STB")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(locked yes)
		(layer "F.Cu")
		(at 88.75 71.42)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP14"
			(at 0 -1.448 0)
			(layer "F.Fab")
		)
		(property "Value" "GPIO5 STRAP"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "PCB FEATURE"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "PCB"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net "GPIO5_STRAP")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 94 84)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C515"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(property "Value" "100nF 100V X7R"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.murata.com/products/productdetail?partno=GRM188R72A104KA35%23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "GRM188R72A104KA35D"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Murata"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_BIAS")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 89 93 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R101"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "220"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07220RL"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_01")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_01")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(locked yes)
		(layer "F.Cu")
		(at 113 109.5 90)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236)")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q113"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "AO3422"
			(at 0 2.4 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.aosmd.com/res/data_sheets/AO3422.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "AO3422"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Alpha & Omega Semiconductor"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_13")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "ZONE5_W")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 74.75 86 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R203"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(property "Value" "100k"
			(at 0 1.43 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07100KL"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_03")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(locked yes)
		(layer "F.Cu")
		(at 78.749631 105.694019 -165)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236)")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q108"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "AO3422"
			(at 0 2.4 15)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.aosmd.com/res/data_sheets/AO3422.pdf"
			(at 0 0 15)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 15)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 15)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "AO3422"
			(at 0 0 15)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Alpha & Omega Semiconductor"
			(at 0 0 15)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 105)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 195)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_08")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 195)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 195)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "ZONE3_N")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 122 111 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R114"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "220"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07220RL"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_14")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_14")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "EL:ESP32-C6-WROOM-1"
		(locked yes)
		(layer "F.Cu")
		(at 100 72.6)
		(descr "ESP32-C6-WROOM-1: https://www.espressif.com/sites/default/files/documentation/esp32-c6-wroom-1_datasheet_en.pdf")
		(tags "esp32-c6")
		(property "Reference" "U1"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "ESP32-C6-WROOM-1-N8"
			(at 0 12 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://documentation.espressif.com/esp32-c6-wroom-1_wroom-1u_datasheet_en.html"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "ESP32-C6-WROOM-1-N8"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Espressif"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "Antenna Area"
			(at 0 -12.75 0)
			(layer "F.SilkS")
		)
		(fp_text user "Antenna Area"
			(at 0 -12.75 0)
			(layer "Eco2.User")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -8.75 -8.26)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "2" smd rect
			(at -8.75 -6.99)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+3V3")
		)
		(pad "3" smd rect
			(at -8.75 -5.72)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "MCU_EN")
		)
		(pad "4" smd rect
			(at -8.75 -4.45)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GPIO4_STRAP")
		)
		(pad "5" smd rect
			(at -8.75 -3.18)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GPIO5_STRAP")
		)
		(pad "6" smd rect
			(at -8.75 -1.91)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "CAN_TX")
		)
		(pad "7" smd rect
			(at -8.75 -0.64)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "CAN_RX")
		)
		(pad "8" smd rect
			(at -8.75 0.63)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "LIGHT_ENABLE")
		)
		(pad "9" smd rect
			(at -8.75 1.9)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB_PRESENT_N")
		)
		(pad "10" smd rect
			(at -8.75 3.17)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "BOOT_GPIO8")
		)
		(pad "11" smd rect
			(at -8.75 4.44)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "SPOT1_PWM")
		)
		(pad "12" smd rect
			(at -8.75 5.71)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "SPOT2_PWM")
		)
		(pad "13" smd rect
			(at -8.75 6.98)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB_DM_MCU")
		)
		(pad "14" smd rect
			(at -8.75 8.25)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB_DP_MCU")
		)
		(pad "15" smd rect
			(at 8.75 8.25 180)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "BOOT_GPIO9")
		)
		(pad "16" smd rect
			(at 8.75 6.98 180)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "SPOT3_PWM")
		)
		(pad "17" smd rect
			(at 8.75 5.71 180)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GPIO19")
		)
		(pad "18" smd rect
			(at 8.75 4.44 180)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GPIO20")
		)
		(pad "19" smd rect
			(at 8.75 3.17 180)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GPIO21")
		)
		(pad "20" smd rect
			(at 8.75 1.9 180)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GPIO22")
		)
		(pad "21" smd rect
			(at 8.75 0.63 180)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GPIO23")
		)
		(pad "22" smd rect
			(at 8.75 -0.64 180)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(U1-NC-Pad22)")
		)
		(pad "23" smd rect
			(at 8.75 -1.91 180)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GPIO15_STRAP")
		)
		(pad "24" smd rect
			(at 8.75 -3.18 180)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "UART_RX")
		)
		(pad "25" smd rect
			(at 8.75 -4.45 180)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "UART_TX")
		)
		(pad "26" smd rect
			(at 8.75 -5.72 180)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "I2C_SCL")
		)
		(pad "27" smd rect
			(at 8.75 -6.99 180)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "I2C_SDA")
		)
		(pad "28" smd rect
			(at 8.75 -8.26 180)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "29" smd rect
			(at -2.755 -3.79 180)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "29" smd rect
			(at -2.755 -2.54 180)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "29" smd rect
			(at -2.755 -1.29 180)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "29" smd rect
			(at -1.505 -3.79 180)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "29" smd rect
			(at -1.505 -2.54 180)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "29" smd rect
			(at -1.505 -1.29 180)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "29" smd rect
			(at -0.255 -3.79 180)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "29" smd rect
			(at -0.255 -2.54 180)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "29" smd rect
			(at -0.255 -1.29 180)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(zone
			(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu")
			(name "antenna keepout")
			(hatch edge 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
				(island_removal_mode 0)
			)
			(polygon
				(pts
					(xy 109 62.85) (xy 91 62.85) (xy 91 56.85) (xy 109 56.85)
				)
			)
		)
		(embedded_fonts no)
		(model "${KICAD8_3RD_PARTY}/3dmodels/com_github_espressif_kicad-libraries/espressif.3dshapes/ESP32-C6-WROOM-1.STEP"
			(offset
				(xyz -9 -9.75 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 125.5 102)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R118"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "220"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07220RL"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_18")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_18")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(locked yes)
		(layer "F.Cu")
		(at 124 124)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3")
		(property "Reference" "H4"
			(at 0 -4.15 0)
			(layer "F.Fab")
		)
		(property "Value" "M3 / 3.2mm NPTH"
			(at 0 4.15 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "mounting_hardware/mounting_hole"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "PCB FEATURE"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "PCB"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 110 114 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R115"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "220"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07220RL"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_15")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_15")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(locked yes)
		(layer "F.Cu")
		(at 74 97.5)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236)")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q106"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "AO3422"
			(at 0 2.4 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.aosmd.com/res/data_sheets/AO3422.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "AO3422"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Alpha & Omega Semiconductor"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_06")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at 0.9375 0)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "ZONE2_C")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fuse:Fuse_Littelfuse-NANO2-451_453"
		(locked yes)
		(layer "F.Cu")
		(at 90 99.5)
		(descr "Littelfuse NANO2 https://www.littelfuse.com/~/media/electronics/datasheets/fuses/littelfuse_fuse_451_453_datasheet.pdf.pdf")
		(tags "Fuse Nano2")
		(property "Reference" "F6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Value" "0.75A ambient zone fuse"
			(at 0 2.7 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.littelfuse.com/assetdocs/fuse-451-and-453-datasheet?assetguid=533cd5cc-956c-4243-867f-6ab5a62f6ba1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0451.750MRL"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Littelfuse"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.455 0)
			(size 1.96 3.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "V24_BUS")
		)
		(pad "2" smd rect
			(at 2.455 0)
			(size 1.96 3.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE3_24V")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Fuse.3dshapes/Fuse_Littelfuse-NANO2-451_453.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(locked yes)
		(layer "F.Cu")
		(at 95.5 127.5)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R22"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "120"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0805FR-07120RL"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "CAN_H")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "CAN_TERM")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-363_SC-70-6"
		(locked yes)
		(layer "F.Cu")
		(at 94 87)
		(descr "SOT, 6 Pin (https://home.jeita.or.jp/tsc/std-pdf/ED-7500A.pdf#page=170, JEDEC MO-203, variant AB, https://www.jedec.org/document_search?search_api_views_fulltext=MO-203)")
		(tags "SOT TO_SOT_SMD SC-88 SOT-363 SC-70-6 US6 UMT6 S-Mini6 TSSOP6")
		(property "Reference" "U13"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "switched ambient gate bias"
			(at 0 1.8 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps22919.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "TPS22919DCKR"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8375 -0.65)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(pad "2" smd roundrect
			(at -0.8375 0)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at -0.8375 0.65)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "LIGHT_ENABLE_SAFE")
		)
		(pad "4" smd roundrect
			(at 0.8375 0.65)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "unconnected-(U13-NC-Pad4)")
		)
		(pad "5" smd roundrect
			(at 0.8375 0)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_BIAS")
		)
		(pad "6" smd roundrect
			(at 0.8375 -0.65)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_BIAS")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 115 94.5 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R121"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "220"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07220RL"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_21")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_21")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fuse:Fuse_Littelfuse-NANO2-451_453"
		(locked yes)
		(layer "F.Cu")
		(at 118.5 91.5 90)
		(descr "Littelfuse NANO2 https://www.littelfuse.com/~/media/electronics/datasheets/fuses/littelfuse_fuse_451_453_datasheet.pdf.pdf")
		(tags "Fuse Nano2")
		(property "Reference" "F8"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Value" "0.75A ambient zone fuse"
			(at 0 2.7 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.littelfuse.com/assetdocs/fuse-451-and-453-datasheet?assetguid=533cd5cc-956c-4243-867f-6ab5a62f6ba1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0451.750MRL"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Littelfuse"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.455 0 90)
			(size 1.96 3.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "V24_BUS")
		)
		(pad "2" smd rect
			(at 2.455 0 90)
			(size 1.96 3.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE5_24V")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Fuse.3dshapes/Fuse_Littelfuse-NANO2-451_453.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 95.5 100.5 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R109"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "220"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07220RL"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_09")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_09")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 85 78 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R5"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-0710KL"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "ARM")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fuse:Fuse_Littelfuse-NANO2-451_453"
		(locked yes)
		(layer "F.Cu")
		(at 82 84 90)
		(descr "Littelfuse NANO2 https://www.littelfuse.com/~/media/electronics/datasheets/fuses/littelfuse_fuse_451_453_datasheet.pdf.pdf")
		(tags "Fuse Nano2")
		(property "Reference" "F5"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Value" "0.75A ambient zone fuse"
			(at 0 2.7 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.littelfuse.com/assetdocs/fuse-451-and-453-datasheet?assetguid=533cd5cc-956c-4243-867f-6ab5a62f6ba1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0451.750MRL"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Littelfuse"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.455 0 90)
			(size 1.96 3.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "V24_BUS")
		)
		(pad "2" smd rect
			(at 2.455 0 90)
			(size 1.96 3.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE2_24V")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Fuse.3dshapes/Fuse_Littelfuse-NANO2-451_453.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(locked yes)
		(layer "F.Cu")
		(at 125.5 110.5 90)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236)")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q118"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "AO3422"
			(at 0 2.4 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.aosmd.com/res/data_sheets/AO3422.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "AO3422"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Alpha & Omega Semiconductor"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_18")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "ZONE6_C")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 107 113)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R20"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "10k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-0710KL"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "CAN_TX")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(locked yes)
		(layer "F.Cu")
		(at 83 70.5)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3")
		(property "Reference" "H1"
			(at 0 -4.15 0)
			(layer "F.Fab")
		)
		(property "Value" "M3 / 3.2mm NPTH"
			(at 0 4.15 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "mounting_hardware/mounting_hole"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "PCB FEATURE"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "PCB"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 108.5 96.5)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R30"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "5.1k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-075K1L"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_CC1")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 100.5 107.5 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C40"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "100n"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "GRM188R72A104KA35D"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Murata"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 86 86 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R31"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "5.1k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-075K1L"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_CC2")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(locked yes)
		(layer "F.Cu")
		(at 115.937776 104.270514 -15)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236)")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q116"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "AO3422"
			(at 0 2.4 165)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.aosmd.com/res/data_sheets/AO3422.pdf"
			(at 0 0 165)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 165)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 165)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "AO3422"
			(at 0 0 165)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Alpha & Omega Semiconductor"
			(at 0 0 165)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 75)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 345)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_16")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 345)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 345)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "ZONE6_W")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fuse:Fuse_Littelfuse-NANO2-451_453"
		(locked yes)
		(layer "F.Cu")
		(at 113 118)
		(descr "Littelfuse NANO2 https://www.littelfuse.com/~/media/electronics/datasheets/fuses/littelfuse_fuse_451_453_datasheet.pdf.pdf")
		(tags "Fuse Nano2")
		(property "Reference" "F3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Value" "1A motor branch fuse"
			(at 0 2.7 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.littelfuse.com/assetdocs/fuse-451-and-453-datasheet?assetguid=533cd5cc-956c-4243-867f-6ab5a62f6ba1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0451001.MRL"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Littelfuse"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.455 0)
			(size 1.96 3.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "V24_BUS")
		)
		(pad "2" smd rect
			(at 2.455 0)
			(size 1.96 3.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "V24_MOTOR2")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Fuse.3dshapes/Fuse_Littelfuse-NANO2-451_453.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 104.5 96)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R11"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "100k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07100KL"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT3_PWM")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(locked yes)
		(layer "F.Cu")
		(at 105 85)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP11"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "I2C_SCL"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom dnp)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net "I2C_SCL")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 76.6 101.8 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R206"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "100k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07100KL"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_06")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(locked yes)
		(layer "F.Cu")
		(at 116.437212 98.561928 5)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236)")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q119"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "AO3422"
			(at 0 2.4 5)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.aosmd.com/res/data_sheets/AO3422.pdf"
			(at 0 0 5)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 5)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 5)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "AO3422"
			(at 0 0 5)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Alpha & Omega Semiconductor"
			(at 0 0 5)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 95)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 5)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_19")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.949998 5)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at 0.937504 0 5)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "ZONE7_W")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(locked yes)
		(layer "F.Cu")
		(at 90 118 180)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236)")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U16"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(property "Value" "NUP2105LT1G"
			(at 0 2.4 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.onsemi.com/products/discrete-power-modules/esd-protection-diodes/nup2105l"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "NUP2105LT1G"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "onsemi"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "CAN_H")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "CAN_L")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fuse:Fuse_Littelfuse-NANO2-451_453"
		(locked yes)
		(layer "F.Cu")
		(at 121 84.5)
		(descr "Littelfuse NANO2 https://www.littelfuse.com/~/media/electronics/datasheets/fuses/littelfuse_fuse_451_453_datasheet.pdf.pdf")
		(tags "Fuse Nano2")
		(property "Reference" "F9"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Value" "0.75A ambient zone fuse"
			(at 0 2.7 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.littelfuse.com/assetdocs/fuse-451-and-453-datasheet?assetguid=533cd5cc-956c-4243-867f-6ab5a62f6ba1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0451.750MRL"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Littelfuse"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.455 0)
			(size 1.96 3.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "V24_BUS")
		)
		(pad "2" smd rect
			(at 2.455 0)
			(size 1.96 3.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE6_24V")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Fuse.3dshapes/Fuse_Littelfuse-NANO2-451_453.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 80 94.5)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R105"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "220"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07220RL"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_05")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_05")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(locked yes)
		(layer "F.Cu")
		(at 81 112 90)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236)")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q111"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "AO3422"
			(at 0 2.4 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.aosmd.com/res/data_sheets/AO3422.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "AO3422"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Alpha & Omega Semiconductor"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_11")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "ZONE4_N")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 111.6125 98.775)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C43"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(property "Value" "1u"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "C1608X7R1E105K080AB"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "TDK"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 118 81)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R34"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "100k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07100KL"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_VBUS")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_SENSE_BASE")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(locked yes)
		(layer "F.Cu")
		(at 98 101)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP10"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "I2C_SDA"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom dnp)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net "I2C_SDA")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(locked yes)
		(layer "F.Cu")
		(at 119 76)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP12"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "PCA_OE"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom dnp)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net "PCA_OE")
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(locked yes)
		(layer "F.Cu")
		(at 84.062223 104.270514 -165)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236)")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q107"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "AO3422"
			(at 0 2.4 15)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.aosmd.com/res/data_sheets/AO3422.pdf"
			(at 0 0 15)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 15)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 15)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "AO3422"
			(at 0 0 15)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Alpha & Omega Semiconductor"
			(at 0 0 15)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 105)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 195)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_07")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 195)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 195)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "ZONE3_W")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 94 92)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "10k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-0710KL"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "MCU_EN")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 104.2 128.6)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R38"
			(at 0 -1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Value" "1k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-071KL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-071KL"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_DM_PARK")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(locked yes)
		(layer "F.Cu")
		(at 76 124)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3")
		(property "Reference" "H3"
			(at 0 -4.15 0)
			(layer "F.Fab")
		)
		(property "Value" "M3 / 3.2mm NPTH"
			(at 0 4.15 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "mounting_hardware/mounting_hole"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "PCB FEATURE"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "PCB"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 86 89)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R111"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "220"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07220RL"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_11")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_11")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 111.6375 87.05)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "100n"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "GRM188R72A104KA35D"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Murata"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
		(locked yes)
		(layer "F.Cu")
		(at 95 108)
		(descr "TSSOP, 28 Pin (JEDEC MO-153 Var AE https://www.jedec.org/document_search?search_api_views_fulltext=MO-153)")
		(tags "TSSOP SO")
		(property "Reference" "U2"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "PCA9685PW,118"
			(at 0 5.8 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "PCA9685PW,118"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "NXP"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -4.225)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "2" smd roundrect
			(at -2.8625 -3.575)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at -2.8625 -2.925)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "4" smd roundrect
			(at -2.8625 -2.275)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "5" smd roundrect
			(at -2.8625 -1.625)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "6" smd roundrect
			(at -2.8625 -0.975)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_01")
		)
		(pad "7" smd roundrect
			(at -2.8625 -0.325)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_02")
		)
		(pad "8" smd roundrect
			(at -2.8625 0.325)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_03")
		)
		(pad "9" smd roundrect
			(at -2.8625 0.975)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_04")
		)
		(pad "10" smd roundrect
			(at -2.8625 1.625)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_05")
		)
		(pad "11" smd roundrect
			(at -2.8625 2.275)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_06")
		)
		(pad "12" smd roundrect
			(at -2.8625 2.925)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_07")
		)
		(pad "13" smd roundrect
			(at -2.8625 3.575)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_08")
		)
		(pad "14" smd roundrect
			(at -2.8625 4.225)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "15" smd roundrect
			(at 2.8625 4.225)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_09")
		)
		(pad "16" smd roundrect
			(at 2.8625 3.575)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_10")
		)
		(pad "17" smd roundrect
			(at 2.8625 2.925)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_11")
		)
		(pad "18" smd roundrect
			(at 2.8625 2.275)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_12")
		)
		(pad "19" smd roundrect
			(at 2.8625 1.625)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_13")
		)
		(pad "20" smd roundrect
			(at 2.8625 0.975)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_14")
		)
		(pad "21" smd roundrect
			(at 2.8625 0.325)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_15")
		)
		(pad "22" smd roundrect
			(at 2.8625 -0.325)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "unconnected-(U2-LED15-Pad22)")
		)
		(pad "23" smd roundrect
			(at 2.8625 -0.975)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PCA_OE")
		)
		(pad "24" smd roundrect
			(at 2.8625 -1.625)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "25" smd roundrect
			(at 2.8625 -2.275)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "26" smd roundrect
			(at 2.8625 -2.925)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "I2C_SCL")
		)
		(pad "27" smd roundrect
			(at 2.8625 -3.575)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "I2C_SDA")
		)
		(pad "28" smd roundrect
			(at 2.8625 -4.225)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-28_4.4x9.7mm_P0.65mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ELF:TI_RSW0010A_UQFN10_1p4x1p8_TMUXHS221F"
		(locked yes)
		(layer "F.Cu")
		(at 104.55 126 -90)
		(descr "TI TMUXHS221F RevA RSW0010A land/paste pp23-24,4224897/A03/2019; exact0.6x0.2 lands,pin1 0.7x0.2; NSMD0.025mm; noEP/drill")
		(tags "Texas UQFN NoLead")
		(property "Reference" "U17"
			(at 0 -2.2 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Value" "TMUXHS221F"
			(at 0 2.2 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmuxhs221f.pdf"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/no_lead"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "TMUXHS221FRSWR"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.55 -0.2 270)
			(size 0.7 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_DP")
			(solder_mask_margin 0.025)
			(solder_paste_margin 0)
			(solder_paste_margin_ratio 0)
		)
		(pad "2" smd roundrect
			(at -0.6 0.2 270)
			(size 0.6 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_DM")
			(solder_mask_margin 0.025)
			(solder_paste_margin 0)
			(solder_paste_margin_ratio 0)
		)
		(pad "3" smd roundrect
			(at -0.4 0.8 270)
			(size 0.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(solder_mask_margin 0.025)
			(solder_paste_margin 0)
			(solder_paste_margin_ratio 0)
		)
		(pad "4" smd roundrect
			(at 0 0.8 270)
			(size 0.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_DM_PARK")
			(solder_mask_margin 0.025)
			(solder_paste_margin 0)
			(solder_paste_margin_ratio 0)
		)
		(pad "5" smd roundrect
			(at 0.4 0.8 270)
			(size 0.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_DP_PARK")
			(solder_mask_margin 0.025)
			(solder_paste_margin 0)
			(solder_paste_margin_ratio 0)
		)
		(pad "6" smd roundrect
			(at 0.6 0.2 270)
			(size 0.6 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_DM_HOST")
			(solder_mask_margin 0.025)
			(solder_paste_margin 0)
			(solder_paste_margin_ratio 0)
		)
		(pad "7" smd roundrect
			(at 0.6 -0.2 270)
			(size 0.6 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_DP_HOST")
			(solder_mask_margin 0.025)
			(solder_paste_margin 0)
			(solder_paste_margin_ratio 0)
		)
		(pad "8" smd roundrect
			(at 0.4 -0.8 270)
			(size 0.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_PRESENT_N")
			(solder_mask_margin 0.025)
			(solder_paste_margin 0)
			(solder_paste_margin_ratio 0)
		)
		(pad "9" smd roundrect
			(at 0 -0.8 270)
			(size 0.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_VBUS")
			(solder_mask_margin 0.025)
			(solder_paste_margin 0)
			(solder_paste_margin_ratio 0)
		)
		(pad "10" smd roundrect
			(at -0.4 -0.8 270)
			(size 0.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_READY_SELECT")
			(solder_mask_margin 0.025)
			(solder_paste_margin 0)
			(solder_paste_margin_ratio 0)
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Texas_RSW0010A_UQFN-10_1.4x1.8mm_P0.4mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(locked yes)
		(layer "F.Cu")
		(at 74.5 110.5 90)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236)")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q109"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "AO3422"
			(at 0 2.4 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.aosmd.com/res/data_sheets/AO3422.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "AO3422"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Alpha & Omega Semiconductor"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_09")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "ZONE3_C")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 122 81)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R35"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "100k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07100KL"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_SENSE_BASE")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(locked yes)
		(layer "F.Cu")
		(at 118.021344 112.618682 -35)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236)")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q114"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "AO3422"
			(at 0 2.4 145)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.aosmd.com/res/data_sheets/AO3422.pdf"
			(at 0 0 145)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 145)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 145)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "AO3422"
			(at 0 0 145)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Alpha & Omega Semiconductor"
			(at 0 0 145)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 55)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.937499 -0.95 325)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_14")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.950001 325)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 325)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "ZONE5_N")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5"
		(locked yes)
		(layer "F.Cu")
		(at 108 87)
		(descr "SOT, 5 Pin (JEDEC MO-178 Var AA https://www.jedec.org/document_search?search_api_views_fulltext=MO-178)")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U6"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "SN74LVC1G04DBVR"
			(at 0 2.4 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "SN74LVC1G04DBVR"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "unconnected-(U6-NC-Pad1)")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "LIGHT_ENABLE_SAFE")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PCA_OE")
		)
		(pad "5" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ELF:Enclosure_J1"
		(layer "F.Cu")
		(at 84.5 126.5 -90)
		(descr "PhoenixContact PTSM0,5 2 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1814702/pdf")
		(tags "PhoenixContact PTSM0.5 2 2.5mm vertical SMD spring clamp terminal block connector ")
		(property "Reference" "J1"
			(at -1.400003 5.53 270)
			(layer "F.Fab")
		)
		(property "Value" "24V INPUT"
			(at -0.2 -4.88 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.phoenixcontact.com/en-us/products/printed-circuit-board-terminal-ptsm-05-2-25-v-smd-r44-1771091"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "1771091"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Phoenix Contact"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0.000002 -0.074999 270)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.25 2.13 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "VIN24_RAW")
		)
		(pad "2" smd rect
			(at 1.25 2.13 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "MP" smd rect
			(at -5.050001 -1.029998 90)
			(size 2.3 5.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "MP" smd rect
			(at 5.05 -1.03 90)
			(size 2.3 5.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_PTSM-0,5-2-2,5-V-SMD_1x02-1MP_P2.50mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 88 76.5)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R4"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "10k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-0710KL"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "LIGHT_ENABLE")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
		(locked yes)
		(layer "F.Cu")
		(at 99.75 89.75 -90)
		(descr "TSSOP, 14 Pin (JEDEC MO-153 variation AB-1, 1.00mm body thickness, https://www.jedec.org/document_search?search_api_views_fulltext=MO-153)")
		(tags "TSSOP SO")
		(property "Reference" "U5"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(property "Value" "74HCS08PWJ"
			(at 0 3.45 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HCS08.pdf"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "74HCS08PWJ"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Nexperia"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -1.95 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT1_PWM")
		)
		(pad "2" smd roundrect
			(at -2.8625 -1.3 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "LIGHT_ENABLE_SAFE")
		)
		(pad "3" smd roundrect
			(at -2.8625 -0.65 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT1_CTRL")
		)
		(pad "4" smd roundrect
			(at -2.8625 0 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT2_PWM")
		)
		(pad "5" smd roundrect
			(at -2.8625 0.65 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "LIGHT_ENABLE_SAFE")
		)
		(pad "6" smd roundrect
			(at -2.8625 1.3 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT2_CTRL")
		)
		(pad "7" smd roundrect
			(at -2.8625 1.95 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "8" smd roundrect
			(at 2.8625 1.95 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT3_CTRL")
		)
		(pad "9" smd roundrect
			(at 2.8625 1.3 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT3_PWM")
		)
		(pad "10" smd roundrect
			(at 2.8625 0.65 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "LIGHT_ENABLE_SAFE")
		)
		(pad "11" smd roundrect
			(at 2.8625 0 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "LIGHT_REQUEST_ARMED")
		)
		(pad "12" smd roundrect
			(at 2.8625 -0.65 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "LIGHT_ENABLE")
		)
		(pad "13" smd roundrect
			(at 2.8625 -1.3 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "ARM")
		)
		(pad "14" smd roundrect
			(at 2.8625 -1.95 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-14_4.4x5mm_P0.65mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ELF:Enclosure_J17"
		(locked yes)
		(layer "F.Cu")
		(at 134 99 -90)
		(descr "JST PH series connector, B2B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf)")
		(tags "connector JST PH vertical")
		(property "Reference" "J17"
			(at 0 -5.45 270)
			(layer "F.Fab")
		)
		(property "Value" "ARM SWITCH"
			(at 0 4.45 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/ePH.pdf"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "connector/SMD_single_row_plus_mounting_pad"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "B2B-PH-SM4-TB(LF)(SN)"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "JST"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -1 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0.5 270)
			(size 1 5.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(pad "2" smd roundrect
			(at 1 0.5 270)
			(size 1 5.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "ARM")
		)
		(pad "MP" smd roundrect
			(at -3.4 -1.75 270)
			(size 1.6 3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
		)
		(pad "MP" smd roundrect
			(at 3.4 -1.75 270)
			(size 1.6 3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_B2B-PH-SM4-TB_1x02-1MP_P2.00mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 88 81.5)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R33"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "0"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603JR-070RL"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_DP")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_DP_MCU")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 88.5 66.5 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "100n"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "GRM188R72A104KA35D"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Murata"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 118 78.5)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R36"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "10k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-0710KL"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_PRESENT_N")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(locked yes)
		(layer "F.Cu")
		(at 78.5 74)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP6"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "GATE_BIAS"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom dnp)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net "GATE_BIAS")
		)
		(embedded_fonts no)
	)
	(footprint "Fuse:Fuse_Littelfuse-NANO2-451_453"
		(locked yes)
		(layer "F.Cu")
		(at 103 116 90)
		(descr "Littelfuse NANO2 https://www.littelfuse.com/~/media/electronics/datasheets/fuses/littelfuse_fuse_451_453_datasheet.pdf.pdf")
		(tags "Fuse Nano2")
		(property "Reference" "F7"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Value" "0.75A ambient zone fuse"
			(at 0 2.7 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.littelfuse.com/assetdocs/fuse-451-and-453-datasheet?assetguid=533cd5cc-956c-4243-867f-6ab5a62f6ba1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0451.750MRL"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Littelfuse"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.455 0 90)
			(size 1.96 3.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "V24_BUS")
		)
		(pad "2" smd rect
			(at 2.455 0 90)
			(size 1.96 3.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ZONE4_24V")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Fuse.3dshapes/Fuse_Littelfuse-NANO2-451_453.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(locked yes)
		(layer "F.Cu")
		(at 78 117 90)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236)")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q501"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(property "Value" "fast reverse gate pull-down"
			(at 0 2.4 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/2N7002BK.pdf"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "2N7002BK,215"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Nexperia"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "EFUSE_DRV")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "VIN24_FUSED")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "EFUSE_BGATE")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 107.2 121.2)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R41"
			(at 0 -1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-0710KL"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "READY_3V3")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_READY_SELECT")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(locked yes)
		(layer "F.Cu")
		(at 117 70.5)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3")
		(property "Reference" "H2"
			(at 0 -4.15 0)
			(layer "F.Fab")
		)
		(property "Value" "M3 / 3.2mm NPTH"
			(at 0 4.15 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "mounting_hardware/mounting_hole"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "PCB FEATURE"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "PCB"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 101 110.5)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C22"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "1u"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "C1608X7R1E105K080AB"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "TDK"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+5V")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 88 79)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R32"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "0"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603JR-070RL"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_DM")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_DM_MCU")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(locked yes)
		(layer "F.Cu")
		(at 84.8 116.9 180)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236)")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q112"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Value" "AO3422"
			(at 0 2.4 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.aosmd.com/res/data_sheets/AO3422.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "AO3422"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Alpha & Omega Semiconductor"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_12")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "ZONE4_C")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 76 93.5)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R103"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "220"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07220RL"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_03")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_03")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 102.2 95.2 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(property "Value" "100n"
			(at 0 1.43 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "GRM188R72A104KA35D"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Murata"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 107 115.5)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C30"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "100n"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "GRM188R72A104KA35D"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Murata"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_VBUS")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
		(locked yes)
		(layer "F.Cu")
		(at 95.5 122 90)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf)")
		(tags "SOIC SO")
		(property "Reference" "U4"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "TCAN1042HGVDRQ1"
			(at 0 3.4 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/tcan1042hgv-q1"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "TCAN1042HGVDRQ1"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -1.905 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "CAN_TX")
		)
		(pad "2" smd roundrect
			(at -2.475 -0.635 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at -2.475 0.635 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+5V")
		)
		(pad "4" smd roundrect
			(at -2.475 1.905 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "CAN_RX")
		)
		(pad "5" smd roundrect
			(at 2.475 1.905 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(pad "6" smd roundrect
			(at 2.475 0.635 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "CAN_L")
		)
		(pad "7" smd roundrect
			(at 2.475 -0.635 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "CAN_H")
		)
		(pad "8" smd roundrect
			(at 2.475 -1.905 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "CAN_STB")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(locked yes)
		(layer "F.Cu")
		(at 80 90.5 90)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236)")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q102"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "AO3422"
			(at 0 2.4 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.aosmd.com/res/data_sheets/AO3422.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "AO3422"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Alpha & Omega Semiconductor"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_02")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "ZONE1_N")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 75 104.5 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R107"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "220"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07220RL"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_07")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_07")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(locked yes)
		(layer "F.Cu")
		(at 78.083716 98.082571 175)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236)")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q105"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "AO3422"
			(at 0 2.4 175)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.aosmd.com/res/data_sheets/AO3422.pdf"
			(at 0 0 175)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 175)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 175)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "AO3422"
			(at 0 0 175)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Alpha & Omega Semiconductor"
			(at 0 0 175)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 85)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.949998 175)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_05")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 175)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at 0.937504 0 175)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "ZONE2_N")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 89.5 105 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C42"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "1u"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "C1608X7R1E105K080AB"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "TDK"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 112.5 97)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R119"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(property "Value" "220"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07220RL"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_19")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_19")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 82 78.5)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R7"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "2.2k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-072K2L"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "I2C_SDA")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 100.6125 103.775)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C41"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(property "Value" "100n"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "GRM188R72A104KA35D"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Murata"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5"
		(locked yes)
		(layer "F.Cu")
		(at 101 127.4 -90)
		(descr "SOT, 5 Pin (JEDEC MO-178 Var AA https://www.jedec.org/document_search?search_api_views_fulltext=MO-178)")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U15"
			(at 0 -2.4 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Value" "ESDS302"
			(at 0 2.4 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/esds302.pdf"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "ESDS302DBVR"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "unconnected-(U15-NC-Pad1)")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "unconnected-(U15-NC-Pad3)")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_DM_HOST")
		)
		(pad "5" smd roundrect
			(at 1.1375 -0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "USB_DP_HOST")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 105 110.5)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R112"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "220"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07220RL"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_12")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_12")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 120.5 102)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R116"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "220"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07220RL"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_16")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_16")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 99.3 120 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C21"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(property "Value" "100n"
			(at 0 1.43 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "GRM188R72A104KA35D"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Murata"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 112 74)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R9"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "100k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07100KL"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT1_PWM")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "F.Cu")
		(at 76.5 90.5 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R102"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "220"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07220RL"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_02")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_02")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
		(locked yes)
		(layer "F.Cu")
		(at 106 103)
		(descr "TSSOP, 28 Pin (JEDEC MO-153 Var AE https://www.jedec.org/document_search?search_api_views_fulltext=MO-153)")
		(tags "TSSOP SO")
		(property "Reference" "U3"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "PCA9685PW,118"
			(at 0 5.8 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "MPN" "PCA9685PW,118"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "NXP"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -4.225)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(pad "2" smd roundrect
			(at -2.8625 -3.575)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at -2.8625 -2.925)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "4" smd roundrect
			(at -2.8625 -2.275)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "5" smd roundrect
			(at -2.8625 -1.625)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "6" smd roundrect
			(at -2.8625 -0.975)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_16")
		)
		(pad "7" smd roundrect
			(at -2.8625 -0.325)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_17")
		)
		(pad "8" smd roundrect
			(at -2.8625 0.325)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "unconnected-(U3-LED2-Pad8)")
		)
		(pad "9" smd roundrect
			(at -2.8625 0.975)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_19")
		)
		(pad "10" smd roundrect
			(at -2.8625 1.625)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "unconnected-(U3-LED4-Pad10)")
		)
		(pad "11" smd roundrect
			(at -2.8625 2.275)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_21")
		)
		(pad "12" smd roundrect
			(at -2.8625 2.925)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "unconnected-(U3-LED6-Pad12)")
		)
		(pad "13" smd roundrect
			(at -2.8625 3.575)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "unconnected-(U3-LED7-Pad13)")
		)
		(pad "14" smd roundrect
			(at -2.8625 4.225)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "15" smd roundrect
			(at 2.8625 4.225)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "unconnected-(U3-LED8-Pad15)")
		)
		(pad "16" smd roundrect
			(at 2.8625 3.575)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "unconnected-(U3-LED9-Pad16)")
		)
		(pad "17" smd roundrect
			(at 2.8625 2.925)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "unconnected-(U3-LED10-Pad17)")
		)
		(pad "18" smd roundrect
			(at 2.8625 2.275)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "unconnected-(U3-LED11-Pad18)")
		)
		(pad "19" smd roundrect
			(at 2.8625 1.625)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_20")
		)
		(pad "20" smd roundrect
			(at 2.8625 0.975)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_18")
		)
		(pad "21" smd roundrect
			(at 2.8625 0.325)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "unconnected-(U3-LED14-Pad21)")
		)
		(pad "22" smd roundrect
			(at 2.8625 -0.325)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "unconnected-(U3-LED15-Pad22)")
		)
		(pad "23" smd roundrect
			(at 2.8625 -0.975)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "PCA_OE")
		)
		(pad "24" smd roundrect
			(at 2.8625 -1.625)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "25" smd roundrect
			(at 2.8625 -2.275)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "26" smd roundrect
			(at 2.8625 -2.925)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "I2C_SCL")
		)
		(pad "27" smd roundrect
			(at 2.8625 -3.575)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "I2C_SDA")
		)
		(pad "28" smd roundrect
			(at 2.8625 -4.225)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-28_4.4x9.7mm_P0.65mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ELF:L_Bourns_SRN6045"
		(locked yes)
		(layer "B.Cu")
		(at 92.6 87.75)
		(descr "Bourns SRN6045 (not SRN6045TA), manufacturer recommended land pattern, SRN6045.pdf REV. 01/20 page 1; pads 2.0x6.0 mm, inner gap 2.3 mm, overall 6.3 mm; nominal body 6.0x6.0 mm, height 4.5 mm maximum. https://www.bourns.com/docs/Product-Datasheets/SRN6045.pdf")
		(tags "Bourns SRN6045 semi-shielded power inductor")
		(property "Reference" "L503"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "220uH +/-20%, .6A RMS .7A saturation"
			(at 0 -4.1 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.bourns.com/docs/Product-Datasheets/SRN6045.pdf"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Height" "4.5 mm maximum"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "SRN6045-221M"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Bourns"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -2.15 0)
			(size 2 6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "SPOT2_LED_MINUS")
		)
		(pad "2" smd rect
			(at 2.15 0)
			(size 2 6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "SPOT2_SW")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 86.5 87 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R202"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "100k"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07100KL"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_02")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 67.5 106 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R308"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "2.2k"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-072K2L"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_BIAS")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_08")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 123.05 101.45)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R521"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "47k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-0747KL"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "V24_SPOT")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 119 107.25 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C516"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "47nF 50V X7R"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C1608X7R1H473K080AA"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "C1608X7R1H473K080AA"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "TDK"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT_EFUSE_DVDT")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT_RTN")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm_ThermalVias"
		(locked yes)
		(layer "B.Cu")
		(at 84.6 112.1 -90)
		(descr "WSON, 6 Pin (http://www.ti.com/lit/ds/symlink/tps61040.pdf#page=35)")
		(tags "WSON NoLead")
		(property "Reference" "U501"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "27V flat-clamp transient protector"
			(at 0 -1.95 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tvs2700.pdf"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/no_lead"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "TVS2700DRVR"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "" smd roundrect
			(at 0 -0.4 270)
			(size 0.87 0.69)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0 0.4 270)
			(size 0.87 0.69)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.8875 0.65 270)
			(size 0.375 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "2" smd roundrect
			(at -0.8875 0 270)
			(size 0.375 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at -0.8875 -0.65 270)
			(size 0.375 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "4" smd roundrect
			(at 0.8875 -0.65 270)
			(size 0.375 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "V24_BUS")
		)
		(pad "5" smd roundrect
			(at 0.8875 0 270)
			(size 0.375 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "V24_BUS")
		)
		(pad "6" smd roundrect
			(at 0.8875 0.65 270)
			(size 0.375 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "V24_BUS")
		)
		(pad "7" thru_hole circle
			(at 0 -0.55 270)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
		)
		(pad "7" smd rect
			(at 0 0 270)
			(size 0.5 1.6)
			(property pad_prop_heatsink)
			(layers "F.Cu")
			(net "GND")
			(zone_connect 2)
		)
		(pad "7" smd rect
			(at 0 0 270)
			(size 1 1.6)
			(property pad_prop_heatsink)
			(layers "B.Cu" "B.Mask")
			(net "GND")
			(zone_connect 2)
		)
		(pad "7" thru_hole circle
			(at 0 0.55 270)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_SON.3dshapes/WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric"
		(locked yes)
		(layer "B.Cu")
		(at 80.4 104.25 -90)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C524"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "10uF 50V X7R"
			(at 0 -2.3 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM32ER71H106KA12-04A.pdf"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "GRM32ER71H106KA12L"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Murata"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net "V24_SPOT")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(locked yes)
		(layer "B.Cu")
		(at 98.5 134 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP1"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "GND"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom dnp)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net "GND")
		)
		(embedded_fonts no)
	)
	(footprint "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm_ThermalVias"
		(locked yes)
		(layer "B.Cu")
		(at 116.5 108.8 90)
		(descr "WSON, 6 Pin (http://www.ti.com/lit/ds/symlink/tps61040.pdf#page=35)")
		(tags "WSON NoLead")
		(property "Reference" "U500"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "27V flat-clamp transient protector"
			(at 0 -1.95 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tvs2700.pdf"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/no_lead"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "TVS2700DRVR"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "" smd roundrect
			(at 0 -0.4 90)
			(size 0.87 0.69)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0 0.4 90)
			(size 0.87 0.69)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.8875 0.65 90)
			(size 0.375 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "2" smd roundrect
			(at -0.8875 0 90)
			(size 0.375 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at -0.8875 -0.65 90)
			(size 0.375 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "4" smd roundrect
			(at 0.8875 -0.65 90)
			(size 0.375 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "V24_SPOT")
		)
		(pad "5" smd roundrect
			(at 0.8875 0 90)
			(size 0.375 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "V24_SPOT")
		)
		(pad "6" smd roundrect
			(at 0.8875 0.65 90)
			(size 0.375 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "V24_SPOT")
		)
		(pad "7" thru_hole circle
			(at 0 -0.55 90)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
		)
		(pad "7" smd rect
			(at 0 0 90)
			(size 0.5 1.6)
			(property pad_prop_heatsink)
			(layers "F.Cu")
			(net "GND")
			(zone_connect 2)
		)
		(pad "7" smd rect
			(at 0 0 90)
			(size 1 1.6)
			(property pad_prop_heatsink)
			(layers "B.Cu" "B.Mask")
			(net "GND")
			(zone_connect 2)
		)
		(pad "7" thru_hole circle
			(at 0 0.55 90)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_SON.3dshapes/WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 102.1 92.2)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R510"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "100k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07100KL"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "+5V")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "BUCK5_FB")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 78.5 95.6 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R528"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "910"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-07910RL"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07910RL"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT3_CTRL")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 81.25 126.25 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C500"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(property "Value" "100nF 100V X7R"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.murata.com/products/productdetail?partno=GRM188R72A104KA35%23"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "GRM188R72A104KA35D"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Murata"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "VIN24_FUSED")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 83.5 80.5 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R302"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "2.2k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-072K2L"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_BIAS")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_02")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 83.5 102.5 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R205"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "100k"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07100KL"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_05")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 91.25 73 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R3"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(property "Value" "10k"
			(at 0 -1.43 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-0710KL"
			(at 0 0 270)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 270)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "BOOT_GPIO8")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 122.5 95.75 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R516"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "402k"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07402KL"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT_EFUSE_MODE")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT_RTN")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 76.5 118.5)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R501"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "140k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07140KL"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "VIN24_FUSED")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "EFUSE_UVLO")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 113 111.5 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R213"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "100k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07100KL"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_13")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(locked yes)
		(layer "B.Cu")
		(at 99.5 79.3)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R524"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "0.300ohm 1% 0.125W"
			(at 0 -1.65 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://industrial.panasonic.com/ww/products/pt/current-sensing-chip-resistors/models/ERJ6RQFR30V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "ERJ-6RQFR30V"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net "V24_SPOT")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net "SPOT2_LED_PLUS")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 127.5 105.5 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R317"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "2.2k"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-072K2L"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_BIAS")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_17")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric"
		(locked yes)
		(layer "B.Cu")
		(at 76.5 104.25 -90)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C523"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "10uF 50V X7R"
			(at 0 -2.3 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM32ER71H106KA12-04A.pdf"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "GRM32ER71H106KA12L"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Murata"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net "V24_SPOT")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SON:Texas_DSG0008A_WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm_ThermalVias"
		(locked yes)
		(layer "B.Cu")
		(at 112 86 90)
		(descr "Texas DSG0008A WSON, 8 Pin (https://www.ti.com/lit/ds/symlink/mspm0c1104.pdf)")
		(tags "Texas WSON NoLead")
		(property "Reference" "U11"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "5V to 3.3V 1A fixed buck"
			(at 0 -1.95 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps62160.pdf"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/no_lead"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "TPS62162DSGR"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "" smd roundrect
			(at 0 -0.4 90)
			(size 0.83 0.74)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0 0.4 90)
			(size 0.83 0.74)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.95 0.75 90)
			(size 0.6 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "2" smd roundrect
			(at -0.95 0.25 90)
			(size 0.6 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "+5V")
		)
		(pad "3" smd roundrect
			(at -0.95 -0.25 90)
			(size 0.6 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "+5V")
		)
		(pad "4" smd roundrect
			(at -0.95 -0.75 90)
			(size 0.6 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "5" smd roundrect
			(at 0.95 -0.75 90)
			(size 0.6 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "6" smd roundrect
			(at 0.95 -0.25 90)
			(size 0.6 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(pad "7" smd roundrect
			(at 0.95 0.25 90)
			(size 0.6 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "BUCK3_SW")
		)
		(pad "8" smd roundrect
			(at 0.95 0.75 90)
			(size 0.6 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "BUCK3_PGOOD")
		)
		(pad "9" thru_hole circle
			(at 0 -0.55 90)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
		)
		(pad "9" smd rect
			(at 0 0 90)
			(size 0.5 1.6)
			(property pad_prop_heatsink)
			(layers "F.Cu")
			(net "GND")
			(zone_connect 2)
		)
		(pad "9" smd rect
			(at 0 0 90)
			(size 0.9 1.6)
			(property pad_prop_heatsink)
			(layers "B.Cu" "B.Mask")
			(net "GND")
			(zone_connect 2)
		)
		(pad "9" thru_hole circle
			(at 0 0.55 90)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_SON.3dshapes/Texas_DSG0008A_WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 77.5 89.4 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R526"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "910"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-07910RL"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07910RL"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT1_CTRL")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 117.25 75.5)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C46"
			(at 0 1.43 180)
			(layer "B.Fab")
		)
		(property "Value" "100n"
			(at 0 -1.43 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.murata.com/products/productdetail?partno=GRM188R72A104KA35%23"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "GRM188R72A104KA35D"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Murata"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 119.5 118 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R215"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "100k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07100KL"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_15")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 65.5 94 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R306"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "2.2k"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-072K2L"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_BIAS")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_06")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 116.5 96.55 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C517"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "100nF 100V X7R"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.murata.com/products/productdetail?partno=GRM188R72A104KA35%23"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "GRM188R72A104KA35D"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Murata"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "V24_BUS")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 94.6 124.55 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C20"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(property "Value" "100n"
			(at 0 -1.43 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "GRM188R72A104KA35D"
			(at 0 0 270)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Murata"
			(at 0 0 270)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "+5V")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric"
		(locked yes)
		(layer "B.Cu")
		(at 88.9 97.3 -90)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C506"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "10uF 50V X7R"
			(at 0 -2.3 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM32ER71H106KA12-04A.pdf"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "GRM32ER71H106KA12L"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Murata"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net "V24_LOGIC")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 70.5 107 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R209"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "100k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07100KL"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_09")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 113 114 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R313"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "2.2k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-072K2L"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_BIAS")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_13")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 88 119)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R211"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(property "Value" "100k"
			(at 0 -1.43 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07100KL"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_11")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 125.5 110.5 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R218"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "100k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07100KL"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_18")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 116 94 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R219"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "100k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07100KL"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_19")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 68 90 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R305"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "2.2k"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-072K2L"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_BIAS")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_05")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 80.45 108.8 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R506"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "10k"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-0710KL"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "EFUSE_PGTH")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 97.75 67.5)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C45"
			(at 0 1.43 180)
			(layer "B.Fab")
		)
		(property "Value" "100n"
			(at 0 -1.43 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.murata.com/products/productdetail?partno=GRM188R72A104KA35%23"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "GRM188R72A104KA35D"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Murata"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMA"
		(locked yes)
		(layer "B.Cu")
		(at 100 87.75 180)
		(descr "Diode SMA (DO-214AC)")
		(tags "Diode SMA (DO-214AC)")
		(property "Reference" "D503"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "60V 1A flyback Schottky"
			(at 0 -2.6 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.diodes.com/datasheet/download/B130.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "B160-13-F"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Diodes Incorporated"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -2 0 180)
			(size 2.5 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1388888889)
			(net "V24_SPOT")
		)
		(pad "2" smd roundrect
			(at 2 0 180)
			(size 2.5 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1388888889)
			(net "SPOT2_SW")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 102.4 94.6)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C508"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "1uF 25V X7R"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C1608X7R1E105K080AB"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "C1608X7R1E105K080AB"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "TDK"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "BUCK5_VCC")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMC"
		(locked yes)
		(layer "B.Cu")
		(at 71 113.5 -90)
		(descr "Diode SMC (DO-214AB)")
		(tags "Diode SMC (DO-214AB)")
		(property "Reference" "D505"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "60V 5A output negative transient Schottky"
			(at 0 -4.2 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.diodes.com/datasheet/download/B520C.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "B560C-13-F"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Diodes Incorporated"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.9 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -3.4 0 180)
			(size 3.3 2.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net "V24_BUS")
		)
		(pad "2" smd roundrect
			(at 3.4 0 180)
			(size 3.3 2.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMC.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-6"
		(locked yes)
		(layer "B.Cu")
		(at 97.75 70)
		(descr "SOT, 6 Pin (JEDEC MO-178 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-178)")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U19"
			(at 0 2.4 180)
			(layer "B.Fab")
		)
		(property "Value" "SN74LVC1G97 AND Schmitt"
			(at 0 -2.4 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc1g97.pdf"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "SN74LVC1G97DBVR"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "LIGHT_REQUEST_ARMED")
		)
		(pad "4" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "LIGHT_ENABLE_SAFE")
		)
		(pad "5" smd roundrect
			(at 1.1375 0)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(pad "6" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "READY_3V3")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric"
		(locked yes)
		(layer "B.Cu")
		(at 104.75 80.1)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C522"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "10uF 50V X7R"
			(at 0 -2.3 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM32ER71H106KA12-04A.pdf"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "GRM32ER71H106KA12L"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Murata"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net "V24_SPOT")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 93 101.5 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R301"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "2.2k"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-072K2L"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_BIAS")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_01")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ELF:TI_PWP0016A_EP3.3x3.3_6ThermalVias_125um"
		(locked yes)
		(layer "B.Cu")
		(at 118.5 101.5 -90)
		(descr "TPS26600 PWP0016A TI4214868/A02/2017 adapted per note9; Cu3.4x3.4/0.1corner chamfers, mask/paste3.3x3.3R0.05 at0.125mm stencil;6x0.2mm holes/0.5mm lands subset of1.1grid; EP17 RTN. Signal centers retained +/-2.875,1.55x0.45 versus TI +/-2.9,1.5x0.45. No opposite broad plate. Specify underpaste via filling/plugging/tenting.")
		(tags "TPS26600 PWP0016A HTSSOP RTN thermal vias 125um")
		(property "Reference" "U14"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "spot branch gated eFuse 0.494A nominal"
			(at 0 -3.45 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2660.pdf"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "TPS26600PWPR"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -2.875 2.275 270)
			(size 1.55 0.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1111111111)
			(net "V24_BUS")
			(solder_mask_margin 0.025)
			(solder_paste_margin 0)
			(solder_paste_margin_ratio 0)
		)
		(pad "2" smd roundrect
			(at -2.875 1.625 270)
			(size 1.55 0.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1111111111)
			(net "V24_BUS")
			(solder_mask_margin 0.025)
			(solder_paste_margin 0)
			(solder_paste_margin_ratio 0)
		)
		(pad "3" smd roundrect
			(at -2.875 0.975 270)
			(size 1.55 0.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1111111111)
			(net "SPOT_RTN")
			(solder_mask_margin 0.025)
			(solder_paste_margin 0)
			(solder_paste_margin_ratio 0)
		)
		(pad "4" smd roundrect
			(at -2.875 0.325 270)
			(size 1.55 0.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1111111111)
			(net "unconnected-(U14-NC-Pad4)")
			(solder_mask_margin 0.025)
			(solder_paste_margin 0)
			(solder_paste_margin_ratio 0)
		)
		(pad "5" smd roundrect
			(at -2.875 -0.325 270)
			(size 1.55 0.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1111111111)
			(net "SPOT_EFUSE_OVP")
			(solder_mask_margin 0.025)
			(solder_paste_margin 0)
			(solder_paste_margin_ratio 0)
		)
		(pad "6" smd roundrect
			(at -2.875 -0.975 270)
			(size 1.55 0.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1111111111)
			(net "SPOT_EFUSE_MODE")
			(solder_mask_margin 0.025)
			(solder_paste_margin 0)
			(solder_paste_margin_ratio 0)
		)
		(pad "7" smd roundrect
			(at -2.875 -1.625 270)
			(size 1.55 0.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1111111111)
			(net "LIGHT_ENABLE_SAFE")
			(solder_mask_margin 0.025)
			(solder_paste_margin 0)
			(solder_paste_margin_ratio 0)
		)
		(pad "8" smd roundrect
			(at -2.875 -2.275 270)
			(size 1.55 0.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1111111111)
			(net "SPOT_RTN")
			(solder_mask_margin 0.025)
			(solder_paste_margin 0)
			(solder_paste_margin_ratio 0)
		)
		(pad "9" smd roundrect
			(at 2.875 -2.275 270)
			(size 1.55 0.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1111111111)
			(net "GND")
			(solder_mask_margin 0.025)
			(solder_paste_margin 0)
			(solder_paste_margin_ratio 0)
		)
		(pad "10" smd roundrect
			(at 2.875 -1.625 270)
			(size 1.55 0.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1111111111)
			(net "SPOT_EFUSE_IMON")
			(solder_mask_margin 0.025)
			(solder_paste_margin 0)
			(solder_paste_margin_ratio 0)
		)
		(pad "11" smd roundrect
			(at 2.875 -0.975 270)
			(size 1.55 0.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1111111111)
			(net "SPOT_EFUSE_ILIM")
			(solder_mask_margin 0.025)
			(solder_paste_margin 0)
			(solder_paste_margin_ratio 0)
		)
		(pad "12" smd roundrect
			(at 2.875 -0.325 270)
			(size 1.55 0.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1111111111)
			(net "SPOT_EFUSE_DVDT")
			(solder_mask_margin 0.025)
			(solder_paste_margin 0)
			(solder_paste_margin_ratio 0)
		)
		(pad "13" smd roundrect
			(at 2.875 0.325 270)
			(size 1.55 0.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1111111111)
			(net "unconnected-(U14-NC-Pad13)")
			(solder_mask_margin 0.025)
			(solder_paste_margin 0)
			(solder_paste_margin_ratio 0)
		)
		(pad "14" smd roundrect
			(at 2.875 0.975 270)
			(size 1.55 0.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1111111111)
			(net "SPOT_EFUSE_FLT_N")
			(solder_mask_margin 0.025)
			(solder_paste_margin 0)
			(solder_paste_margin_ratio 0)
		)
		(pad "15" smd roundrect
			(at 2.875 1.625 270)
			(size 1.55 0.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1111111111)
			(net "V24_SPOT")
			(solder_mask_margin 0.025)
			(solder_paste_margin 0)
			(solder_paste_margin_ratio 0)
		)
		(pad "16" smd roundrect
			(at 2.875 2.275 270)
			(size 1.55 0.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1111111111)
			(net "V24_SPOT")
			(solder_mask_margin 0.025)
			(solder_paste_margin 0)
			(solder_paste_margin_ratio 0)
		)
		(pad "17" thru_hole circle
			(at -1.1 -1.1 270)
			(size 0.5 0.5)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "SPOT_RTN")
		)
		(pad "17" thru_hole circle
			(at -1.1 0 270)
			(size 0.5 0.5)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "SPOT_RTN")
		)
		(pad "17" thru_hole circle
			(at -1.1 1.1 270)
			(size 0.5 0.5)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "SPOT_RTN")
		)
		(pad "17" thru_hole circle
			(at 0 0 270)
			(size 0.5 0.5)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "SPOT_RTN")
		)
		(pad "17" smd roundrect
			(at 0 0 270)
			(size 3.3 3.3)
			(property pad_prop_heatsink)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.01515151515)
			(net "SPOT_RTN")
			(solder_mask_margin 0)
			(solder_paste_margin 0)
			(solder_paste_margin_ratio 0)
			(zone_connect 2)
		)
		(pad "17" smd roundrect
			(at 0 0 270)
			(size 3.4 3.4)
			(layers "B.Cu")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.02941176471)
			(chamfer top_left top_right bottom_left bottom_right)
			(net "SPOT_RTN")
			(thermal_bridge_angle 45)
		)
		(pad "17" thru_hole circle
			(at 0 1.1 270)
			(size 0.5 0.5)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "SPOT_RTN")
		)
		(pad "17" thru_hole circle
			(at 1.1 1.1 270)
			(size 0.5 0.5)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "SPOT_RTN")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_SO.3dshapes/HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3x3mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ELF:CP_CDE_AFK_CaseP_D16_H17_Provisional"
		(locked yes)
		(layer "B.Cu")
		(at 100 114)
		(descr "CDE AFK case P, AFK108M50P44T-F. ENGINEERING-DERIVED PROVISIONAL lands, not manufacturer-recommended. AFK.pdf p1 body/terminal dimensions and p5 restrictive reflow profile. Requires assembler land/process approval before release. No main-stencil paste; factory post-reflow installation. https://www.cde.com/resources/catalogs/AFK.pdf")
		(tags "CDE AFK case P electrolytic polarized provisional")
		(property "Reference" "C504"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(property "Value" "1000uF 50V low ESR"
			(at 0 -9.55 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.cde.com/resources/catalogs/AFK.pdf"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Height" "17.0 mm maximum"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Assembly" "Factory post-reflow installation; no main stencil paste; qualified local profile required; 230C peak/5s, >=200C/20s, one reflow per CDE p5"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Verification" "PROVISIONAL engineering lands; case dimensions visually verified; assembler validation required before release"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "AFK108M50P44T-F"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Cornell Dubilier / Knowles"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "+"
			(at -9.25 2.1 180)
			(layer "B.SilkS")
		)
		(fp_text user "+"
			(at -5.5 4 180)
			(layer "B.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(fp_text user "-"
			(at 5.5 4 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -6.5 0)
			(size 7 2.3)
			(layers "B.Cu" "B.Mask")
			(net "V24_BUS")
		)
		(pad "2" smd rect
			(at 6.5 0)
			(size 7 2.3)
			(layers "B.Cu" "B.Mask")
			(net "GND")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 89 93 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R201"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "100k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07100KL"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_01")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 109 103.5 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R216"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "100k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07100KL"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_16")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(locked yes)
		(layer "B.Cu")
		(at 88.25 115 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C501"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(property "Value" "1uF 100V X7R"
			(at 0 -1.85 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C3216X7R2A105K160AA"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "C3216X7R2A105K160AA"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "TDK"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net "VIN24_FUSED")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 122 90 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R320"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "2.2k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-072K2L"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_BIAS")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_20")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMA"
		(locked yes)
		(layer "B.Cu")
		(at 83.25 85.5 -90)
		(descr "Diode SMA (DO-214AC)")
		(tags "Diode SMA (DO-214AC)")
		(property "Reference" "D502"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "60V 1A flyback Schottky"
			(at 0 -2.6 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.diodes.com/datasheet/download/B130.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "B160-13-F"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Diodes Incorporated"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -2 0 270)
			(size 2.5 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1388888889)
			(net "V24_SPOT")
		)
		(pad "2" smd roundrect
			(at 2 0 270)
			(size 2.5 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1388888889)
			(net "SPOT1_SW")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 127 101.5 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R221"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "100k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07100KL"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_21")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 105 70 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R42"
			(at 0 1.43 270)
			(layer "B.Fab")
		)
		(property "Value" "1k"
			(at 0 -1.43 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-071KL"
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-071KL"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "READY_3V3")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "MCU_EN")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 101 101 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R310"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "2.2k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-072K2L"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_BIAS")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_10")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 102.1 97.3 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C509"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "100nF 100V X7R"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.murata.com/products/productdetail?partno=GRM188R72A104KA35%23"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "GRM188R72A104KA35D"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Murata"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "BUCK5_BOOT")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "BUCK5_SW")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 84.7 117.7 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C502"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "100nF 100V X7R"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.murata.com/products/productdetail?partno=GRM188R72A104KA35%23"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "GRM188R72A104KA35D"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Murata"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "VIN24_RPP")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(locked yes)
		(layer "B.Cu")
		(at 74.8 86 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R523"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "0.300ohm 1% 0.125W"
			(at 0 -1.65 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://industrial.panasonic.com/ww/products/pt/current-sensing-chip-resistors/models/ERJ6RQFR30V"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "ERJ-6RQFR30V"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net "V24_SPOT")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net "SPOT1_LED_PLUS")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 66 110.5 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R309"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "2.2k"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-072K2L"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_BIAS")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_09")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 76.95 108.8 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R509"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "10k"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-0710KL"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "EFUSE_PGOOD")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMA"
		(locked yes)
		(layer "B.Cu")
		(at 112.9 106.3 -90)
		(descr "Diode SMA (DO-214AC)")
		(tags "Diode SMA (DO-214AC)")
		(property "Reference" "D501"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "60V output negative transient Schottky"
			(at 0 -2.6 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.diodes.com/datasheet/download/B130.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "B160-13-F"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Diodes Incorporated"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -2 0 270)
			(size 2.5 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1388888889)
			(net "V24_SPOT")
		)
		(pad "2" smd roundrect
			(at 2 0 270)
			(size 2.5 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1388888889)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ELF:L_Bourns_SRN6045"
		(locked yes)
		(layer "B.Cu")
		(at 72.75 92.1 -90)
		(descr "Bourns SRN6045 (not SRN6045TA), manufacturer recommended land pattern, SRN6045.pdf REV. 01/20 page 1; pads 2.0x6.0 mm, inner gap 2.3 mm, overall 6.3 mm; nominal body 6.0x6.0 mm, height 4.5 mm maximum. https://www.bourns.com/docs/Product-Datasheets/SRN6045.pdf")
		(tags "Bourns SRN6045 semi-shielded power inductor")
		(property "Reference" "L504"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "220uH +/-20%, .6A RMS .7A saturation"
			(at 0 -4.1 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.bourns.com/docs/Product-Datasheets/SRN6045.pdf"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Height" "4.5 mm maximum"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "SRN6045-221M"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Bourns"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -2.15 0 270)
			(size 2 6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "SPOT3_LED_MINUS")
		)
		(pad "2" smd rect
			(at 2.15 0 270)
			(size 2 6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "SPOT3_SW")
		)
		(embedded_fonts no)
	)
	(footprint "Inductor_SMD:L_Bourns-SRN4018"
		(locked yes)
		(layer "B.Cu")
		(at 112.3 81.6 90)
		(descr "Bourns SRN4018 series SMD inductor, https://www.bourns.com/docs/Product-Datasheets/SRN4018.pdf")
		(tags "Bourns SRN4018 SMD inductor")
		(property "Reference" "L501"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "2.2uH 2.9A RMS 3A sat"
			(at 0 3.1 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.bourns.com/docs/product-datasheets/srn4018.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "SRN4018-2R2M"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Bourns"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.525 0 90)
			(size 1.5 3.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "BUCK3_SW")
		)
		(pad "2" smd rect
			(at 1.525 0 90)
			(size 1.5 3.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "+3V3")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Bourns-SRN4018.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 96.1 82 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R527"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "910"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-07910RL"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07910RL"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT2_CTRL")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 102.2 126.3 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R37"
			(at 0 1.43 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Value" "1k"
			(at 0 -1.43 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-071KL"
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-071KL"
			(at 0 0 270)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 270)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "USB_DP_PARK")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(locked yes)
		(layer "B.Cu")
		(at 81.2 99 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R525"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "0.300ohm 1% 0.125W"
			(at 0 -1.65 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://industrial.panasonic.com/ww/products/pt/current-sensing-chip-resistors/models/ERJ6RQFR30V"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "ERJ-6RQFR30V"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net "V24_SPOT")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net "SPOT3_LED_PLUS")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 115.5 86 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R513"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "10k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-0710KL"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "BUCK3_PGOOD")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 102 67.5)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C44"
			(at 0 1.43 180)
			(layer "B.Fab")
		)
		(property "Value" "100n"
			(at 0 -1.43 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.murata.com/products/productdetail?partno=GRM188R72A104KA35%23"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "GRM188R72A104KA35D"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Murata"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric"
		(locked yes)
		(layer "B.Cu")
		(at 89 66.8 180)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(property "Value" "22uF 25V X7R"
			(at 0 -2.3 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.murata.com/-/media/webrenewal/tool/library/common-pdf/dynamic-model/component-list-d-mlcc-2504.ashx?cvid=20250523010405000000&la=en"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "GRM32ER71E226KE15L"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Murata"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 180)
			(size 1.15 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net "+3V3")
		)
		(pad "2" smd roundrect
			(at 1.475 0 180)
			(size 1.15 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 78 128.75)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R312"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(property "Value" "2.2k"
			(at 0 -1.43 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-072K2L"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_BIAS")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_12")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 100 103.5 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R307"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "2.2k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-072K2L"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_BIAS")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_07")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ELF:TI_DDA0008B_EP2.71x3.4_ThermalVias_125um"
		(locked yes)
		(layer "B.Cu")
		(at 97 96)
		(descr "LMR36510 DDA0008B; TI drawing 4214849/B 09/2025. Thermal copper 2.95x4.9; mask/paste 2.71x3.4 for 0.125mm stencil; eight 0.2mm holes with 0.5mm lands at x +/-0.65, y +/-0.65,+/-1.95. Opposite-face mask closed; under-paste via treatment required.")
		(tags "TI LMR36510 DDA0008B PowerPAD thermal vias 125um stencil")
		(property "Reference" "U10"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "24V to 5V 1A buck"
			(at 0 -3.5 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lmr36510.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "LMR36510ADDAR"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -2.7 1.905)
			(size 1.55 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.08333333333)
			(net "GND")
		)
		(pad "2" smd roundrect
			(at -2.7 0.635)
			(size 1.55 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.08333333333)
			(net "V24_LOGIC")
		)
		(pad "3" smd roundrect
			(at -2.7 -0.635)
			(size 1.55 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.08333333333)
			(net "V24_LOGIC")
		)
		(pad "4" smd roundrect
			(at -2.7 -1.905)
			(size 1.55 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.08333333333)
			(net "BUCK5_PGOOD")
		)
		(pad "5" smd roundrect
			(at 2.7 -1.905)
			(size 1.55 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.08333333333)
			(net "BUCK5_FB")
		)
		(pad "6" smd roundrect
			(at 2.7 -0.635)
			(size 1.55 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.08333333333)
			(net "BUCK5_VCC")
		)
		(pad "7" smd roundrect
			(at 2.7 0.635)
			(size 1.55 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.08333333333)
			(net "BUCK5_BOOT")
		)
		(pad "8" smd roundrect
			(at 2.7 1.905)
			(size 1.55 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.08333333333)
			(net "BUCK5_SW")
		)
		(pad "9" thru_hole circle
			(at -0.65 -1.95)
			(size 0.5 0.5)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
		)
		(pad "9" thru_hole circle
			(at -0.65 -0.65)
			(size 0.5 0.5)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
		)
		(pad "9" thru_hole circle
			(at -0.65 0.65)
			(size 0.5 0.5)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
		)
		(pad "9" thru_hole circle
			(at -0.65 1.95)
			(size 0.5 0.5)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
		)
		(pad "9" smd rect
			(at 0 0)
			(size 2.71 3.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "GND")
			(solder_mask_margin 0)
			(solder_paste_margin 0)
			(solder_paste_margin_ratio 0)
		)
		(pad "9" smd rect
			(at 0 0)
			(size 2.95 4.9)
			(layers "F.Cu")
			(net "GND")
		)
		(pad "9" smd rect
			(at 0 0)
			(size 2.95 4.9)
			(layers "B.Cu")
			(net "GND")
		)
		(pad "9" thru_hole circle
			(at 0.65 -1.95)
			(size 0.5 0.5)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
		)
		(pad "9" thru_hole circle
			(at 0.65 -0.65)
			(size 0.5 0.5)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
		)
		(pad "9" thru_hole circle
			(at 0.65 0.65)
			(size 0.5 0.5)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
		)
		(pad "9" thru_hole circle
			(at 0.65 1.95)
			(size 0.5 0.5)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_SO.3dshapes/HTSOP-8-1EP_3.9x4.9mm_Pitch1.27mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 82.2 112.1 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C505"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "100nF 100V X7R"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.murata.com/products/productdetail?partno=GRM188R72A104KA35%23"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "GRM188R72A104KA35D"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Murata"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "V24_BUS")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 83.5 98.5 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R204"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "100k"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07100KL"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_04")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 119.5 120.5 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R315"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "2.2k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-072K2L"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_BIAS")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_15")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(locked yes)
		(layer "B.Cu")
		(at 116.5 91.5 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP9"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "V24_SPOT"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom dnp)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net "V24_SPOT")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 122 92.5 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R220"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "100k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07100KL"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_20")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:Texas_RGE0024H_VQFN-24-1EP_4x4mm_P0.5mm_EP2.7x2.7mm_ThermalVias"
		(locked yes)
		(layer "B.Cu")
		(at 81 116.5 90)
		(descr "Texas RGE0024H VQFN, 24 Pin (http://www.ti.com/lit/ds/symlink/tlc5971.pdf#page=40)")
		(tags "Texas VQFN NoLead")
		(property "Reference" "U12"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "24V input eFuse / 4.5A nominal"
			(at 0 -3.33 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2663.pdf"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/no_lead"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "TPS26630RGER"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "" smd roundrect
			(at -0.675 -0.675 90)
			(size 1.17 1.17)
			(layers "B.Paste")
			(roundrect_rratio 0.213675)
		)
		(pad "" smd roundrect
			(at -0.675 0.675 90)
			(size 1.17 1.17)
			(layers "B.Paste")
			(roundrect_rratio 0.213675)
		)
		(pad "" smd roundrect
			(at 0.675 -0.675 90)
			(size 1.17 1.17)
			(layers "B.Paste")
			(roundrect_rratio 0.213675)
		)
		(pad "" smd roundrect
			(at 0.675 0.675 90)
			(size 1.17 1.17)
			(layers "B.Paste")
			(roundrect_rratio 0.213675)
		)
		(pad "1" smd roundrect
			(at -1.9625 1.25 90)
			(size 0.825 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "VIN24_RPP")
		)
		(pad "2" smd roundrect
			(at -1.9625 0.75 90)
			(size 0.825 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "VIN24_RPP")
		)
		(pad "3" smd roundrect
			(at -1.9625 0.25 90)
			(size 0.825 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "EFUSE_BGATE")
		)
		(pad "4" smd roundrect
			(at -1.9625 -0.25 90)
			(size 0.825 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "EFUSE_DRV")
		)
		(pad "5" smd roundrect
			(at -1.9625 -0.75 90)
			(size 0.825 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "VIN24_FUSED")
		)
		(pad "6" smd roundrect
			(at -1.9625 -1.25 90)
			(size 0.825 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "EFUSE_UVLO")
		)
		(pad "7" smd roundrect
			(at -1.25 -1.9625 90)
			(size 0.25 0.825)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "EFUSE_OVP")
		)
		(pad "8" smd roundrect
			(at -0.75 -1.9625 90)
			(size 0.25 0.825)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "9" smd roundrect
			(at -0.25 -1.9625 90)
			(size 0.25 0.825)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "EFUSE_DVDT")
		)
		(pad "10" smd roundrect
			(at 0.25 -1.9625 90)
			(size 0.25 0.825)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "EFUSE_ILIM")
		)
		(pad "11" smd roundrect
			(at 0.75 -1.9625 90)
			(size 0.25 0.825)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "unconnected-(U12-MODE-Pad11)")
		)
		(pad "12" smd roundrect
			(at 1.25 -1.9625 90)
			(size 0.25 0.825)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "EFUSE_RESET_N")
		)
		(pad "13" smd roundrect
			(at 1.9625 -1.25 90)
			(size 0.825 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "EFUSE_IMON")
		)
		(pad "14" smd roundrect
			(at 1.9625 -0.75 90)
			(size 0.825 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "EFUSE_FLT_N")
		)
		(pad "15" smd roundrect
			(at 1.9625 -0.25 90)
			(size 0.825 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "EFUSE_PGTH")
		)
		(pad "16" smd roundrect
			(at 1.9625 0.25 90)
			(size 0.825 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "EFUSE_PGOOD")
		)
		(pad "17" smd roundrect
			(at 1.9625 0.75 90)
			(size 0.825 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "V24_BUS")
		)
		(pad "18" smd roundrect
			(at 1.9625 1.25 90)
			(size 0.825 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "V24_BUS")
		)
		(pad "19" smd roundrect
			(at 1.25 1.9625 90)
			(size 0.25 0.825)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "unconnected-(U12-DNC-Pad19)")
		)
		(pad "20" smd roundrect
			(at 0.75 1.9625 90)
			(size 0.25 0.825)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "unconnected-(U12-DNC-Pad20)")
		)
		(pad "21" smd roundrect
			(at 0.25 1.9625 90)
			(size 0.25 0.825)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "unconnected-(U12-DNC-Pad21)")
		)
		(pad "22" smd roundrect
			(at -0.25 1.9625 90)
			(size 0.25 0.825)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "unconnected-(U12-DNC-Pad22)")
		)
		(pad "23" smd roundrect
			(at -0.75 1.9625 90)
			(size 0.25 0.825)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "unconnected-(U12-DNC-Pad23)")
		)
		(pad "24" smd roundrect
			(at -1.25 1.9625 90)
			(size 0.25 0.825)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "unconnected-(U12-DNC-Pad24)")
		)
		(pad "25" thru_hole circle
			(at -1.1 -1.1 90)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
		)
		(pad "25" thru_hole circle
			(at -1.1 0 90)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
		)
		(pad "25" thru_hole circle
			(at -1.1 1.1 90)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
		)
		(pad "25" thru_hole circle
			(at 0 -1.1 90)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
		)
		(pad "25" thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
		)
		(pad "25" smd rect
			(at 0 0 90)
			(size 2.7 2.7)
			(property pad_prop_heatsink)
			(layers "F.Cu")
			(net "GND")
			(zone_connect 2)
		)
		(pad "25" smd rect
			(at 0 0 90)
			(size 2.7 2.7)
			(property pad_prop_heatsink)
			(layers "B.Cu" "B.Mask")
			(net "GND")
			(zone_connect 2)
		)
		(pad "25" thru_hole circle
			(at 0 1.1 90)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
		)
		(pad "25" thru_hole circle
			(at 1.1 -1.1 90)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
		)
		(pad "25" thru_hole circle
			(at 1.1 0 90)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
		)
		(pad "25" thru_hole circle
			(at 1.1 1.1 90)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Texas_RGE0024H_VQFN-24-1EP_4x4mm_P0.5mm_EP2.7x2.7mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 119 95.75 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R517"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "210k"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07210KL"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "V24_BUS")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT_EFUSE_OVP")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 76.6 111.5 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R504"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "10k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-0710KL"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "EFUSE_OVP")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:TSOT-23-5"
		(locked yes)
		(layer "B.Cu")
		(at 77.5 99.5 -90)
		(descr "TSOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/MO-193D.pdf variant AB)")
		(tags "TSOT TO_SOT_SMD")
		(property "Reference" "U9"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "333mA spotlight CC driver"
			(at 0 -2.4 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.diodes.com/datasheet/download/AL8860.pdf"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "AL8860WT-7"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Diodes Incorporated"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 0.95 270)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT3_SW")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 270)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at -1.1375 -0.95 270)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT3_CTRL")
		)
		(pad "4" smd roundrect
			(at 1.1375 -0.95 270)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT3_LED_PLUS")
		)
		(pad "5" smd roundrect
			(at 1.1375 0.95 270)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "V24_SPOT")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TSOT-23-5.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMA"
		(locked yes)
		(layer "B.Cu")
		(at 72.75 99.5 90)
		(descr "Diode SMA (DO-214AC)")
		(tags "Diode SMA (DO-214AC)")
		(property "Reference" "D504"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "60V 1A flyback Schottky"
			(at 0 -2.6 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.diodes.com/datasheet/download/B130.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "B160-13-F"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Diodes Incorporated"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -2 0 90)
			(size 2.5 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1388888889)
			(net "V24_SPOT")
		)
		(pad "2" smd roundrect
			(at 2 0 90)
			(size 2.5 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1388888889)
			(net "SPOT3_SW")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 71 120.5 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R311"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "2.2k"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-072K2L"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_BIAS")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_11")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ELF:L_Bourns_SRP7050TA"
		(locked yes)
		(layer "B.Cu")
		(at 108.7 98)
		(descr "Bourns SRP7050TA, manufacturer recommended land pattern, SRP7050TA.pdf REV. 06/26 page 1; pads 2.95x3.5 mm, inner gap 2.5 mm, overall 8.4 mm; body 7.3x6.6 mm, maximum height 5.0 mm. https://www.bourns.com/docs/Product-Datasheets/SRP7050TA.pdf")
		(tags "Bourns SRP7050TA shielded power inductor")
		(property "Reference" "L500"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "22uH 2.5A RMS 5.5A sat"
			(at 0 -4.4 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.bourns.com/docs/Product-Datasheets/SRP7050TA.pdf"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Height" "5.0 mm maximum"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "SRP7050TA-220M"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Bourns"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -2.725 0)
			(size 2.95 3.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "BUCK5_SW")
		)
		(pad "2" smd rect
			(at 2.725 0)
			(size 2.95 3.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "+5V")
		)
		(embedded_fonts no)
	)
	(footprint "ELF:JST_PA_BM04B_PASS_TFT_1x04_P2mm_Vertical"
		(locked yes)
		(layer "B.Cu")
		(at 88.5 130 160)
		(property "Reference" "J12"
			(at 0 3.850001 340)
			(layer "B.Fab")
		)
		(property "Value" "MOTOR 1"
			(at 0 -3.850001 340)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/ePA-F.pdf"
			(at 0 0 340)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 340)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "BM04B-PASS-TFT(LF)(SN)"
			(at 0 0 340)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "JST"
			(at 0 0 340)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" smd rect
			(at -3 -3.5 160)
			(size 1 2.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "V24_MOTOR1")
		)
		(pad "2" smd rect
			(at -1 -3.5 160)
			(size 1 2.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "GND")
		)
		(pad "3" smd rect
			(at 1 -3.5 160)
			(size 1 2.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "CAN_H")
		)
		(pad "4" smd rect
			(at 3 -3.5 160)
			(size 1 2.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "CAN_L")
		)
		(pad "MP" smd rect
			(at -5.2 1.050001 160)
			(size 1.8 3.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "MP" smd rect
			(at 5.2 1.05 160)
			(size 1.8 3.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_JST:JST_GH_BM04B-GHS-TBT_1x04-1MP_P1.25mm_Vertical"
		(locked yes)
		(layer "B.Cu")
		(at 134.4 100.6 90)
		(descr "JST GH series connector, BM04B-GHS-TBT (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf)")
		(tags "connector JST GH vertical")
		(property "Reference" "J8"
			(at 0 4 270)
			(layer "B.Fab")
		)
		(property "Value" "ZONE 7"
			(at 0 -4 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eGH.pdf"
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "connector/SMD_single_row_plus_mounting_pad"
			(at 0 0 270)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "BM04B-GHS-TBT(LF)(SN)"
			(at 0 0 270)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "JST"
			(at 0 0 270)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.5 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.875 -1.95 90)
			(size 0.6 1.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "ZONE7_24V")
		)
		(pad "2" smd roundrect
			(at -0.625 -1.95 90)
			(size 0.6 1.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "ZONE7_W")
		)
		(pad "3" smd roundrect
			(at 0.625 -1.95 90)
			(size 0.6 1.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "ZONE7_N")
		)
		(pad "4" smd roundrect
			(at 1.875 -1.95 90)
			(size 0.6 1.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "ZONE7_C")
		)
		(pad "MP" smd roundrect
			(at -3.725 1.4 90)
			(size 1 2.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "MP" smd roundrect
			(at 3.725 1.4 90)
			(size 1 2.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_JST.3dshapes/JST_GH_BM04B-GHS-TBT_1x04-1MP_P1.25mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 98.5 91.6)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R511"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "24.9k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-0724K9L"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "BUCK5_FB")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ELF:L_Bourns_SRN6045"
		(locked yes)
		(layer "B.Cu")
		(at 83.25 92.9 90)
		(descr "Bourns SRN6045 (not SRN6045TA), manufacturer recommended land pattern, SRN6045.pdf REV. 01/20 page 1; pads 2.0x6.0 mm, inner gap 2.3 mm, overall 6.3 mm; nominal body 6.0x6.0 mm, height 4.5 mm maximum. https://www.bourns.com/docs/Product-Datasheets/SRN6045.pdf")
		(tags "Bourns SRN6045 semi-shielded power inductor")
		(property "Reference" "L502"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "220uH +/-20%, .6A RMS .7A saturation"
			(at 0 -4.1 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.bourns.com/docs/Product-Datasheets/SRN6045.pdf"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Height" "4.5 mm maximum"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "SRN6045-221M"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Bourns"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -2.15 0 90)
			(size 2 6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "SPOT1_LED_MINUS")
		)
		(pad "2" smd rect
			(at 2.15 0 90)
			(size 2 6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "SPOT1_SW")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 73.5 105.5 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R208"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "100k"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07100KL"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_08")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 108.5 125.4 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R40"
			(at 0 1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-0710KL"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "USB_VBUS")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:TSOT-23-5"
		(locked yes)
		(layer "B.Cu")
		(at 78.5 85.5 90)
		(descr "TSOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/MO-193D.pdf variant AB)")
		(tags "TSOT TO_SOT_SMD")
		(property "Reference" "U7"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "333mA spotlight CC driver"
			(at 0 -2.4 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.diodes.com/datasheet/download/AL8860.pdf"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "AL8860WT-7"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Diodes Incorporated"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT1_SW")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 90)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at -1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT1_CTRL")
		)
		(pad "4" smd roundrect
			(at 1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT1_LED_PLUS")
		)
		(pad "5" smd roundrect
			(at 1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "V24_SPOT")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TSOT-23-5.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric"
		(locked yes)
		(layer "B.Cu")
		(at 104.75 84)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C521"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "10uF 50V X7R"
			(at 0 -2.3 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM32ER71H106KA12-04A.pdf"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "GRM32ER71H106KA12L"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Murata"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net "V24_SPOT")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 73.5 119.35)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R502"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(property "Value" "10k"
			(at 0 -1.43 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-0710KL"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "EFUSE_UVLO")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 121 111 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R316"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "2.2k"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-072K2L"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_BIAS")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_16")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 120.75 95.75 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R518"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "10k"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-0710KL"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT_EFUSE_OVP")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT_RTN")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric"
		(locked yes)
		(layer "B.Cu")
		(at 75.6 80.75 90)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C520"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "10uF 50V X7R"
			(at 0 -2.3 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM32ER71H106KA12-04A.pdf"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "GRM32ER71H106KA12L"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Murata"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net "V24_SPOT")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 118 112.5 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R214"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "100k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07100KL"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_14")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 97 100.5 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R512"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "10k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-0710KL"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "BUCK5_PGOOD")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 128.5 110 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R318"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "2.2k"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-072K2L"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_BIAS")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_18")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric"
		(locked yes)
		(layer "B.Cu")
		(at 107 92)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C510"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "22uF 25V X7R"
			(at 0 -2.3 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM32ER71E226KE15-01.pdf"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "GRM32ER71E226KE15L"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Murata"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net "+5V")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 76.6 113.25)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R503"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "210k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07210KL"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "VIN24_FUSED")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "EFUSE_OVP")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric"
		(locked yes)
		(layer "B.Cu")
		(at 107 88.2)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C511"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "22uF 25V X7R"
			(at 0 -2.3 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM32ER71E226KE15-01.pdf"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "GRM32ER71E226KE15L"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Murata"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net "+5V")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 79.6 112.2 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R507"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "10k"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-0710KL"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "EFUSE_IMON")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 118 115 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R314"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "2.2k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-072K2L"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_BIAS")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_14")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 100 73 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(property "Value" "1u"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "C1608X7R1E105K080AB"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "TDK"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "MCU_EN")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 123.05 99.3)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R514"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "4.7k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://yageogroup.com/component-documentation/download/specsheet/RC0603FR-074K7L"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-074K7L"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "LIGHT_ENABLE_SAFE")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 76.6 116.75 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C503"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "100nF 100V X7R"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.murata.com/products/productdetail?partno=GRM188R72A104KA35%23"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "GRM188R72A104KA35D"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Murata"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "EFUSE_DVDT")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "EL:JST_GH_BM06B-GHS-TBT_1x06-1MP_P1.25mm_Vertical"
		(locked yes)
		(layer "B.Cu")
		(at 127 116 180)
		(descr "JST GH series connector, BM06B-GHS-TBT (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf)")
		(tags "connector JST GH vertical")
		(property "Reference" "J9"
			(at 0 4.1 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "SPOTLIGHT 3 PAIRS"
			(at 0 -4 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eGH.pdf"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "connector/SMD_single_row_plus_mounting_pad"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "BM06B-GHS-TBT(LF)(SN)"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "JST"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.5 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -3.125 -1.95 180)
			(size 0.6 1.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT1_LED_PLUS")
		)
		(pad "2" smd roundrect
			(at -1.875 -1.95 180)
			(size 0.6 1.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT1_LED_MINUS")
		)
		(pad "3" smd roundrect
			(at -0.625 -1.95 180)
			(size 0.6 1.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT2_LED_PLUS")
		)
		(pad "4" smd roundrect
			(at 0.625 -1.95 180)
			(size 0.6 1.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT2_LED_MINUS")
		)
		(pad "5" smd roundrect
			(at 1.875 -1.95 180)
			(size 0.6 1.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT3_LED_PLUS")
		)
		(pad "6" smd roundrect
			(at 3.125 -1.95 180)
			(size 0.6 1.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT3_LED_MINUS")
		)
		(pad "MP" smd roundrect
			(at -4.975 1.4 180)
			(size 1 2.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "MP" smd roundrect
			(at 4.975 1.4 180)
			(size 1 2.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_JST.3dshapes/JST_GH_BM06B-GHS-TBT_1x06-1MP_P1.25mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 125 103.2)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R520"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "10k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-0710KL"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT_EFUSE_FLT_N")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(locked yes)
		(layer "B.Cu")
		(at 65 107 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP8"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "EFUSE_RESET_N"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom dnp)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net "EFUSE_RESET_N")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(locked yes)
		(layer "B.Cu")
		(at 116.5 88.5 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP5"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "+3V3"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom dnp)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net "+3V3")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 120.75 107.25 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R515"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "24.3k"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-0724K3L"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT_EFUSE_ILIM")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT_RTN")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ELF:SOT-23-6_FabPin1"
		(locked yes)
		(layer "B.Cu")
		(at 102 70)
		(descr "SOT, 6 Pin (JEDEC MO-178 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-178)")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U18"
			(at 0 2.4 180)
			(layer "B.Fab")
		)
		(property "Value" "TPS3808G33"
			(at 0 -2.4 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps3808.pdf"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "TPS3808G33DBVR"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "READY_3V3")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(pad "4" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "unconnected-(U18-CT-Pad4)")
		)
		(pad "5" smd roundrect
			(at 1.1375 0)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(pad "6" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 125 106.5 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R217"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "100k"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07100KL"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_17")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 82.2 108.8 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R505"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "165k"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07165KL"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "V24_BUS")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "EFUSE_PGTH")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric"
		(locked yes)
		(layer "B.Cu")
		(at 117.4 82)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C513"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "22uF 25V X7R"
			(at 0 -2.3 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM32ER71E226KE15-01.pdf"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "GRM32ER71E226KE15L"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Murata"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net "+3V3")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-563"
		(locked yes)
		(layer "B.Cu")
		(at 114.75 75.5 -90)
		(descr "SOT, 6 Pin (https://www.jedec.org/system/files/docs/MO-293B.pdf)")
		(tags "SOT TO_SOT_SMD JEDEC-MO-293-UAAD Texas-DRL-6")
		(property "Reference" "U20"
			(at 0 1.65 90)
			(layer "B.Fab")
		)
		(property "Value" "TMP112AIDRLR"
			(at 0 -1.65 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmp112.pdf"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "TMP112AIDRLR"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7125 0.5 270)
			(size 0.675 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "I2C_SCL")
		)
		(pad "2" smd roundrect
			(at -0.7125 0 270)
			(size 0.675 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at -0.7125 -0.5 270)
			(size 0.675 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "unconnected-(U20-ALERT-Pad3)")
		)
		(pad "4" smd roundrect
			(at 0.7125 -0.5 270)
			(size 0.675 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "5" smd roundrect
			(at 0.7125 0 270)
			(size 0.675 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(pad "6" smd roundrect
			(at 0.7125 0.5 270)
			(size 0.675 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "I2C_SDA")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-563.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMB"
		(locked yes)
		(layer "B.Cu")
		(at 83.75 122.5)
		(descr "Diode SMB (DO-214AA)")
		(tags "Diode SMB (DO-214AA)")
		(property "Reference" "D500"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(property "Value" "SMBJ33CA 33V bidirectional TVS"
			(at 0 -3.1 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.littelfuse.com/~/media/electronics/datasheets/tvs_diodes/littelfuse_tvs_diode_smbj_datasheet.pdf.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "SMBJ33CA"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Littelfuse"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 3 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -2.15 0)
			(size 2.5 2.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1086956522)
			(net "VIN24_FUSED")
		)
		(pad "2" smd roundrect
			(at 2.15 0)
			(size 2.5 2.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1086956522)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMB.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric"
		(locked yes)
		(layer "B.Cu")
		(at 79.5 80.75 90)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C519"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "10uF 50V X7R"
			(at 0 -2.3 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM32ER71H106KA12-04A.pdf"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "GRM32ER71H106KA12L"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Murata"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net "V24_SPOT")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SON:VSON-8_3.3x3.3mm_P0.65mm_NexFET"
		(locked yes)
		(layer "B.Cu")
		(at 91.25 125)
		(descr "8-Lead Plastic Dual Flat, No Lead Package (MF) - 3.3x3.3x1 mm Body [VSON] http://www.ti.com/lit/ds/symlink/csd87334q3d.pdf")
		(tags "VSON 0.65")
		(property "Reference" "Q500"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(property "Value" "100V reverse blocking MOSFET"
			(at 0 -2.8 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/csd19537q3.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "CSD19537Q3"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0.526 -0.242 0)
			(layer "B.Fab")
		)
		(pad "" smd rect
			(at -0.09 -0.61)
			(size 0.57 0.738)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at -0.09 0.61)
			(size 0.57 0.738)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at 0.86 -0.61)
			(size 0.57 0.738)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at 0.86 0.61)
			(size 0.57 0.738)
			(layers "B.Paste")
		)
		(pad "" smd roundrect
			(at 1.44 -0.9725)
			(size 0.63 0.5)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 1.44 -0.33)
			(size 0.63 0.5)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 1.44 0.33)
			(size 0.63 0.5)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 1.44 0.9725)
			(size 0.63 0.5)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -1.44 0.97)
			(size 0.63 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "VIN24_FUSED")
		)
		(pad "2" smd roundrect
			(at -1.44 0.33)
			(size 0.63 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "VIN24_FUSED")
		)
		(pad "3" smd roundrect
			(at -1.44 -0.33)
			(size 0.63 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "VIN24_FUSED")
		)
		(pad "4" smd roundrect
			(at -1.44 -0.97)
			(size 0.63 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "EFUSE_BGATE")
		)
		(pad "5" smd custom
			(at 0.385 0)
			(size 1.9 2.45)
			(layers "B.Cu" "B.Mask")
			(net "VIN24_RPP")
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 1.371 0.72) (xy 0.95 0.72) (xy 0.95 0.58) (xy 1.37 0.58) (xy 1.37 0.08) (xy 0.95 0.08) (xy 0.95 -0.08)
						(xy 1.37 -0.08) (xy 1.37 -0.58) (xy 0.95 -0.58) (xy 0.95 -0.72) (xy 1.37 -0.72) (xy 1.37 -1.225)
						(xy -0.95 -1.225) (xy -0.95 1.225) (xy 1.371 1.225)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_SON.3dshapes/VSON-8_3.3x3.3mm_P0.65mm_NexFET.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 105 125.6 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C31"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "100n"
			(at 0 -1.43 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "GRM188R72A104KA35D"
			(at 0 0 270)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Murata"
			(at 0 0 270)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "USB_VBUS")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(locked yes)
		(layer "B.Cu")
		(at 88 108.25)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP3"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(property "Value" "V24_BUS"
			(at 0 -1.55 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom dnp)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 180)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net "V24_BUS")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 96 103 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R304"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "2.2k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-072K2L"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_BIAS")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_04")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 116.5 106.45 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C518"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "100nF 100V X7R"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.murata.com/products/productdetail?partno=GRM188R72A104KA35%23"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "GRM188R72A104KA35D"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Murata"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "V24_SPOT")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(locked yes)
		(layer "B.Cu")
		(at 103.5 103.5 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP4"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "+5V"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom dnp)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net "+5V")
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:TSOT-23-5"
		(locked yes)
		(layer "B.Cu")
		(at 100 83)
		(descr "TSOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/MO-193D.pdf variant AB)")
		(tags "TSOT TO_SOT_SMD")
		(property "Reference" "U8"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "333mA spotlight CC driver"
			(at 0 -2.4 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.diodes.com/datasheet/download/AL8860.pdf"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "AL8860WT-7"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Diodes Incorporated"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT2_SW")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "3" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT2_CTRL")
		)
		(pad "4" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT2_LED_PLUS")
		)
		(pad "5" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "V24_SPOT")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TSOT-23-5.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ELF:Expansion_SolderPads_1x07_P1p27mm"
		(layer "B.Cu")
		(at 106 75.04)
		(property "Reference" "J18"
			(at 0 1.5 180)
			(layer "B.Fab")
		)
		(property "Value" "GPIO EXPANSION 3V3"
			(at 0 -1.5 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "PCB FEATURE"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "PCB"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" smd circle
			(at -3.81 0)
			(size 0.85 0.85)
			(layers "B.Cu" "B.Mask")
			(net "+3V3")
		)
		(pad "2" smd circle
			(at -2.54 0)
			(size 0.85 0.85)
			(layers "B.Cu" "B.Mask")
			(net "GND")
		)
		(pad "3" smd circle
			(at -1.27 0)
			(size 0.85 0.85)
			(layers "B.Cu" "B.Mask")
			(net "GPIO19")
		)
		(pad "4" smd circle
			(at 0 0)
			(size 0.85 0.85)
			(layers "B.Cu" "B.Mask")
			(net "GPIO20")
		)
		(pad "5" smd circle
			(at 1.27 0)
			(size 0.85 0.85)
			(layers "B.Cu" "B.Mask")
			(net "GPIO21")
		)
		(pad "6" smd circle
			(at 2.54 0)
			(size 0.85 0.85)
			(layers "B.Cu" "B.Mask")
			(net "GPIO22")
		)
		(pad "7" smd circle
			(at 3.81 0)
			(size 0.85 0.85)
			(layers "B.Cu" "B.Mask")
			(net "GPIO23")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(locked yes)
		(layer "B.Cu")
		(at 91.9 97.3 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor")
		(property "Reference" "C507"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "220nF 50V X7R"
			(at 0 -1.68 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C2012X7R1H224K125AA"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "C2012X7R1H224K125AA"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "TDK"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "V24_LOGIC")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 88.5 111 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R210"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "100k"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07100KL"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_10")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 122.5 107.25 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R519"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "10k"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-0710KL"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT_EFUSE_IMON")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT_RTN")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 119 92 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R319"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "2.2k"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-072K2L"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_BIAS")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_19")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 107.3 123.9 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R39"
			(at 0 1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Value" "33k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0733KL"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-0733KL"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "USB_READY_SELECT")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ELF:JST_PA_BM04B_PASS_TFT_1x04_P2mm_Vertical"
		(locked yes)
		(layer "B.Cu")
		(at 113 129.5 -160)
		(property "Reference" "J13"
			(at 0 3.850001 20)
			(layer "B.Fab")
		)
		(property "Value" "MOTOR 2"
			(at 0 -3.850001 20)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/ePA-F.pdf"
			(at 0 0 20)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 20)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "BM04B-PASS-TFT(LF)(SN)"
			(at 0 0 20)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "JST"
			(at 0 0 20)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" smd rect
			(at -3 -3.5 200)
			(size 1 2.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "V24_MOTOR2")
		)
		(pad "2" smd rect
			(at -1 -3.5 200)
			(size 1 2.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "GND")
		)
		(pad "3" smd rect
			(at 1 -3.5 200)
			(size 1 2.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "CAN_H")
		)
		(pad "4" smd rect
			(at 3 -3.5 200)
			(size 1 2.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "CAN_L")
		)
		(pad "MP" smd rect
			(at -5.2 1.05 200)
			(size 1.8 3.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "MP" smd rect
			(at 5.2 1.050001 200)
			(size 1.8 3.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric"
		(locked yes)
		(layer "B.Cu")
		(at 112.3 89.4)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C512"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "22uF 25V X7R"
			(at 0 -2.3 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.murata.com/-/media/webrenewal/tool/library/common-pdf/dynamic-model/component-list-d-mlcc-2504.ashx?cvid=20250523010405000000&la=en"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "GRM32ER71E226KE15L"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Murata"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net "+5V")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 78.7 108.8 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R508"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "10k"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-0710KL"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "EFUSE_FLT_N")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 76.6 115 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R500"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "4.02k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-074K02L"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "EFUSE_ILIM")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 90.5 103 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R207"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "100k"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07100KL"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_07")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 130 102 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R321"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "2.2k"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-072K2L"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_BIAS")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_21")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 95 76.75 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R10"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(property "Value" "100k"
			(at 0 -1.43 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07100KL"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "SPOT2_PWM")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(locked yes)
		(layer "B.Cu")
		(at 72.5 82 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R303"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Value" "2.2k"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "MPN" "RC0603FR-072K2L"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Yageo"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GATE_BIAS")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "PWM_03")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fuse:Fuse_Littelfuse-NANO2-451_453"
		(locked yes)
		(layer "B.Cu")
		(at 90 82 180)
		(descr "Littelfuse NANO2 https://www.littelfuse.com/~/media/electronics/datasheets/fuses/littelfuse_fuse_451_453_datasheet.pdf.pdf")
		(tags "Fuse Nano2")
		(property "Reference" "F11"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Value" "0.5A logic branch fuse"
			(at 0 -2.7 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.littelfuse.com/assetdocs/fuse-451-and-453-datasheet?assetguid=533cd5cc-956c-4243-867f-6ab5a62f6ba1"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "0451.500MRL"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Littelfuse"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -2.455 0 180)
			(size 1.96 3.15)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "V24_BUS")
		)
		(pad "2" smd rect
			(at 2.455 0 180)
			(size 1.96 3.15)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "V24_LOGIC")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Fuse.3dshapes/Fuse_Littelfuse-NANO2-451_453.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 90.910995 63)
		(end 109.089004 63)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 109.089004 63)
		(mid 100 138.1)
		(end 90.910995 63)
		(layer "Edge.Cuts")
	)
	(gr_text "1"
		(at 70 83.75 0)
		(layer "F.SilkS")
	)
	(gr_text "30"
		(at 72 115.25 0)
		(layer "F.SilkS")
	)
	(gr_text "J1"
		(at 79 128.5 0)
		(layer "F.SilkS")
	)
	(gr_text "G4*"
		(at 86.25 65.9 0)
		(layer "F.SilkS")
	)
	(gr_text "G15*"
		(at 112 67.19 0)
		(layer "F.SilkS")
	)
	(gr_text "J16 BRAKE"
		(at 113.8 120.699999 0)
		(layer "F.SilkS")
	)
	(gr_text "BOOT"
		(at 115 85.5 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 119.159999 125.699999 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 127.182622 89.046988 0)
		(layer "F.SilkS")
	)
	(gr_text "J15 UART"
		(at 130.36131 90.84229 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 132 96 0)
		(layer "F.SilkS")
	)
	(gr_text "J17 ARM"
		(at 134 93 0)
		(layer "F.SilkS")
	)
	(gr_text "J2 LED Z1-6"
		(at 66 99 90)
		(layer "F.SilkS")
	)
	(gr_text "CAN TERM"
		(at 92.5 131 90)
		(layer "F.SilkS")
	)
	(gr_text "RESET"
		(at 103.5 91.5 90)
		(layer "F.SilkS")
	)
	(gr_text "J14 USB"
		(at 106.5 134.425 90)
		(layer "F.SilkS")
	)
	(gr_text "J9 SPOT"
		(at 127 111.9 0)
		(layer "B.SilkS")
	)
	(gr_text "1"
		(at 130.125 119.45 0)
		(layer "B.SilkS")
	)
	(gr_text "J12 M1"
		(at 96 127.5 0)
		(layer "B.SilkS")
	)
	(gr_text ""
		(at 100 65 0)
		(layer "B.SilkS")
	)
	(gr_text "1"
		(at 100.69 75.54 0)
		(layer "B.SilkS")
	)
	(gr_text "J18 GPIO"
		(at 106 73.04 0)
		(layer "B.SilkS")
	)
	(gr_text "J13 M2"
		(at 112.5 124.5 0)
		(layer "B.SilkS")
	)
	(gr_text "TEMP"
		(at 114.75 78 0)
		(layer "B.SilkS")
	)
	(gr_text "J8 Z7"
		(at 128.9 99.6 0)
		(layer "B.SilkS")
	)
	(gr_text "1"
		(at 131.449999 104.475 0)
		(layer "B.SilkS")
	)
	(gr_text "engineered lighting"
		(at 81.75 75.37 0)
		(layer "B.SilkS")
	)
	(gr_text "LIGHT v0.2"
		(at 81.75 76.95 0)
		(layer "B.SilkS")
	)
	(gr_text "engineered.lighting"
		(at 100.4 64.849999 0)
		(layer "B.SilkS")
	)
	(gr_text "\"A room is not a room"
		(at 126.5 85.02 0)
		(layer "B.SilkS")
	)
	(gr_text "without natural light.\""
		(at 126.5 86.17 0)
		(layer "B.SilkS")
	)
	(gr_text "— Louis Kahn"
		(at 126.5 87.32 0)
		(layer "B.SilkS")
	)
	(zone
		(layer "F.Cu")
		(name "ELF_MOLEX_BODY_J16_VIAS")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(keepout
			(tracks allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 117.234997 122.725) (xy 117.235001 130.674996) (xy 109.635003 130.674995) (xy 109.635 122.724998)
			)
		)
	)
	(zone
		(net "VIN24_FUSED")
		(layer "F.Cu")
		(name "MAIN_PROBE_FUSED_front_distributed_collector")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.15)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.4)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 80.25 121.9) (xy 79.5 123.05) (xy 78 123.05) (xy 77.25 121.9) (xy 77.25 118.9) (xy 79.6 118.9)
				(xy 79.6 120) (xy 80.25 120.5)
			)
		)
	)
	(zone
		(layer "F.Cu")
		(name "ELF_MOLEX_BODY_J16_COPPER")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(keepout
			(tracks not_allowed)
			(vias allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 109.665001 123.249985) (xy 109.669198 123.291077) (xy 109.691257 123.357647) (xy 109.728074 123.417336)
				(xy 109.777663 123.466925) (xy 109.837352 123.503742) (xy 109.903922 123.525801) (xy 109.945013 123.529999)
				(xy 112.384986 123.529998) (xy 112.426078 123.525801) (xy 112.492648 123.503742) (xy 112.552337 123.466925)
				(xy 112.601926 123.417336) (xy 112.638743 123.357647) (xy 112.660802 123.291077) (xy 112.665 123.249986)
				(xy 112.664999 122.724998) (xy 117.234997 122.725) (xy 117.234998 125.099999) (xy 116.665013 125.1)
				(xy 116.623921 125.104197) (xy 116.557351 125.126256) (xy 116.497662 125.163073) (xy 116.448073 125.212662)
				(xy 116.411256 125.272351) (xy 116.389197 125.338921) (xy 116.384999 125.380012) (xy 116.385 126.019985)
				(xy 116.389197 126.061077) (xy 116.411256 126.127647) (xy 116.448073 126.187336) (xy 116.497662 126.236925)
				(xy 116.557351 126.273742) (xy 116.623921 126.295801) (xy 116.665012 126.299999) (xy 117.234998 126.299998)
				(xy 117.234998 127.099998) (xy 116.665014 127.099999) (xy 116.623922 127.104196) (xy 116.557352 127.126255)
				(xy 116.497663 127.163072) (xy 116.448074 127.212661) (xy 116.411257 127.27235) (xy 116.389198 127.33892)
				(xy 116.385 127.380011) (xy 116.385001 128.019984) (xy 116.389198 128.061076) (xy 116.411257 128.127646)
				(xy 116.448074 128.187335) (xy 116.497663 128.236924) (xy 116.557352 128.273741) (xy 116.623922 128.2958)
				(xy 116.665013 128.299998) (xy 117.234999 128.299997) (xy 117.235001 130.674996) (xy 112.664999 130.674995)
				(xy 112.664999 130.150013) (xy 112.660802 130.108921) (xy 112.638743 130.042351) (xy 112.601926 129.982662)
				(xy 112.552337 129.933073) (xy 112.492648 129.896256) (xy 112.426078 129.874197) (xy 112.384987 129.869999)
				(xy 109.945014 129.87) (xy 109.903922 129.874197) (xy 109.837352 129.896256) (xy 109.777663 129.933073)
				(xy 109.728074 129.982662) (xy 109.691257 130.042351) (xy 109.669198 130.108921) (xy 109.665 130.150012)
				(xy 109.665 130.674995) (xy 109.635003 130.674995) (xy 109.635 122.724998) (xy 109.665 122.724998)
			)
		)
	)
	(zone
		(layers "F.Cu" "B.Cu")
		(name "M3_H2_SURFACE")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 121 70.5) (xy 120.991435 70.761612) (xy 120.965779 71.022104) (xy 120.923141 71.280361) (xy 120.863703 71.535276)
				(xy 120.78772 71.785757) (xy 120.695518 72.030733) (xy 120.58749 72.269154) (xy 120.464101 72.5)
				(xy 120.325878 72.72228) (xy 120.173413 72.935045) (xy 120.007359 73.137383) (xy 119.828427 73.328427)
				(xy 119.637383 73.507359) (xy 119.435045 73.673413) (xy 119.22228 73.825878) (xy 119 73.964101)
				(xy 118.769154 74.08749) (xy 118.530733 74.195518) (xy 118.285757 74.28772) (xy 118.035276 74.363703)
				(xy 117.780361 74.423141) (xy 117.522104 74.465779) (xy 117.261612 74.491435) (xy 117 74.5) (xy 116.738387 74.491435)
				(xy 116.477895 74.465779) (xy 116.219638 74.423141) (xy 115.964723 74.363703) (xy 115.714242 74.28772)
				(xy 115.469266 74.195518) (xy 115.230845 74.08749) (xy 115 73.964101) (xy 114.777719 73.825878)
				(xy 114.564954 73.673413) (xy 114.362616 73.507359) (xy 114.171572 73.328427) (xy 113.99264 73.137383)
				(xy 113.826586 72.935045) (xy 113.674121 72.72228) (xy 113.535898 72.5) (xy 113.412509 72.269154)
				(xy 113.304481 72.030733) (xy 113.212279 71.785757) (xy 113.136296 71.535276) (xy 113.076858 71.280361)
				(xy 113.03422 71.022104) (xy 113.008564 70.761612) (xy 113 70.5) (xy 113.008564 70.238387) (xy 113.03422 69.977895)
				(xy 113.076858 69.719638) (xy 113.136296 69.464723) (xy 113.212279 69.214242) (xy 113.304481 68.969266)
				(xy 113.412509 68.730845) (xy 113.535898 68.5) (xy 113.674121 68.277719) (xy 113.826586 68.064954)
				(xy 113.99264 67.862616) (xy 114.171572 67.671572) (xy 114.362616 67.49264) (xy 114.564954 67.326586)
				(xy 114.777719 67.174121) (xy 115 67.035898) (xy 115.230845 66.912509) (xy 115.469266 66.804481)
				(xy 115.714242 66.712279) (xy 115.964723 66.636296) (xy 116.219638 66.576858) (xy 116.477895 66.53422)
				(xy 116.738387 66.508564) (xy 117 66.5) (xy 117.261612 66.508564) (xy 117.522104 66.53422) (xy 117.780361 66.576858)
				(xy 118.035276 66.636296) (xy 118.285757 66.712279) (xy 118.530733 66.804481) (xy 118.769154 66.912509)
				(xy 119 67.035898) (xy 119.22228 67.174121) (xy 119.435045 67.326586) (xy 119.637383 67.49264) (xy 119.828427 67.671572)
				(xy 120.007359 67.862616) (xy 120.173413 68.064954) (xy 120.325878 68.277719) (xy 120.464101 68.5)
				(xy 120.58749 68.730845) (xy 120.695518 68.969266) (xy 120.78772 69.214242) (xy 120.863703 69.464723)
				(xy 120.923141 69.719638) (xy 120.965779 69.977895) (xy 120.991435 70.238387)
			)
		)
	)
	(zone
		(layers "F.Cu" "B.Cu")
		(name "M3_H1_SURFACE")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 87 70.5) (xy 86.991435 70.761612) (xy 86.965779 71.022104) (xy 86.923141 71.280361) (xy 86.863703 71.535276)
				(xy 86.78772 71.785757) (xy 86.695518 72.030733) (xy 86.58749 72.269154) (xy 86.464101 72.5) (xy 86.325878 72.72228)
				(xy 86.173413 72.935045) (xy 86.007359 73.137383) (xy 85.828427 73.328427) (xy 85.637383 73.507359)
				(xy 85.435045 73.673413) (xy 85.22228 73.825878) (xy 85 73.964101) (xy 84.769154 74.08749) (xy 84.530733 74.195518)
				(xy 84.285757 74.28772) (xy 84.035276 74.363703) (xy 83.780361 74.423141) (xy 83.522104 74.465779)
				(xy 83.261612 74.491435) (xy 83 74.5) (xy 82.738387 74.491435) (xy 82.477895 74.465779) (xy 82.219638 74.423141)
				(xy 81.964723 74.363703) (xy 81.714242 74.28772) (xy 81.469266 74.195518) (xy 81.230845 74.08749)
				(xy 81 73.964101) (xy 80.777719 73.825878) (xy 80.564954 73.673413) (xy 80.362616 73.507359) (xy 80.171572 73.328427)
				(xy 79.99264 73.137383) (xy 79.826586 72.935045) (xy 79.674121 72.72228) (xy 79.535898 72.5) (xy 79.412509 72.269154)
				(xy 79.304481 72.030733) (xy 79.212279 71.785757) (xy 79.136296 71.535276) (xy 79.076858 71.280361)
				(xy 79.03422 71.022104) (xy 79.008564 70.761612) (xy 79 70.5) (xy 79.008564 70.238387) (xy 79.03422 69.977895)
				(xy 79.076858 69.719638) (xy 79.136296 69.464723) (xy 79.212279 69.214242) (xy 79.304481 68.969266)
				(xy 79.412509 68.730845) (xy 79.535898 68.5) (xy 79.674121 68.277719) (xy 79.826586 68.064954) (xy 79.99264 67.862616)
				(xy 80.171572 67.671572) (xy 80.362616 67.49264) (xy 80.564954 67.326586) (xy 80.777719 67.174121)
				(xy 81 67.035898) (xy 81.230845 66.912509) (xy 81.469266 66.804481) (xy 81.714242 66.712279) (xy 81.964723 66.636296)
				(xy 82.219638 66.576858) (xy 82.477895 66.53422) (xy 82.738387 66.508564) (xy 83 66.5) (xy 83.261612 66.508564)
				(xy 83.522104 66.53422) (xy 83.780361 66.576858) (xy 84.035276 66.636296) (xy 84.285757 66.712279)
				(xy 84.530733 66.804481) (xy 84.769154 66.912509) (xy 85 67.035898) (xy 85.22228 67.174121) (xy 85.435045 67.326586)
				(xy 85.637383 67.49264) (xy 85.828427 67.671572) (xy 86.007359 67.862616) (xy 86.173413 68.064954)
				(xy 86.325878 68.277719) (xy 86.464101 68.5) (xy 86.58749 68.730845) (xy 86.695518 68.969266) (xy 86.78772 69.214242)
				(xy 86.863703 69.464723) (xy 86.923141 69.719638) (xy 86.965779 69.977895) (xy 86.991435 70.238387)
			)
		)
	)
	(zone
		(layers "F.Cu" "B.Cu")
		(name "M3_H4_SURFACE")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 128 124) (xy 127.991435 124.261612) (xy 127.965779 124.522104) (xy 127.923141 124.780361) (xy 127.863703 125.035276)
				(xy 127.78772 125.285757) (xy 127.695518 125.530733) (xy 127.58749 125.769154) (xy 127.464101 126)
				(xy 127.325878 126.22228) (xy 127.173413 126.435045) (xy 127.007359 126.637383) (xy 126.828427 126.828427)
				(xy 126.637383 127.007359) (xy 126.435045 127.173413) (xy 126.22228 127.325878) (xy 126 127.464101)
				(xy 125.769154 127.58749) (xy 125.530733 127.695518) (xy 125.285757 127.78772) (xy 125.035276 127.863703)
				(xy 124.780361 127.923141) (xy 124.522104 127.965779) (xy 124.261612 127.991435) (xy 124 128) (xy 123.738387 127.991435)
				(xy 123.477895 127.965779) (xy 123.219638 127.923141) (xy 122.964723 127.863703) (xy 122.714242 127.78772)
				(xy 122.469266 127.695518) (xy 122.230845 127.58749) (xy 122 127.464101) (xy 121.777719 127.325878)
				(xy 121.564954 127.173413) (xy 121.362616 127.007359) (xy 121.171572 126.828427) (xy 120.99264 126.637383)
				(xy 120.826586 126.435045) (xy 120.674121 126.22228) (xy 120.535898 126) (xy 120.412509 125.769154)
				(xy 120.304481 125.530733) (xy 120.212279 125.285757) (xy 120.136296 125.035276) (xy 120.076858 124.780361)
				(xy 120.03422 124.522104) (xy 120.008564 124.261612) (xy 120 124) (xy 120.008564 123.738387) (xy 120.03422 123.477895)
				(xy 120.076858 123.219638) (xy 120.136296 122.964723) (xy 120.212279 122.714242) (xy 120.304481 122.469266)
				(xy 120.412509 122.230845) (xy 120.535898 122) (xy 120.674121 121.777719) (xy 120.826586 121.564954)
				(xy 120.99264 121.362616) (xy 121.171572 121.171572) (xy 121.362616 120.99264) (xy 121.564954 120.826586)
				(xy 121.777719 120.674121) (xy 122 120.535898) (xy 122.230845 120.412509) (xy 122.469266 120.304481)
				(xy 122.714242 120.212279) (xy 122.964723 120.136296) (xy 123.219638 120.076858) (xy 123.477895 120.03422)
				(xy 123.738387 120.008564) (xy 124 120) (xy 124.261612 120.008564) (xy 124.522104 120.03422) (xy 124.780361 120.076858)
				(xy 125.035276 120.136296) (xy 125.285757 120.212279) (xy 125.530733 120.304481) (xy 125.769154 120.412509)
				(xy 126 120.535898) (xy 126.22228 120.674121) (xy 126.435045 120.826586) (xy 126.637383 120.99264)
				(xy 126.828427 121.171572) (xy 127.007359 121.362616) (xy 127.173413 121.564954) (xy 127.325878 121.777719)
				(xy 127.464101 122) (xy 127.58749 122.230845) (xy 127.695518 122.469266) (xy 127.78772 122.714242)
				(xy 127.863703 122.964723) (xy 127.923141 123.219638) (xy 127.965779 123.477895) (xy 127.991435 123.738387)
			)
		)
	)
	(zone
		(layers "F.Cu" "B.Cu")
		(name "M3_H3_SURFACE")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 80 124) (xy 79.991435 124.261612) (xy 79.965779 124.522104) (xy 79.923141 124.780361) (xy 79.863703 125.035276)
				(xy 79.78772 125.285757) (xy 79.695518 125.530733) (xy 79.58749 125.769154) (xy 79.464101 126) (xy 79.325878 126.22228)
				(xy 79.173413 126.435045) (xy 79.007359 126.637383) (xy 78.828427 126.828427) (xy 78.637383 127.007359)
				(xy 78.435045 127.173413) (xy 78.22228 127.325878) (xy 78 127.464101) (xy 77.769154 127.58749) (xy 77.530733 127.695518)
				(xy 77.285757 127.78772) (xy 77.035276 127.863703) (xy 76.780361 127.923141) (xy 76.522104 127.965779)
				(xy 76.261612 127.991435) (xy 76 128) (xy 75.738387 127.991435) (xy 75.477895 127.965779) (xy 75.219638 127.923141)
				(xy 74.964723 127.863703) (xy 74.714242 127.78772) (xy 74.469266 127.695518) (xy 74.230845 127.58749)
				(xy 74 127.464101) (xy 73.777719 127.325878) (xy 73.564954 127.173413) (xy 73.362616 127.007359)
				(xy 73.171572 126.828427) (xy 72.99264 126.637383) (xy 72.826586 126.435045) (xy 72.674121 126.22228)
				(xy 72.535898 126) (xy 72.412509 125.769154) (xy 72.304481 125.530733) (xy 72.212279 125.285757)
				(xy 72.136296 125.035276) (xy 72.076858 124.780361) (xy 72.03422 124.522104) (xy 72.008564 124.261612)
				(xy 72 124) (xy 72.008564 123.738387) (xy 72.03422 123.477895) (xy 72.076858 123.219638) (xy 72.136296 122.964723)
				(xy 72.212279 122.714242) (xy 72.304481 122.469266) (xy 72.412509 122.230845) (xy 72.535898 122)
				(xy 72.674121 121.777719) (xy 72.826586 121.564954) (xy 72.99264 121.362616) (xy 73.171572 121.171572)
				(xy 73.362616 120.99264) (xy 73.564954 120.826586) (xy 73.777719 120.674121) (xy 74 120.535898)
				(xy 74.230845 120.412509) (xy 74.469266 120.304481) (xy 74.714242 120.212279) (xy 74.964723 120.136296)
				(xy 75.219638 120.076858) (xy 75.477895 120.03422) (xy 75.738387 120.008564) (xy 76 120) (xy 76.261612 120.008564)
				(xy 76.522104 120.03422) (xy 76.780361 120.076858) (xy 77.035276 120.136296) (xy 77.285757 120.212279)
				(xy 77.530733 120.304481) (xy 77.769154 120.412509) (xy 78 120.535898) (xy 78.22228 120.674121)
				(xy 78.435045 120.826586) (xy 78.637383 120.99264) (xy 78.828427 121.171572) (xy 79.007359 121.362616)
				(xy 79.173413 121.564954) (xy 79.325878 121.777719) (xy 79.464101 122) (xy 79.58749 122.230845)
				(xy 79.695518 122.469266) (xy 79.78772 122.714242) (xy 79.863703 122.964723) (xy 79.923141 123.219638)
				(xy 79.965779 123.477895) (xy 79.991435 123.738387)
			)
		)
	)
	(zone
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu")
		(name "M3_H1_BORE")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 84.85 70.5) (xy 84.846039 70.620995) (xy 84.834172 70.741473) (xy 84.814452 70.860917) (xy 84.786962 70.978815)
				(xy 84.75182 71.094663) (xy 84.709177 71.207964) (xy 84.659214 71.318234) (xy 84.602146 71.425)
				(xy 84.538218 71.527804) (xy 84.467703 71.626208) (xy 84.390903 71.719789) (xy 84.308147 71.808147)
				(xy 84.219789 71.890903) (xy 84.126208 71.967703) (xy 84.027804 72.038218) (xy 83.925 72.102146)
				(xy 83.818234 72.159214) (xy 83.707964 72.209177) (xy 83.594663 72.25182) (xy 83.478815 72.286962)
				(xy 83.360917 72.314452) (xy 83.241473 72.334172) (xy 83.120995 72.346039) (xy 83 72.35) (xy 82.879004 72.346039)
				(xy 82.758526 72.334172) (xy 82.639082 72.314452) (xy 82.521184 72.286962) (xy 82.405336 72.25182)
				(xy 82.292035 72.209177) (xy 82.181765 72.159214) (xy 82.075 72.102146) (xy 81.972195 72.038218)
				(xy 81.873791 71.967703) (xy 81.78021 71.890903) (xy 81.691852 71.808147) (xy 81.609096 71.719789)
				(xy 81.532296 71.626208) (xy 81.461781 71.527804) (xy 81.397853 71.425) (xy 81.340785 71.318234)
				(xy 81.290822 71.207964) (xy 81.248179 71.094663) (xy 81.213037 70.978815) (xy 81.185547 70.860917)
				(xy 81.165827 70.741473) (xy 81.15396 70.620995) (xy 81.15 70.5) (xy 81.15396 70.379004) (xy 81.165827 70.258526)
				(xy 81.185547 70.139082) (xy 81.213037 70.021184) (xy 81.248179 69.905336) (xy 81.290822 69.792035)
				(xy 81.340785 69.681765) (xy 81.397853 69.575) (xy 81.461781 69.472195) (xy 81.532296 69.373791)
				(xy 81.609096 69.28021) (xy 81.691852 69.191852) (xy 81.78021 69.109096) (xy 81.873791 69.032296)
				(xy 81.972195 68.961781) (xy 82.075 68.897853) (xy 82.181765 68.840785) (xy 82.292035 68.790822)
				(xy 82.405336 68.748179) (xy 82.521184 68.713037) (xy 82.639082 68.685547) (xy 82.758526 68.665827)
				(xy 82.879004 68.65396) (xy 83 68.65) (xy 83.120995 68.65396) (xy 83.241473 68.665827) (xy 83.360917 68.685547)
				(xy 83.478815 68.713037) (xy 83.594663 68.748179) (xy 83.707964 68.790822) (xy 83.818234 68.840785)
				(xy 83.925 68.897853) (xy 84.027804 68.961781) (xy 84.126208 69.032296) (xy 84.219789 69.109096)
				(xy 84.308147 69.191852) (xy 84.390903 69.28021) (xy 84.467703 69.373791) (xy 84.538218 69.472195)
				(xy 84.602146 69.575) (xy 84.659214 69.681765) (xy 84.709177 69.792035) (xy 84.75182 69.905336)
				(xy 84.786962 70.021184) (xy 84.814452 70.139082) (xy 84.834172 70.258526) (xy 84.846039 70.379004)
			)
		)
	)
	(zone
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu")
		(name "M3_H4_BORE")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 125.85 124) (xy 125.846039 124.120995) (xy 125.834172 124.241473) (xy 125.814452 124.360917)
				(xy 125.786962 124.478815) (xy 125.75182 124.594663) (xy 125.709177 124.707964) (xy 125.659214 124.818234)
				(xy 125.602146 124.925) (xy 125.538218 125.027804) (xy 125.467703 125.126208) (xy 125.390903 125.219789)
				(xy 125.308147 125.308147) (xy 125.219789 125.390903) (xy 125.126208 125.467703) (xy 125.027804 125.538218)
				(xy 124.925 125.602146) (xy 124.818234 125.659214) (xy 124.707964 125.709177) (xy 124.594663 125.75182)
				(xy 124.478815 125.786962) (xy 124.360917 125.814452) (xy 124.241473 125.834172) (xy 124.120995 125.846039)
				(xy 124 125.85) (xy 123.879004 125.846039) (xy 123.758526 125.834172) (xy 123.639082 125.814452)
				(xy 123.521184 125.786962) (xy 123.405336 125.75182) (xy 123.292035 125.709177) (xy 123.181765 125.659214)
				(xy 123.075 125.602146) (xy 122.972195 125.538218) (xy 122.873791 125.467703) (xy 122.78021 125.390903)
				(xy 122.691852 125.308147) (xy 122.609096 125.219789) (xy 122.532296 125.126208) (xy 122.461781 125.027804)
				(xy 122.397853 124.925) (xy 122.340785 124.818234) (xy 122.290822 124.707964) (xy 122.248179 124.594663)
				(xy 122.213037 124.478815) (xy 122.185547 124.360917) (xy 122.165827 124.241473) (xy 122.15396 124.120995)
				(xy 122.15 124) (xy 122.15396 123.879004) (xy 122.165827 123.758526) (xy 122.185547 123.639082)
				(xy 122.213037 123.521184) (xy 122.248179 123.405336) (xy 122.290822 123.292035) (xy 122.340785 123.181765)
				(xy 122.397853 123.075) (xy 122.461781 122.972195) (xy 122.532296 122.873791) (xy 122.609096 122.78021)
				(xy 122.691852 122.691852) (xy 122.78021 122.609096) (xy 122.873791 122.532296) (xy 122.972195 122.461781)
				(xy 123.075 122.397853) (xy 123.181765 122.340785) (xy 123.292035 122.290822) (xy 123.405336 122.248179)
				(xy 123.521184 122.213037) (xy 123.639082 122.185547) (xy 123.758526 122.165827) (xy 123.879004 122.15396)
				(xy 124 122.15) (xy 124.120995 122.15396) (xy 124.241473 122.165827) (xy 124.360917 122.185547)
				(xy 124.478815 122.213037) (xy 124.594663 122.248179) (xy 124.707964 122.290822) (xy 124.818234 122.340785)
				(xy 124.925 122.397853) (xy 125.027804 122.461781) (xy 125.126208 122.532296) (xy 125.219789 122.609096)
				(xy 125.308147 122.691852) (xy 125.390903 122.78021) (xy 125.467703 122.873791) (xy 125.538218 122.972195)
				(xy 125.602146 123.075) (xy 125.659214 123.181765) (xy 125.709177 123.292035) (xy 125.75182 123.405336)
				(xy 125.786962 123.521184) (xy 125.814452 123.639082) (xy 125.834172 123.758526) (xy 125.846039 123.879004)
			)
		)
	)
	(zone
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu")
		(name "M3_H2_BORE")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 118.85 70.5) (xy 118.846039 70.620995) (xy 118.834172 70.741473) (xy 118.814452 70.860917) (xy 118.786962 70.978815)
				(xy 118.75182 71.094663) (xy 118.709177 71.207964) (xy 118.659214 71.318234) (xy 118.602146 71.425)
				(xy 118.538218 71.527804) (xy 118.467703 71.626208) (xy 118.390903 71.719789) (xy 118.308147 71.808147)
				(xy 118.219789 71.890903) (xy 118.126208 71.967703) (xy 118.027804 72.038218) (xy 117.925 72.102146)
				(xy 117.818234 72.159214) (xy 117.707964 72.209177) (xy 117.594663 72.25182) (xy 117.478815 72.286962)
				(xy 117.360917 72.314452) (xy 117.241473 72.334172) (xy 117.120995 72.346039) (xy 117 72.35) (xy 116.879004 72.346039)
				(xy 116.758526 72.334172) (xy 116.639082 72.314452) (xy 116.521184 72.286962) (xy 116.405336 72.25182)
				(xy 116.292035 72.209177) (xy 116.181765 72.159214) (xy 116.075 72.102146) (xy 115.972195 72.038218)
				(xy 115.873791 71.967703) (xy 115.78021 71.890903) (xy 115.691852 71.808147) (xy 115.609096 71.719789)
				(xy 115.532296 71.626208) (xy 115.461781 71.527804) (xy 115.397853 71.425) (xy 115.340785 71.318234)
				(xy 115.290822 71.207964) (xy 115.248179 71.094663) (xy 115.213037 70.978815) (xy 115.185547 70.860917)
				(xy 115.165827 70.741473) (xy 115.15396 70.620995) (xy 115.15 70.5) (xy 115.15396 70.379004) (xy 115.165827 70.258526)
				(xy 115.185547 70.139082) (xy 115.213037 70.021184) (xy 115.248179 69.905336) (xy 115.290822 69.792035)
				(xy 115.340785 69.681765) (xy 115.397853 69.575) (xy 115.461781 69.472195) (xy 115.532296 69.373791)
				(xy 115.609096 69.28021) (xy 115.691852 69.191852) (xy 115.78021 69.109096) (xy 115.873791 69.032296)
				(xy 115.972195 68.961781) (xy 116.075 68.897853) (xy 116.181765 68.840785) (xy 116.292035 68.790822)
				(xy 116.405336 68.748179) (xy 116.521184 68.713037) (xy 116.639082 68.685547) (xy 116.758526 68.665827)
				(xy 116.879004 68.65396) (xy 117 68.65) (xy 117.120995 68.65396) (xy 117.241473 68.665827) (xy 117.360917 68.685547)
				(xy 117.478815 68.713037) (xy 117.594663 68.748179) (xy 117.707964 68.790822) (xy 117.818234 68.840785)
				(xy 117.925 68.897853) (xy 118.027804 68.961781) (xy 118.126208 69.032296) (xy 118.219789 69.109096)
				(xy 118.308147 69.191852) (xy 118.390903 69.28021) (xy 118.467703 69.373791) (xy 118.538218 69.472195)
				(xy 118.602146 69.575) (xy 118.659214 69.681765) (xy 118.709177 69.792035) (xy 118.75182 69.905336)
				(xy 118.786962 70.021184) (xy 118.814452 70.139082) (xy 118.834172 70.258526) (xy 118.846039 70.379004)
			)
		)
	)
	(zone
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu")
		(name "M3_H3_BORE")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 77.85 124) (xy 77.846039 124.120995) (xy 77.834172 124.241473) (xy 77.814452 124.360917) (xy 77.786962 124.478815)
				(xy 77.75182 124.594663) (xy 77.709177 124.707964) (xy 77.659214 124.818234) (xy 77.602146 124.925)
				(xy 77.538218 125.027804) (xy 77.467703 125.126208) (xy 77.390903 125.219789) (xy 77.308147 125.308147)
				(xy 77.219789 125.390903) (xy 77.126208 125.467703) (xy 77.027804 125.538218) (xy 76.925 125.602146)
				(xy 76.818234 125.659214) (xy 76.707964 125.709177) (xy 76.594663 125.75182) (xy 76.478815 125.786962)
				(xy 76.360917 125.814452) (xy 76.241473 125.834172) (xy 76.120995 125.846039) (xy 76 125.85) (xy 75.879004 125.846039)
				(xy 75.758526 125.834172) (xy 75.639082 125.814452) (xy 75.521184 125.786962) (xy 75.405336 125.75182)
				(xy 75.292035 125.709177) (xy 75.181765 125.659214) (xy 75.075 125.602146) (xy 74.972195 125.538218)
				(xy 74.873791 125.467703) (xy 74.78021 125.390903) (xy 74.691852 125.308147) (xy 74.609096 125.219789)
				(xy 74.532296 125.126208) (xy 74.461781 125.027804) (xy 74.397853 124.925) (xy 74.340785 124.818234)
				(xy 74.290822 124.707964) (xy 74.248179 124.594663) (xy 74.213037 124.478815) (xy 74.185547 124.360917)
				(xy 74.165827 124.241473) (xy 74.15396 124.120995) (xy 74.15 124) (xy 74.15396 123.879004) (xy 74.165827 123.758526)
				(xy 74.185547 123.639082) (xy 74.213037 123.521184) (xy 74.248179 123.405336) (xy 74.290822 123.292035)
				(xy 74.340785 123.181765) (xy 74.397853 123.075) (xy 74.461781 122.972195) (xy 74.532296 122.873791)
				(xy 74.609096 122.78021) (xy 74.691852 122.691852) (xy 74.78021 122.609096) (xy 74.873791 122.532296)
				(xy 74.972195 122.461781) (xy 75.075 122.397853) (xy 75.181765 122.340785) (xy 75.292035 122.290822)
				(xy 75.405336 122.248179) (xy 75.521184 122.213037) (xy 75.639082 122.185547) (xy 75.758526 122.165827)
				(xy 75.879004 122.15396) (xy 76 122.15) (xy 76.120995 122.15396) (xy 76.241473 122.165827) (xy 76.360917 122.185547)
				(xy 76.478815 122.213037) (xy 76.594663 122.248179) (xy 76.707964 122.290822) (xy 76.818234 122.340785)
				(xy 76.925 122.397853) (xy 77.027804 122.461781) (xy 77.126208 122.532296) (xy 77.219789 122.609096)
				(xy 77.308147 122.691852) (xy 77.390903 122.78021) (xy 77.467703 122.873791) (xy 77.538218 122.972195)
				(xy 77.602146 123.075) (xy 77.659214 123.181765) (xy 77.709177 123.292035) (xy 77.75182 123.405336)
				(xy 77.786962 123.521184) (xy 77.814452 123.639082) (xy 77.834172 123.758526) (xy 77.846039 123.879004)
			)
		)
	)
	(zone
		(net "VIN24_FUSED")
		(layer "B.Cu")
		(name "MOUNT_REV_Q500_SOURCE_COLLECTOR")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(fill yes
			(thermal_gap 0.3)
			(thermal_bridge_width 0.4)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 88.1 124.42) (xy 90.13 124.42) (xy 90.13 126.3) (xy 88.1 126.3)
			)
		)
	)
	(zone
		(net "GND")
		(layer "B.Cu")
		(name "MAIN_PROBE_D505_anode_direct_3mm_collector")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.15)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.4)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 69.45 114.3) (xy 72.55 114.3) (xy 72.55 115.5) (xy 72.5 115.5) (xy 72.5 116.9) (xy 69.5 116.9)
				(xy 69.5 115.5) (xy 69.45 115.5)
			)
		)
	)
	(zone
		(net "GND")
		(layer "B.Cu")
		(name "MAIN_PROBE_J1_GND_distributed_collector")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.15)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.4)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 86.7 116.15) (xy 89.8 116.15) (xy 89.8 117.35) (xy 86.7 117.35)
			)
		)
	)
	(zone
		(net "GND")
		(layer "B.Cu")
		(name "MAIN_PROBE_C504_2_3mm_collector")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.15)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.4)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 108.95 119) (xy 113.05 119) (xy 113.05 122) (xy 108.95 122)
			)
		)
	)
	(zone
		(net "SPOT_RTN")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 123.4 108.975) (xy 116.625 108.975) (xy 116.625 97.95) (xy 119.75 97.95) (xy 119.75 94.025)
				(xy 123.4 94.025)
			)
		)
	)
	(zone
		(net "VIN24_FUSED")
		(layer "B.Cu")
		(name "MAIN_PROBE_FUSED_back_distributed_collector")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.15)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.4)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 79.475 119.225) (xy 79.475 121.4) (xy 80.25 122.5) (xy 80.25 124) (xy 84.25 124) (xy 84.25 127)
				(xy 77.25 127) (xy 77.25 125.5) (xy 77.25 121.6) (xy 78.025 121.05) (xy 78.025 119) (xy 79.25 119)
			)
		)
	)
	(zone
		(layer "B.Cu")
		(name "Preserve SPOT_RTN reference copper")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 123.4 98.6926) (xy 123.381093 98.750791) (xy 123.371005 98.762602) (xy 123.346951 98.786655)
				(xy 123.34695 98.786658) (xy 123.289354 98.899695) (xy 123.2745 98.993477) (xy 123.2745 99.60652)
				(xy 123.274501 99.606523) (xy 123.289352 99.700299) (xy 123.289354 99.700304) (xy 123.34695 99.813342)
				(xy 123.371005 99.837397) (xy 123.398781 99.891912) (xy 123.4 99.907399) (xy 123.4 100.8426) (xy 123.381093 100.900791)
				(xy 123.371005 100.912602) (xy 123.346951 100.936655) (xy 123.34695 100.936658) (xy 123.289354 101.049695)
				(xy 123.2745 101.143477) (xy 123.2745 101.75652) (xy 123.274501 101.756523) (xy 123.289352 101.850299)
				(xy 123.289354 101.850304) (xy 123.34695 101.963342) (xy 123.371005 101.987397) (xy 123.398781 102.041912)
				(xy 123.4 102.057399) (xy 123.4 103.70518) (xy 123.381093 103.763371) (xy 123.350501 103.790916)
				(xy 123.267689 103.838728) (xy 123.174497 103.93192) (xy 123.10861 104.046039) (xy 123.108609 104.046044)
				(xy 123.074501 104.173338) (xy 123.074501 104.305122) (xy 123.084833 104.343682) (xy 123.10861 104.43242)
				(xy 123.174497 104.546539) (xy 123.174499 104.546541) (xy 123.174501 104.546544) (xy 123.267687 104.63973)
				(xy 123.3505 104.687542) (xy 123.391441 104.73301) (xy 123.4 104.773278) (xy 123.4 108.876) (xy 123.381093 108.934191)
				(xy 123.331593 108.970155) (xy 123.301 108.975) (xy 117.5995 108.975) (xy 117.541309 108.956093)
				(xy 117.505345 108.906593) (xy 117.5005 108.876) (xy 117.5005 108.280253) (xy 117.500498 108.280241)
				(xy 117.49307 108.242897) (xy 117.499602 108.183594) (xy 117.503209 108.175423) (xy 117.503211 108.175422)
				(xy 117.547646 108.074786) (xy 117.5505 108.050185) (xy 117.550499 107.833841) (xy 117.563766 107.784336)
				(xy 117.565671 107.781037) (xy 117.572116 107.77126) (xy 117.590285 107.746965) (xy 117.598774 107.725725)
				(xy 117.604956 107.71299) (xy 117.616392 107.693186) (xy 117.617323 107.689707) (xy 117.624244 107.66388)
				(xy 117.624244 107.663879) (xy 117.625763 107.658208) (xy 117.639201 107.624596) (xy 117.642743 107.59484)
				(xy 117.6505 107.565892) (xy 117.6505 107.535557) (xy 117.651194 107.523854) (xy 117.685706 107.23395)
				(xy 117.698595 107.125676) (xy 117.724249 107.07013) (xy 117.751962 107.049168) (xy 117.75322 107.048528)
				(xy 117.848528 106.95322) (xy 117.909719 106.833126) (xy 117.9255 106.733488) (xy 117.9255 106.166512)
				(xy 117.909719 106.066874) (xy 117.909716 106.066869) (xy 117.909716 106.066867) (xy 117.848529 105.946782)
				(xy 117.848528 105.94678) (xy 117.770974 105.869226) (xy 117.791341 105.861939) (xy 117.835698 105.84096)
				(xy 117.877785 105.815734) (xy 117.917196 105.786505) (xy 117.953553 105.753553) (xy 117.986505 105.717196)
				(xy 118.015734 105.677785) (xy 118.04096 105.635698) (xy 118.061939 105.591341) (xy 118.07847 105.545142)
				(xy 118.090392 105.497545) (xy 118.097592 105.449008) (xy 118.1 105.4) (xy 118.097592 105.350991)
				(xy 118.097519 105.3505) (xy 118.374673 105.3505) (xy 118.374674 105.3505) (xy 118.44774 105.335966)
				(xy 118.447746 105.335961) (xy 118.456752 105.332233) (xy 118.457586 105.334248) (xy 118.466267 105.331799)
				(xy 118.486125 105.32209) (xy 118.494176 105.323926) (xy 118.50388 105.321189) (xy 118.546391 105.332655)
				(xy 118.550823 105.335006) (xy 118.55226 105.335966) (xy 118.552856 105.336084) (xy 118.558117 105.338875)
				(xy 118.576273 105.357639) (xy 118.596135 105.374601) (xy 118.597899 105.37999) (xy 118.600664 105.382847)
				(xy 118.602056 105.392681) (xy 118.610384 105.418112) (xy 118.638875 105.760008) (xy 118.624865 105.819567)
				(xy 118.585163 105.856438) (xy 118.496781 105.901471) (xy 118.40147 105.996782) (xy 118.340283 106.116867)
				(xy 118.340281 106.116874) (xy 118.3245 106.21651) (xy 118.3245 106.733489) (xy 118.340281 106.833125)
				(xy 118.340283 106.833132) (xy 118.401385 106.95305) (xy 118.401472 106.95322) (xy 118.49678 107.048528)
				(xy 118.496782 107.048529) (xy 118.616867 107.109716) (xy 118.616869 107.109716) (xy 118.616874 107.109719)
				(xy 118.692541 107.121703) (xy 118.71651 107.1255) (xy 118.716512 107.1255) (xy 119.28349 107.1255)
				(xy 119.304885 107.122111) (xy 119.383126 107.109719) (xy 119.50322 107.048528) (xy 119.598528 106.95322)
				(xy 119.659719 106.833126) (xy 119.6755 106.733488) (xy 119.6755 106.216512) (xy 119.675336 106.215479)
				(xy 119.669253 106.17707) (xy 119.659719 106.116874) (xy 119.659716 106.116869) (xy 119.659716 106.116867)
				(xy 119.598529 105.996782) (xy 119.598528 105.99678) (xy 119.50322 105.901472) (xy 119.503217 105.90147)
				(xy 119.383132 105.840283) (xy 119.383127 105.840281) (xy 119.383126 105.840281) (xy 119.343799 105.834052)
				(xy 119.323569 105.830848) (xy 119.269052 105.80307) (xy 119.241275 105.748554) (xy 119.2404 105.741307)
				(xy 119.226395 105.573251) (xy 119.240404 105.513694) (xy 119.286747 105.473743) (xy 119.347721 105.468662)
				(xy 119.395057 105.495028) (xy 120.045504 106.145475) (xy 120.073281 106.199992) (xy 120.0745 106.215479)
				(xy 120.0745 106.65652) (xy 120.074501 106.656523) (xy 120.089352 106.750299) (xy 120.089354 106.750304)
				(xy 120.14695 106.863342) (xy 120.236658 106.95305) (xy 120.349696 107.010646) (xy 120.443481 107.0255)
				(xy 121.056518 107.025499) (xy 121.05652 107.025499) (xy 121.056521 107.025498) (xy 121.103411 107.018072)
				(xy 121.150299 107.010647) (xy 121.150299 107.010646) (xy 121.150304 107.010646) (xy 121.263342 106.95305)
				(xy 121.35305 106.863342) (xy 121.410646 106.750304) (xy 121.4255 106.656519) (xy 121.425499 106.193482)
				(xy 121.413367 106.116874) (xy 121.410647 106.0997) (xy 121.410646 106.099698) (xy 121.410646 106.099696)
				(xy 121.35305 105.986658) (xy 121.263342 105.89695) (xy 121.260487 105.895495) (xy 121.203819 105.866621)
				(xy 121.160555 105.823356) (xy 121.150984 105.762924) (xy 121.163029 105.728912) (xy 121.17755 105.703762)
				(xy 121.22302 105.662822) (xy 121.283871 105.656428) (xy 121.333289 105.68326) (xy 121.795504 106.145475)
				(xy 121.823281 106.199992) (xy 121.8245 106.215479) (xy 121.8245 106.65652) (xy 121.824501 106.656523)
				(xy 121.839352 106.750299) (xy 121.839354 106.750304) (xy 121.89695 106.863342) (xy 121.986658 106.95305)
				(xy 122.099696 107.010646) (xy 122.193481 107.0255) (xy 122.806518 107.025499) (xy 122.80652 107.025499)
				(xy 122.806521 107.025498) (xy 122.853411 107.018072) (xy 122.900299 107.010647) (xy 122.900299 107.010646)
				(xy 122.900304 107.010646) (xy 123.013342 106.95305) (xy 123.10305 106.863342) (xy 123.160646 106.750304)
				(xy 123.1755 106.656519) (xy 123.175499 106.193482) (xy 123.163367 106.116874) (xy 123.160647 106.0997)
				(xy 123.160646 106.099698) (xy 123.160646 106.099696) (xy 123.10305 105.986658) (xy 123.013342 105.89695)
				(xy 122.900304 105.839354) (xy 122.900305 105.839354) (xy 122.806522 105.8245) (xy 122.806519 105.8245)
				(xy 122.365479 105.8245) (xy 122.307288 105.805593) (xy 122.295475 105.795504) (xy 121.629496 105.129525)
				(xy 121.601719 105.075008) (xy 121.6005 105.059521) (xy 121.6005 103.385439) (xy 121.6005 103.385438)
				(xy 121.58859 103.340989) (xy 121.58859 103.340988) (xy 121.58859 103.340987) (xy 121.580021 103.30901)
				(xy 121.58002 103.309008) (xy 121.540463 103.240493) (xy 121.540461 103.240491) (xy 121.54046 103.240489)
				(xy 121.284511 102.98454) (xy 121.284508 102.984538) (xy 121.215992 102.94498) (xy 121.215988 102.944978)
				(xy 121.139564 102.9245) (xy 121.139562 102.9245) (xy 120.460438 102.9245) (xy 120.460435 102.9245)
				(xy 120.384011 102.944978) (xy 120.384007 102.94498) (xy 120.315489 102.984539) (xy 119.915605 103.384422)
				(xy 119.877405 103.408171) (xy 119.871267 103.410252) (xy 119.85226 103.414034) (xy 119.844153 103.41945)
				(xy 119.831803 103.42364) (xy 119.813616 103.423874) (xy 119.796112 103.428811) (xy 119.782165 103.424279)
				(xy 119.770622 103.424428) (xy 119.760417 103.417212) (xy 119.757386 103.416227) (xy 119.756749 103.417766)
				(xy 119.747742 103.414035) (xy 119.74774 103.414034) (xy 119.747736 103.414033) (xy 119.674684 103.399501)
				(xy 119.674674 103.3995) (xy 119.275326 103.3995) (xy 119.275325 103.3995) (xy 119.275315 103.399501)
				(xy 119.202263 103.414033) (xy 119.202261 103.414033) (xy 119.20226 103.414034) (xy 119.202259 103.414034)
				(xy 119.193251 103.417766) (xy 119.192416 103.415751) (xy 119.146112 103.428811) (xy 119.107386 103.416227)
				(xy 119.106749 103.417766) (xy 119.097742 103.414035) (xy 119.09774 103.414034) (xy 119.097736 103.414033)
				(xy 119.024684 103.399501) (xy 119.024674 103.3995) (xy 118.625326 103.3995) (xy 118.625325 103.3995)
				(xy 118.625315 103.399501) (xy 118.552263 103.414033) (xy 118.552261 103.414033) (xy 118.55226 103.414034)
				(xy 118.552259 103.414034) (xy 118.543251 103.417766) (xy 118.542416 103.415751) (xy 118.496112 103.428811)
				(xy 118.457386 103.416227) (xy 118.456749 103.417766) (xy 118.447742 103.414035) (xy 118.44774 103.414034)
				(xy 118.447736 103.414033) (xy 118.374684 103.399501) (xy 118.374674 103.3995) (xy 117.975326 103.3995)
				(xy 117.975325 103.3995) (xy 117.975315 103.399501) (xy 117.902263 103.414033) (xy 117.902261 103.414033)
				(xy 117.90226 103.414034) (xy 117.902259 103.414034) (xy 117.893251 103.417766) (xy 117.892416 103.415751)
				(xy 117.846112 103.428811) (xy 117.807386 103.416227) (xy 117.806749 103.417766) (xy 117.797742 103.414035)
				(xy 117.79774 103.414034) (xy 117.797736 103.414033) (xy 117.724684 103.399501) (xy 117.724674 103.3995)
				(xy 117.325326 103.3995) (xy 117.325325 103.3995) (xy 117.325315 103.399501) (xy 117.252263 103.414033)
				(xy 117.252261 103.414033) (xy 117.25226 103.414034) (xy 117.252259 103.414034) (xy 117.243251 103.417766)
				(xy 117.242416 103.415751) (xy 117.196112 103.428811) (xy 117.157386 103.416227) (xy 117.156749 103.417766)
				(xy 117.147742 103.414035) (xy 117.14774 103.414034) (xy 117.147736 103.414033) (xy 117.074684 103.399501)
				(xy 117.074674 103.3995) (xy 116.724 103.3995) (xy 116.665809 103.380593) (xy 116.629845 103.331093)
				(xy 116.625 103.3005) (xy 116.625 99.984108) (xy 116.625 99.6995) (xy 116.643907 99.641309) (xy 116.693407 99.605345)
				(xy 116.724 99.6005) (xy 117.074673 99.6005) (xy 117.074674 99.6005) (xy 117.14774 99.585966) (xy 117.230601 99.530601)
				(xy 117.285966 99.44774) (xy 117.3005 99.374674) (xy 117.3005 98.049) (xy 117.319407 97.990809)
				(xy 117.368907 97.954845) (xy 117.3995 97.95) (xy 117.6505 97.95) (xy 117.708691 97.968907) (xy 117.744655 98.018407)
				(xy 117.7495 98.049) (xy 117.7495 99.374672) (xy 117.749501 99.374684) (xy 117.764033 99.447736)
				(xy 117.764035 99.447742) (xy 117.819397 99.530599) (xy 117.819399 99.530601) (xy 117.90226 99.585966)
				(xy 117.957808 99.597015) (xy 117.975315 99.600498) (xy 117.97532 99.600498) (xy 117.975326 99.6005)
				(xy 117.975327 99.6005) (xy 118.374673 99.6005) (xy 118.374674 99.6005) (xy 118.44774 99.585966)
				(xy 118.447746 99.585961) (xy 118.456752 99.582233) (xy 118.457586 99.584248) (xy 118.50388 99.571189)
				(xy 118.54261 99.583773) (xy 118.543248 99.582233) (xy 118.552255 99.585962) (xy 118.55226 99.585966)
				(xy 118.607808 99.597015) (xy 118.625315 99.600498) (xy 118.62532 99.600498) (xy 118.625326 99.6005)
				(xy 118.625327 99.6005) (xy 119.024673 99.6005) (xy 119.024674 99.6005) (xy 119.09774 99.585966)
				(xy 119.097746 99.585961) (xy 119.106752 99.582233) (xy 119.107586 99.584248) (xy 119.15388 99.571189)
				(xy 119.19261 99.583773) (xy 119.193248 99.582233) (xy 119.202255 99.585962) (xy 119.20226 99.585966)
				(xy 119.257808 99.597015) (xy 119.275315 99.600498) (xy 119.27532 99.600498) (xy 119.275326 99.6005)
				(xy 119.275327 99.6005) (xy 119.674673 99.6005) (xy 119.674674 99.6005) (xy 119.74774 99.585966)
				(xy 119.747746 99.585961) (xy 119.756752 99.582233) (xy 119.757586 99.584248) (xy 119.80388 99.571189)
				(xy 119.84261 99.583773) (xy 119.843248 99.582233) (xy 119.852255 99.585962) (xy 119.85226 99.585966)
				(xy 119.907808 99.597015) (xy 119.925315 99.600498) (xy 119.92532 99.600498) (xy 119.925326 99.6005)
				(xy 119.925327 99.6005) (xy 120.324673 99.6005) (xy 120.324674 99.6005) (xy 120.39774 99.585966)
				(xy 120.480601 99.530601) (xy 120.535966 99.44774) (xy 120.5505 99.374674) (xy 120.5505 97.875326)
				(xy 120.550499 97.875324) (xy 120.550499 97.875317) (xy 120.534286 97.793816) (xy 120.541476 97.733054)
				(xy 120.583008 97.688124) (xy 120.631383 97.6755) (xy 121.05 97.6755) (xy 121.05 97.943224) (xy 121.046446 97.946446)
				(xy 121.013494 97.982803) (xy 120.984265 98.022214) (xy 120.959039 98.064301) (xy 120.93806 98.108658)
				(xy 120.921529 98.154857) (xy 120.909607 98.202454) (xy 120.902407 98.250991) (xy 120.9 98.3) (xy 120.902407 98.349008)
				(xy 120.909607 98.397545) (xy 120.921529 98.445142) (xy 120.93806 98.491341) (xy 120.959039 98.535698)
				(xy 120.984265 98.577785) (xy 121.013494 98.617196) (xy 121.046446 98.653553) (xy 121.082803 98.686505)
				(xy 121.122214 98.715734) (xy 121.164301 98.74096) (xy 121.208658 98.761939) (xy 121.254857 98.77847)
				(xy 121.302454 98.790392) (xy 121.350991 98.797592) (xy 121.357021 98.797888) (xy 121.6245 99.122104)
				(xy 121.6245 99.5539) (xy 121.605593 99.612091) (xy 121.556093 99.648055) (xy 121.494907 99.648055)
				(xy 121.476 99.639636) (xy 121.378959 99.583609) (xy 121.378961 99.583609) (xy 121.329569 99.570375)
				(xy 121.251662 99.5495) (xy 121.119878 99.5495) (xy 121.04197 99.570375) (xy 120.992579 99.583609)
				(xy 120.87846 99.649496) (xy 120.785266 99.74269) (xy 120.719379 99.856809) (xy 120.706989 99.90305)
				(xy 120.68527 99.984108) (xy 120.68527 100.115892) (xy 120.693008 100.14477) (xy 120.719379 100.24319)
				(xy 120.785266 100.357309) (xy 120.785271 100.357315) (xy 120.807953 100.379998) (xy 120.835729 100.434515)
				(xy 120.826157 100.494947) (xy 120.807953 100.520002) (xy 120.785271 100.542684) (xy 120.785266 100.54269)
				(xy 120.719379 100.656809) (xy 120.719378 100.656814) (xy 120.68527 100.784108) (xy 120.68527 100.915892)
				(xy 120.714639 101.0255) (xy 120.719379 101.04319) (xy 120.785266 101.157309) (xy 120.785268 101.157311)
				(xy 120.78527 101.157314) (xy 120.878456 101.2505) (xy 120.878458 101.250501) (xy 120.87846 101.250503)
				(xy 120.99258 101.31639) (xy 120.992578 101.31639) (xy 120.992582 101.316391) (xy 120.992584 101.316392)
				(xy 121.119878 101.3505) (xy 121.11988 101.3505) (xy 121.25166 101.3505) (xy 121.251662 101.3505)
				(xy 121.348654 101.324511) (xy 121.356628 101.324929) (xy 121.363926 101.32168) (xy 121.386605 101.3265)
				(xy 121.409753 101.327714) (xy 121.423775 101.334401) (xy 121.575 101.42171) (xy 121.615941 101.46718)
				(xy 121.6245 101.507447) (xy 121.6245 101.75652) (xy 121.624501 101.756523) (xy 121.639352 101.850299)
				(xy 121.639354 101.850304) (xy 121.69695 101.963342) (xy 121.786658 102.05305) (xy 121.899696 102.110646)
				(xy 121.993481 102.1255) (xy 122.456518 102.125499) (xy 122.45652 102.125499) (xy 122.456521 102.125498)
				(xy 122.503411 102.118072) (xy 122.550299 102.110647) (xy 122.550299 102.110646) (xy 122.550304 102.110646)
				(xy 122.663342 102.05305) (xy 122.75305 101.963342) (xy 122.810646 101.850304) (xy 122.8255 101.756519)
				(xy 122.825499 101.143482) (xy 122.822651 101.1255) (xy 122.810647 101.0497) (xy 122.810646 101.049698)
				(xy 122.810646 101.049696) (xy 122.75305 100.936658) (xy 122.663342 100.84695) (xy 122.550304 100.789354)
				(xy 122.550305 100.789354) (xy 122.456522 100.7745) (xy 122.456519 100.7745) (xy 122.147621 100.7745)
				(xy 122.08943 100.755593) (xy 122.068128 100.734508) (xy 121.694272 100.230868) (xy 121.67477 100.172874)
				(xy 121.675025 100.164689) (xy 121.675705 100.155317) (xy 121.68627 100.115892) (xy 121.68627 100.00986)
				(xy 121.68653 100.006281) (xy 121.696777 99.981111) (xy 121.705177 99.955261) (xy 121.708196 99.953067)
				(xy 121.709603 99.949612) (xy 121.732685 99.935275) (xy 121.754677 99.919297) (xy 121.75841 99.919297)
				(xy 121.761578 99.917329) (xy 121.788676 99.919297) (xy 121.815863 99.919297) (xy 121.821642 99.921691)
				(xy 121.822603 99.921761) (xy 121.823367 99.922405) (xy 121.830205 99.925238) (xy 121.899696 99.960646)
				(xy 121.993481 99.9755) (xy 122.456518 99.975499) (xy 122.45652 99.975499) (xy 122.456521 99.975498)
				(xy 122.503411 99.968072) (xy 122.550299 99.960647) (xy 122.550299 99.960646) (xy 122.550304 99.960646)
				(xy 122.663342 99.90305) (xy 122.75305 99.813342) (xy 122.810646 99.700304) (xy 122.8255 99.606519)
				(xy 122.825499 98.993482) (xy 122.825498 98.993478) (xy 122.825498 98.993476) (xy 122.810647 98.8997)
				(xy 122.810646 98.899698) (xy 122.810646 98.899696) (xy 122.75305 98.786658) (xy 122.663342 98.69695)
				(xy 122.550304 98.639354) (xy 122.550305 98.639354) (xy 122.456522 98.6245) (xy 122.121449 98.6245)
				(xy 121.89707 98.352525) (xy 121.897592 98.349008) (xy 121.9 98.3) (xy 121.897592 98.250991) (xy 121.890392 98.202454)
				(xy 121.87847 98.154857) (xy 121.861939 98.108658) (xy 121.84096 98.064301) (xy 121.815734 98.022214)
				(xy 121.786505 97.982803) (xy 121.753553 97.946446) (xy 121.75 97.943225) (xy 121.75 97.672702)
				(xy 121.815989 97.655021) (xy 121.884511 97.61546) (xy 121.912485 97.587485) (xy 121.940461 97.559511)
				(xy 122.295474 97.204496) (xy 122.349991 97.176718) (xy 122.365478 97.175499) (xy 122.806521 97.175499)
				(xy 122.806522 97.175498) (xy 122.853411 97.168072) (xy 122.900299 97.160647) (xy 122.900299 97.160646)
				(xy 122.900304 97.160646) (xy 123.013342 97.10305) (xy 123.10305 97.013342) (xy 123.160646 96.900304)
				(xy 123.1755 96.806519) (xy 123.175499 96.543203) (xy 123.4 96.392551)
			)
		)
	)
	(zone
		(net "V24_BUS")
		(layer "B.Cu")
		(name "MAIN_PROBE_U12_OUT_3mm_collector")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.15)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.4)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 87.7 115.82) (xy 83.6 115.82) (xy 83.6 114.82) (xy 81.625 114.82) (xy 81.625 112.82) (xy 83.75 112.82)
				(xy 87.7 112.82)
			)
		)
	)
	(zone
		(net "V24_BUS")
		(layer "B.Cu")
		(name "MAIN_PROBE_D505_1_3mm_collector")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.15)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.4)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 68.95 111.1) (xy 73.05 111.1) (xy 73.05 114.1) (xy 68.95 114.1)
			)
		)
	)
	(zone
		(net "VIN24_RPP")
		(layer "B.Cu")
		(name "MAIN_PROBE_RPP_taper_3mm")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.15)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.4)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 83.5 120.05) (xy 83.5 121.7) (xy 80.5 121.7) (xy 80.5 120.5) (xy 81.45 120.05) (xy 81.45 119.05)
				(xy 82.55 119.05)
			)
		)
	)
	(zone
		(net "GND")
		(layer "In1.Cu")
		(name "Continuous top-side GND reference")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.4)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 109.559891 63.633056) (xy 110.734297 63.962245) (xy 111.896422 64.329003) (xy 113.046091 64.733239)
				(xy 114.182053 65.174517) (xy 115.303118 65.652373) (xy 116.408078 66.16629) (xy 117.495824 66.715753)
				(xy 118.565212 67.300186) (xy 119.615078 67.918952) (xy 120.644335 68.571409) (xy 121.651947 69.256901)
				(xy 122.636779 69.974659) (xy 123.597832 70.723948) (xy 124.534137 71.504018) (xy 125.444644 72.313994)
				(xy 126.328443 73.153064) (xy 127.184568 74.020313) (xy 128.01215 74.914858) (xy 128.810328 75.835772)
				(xy 129.578204 76.782018) (xy 130.315054 77.752701) (xy 131.020044 78.746725) (xy 131.692449 79.763066)
				(xy 132.331585 80.80069) (xy 132.936751 81.858466) (xy 133.507317 82.935283) (xy 134.042693 84.030031)
				(xy 134.542306 85.141537) (xy 135.005657 86.268694) (xy 135.432232 87.410251) (xy 135.821588 88.56502)
				(xy 136.173317 89.731798) (xy 136.487055 90.909364) (xy 136.762472 92.096491) (xy 136.99928 93.291939)
				(xy 137.197216 94.494373) (xy 137.35609 95.702634) (xy 137.475727 96.915404) (xy 137.556001 98.13141)
				(xy 137.596828 99.349348) (xy 137.598168 100.568024) (xy 137.560016 101.786079) (xy 137.482414 103.002252)
				(xy 137.365445 104.215255) (xy 137.209228 105.423855) (xy 137.013926 106.626771) (xy 136.779752 107.822699)
				(xy 136.506945 109.01043) (xy 136.195792 110.188695) (xy 135.846626 111.356244) (xy 135.459806 112.511876)
				(xy 135.035749 113.654345) (xy 134.574882 114.782502) (xy 134.077705 115.895121) (xy 133.544729 116.991055)
				(xy 132.976526 118.069133) (xy 132.373691 119.128226) (xy 131.736848 120.167234) (xy 131.066678 121.18505)
				(xy 130.363855 122.180647) (xy 129.629167 123.152912) (xy 128.863338 124.100884) (xy 128.067214 125.023515)
				(xy 127.241584 125.919894) (xy 126.387381 126.789007) (xy 125.505414 127.630032) (xy 124.59669 128.442004)
				(xy 123.662119 129.224115) (xy 122.702701 129.975526) (xy 121.719424 130.695463) (xy 120.713356 131.383144)
				(xy 119.685522 132.03787) (xy 118.637026 132.658936) (xy 117.568923 133.245718) (xy 116.482388 133.79757)
				(xy 115.378535 134.313926) (xy 114.25855 134.794232) (xy 113.123548 135.238009) (xy 111.974798 135.644762)
				(xy 110.813434 136.014087) (xy 109.640764 136.34557) (xy 108.457935 136.638889) (xy 107.266212 136.893726)
				(xy 106.066899 137.109805) (xy 104.861172 137.286913) (xy 103.650352 137.424854) (xy 102.43568 137.52349)
				(xy 101.218487 137.582711) (xy 100 137.602458) (xy 98.781513 137.582711) (xy 97.56432 137.52349)
				(xy 96.349648 137.424854) (xy 95.138828 137.286913) (xy 93.933101 137.109805) (xy 92.733788 136.893726)
				(xy 91.542065 136.638889) (xy 90.359235 136.345571) (xy 89.186547 136.014083) (xy 88.025211 135.644766)
				(xy 86.876461 135.238014) (xy 85.741451 134.794233) (xy 84.621465 134.313926) (xy 83.517612 133.797571)
				(xy 82.431077 133.245719) (xy 81.362974 132.658937) (xy 80.314477 132.03787) (xy 79.286659 131.383154)
				(xy 78.280547 130.695443) (xy 77.297314 129.975539) (xy 76.337881 129.224116) (xy 75.40331 128.442005)
				(xy 74.494586 127.630033) (xy 73.612634 126.789023) (xy 72.7584 125.919879) (xy 71.932801 125.023533)
				(xy 71.136648 124.100867) (xy 70.370833 123.152913) (xy 69.636144 122.180648) (xy 68.933321 121.18505)
				(xy 68.263152 120.167235) (xy 67.626309 119.128227) (xy 67.023473 118.069134) (xy 66.455264 116.991044)
				(xy 65.922301 115.895135) (xy 65.425113 114.782493) (xy 64.964255 113.654357) (xy 64.540194 112.511876)
				(xy 64.153373 111.356244) (xy 63.804207 110.188696) (xy 63.493055 109.010431) (xy 63.220247 107.8227)
				(xy 62.986073 106.626772) (xy 62.790771 105.423856) (xy 62.634554 104.215256) (xy 62.517585 103.002253)
				(xy 62.439983 101.78608) (xy 62.401831 100.568025) (xy 62.403171 99.349349) (xy 62.443998 98.131411)
				(xy 62.524272 96.915405) (xy 62.643909 95.702635) (xy 62.802783 94.494369) (xy 63.000722 93.291915)
				(xy 63.23752 92.096522) (xy 63.512944 90.909364) (xy 63.826678 89.731808) (xy 64.178417 88.565003)
				(xy 64.567763 87.410261) (xy 64.994351 86.268668) (xy 65.457686 85.141552) (xy 65.9573 84.030043)
				(xy 66.492681 82.935283) (xy 67.063259 81.858444) (xy 67.668409 80.8007) (xy 68.30754 79.763079)
				(xy 68.979965 78.746711) (xy 69.684933 77.752716) (xy 70.421794 76.782019) (xy 71.189684 75.835757)
				(xy 71.987834 74.914874) (xy 72.81543 74.020314) (xy 73.671556 73.153064) (xy 74.555354 72.313994)
				(xy 75.465876 71.504005) (xy 76.402137 70.723973) (xy 77.363235 69.974648) (xy 78.348051 69.256902)
				(xy 79.355664 68.571409) (xy 80.38492 67.918953) (xy 81.434773 67.300195) (xy 82.504189 66.715747)
				(xy 83.591909 66.166297) (xy 84.696893 65.652368) (xy 85.817945 65.174517) (xy 86.953907 64.73324)
				(xy 88.103576 64.329003) (xy 89.265701 63.962245) (xy 90.440107 63.633056) (xy 90.972525 63.5) (xy 109.027474 63.5)
			)
		)
	)
	(zone
		(net "V24_BUS")
		(layer "In2.Cu")
		(name "Dedicated 24V distribution")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.4)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 131.020044 78.746725) (xy 131.692449 79.763066) (xy 132.331585 80.80069) (xy 132.936751 81.858466)
				(xy 133.507317 82.935283) (xy 134.042693 84.030031) (xy 134.542306 85.141537) (xy 135.005657 86.268694)
				(xy 135.432232 87.410251) (xy 135.821588 88.56502) (xy 136.173317 89.731798) (xy 136.487055 90.909364)
				(xy 136.762472 92.096491) (xy 136.99928 93.291939) (xy 137.197216 94.494373) (xy 137.35609 95.702634)
				(xy 137.475727 96.915404) (xy 137.556001 98.13141) (xy 137.596828 99.349348) (xy 137.598168 100.568024)
				(xy 137.560016 101.786079) (xy 137.482414 103.002252) (xy 137.365445 104.215255) (xy 137.209228 105.423855)
				(xy 137.013926 106.626771) (xy 136.779752 107.822699) (xy 136.506945 109.01043) (xy 136.195792 110.188695)
				(xy 135.846626 111.356244) (xy 135.459806 112.511876) (xy 135.035749 113.654345) (xy 134.574882 114.782502)
				(xy 134.077705 115.895121) (xy 133.544729 116.991055) (xy 132.976526 118.069133) (xy 132.373691 119.128226)
				(xy 131.736848 120.167234) (xy 131.066678 121.18505) (xy 130.363855 122.180647) (xy 129.629167 123.152912)
				(xy 128.863338 124.100884) (xy 128.067214 125.023515) (xy 127.241584 125.919894) (xy 126.387381 126.789007)
				(xy 125.505414 127.630032) (xy 124.59669 128.442004) (xy 123.662119 129.224115) (xy 122.702701 129.975526)
				(xy 121.719424 130.695463) (xy 120.713356 131.383144) (xy 119.685522 132.03787) (xy 118.637026 132.658936)
				(xy 117.568923 133.245718) (xy 116.482388 133.79757) (xy 115.378535 134.313926) (xy 114.25855 134.794232)
				(xy 113.123548 135.238009) (xy 111.974798 135.644762) (xy 110.813434 136.014087) (xy 109.640764 136.34557)
				(xy 108.457935 136.638889) (xy 107.266212 136.893726) (xy 106.066899 137.109805) (xy 104.861172 137.286913)
				(xy 103.650352 137.424854) (xy 102.43568 137.52349) (xy 101.218487 137.582711) (xy 100 137.602458)
				(xy 98.781513 137.582711) (xy 97.56432 137.52349) (xy 96.349648 137.424854) (xy 95.138828 137.286913)
				(xy 93.933101 137.109805) (xy 92.733788 136.893726) (xy 91.542065 136.638889) (xy 90.359235 136.345571)
				(xy 89.186547 136.014083) (xy 88.025211 135.644766) (xy 86.876461 135.238014) (xy 85.741451 134.794233)
				(xy 84.621465 134.313926) (xy 83.517612 133.797571) (xy 82.431077 133.245719) (xy 81.362974 132.658937)
				(xy 80.314477 132.03787) (xy 79.286659 131.383154) (xy 78.280547 130.695443) (xy 77.297314 129.975539)
				(xy 76.337881 129.224116) (xy 75.40331 128.442005) (xy 74.494586 127.630033) (xy 73.612634 126.789023)
				(xy 72.7584 125.919879) (xy 71.932801 125.023533) (xy 71.136648 124.100867) (xy 70.370833 123.152913)
				(xy 69.636144 122.180648) (xy 68.933321 121.18505) (xy 68.263152 120.167235) (xy 67.626309 119.128227)
				(xy 67.023473 118.069134) (xy 66.455264 116.991044) (xy 65.922301 115.895135) (xy 65.425113 114.782493)
				(xy 64.964255 113.654357) (xy 64.540194 112.511876) (xy 64.153373 111.356244) (xy 63.804207 110.188696)
				(xy 63.493055 109.010431) (xy 63.220247 107.8227) (xy 62.986073 106.626772) (xy 62.790771 105.423856)
				(xy 62.634554 104.215256) (xy 62.517585 103.002253) (xy 62.439983 101.78608) (xy 62.401831 100.568025)
				(xy 62.403171 99.349349) (xy 62.443998 98.131411) (xy 62.524272 96.915405) (xy 62.643909 95.702635)
				(xy 62.802783 94.494369) (xy 63.000722 93.291915) (xy 63.23752 92.096522) (xy 63.512944 90.909364)
				(xy 63.826678 89.731808) (xy 64.178417 88.565003) (xy 64.567763 87.410261) (xy 64.994351 86.268668)
				(xy 65.457686 85.141552) (xy 65.9573 84.030043) (xy 66.492681 82.935283) (xy 67.063259 81.858444)
				(xy 67.668409 80.8007) (xy 68.30754 79.763079) (xy 68.979965 78.746711) (xy 69.43863 78.1) (xy 130.561368 78.1)
			)
		)
	)
	(zone
		(net "GND")
		(layer "In3.Cu")
		(name "Inner signal GND reference")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.4)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 109.559891 63.633056) (xy 110.734297 63.962245) (xy 111.896422 64.329003) (xy 113.046091 64.733239)
				(xy 114.182053 65.174517) (xy 115.303118 65.652373) (xy 116.408078 66.16629) (xy 117.495824 66.715753)
				(xy 118.565212 67.300186) (xy 119.615078 67.918952) (xy 120.644335 68.571409) (xy 121.651947 69.256901)
				(xy 122.636779 69.974659) (xy 123.597832 70.723948) (xy 124.534137 71.504018) (xy 125.444644 72.313994)
				(xy 126.328443 73.153064) (xy 127.184568 74.020313) (xy 128.01215 74.914858) (xy 128.810328 75.835772)
				(xy 129.578204 76.782018) (xy 130.315054 77.752701) (xy 131.020044 78.746725) (xy 131.692449 79.763066)
				(xy 132.331585 80.80069) (xy 132.936751 81.858466) (xy 133.507317 82.935283) (xy 134.042693 84.030031)
				(xy 134.542306 85.141537) (xy 135.005657 86.268694) (xy 135.432232 87.410251) (xy 135.821588 88.56502)
				(xy 136.173317 89.731798) (xy 136.487055 90.909364) (xy 136.762472 92.096491) (xy 136.99928 93.291939)
				(xy 137.197216 94.494373) (xy 137.35609 95.702634) (xy 137.475727 96.915404) (xy 137.556001 98.13141)
				(xy 137.596828 99.349348) (xy 137.598168 100.568024) (xy 137.560016 101.786079) (xy 137.482414 103.002252)
				(xy 137.365445 104.215255) (xy 137.209228 105.423855) (xy 137.013926 106.626771) (xy 136.779752 107.822699)
				(xy 136.506945 109.01043) (xy 136.195792 110.188695) (xy 135.846626 111.356244) (xy 135.459806 112.511876)
				(xy 135.035749 113.654345) (xy 134.574882 114.782502) (xy 134.077705 115.895121) (xy 133.544729 116.991055)
				(xy 132.976526 118.069133) (xy 132.373691 119.128226) (xy 131.736848 120.167234) (xy 131.066678 121.18505)
				(xy 130.363855 122.180647) (xy 129.629167 123.152912) (xy 128.863338 124.100884) (xy 128.067214 125.023515)
				(xy 127.241584 125.919894) (xy 126.387381 126.789007) (xy 125.505414 127.630032) (xy 124.59669 128.442004)
				(xy 123.662119 129.224115) (xy 122.702701 129.975526) (xy 121.719424 130.695463) (xy 120.713356 131.383144)
				(xy 119.685522 132.03787) (xy 118.637026 132.658936) (xy 117.568923 133.245718) (xy 116.482388 133.79757)
				(xy 115.378535 134.313926) (xy 114.25855 134.794232) (xy 113.123548 135.238009) (xy 111.974798 135.644762)
				(xy 110.813434 136.014087) (xy 109.640764 136.34557) (xy 108.457935 136.638889) (xy 107.266212 136.893726)
				(xy 106.066899 137.109805) (xy 104.861172 137.286913) (xy 103.650352 137.424854) (xy 102.43568 137.52349)
				(xy 101.218487 137.582711) (xy 100 137.602458) (xy 98.781513 137.582711) (xy 97.56432 137.52349)
				(xy 96.349648 137.424854) (xy 95.138828 137.286913) (xy 93.933101 137.109805) (xy 92.733788 136.893726)
				(xy 91.542065 136.638889) (xy 90.359235 136.345571) (xy 89.186547 136.014083) (xy 88.025211 135.644766)
				(xy 86.876461 135.238014) (xy 85.741451 134.794233) (xy 84.621465 134.313926) (xy 83.517612 133.797571)
				(xy 82.431077 133.245719) (xy 81.362974 132.658937) (xy 80.314477 132.03787) (xy 79.286659 131.383154)
				(xy 78.280547 130.695443) (xy 77.297314 129.975539) (xy 76.337881 129.224116) (xy 75.40331 128.442005)
				(xy 74.494586 127.630033) (xy 73.612634 126.789023) (xy 72.7584 125.919879) (xy 71.932801 125.023533)
				(xy 71.136648 124.100867) (xy 70.370833 123.152913) (xy 69.636144 122.180648) (xy 68.933321 121.18505)
				(xy 68.263152 120.167235) (xy 67.626309 119.128227) (xy 67.023473 118.069134) (xy 66.455264 116.991044)
				(xy 65.922301 115.895135) (xy 65.425113 114.782493) (xy 64.964255 113.654357) (xy 64.540194 112.511876)
				(xy 64.153373 111.356244) (xy 63.804207 110.188696) (xy 63.493055 109.010431) (xy 63.220247 107.8227)
				(xy 62.986073 106.626772) (xy 62.790771 105.423856) (xy 62.634554 104.215256) (xy 62.517585 103.002253)
				(xy 62.439983 101.78608) (xy 62.401831 100.568025) (xy 62.403171 99.349349) (xy 62.443998 98.131411)
				(xy 62.524272 96.915405) (xy 62.643909 95.702635) (xy 62.802783 94.494369) (xy 63.000722 93.291915)
				(xy 63.23752 92.096522) (xy 63.512944 90.909364) (xy 63.826678 89.731808) (xy 64.178417 88.565003)
				(xy 64.567763 87.410261) (xy 64.994351 86.268668) (xy 65.457686 85.141552) (xy 65.9573 84.030043)
				(xy 66.492681 82.935283) (xy 67.063259 81.858444) (xy 67.668409 80.8007) (xy 68.30754 79.763079)
				(xy 68.979965 78.746711) (xy 69.684933 77.752716) (xy 70.421794 76.782019) (xy 71.189684 75.835757)
				(xy 71.987834 74.914874) (xy 72.81543 74.020314) (xy 73.671556 73.153064) (xy 74.555354 72.313994)
				(xy 75.465876 71.504005) (xy 76.402137 70.723973) (xy 77.363235 69.974648) (xy 78.348051 69.256902)
				(xy 79.355664 68.571409) (xy 80.38492 67.918953) (xy 81.434773 67.300195) (xy 82.504189 66.715747)
				(xy 83.591909 66.166297) (xy 84.696893 65.652368) (xy 85.817945 65.174517) (xy 86.953907 64.73324)
				(xy 88.103576 64.329003) (xy 89.265701 63.962245) (xy 90.440107 63.633056) (xy 90.972525 63.5) (xy 109.027474 63.5)
			)
		)
	)
	(zone
		(net "VIN24_RPP")
		(layer "In4.Cu")
		(name "MOUNT_REV_Q500_In4_ARRAY")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(fill yes
			(thermal_gap 0.3)
			(thermal_bridge_width 0.4)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 92.235 122.85) (xy 94.035 122.85) (xy 94.035 127.9) (xy 92.235 127.9)
			)
		)
	)
	(zone
		(net "VIN24_FUSED")
		(layer "In4.Cu")
		(name "MOUNT_REV_F1_In4_ARRAY")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(fill yes
			(thermal_gap 0.3)
			(thermal_bridge_width 0.4)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 90.899999 119.645) (xy 92.95 119.645) (xy 92.95 123.445) (xy 90.899999 123.445)
			)
		)
	)
	(zone
		(net "GND")
		(layer "In6.Cu")
		(name "Continuous bottom-side GND reference")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.4)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 109.559891 63.633056) (xy 110.734297 63.962245) (xy 111.896422 64.329003) (xy 113.046091 64.733239)
				(xy 114.182053 65.174517) (xy 115.303118 65.652373) (xy 116.408078 66.16629) (xy 117.495824 66.715753)
				(xy 118.565212 67.300186) (xy 119.615078 67.918952) (xy 120.644335 68.571409) (xy 121.651947 69.256901)
				(xy 122.636779 69.974659) (xy 123.597832 70.723948) (xy 124.534137 71.504018) (xy 125.444644 72.313994)
				(xy 126.328443 73.153064) (xy 127.184568 74.020313) (xy 128.01215 74.914858) (xy 128.810328 75.835772)
				(xy 129.578204 76.782018) (xy 130.315054 77.752701) (xy 131.020044 78.746725) (xy 131.692449 79.763066)
				(xy 132.331585 80.80069) (xy 132.936751 81.858466) (xy 133.507317 82.935283) (xy 134.042693 84.030031)
				(xy 134.542306 85.141537) (xy 135.005657 86.268694) (xy 135.432232 87.410251) (xy 135.821588 88.56502)
				(xy 136.173317 89.731798) (xy 136.487055 90.909364) (xy 136.762472 92.096491) (xy 136.99928 93.291939)
				(xy 137.197216 94.494373) (xy 137.35609 95.702634) (xy 137.475727 96.915404) (xy 137.556001 98.13141)
				(xy 137.596828 99.349348) (xy 137.598168 100.568024) (xy 137.560016 101.786079) (xy 137.482414 103.002252)
				(xy 137.365445 104.215255) (xy 137.209228 105.423855) (xy 137.013926 106.626771) (xy 136.779752 107.822699)
				(xy 136.506945 109.01043) (xy 136.195792 110.188695) (xy 135.846626 111.356244) (xy 135.459806 112.511876)
				(xy 135.035749 113.654345) (xy 134.574882 114.782502) (xy 134.077705 115.895121) (xy 133.544729 116.991055)
				(xy 132.976526 118.069133) (xy 132.373691 119.128226) (xy 131.736848 120.167234) (xy 131.066678 121.18505)
				(xy 130.363855 122.180647) (xy 129.629167 123.152912) (xy 128.863338 124.100884) (xy 128.067214 125.023515)
				(xy 127.241584 125.919894) (xy 126.387381 126.789007) (xy 125.505414 127.630032) (xy 124.59669 128.442004)
				(xy 123.662119 129.224115) (xy 122.702701 129.975526) (xy 121.719424 130.695463) (xy 120.713356 131.383144)
				(xy 119.685522 132.03787) (xy 118.637026 132.658936) (xy 117.568923 133.245718) (xy 116.482388 133.79757)
				(xy 115.378535 134.313926) (xy 114.25855 134.794232) (xy 113.123548 135.238009) (xy 111.974798 135.644762)
				(xy 110.813434 136.014087) (xy 109.640764 136.34557) (xy 108.457935 136.638889) (xy 107.266212 136.893726)
				(xy 106.066899 137.109805) (xy 104.861172 137.286913) (xy 103.650352 137.424854) (xy 102.43568 137.52349)
				(xy 101.218487 137.582711) (xy 100 137.602458) (xy 98.781513 137.582711) (xy 97.56432 137.52349)
				(xy 96.349648 137.424854) (xy 95.138828 137.286913) (xy 93.933101 137.109805) (xy 92.733788 136.893726)
				(xy 91.542065 136.638889) (xy 90.359235 136.345571) (xy 89.186547 136.014083) (xy 88.025211 135.644766)
				(xy 86.876461 135.238014) (xy 85.741451 134.794233) (xy 84.621465 134.313926) (xy 83.517612 133.797571)
				(xy 82.431077 133.245719) (xy 81.362974 132.658937) (xy 80.314477 132.03787) (xy 79.286659 131.383154)
				(xy 78.280547 130.695443) (xy 77.297314 129.975539) (xy 76.337881 129.224116) (xy 75.40331 128.442005)
				(xy 74.494586 127.630033) (xy 73.612634 126.789023) (xy 72.7584 125.919879) (xy 71.932801 125.023533)
				(xy 71.136648 124.100867) (xy 70.370833 123.152913) (xy 69.636144 122.180648) (xy 68.933321 121.18505)
				(xy 68.263152 120.167235) (xy 67.626309 119.128227) (xy 67.023473 118.069134) (xy 66.455264 116.991044)
				(xy 65.922301 115.895135) (xy 65.425113 114.782493) (xy 64.964255 113.654357) (xy 64.540194 112.511876)
				(xy 64.153373 111.356244) (xy 63.804207 110.188696) (xy 63.493055 109.010431) (xy 63.220247 107.8227)
				(xy 62.986073 106.626772) (xy 62.790771 105.423856) (xy 62.634554 104.215256) (xy 62.517585 103.002253)
				(xy 62.439983 101.78608) (xy 62.401831 100.568025) (xy 62.403171 99.349349) (xy 62.443998 98.131411)
				(xy 62.524272 96.915405) (xy 62.643909 95.702635) (xy 62.802783 94.494369) (xy 63.000722 93.291915)
				(xy 63.23752 92.096522) (xy 63.512944 90.909364) (xy 63.826678 89.731808) (xy 64.178417 88.565003)
				(xy 64.567763 87.410261) (xy 64.994351 86.268668) (xy 65.457686 85.141552) (xy 65.9573 84.030043)
				(xy 66.492681 82.935283) (xy 67.063259 81.858444) (xy 67.668409 80.8007) (xy 68.30754 79.763079)
				(xy 68.979965 78.746711) (xy 69.684933 77.752716) (xy 70.421794 76.782019) (xy 71.189684 75.835757)
				(xy 71.987834 74.914874) (xy 72.81543 74.020314) (xy 73.671556 73.153064) (xy 74.555354 72.313994)
				(xy 75.465876 71.504005) (xy 76.402137 70.723973) (xy 77.363235 69.974648) (xy 78.348051 69.256902)
				(xy 79.355664 68.571409) (xy 80.38492 67.918953) (xy 81.434773 67.300195) (xy 82.504189 66.715747)
				(xy 83.591909 66.166297) (xy 84.696893 65.652368) (xy 85.817945 65.174517) (xy 86.953907 64.73324)
				(xy 88.103576 64.329003) (xy 89.265701 63.962245) (xy 90.440107 63.633056) (xy 90.972525 63.5) (xy 109.027474 63.5)
			)
		)
	)
	(embedded_fonts no)
)
