(kicad_sch
  (version 20250114)
  (generator "engineered-lighting")
  (generator_version "0.2")
  (paper "A3")
  (title_block
    (title "Pwm")
    (date "2026-09-06")
    (rev "A draft")
    (company "Engineered Lighting")
    (comment 1 "ENGINEERING DRAFT - see release status before fabrication"))
  (lib_symbols
    (symbol "Driver_LED:PCA9685PW"
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "U"
        (at -12.7 22.225 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "PCA9685PW"
        (at 1.27 22.225 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
        (at 0.635 -24.765 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/PCA9685.pdf"
        (at -10.16 17.78 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "16-channel 12-bit PWM Fm+ I2C-bus LED controller RGBA TSSOP"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "PWM LED driver I2C TSSOP"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "PCA9685PW_0_1"
        (rectangle
          (start -12.7 20.32)
          (end 12.7 -22.86)
          (fill
            (type background))))
      (symbol "PCA9685PW_1_1"
        (pin input line
          (at -17.78 -5.08 0)
          (length 5.08)
          (name "A0")
          (number "1"))
        (pin input line
          (at -17.78 -7.62 0)
          (length 5.08)
          (name "A1")
          (number "2"))
        (pin input line
          (at -17.78 -10.16 0)
          (length 5.08)
          (name "A2")
          (number "3"))
        (pin input line
          (at -17.78 -12.7 0)
          (length 5.08)
          (name "A3")
          (number "4"))
        (pin input line
          (at -17.78 -15.24 0)
          (length 5.08)
          (name "A4")
          (number "5"))
        (pin output line
          (at 17.78 17.78 180)
          (length 5.08)
          (name "LED0")
          (number "6"))
        (pin output line
          (at 17.78 15.24 180)
          (length 5.08)
          (name "LED1")
          (number "7"))
        (pin output line
          (at 17.78 12.7 180)
          (length 5.08)
          (name "LED2")
          (number "8"))
        (pin output line
          (at 17.78 10.16 180)
          (length 5.08)
          (name "LED3")
          (number "9"))
        (pin output line
          (at 17.78 7.62 180)
          (length 5.08)
          (name "LED4")
          (number "10"))
        (pin output line
          (at 17.78 5.08 180)
          (length 5.08)
          (name "LED5")
          (number "11"))
        (pin output line
          (at 17.78 2.54 180)
          (length 5.08)
          (name "LED6")
          (number "12"))
        (pin output line
          (at 17.78 0 180)
          (length 5.08)
          (name "LED7")
          (number "13"))
        (pin power_in line
          (at 0 -27.94 90)
          (length 5.08)
          (name "VSS")
          (number "14"))
        (pin output line
          (at 17.78 -2.54 180)
          (length 5.08)
          (name "LED8")
          (number "15"))
        (pin output line
          (at 17.78 -5.08 180)
          (length 5.08)
          (name "LED9")
          (number "16"))
        (pin output line
          (at 17.78 -7.62 180)
          (length 5.08)
          (name "LED10")
          (number "17"))
        (pin output line
          (at 17.78 -10.16 180)
          (length 5.08)
          (name "LED11")
          (number "18"))
        (pin output line
          (at 17.78 -12.7 180)
          (length 5.08)
          (name "LED12")
          (number "19"))
        (pin output line
          (at 17.78 -15.24 180)
          (length 5.08)
          (name "LED13")
          (number "20"))
        (pin output line
          (at 17.78 -17.78 180)
          (length 5.08)
          (name "LED14")
          (number "21"))
        (pin output line
          (at 17.78 -20.32 180)
          (length 5.08)
          (name "LED15")
          (number "22"))
        (pin input line
          (at -17.78 10.16 0)
          (length 5.08)
          (name "~{OE}")
          (number "23"))
        (pin input line
          (at -17.78 -17.78 0)
          (length 5.08)
          (name "A5")
          (number "24"))
        (pin input line
          (at -17.78 12.7 0)
          (length 5.08)
          (name "EXTCLK")
          (number "25"))
        (pin input line
          (at -17.78 17.78 0)
          (length 5.08)
          (name "SCL")
          (number "26"))
        (pin bidirectional line
          (at -17.78 15.24 0)
          (length 5.08)
          (name "SDA")
          (number "27"))
        (pin power_in line
          (at 0 25.4 270)
          (length 5.08)
          (name "VDD")
          (number "28")))
      (embedded_fonts no))
    (symbol "Device:C"
      (pin_numbers
        (hide yes))
      (pin_names
        (offset 0.254))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "C"
        (at 0.635 2.54 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "C"
        (at 0.635 -2.54 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" ""
        (at 0.9652 -3.81 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Unpolarized capacitor"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "cap capacitor"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "C_*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762))
          (fill
            (type none)))
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762))
          (fill
            (type none))))
      (symbol "C_1_1"
        (pin passive line
          (at 0 3.81 270)
          (length 2.794)
          (name "")
          (number "1"))
        (pin passive line
          (at 0 -3.81 90)
          (length 2.794)
          (name "")
          (number "2")))
      (embedded_fonts no)))
  (symbol
    (lib_id "Driver_LED:PCA9685PW")
    (at 96.52 104.14 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "U2"
      (at 116.84 69.85 0.0))
    (property "Value" "PCA9685PW,118"
      (at 116.84 72.39 0.0))
    (property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
      (at 96.52 104.14 0.0)
      (hide yes))
    (property "MPN" "PCA9685PW,118"
      (at 96.52 104.14 0.0)
      (hide yes))
    (property "Manufacturer" "NXP"
      (at 96.52 104.14 0.0)
      (hide yes))
    (property "Datasheet" ""
      (at 96.52 104.14 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "U2")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28"))
  (wire
    (pts
      (xy 78.74 109.22)
      (xy 71.12 109.22)))
  (global_label "GND"
    (shape passive)
    (at 71.12 109.22 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 71.12 109.22 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 78.74 111.76)
      (xy 71.12 111.76)))
  (global_label "GND"
    (shape passive)
    (at 71.12 111.76 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 71.12 111.76 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 78.74 114.3)
      (xy 71.12 114.3)))
  (global_label "GND"
    (shape passive)
    (at 71.12 114.3 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 71.12 114.3 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 78.74 116.84)
      (xy 71.12 116.84)))
  (global_label "GND"
    (shape passive)
    (at 71.12 116.84 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 71.12 116.84 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 78.74 119.38)
      (xy 71.12 119.38)))
  (global_label "GND"
    (shape passive)
    (at 71.12 119.38 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 71.12 119.38 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 114.3 86.36)
      (xy 123.19 86.36)))
  (global_label "PWM_01"
    (shape passive)
    (at 123.19 86.36 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 123.19 86.36 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 114.3 88.9)
      (xy 123.19 88.9)))
  (global_label "PWM_02"
    (shape passive)
    (at 123.19 88.9 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 123.19 88.9 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 114.3 91.44)
      (xy 123.19 91.44)))
  (global_label "PWM_03"
    (shape passive)
    (at 123.19 91.44 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 123.19 91.44 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 114.3 93.98)
      (xy 123.19 93.98)))
  (global_label "PWM_04"
    (shape passive)
    (at 123.19 93.98 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 123.19 93.98 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 114.3 96.52)
      (xy 123.19 96.52)))
  (global_label "PWM_05"
    (shape passive)
    (at 123.19 96.52 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 123.19 96.52 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 114.3 99.06)
      (xy 123.19 99.06)))
  (global_label "PWM_06"
    (shape passive)
    (at 123.19 99.06 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 123.19 99.06 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 114.3 101.6)
      (xy 123.19 101.6)))
  (global_label "PWM_07"
    (shape passive)
    (at 123.19 101.6 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 123.19 101.6 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 114.3 104.14)
      (xy 123.19 104.14)))
  (global_label "PWM_08"
    (shape passive)
    (at 123.19 104.14 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 123.19 104.14 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 96.52 132.08)
      (xy 96.52 139.7)))
  (global_label "GND"
    (shape passive)
    (at 96.52 139.7 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 96.52 139.7 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 114.3 106.68)
      (xy 123.19 106.68)))
  (global_label "PWM_09"
    (shape passive)
    (at 123.19 106.68 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 123.19 106.68 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 114.3 109.22)
      (xy 123.19 109.22)))
  (global_label "PWM_10"
    (shape passive)
    (at 123.19 109.22 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 123.19 109.22 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 114.3 111.76)
      (xy 123.19 111.76)))
  (global_label "PWM_11"
    (shape passive)
    (at 123.19 111.76 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 123.19 111.76 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 114.3 114.3)
      (xy 123.19 114.3)))
  (global_label "PWM_12"
    (shape passive)
    (at 123.19 114.3 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 123.19 114.3 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 114.3 116.84)
      (xy 123.19 116.84)))
  (global_label "PWM_13"
    (shape passive)
    (at 123.19 116.84 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 123.19 116.84 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 114.3 119.38)
      (xy 123.19 119.38)))
  (global_label "PWM_14"
    (shape passive)
    (at 123.19 119.38 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 123.19 119.38 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 114.3 121.92)
      (xy 123.19 121.92)))
  (global_label "PWM_15"
    (shape passive)
    (at 123.19 121.92 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 123.19 121.92 0.0)
      (hide yes)))
  (no_connect
    (at 114.3 124.46))
  (wire
    (pts
      (xy 78.74 93.98)
      (xy 69.85 93.98)))
  (global_label "PCA_OE"
    (shape passive)
    (at 69.85 93.98 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 69.85 93.98 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 78.74 121.92)
      (xy 71.12 121.92)))
  (global_label "GND"
    (shape passive)
    (at 71.12 121.92 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 71.12 121.92 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 78.74 91.44)
      (xy 71.12 91.44)))
  (global_label "GND"
    (shape passive)
    (at 71.12 91.44 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 71.12 91.44 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 78.74 86.36)
      (xy 68.58 86.36)))
  (global_label "I2C_SCL"
    (shape passive)
    (at 68.58 86.36 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 68.58 86.36 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 78.74 88.9)
      (xy 68.58 88.9)))
  (global_label "I2C_SDA"
    (shape passive)
    (at 68.58 88.9 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 68.58 88.9 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 96.52 78.74)
      (xy 96.52 71.12)))
  (global_label "+3V3"
    (shape passive)
    (at 96.52 71.12 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 96.52 71.12 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:C")
    (at 45.72 205.74 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C40"
      (at 50.8 204.47 0.0))
    (property "Value" "100n"
      (at 50.8 207.01 0.0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
      (at 45.72 205.74 0.0)
      (hide yes))
    (property "MPN" "GRM188R72A104KA35D"
      (at 45.72 205.74 0.0)
      (hide yes))
    (property "Manufacturer" "Murata"
      (at 45.72 205.74 0.0)
      (hide yes))
    (property "Datasheet" ""
      (at 45.72 205.74 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C40")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 45.72 201.93)
      (xy 45.72 194.31)))
  (global_label "+3V3"
    (shape passive)
    (at 45.72 194.31 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 45.72 194.31 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 45.72 209.55)
      (xy 45.72 217.17)))
  (global_label "GND"
    (shape passive)
    (at 45.72 217.17 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 45.72 217.17 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:C")
    (at 101.6 205.74 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C42"
      (at 106.68 204.47 0.0))
    (property "Value" "1u"
      (at 106.68 207.01 0.0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
      (at 101.6 205.74 0.0)
      (hide yes))
    (property "MPN" "C1608X7R1E105K080AB"
      (at 101.6 205.74 0.0)
      (hide yes))
    (property "Manufacturer" "TDK"
      (at 101.6 205.74 0.0)
      (hide yes))
    (property "Datasheet" ""
      (at 101.6 205.74 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C42")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 101.6 201.93)
      (xy 101.6 194.31)))
  (global_label "+3V3"
    (shape passive)
    (at 101.6 194.31 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 101.6 194.31 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 101.6 209.55)
      (xy 101.6 217.17)))
  (global_label "GND"
    (shape passive)
    (at 101.6 217.17 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 101.6 217.17 0.0)
      (hide yes)))
  (symbol
    (lib_id "Driver_LED:PCA9685PW")
    (at 287.02 104.14 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "U3"
      (at 307.34 69.85 0.0))
    (property "Value" "PCA9685PW,118"
      (at 307.34 72.39 0.0))
    (property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
      (at 287.02 104.14 0.0)
      (hide yes))
    (property "MPN" "PCA9685PW,118"
      (at 287.02 104.14 0.0)
      (hide yes))
    (property "Manufacturer" "NXP"
      (at 287.02 104.14 0.0)
      (hide yes))
    (property "Datasheet" ""
      (at 287.02 104.14 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "U3")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28"))
  (wire
    (pts
      (xy 269.24 109.22)
      (xy 261.62 109.22)))
  (global_label "+3V3"
    (shape passive)
    (at 261.62 109.22 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 261.62 109.22 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 269.24 111.76)
      (xy 261.62 111.76)))
  (global_label "GND"
    (shape passive)
    (at 261.62 111.76 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 261.62 111.76 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 269.24 114.3)
      (xy 261.62 114.3)))
  (global_label "GND"
    (shape passive)
    (at 261.62 114.3 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 261.62 114.3 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 269.24 116.84)
      (xy 261.62 116.84)))
  (global_label "GND"
    (shape passive)
    (at 261.62 116.84 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 261.62 116.84 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 269.24 119.38)
      (xy 261.62 119.38)))
  (global_label "GND"
    (shape passive)
    (at 261.62 119.38 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 261.62 119.38 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 304.8 86.36)
      (xy 313.69 86.36)))
  (global_label "PWM_16"
    (shape passive)
    (at 313.69 86.36 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 313.69 86.36 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 304.8 88.9)
      (xy 313.69 88.9)))
  (global_label "PWM_17"
    (shape passive)
    (at 313.69 88.9 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 313.69 88.9 0.0)
      (hide yes)))
  (no_connect
    (at 304.8 91.44))
  (wire
    (pts
      (xy 304.8 93.98)
      (xy 313.69 93.98)))
  (global_label "PWM_19"
    (shape passive)
    (at 313.69 93.98 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 313.69 93.98 0.0)
      (hide yes)))
  (no_connect
    (at 304.8 96.52))
  (wire
    (pts
      (xy 304.8 99.06)
      (xy 313.69 99.06)))
  (global_label "PWM_21"
    (shape passive)
    (at 313.69 99.06 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 313.69 99.06 0.0)
      (hide yes)))
  (no_connect
    (at 304.8 101.6))
  (no_connect
    (at 304.8 104.14))
  (wire
    (pts
      (xy 287.02 132.08)
      (xy 287.02 139.7)))
  (global_label "GND"
    (shape passive)
    (at 287.02 139.7 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 287.02 139.7 0.0)
      (hide yes)))
  (no_connect
    (at 304.8 106.68))
  (no_connect
    (at 304.8 109.22))
  (no_connect
    (at 304.8 111.76))
  (no_connect
    (at 304.8 114.3))
  (wire
    (pts
      (xy 304.8 116.84)
      (xy 313.69 116.84)))
  (global_label "PWM_20"
    (shape passive)
    (at 313.69 116.84 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 313.69 116.84 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 304.8 119.38)
      (xy 313.69 119.38)))
  (global_label "PWM_18"
    (shape passive)
    (at 313.69 119.38 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 313.69 119.38 0.0)
      (hide yes)))
  (no_connect
    (at 304.8 121.92))
  (no_connect
    (at 304.8 124.46))
  (wire
    (pts
      (xy 269.24 93.98)
      (xy 260.35 93.98)))
  (global_label "PCA_OE"
    (shape passive)
    (at 260.35 93.98 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 260.35 93.98 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 269.24 121.92)
      (xy 261.62 121.92)))
  (global_label "GND"
    (shape passive)
    (at 261.62 121.92 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 261.62 121.92 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 269.24 91.44)
      (xy 261.62 91.44)))
  (global_label "GND"
    (shape passive)
    (at 261.62 91.44 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 261.62 91.44 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 269.24 86.36)
      (xy 259.08 86.36)))
  (global_label "I2C_SCL"
    (shape passive)
    (at 259.08 86.36 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 259.08 86.36 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 269.24 88.9)
      (xy 259.08 88.9)))
  (global_label "I2C_SDA"
    (shape passive)
    (at 259.08 88.9 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 259.08 88.9 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 287.02 78.74)
      (xy 287.02 71.12)))
  (global_label "+3V3"
    (shape passive)
    (at 287.02 71.12 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 287.02 71.12 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:C")
    (at 243.84 205.74 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C41"
      (at 248.92 204.47 0.0))
    (property "Value" "100n"
      (at 248.92 207.01 0.0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
      (at 243.84 205.74 0.0)
      (hide yes))
    (property "MPN" "GRM188R72A104KA35D"
      (at 243.84 205.74 0.0)
      (hide yes))
    (property "Manufacturer" "Murata"
      (at 243.84 205.74 0.0)
      (hide yes))
    (property "Datasheet" ""
      (at 243.84 205.74 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C41")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 243.84 201.93)
      (xy 243.84 194.31)))
  (global_label "+3V3"
    (shape passive)
    (at 243.84 194.31 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 243.84 194.31 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 243.84 209.55)
      (xy 243.84 217.17)))
  (global_label "GND"
    (shape passive)
    (at 243.84 217.17 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 243.84 217.17 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:C")
    (at 299.72 205.74 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C43"
      (at 304.8 204.47 0.0))
    (property "Value" "1u"
      (at 304.8 207.01 0.0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
      (at 299.72 205.74 0.0)
      (hide yes))
    (property "MPN" "C1608X7R1E105K080AB"
      (at 299.72 205.74 0.0)
      (hide yes))
    (property "Manufacturer" "TDK"
      (at 299.72 205.74 0.0)
      (hide yes))
    (property "Datasheet" ""
      (at 299.72 205.74 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C43")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 299.72 201.93)
      (xy 299.72 194.31)))
  (global_label "+3V3"
    (shape passive)
    (at 299.72 194.31 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 299.72 194.31 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 299.72 209.55)
      (xy 299.72 217.17)))
  (global_label "GND"
    (shape passive)
    (at 299.72 217.17 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 299.72 217.17 0.0)
      (hide yes)))
  (text "PWM"
    (at 20.32 15.24 0))
  (text "U2 address 0x40 / zones 1-5"
    (at 35.56 35.56 0))
  (text "U3 address 0x41 / zones 6-7"
    (at 233.68 35.56 0))
  (text "24 outputs total: 21 here + 3 direct spotlight PWM.\nOUTDRV=0, OUTNE=00; INVRT/duty encoding must be verified with outputs inhibited."
    (at 20.32 248.92 0))
  (embedded_fonts no))