(kicad_sch
  (version 20250114)
  (generator "engineered-lighting")
  (generator_version "0.2")
  (paper "A2")
  (title_block
    (title "Upper LED flex / 30-contact main-board connection")
    (date "2026-09-06")
    (rev "0.3 ENGINEERING REVIEW")
    (company "Engineered Lighting")
    (comment 1 "ENGINEERING DRAFT - see release status before fabrication"))
  (lib_symbols
    (symbol "Connector_Generic:Conn_01x04"
      (pin_names
        (offset 1.016)
        (hide yes))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "J"
        (at 0 5.08 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "Conn_01x04"
        (at 0 -7.62 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "connector"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "Connector*:*_1x??_*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "Conn_01x04_1_1"
        (rectangle
          (start -1.27 3.81)
          (end 1.27 -6.35)
          (fill
            (type background)))
        (rectangle
          (start -1.27 2.667)
          (end 0 2.413)
          (fill
            (type none)))
        (rectangle
          (start -1.27 0.127)
          (end 0 -0.127)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -2.413)
          (end 0 -2.667)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -4.953)
          (end 0 -5.207)
          (fill
            (type none)))
        (pin passive line
          (at -5.08 2.54 0)
          (length 3.81)
          (name "Pin_1")
          (number "1"))
        (pin passive line
          (at -5.08 0 0)
          (length 3.81)
          (name "Pin_2")
          (number "2"))
        (pin passive line
          (at -5.08 -2.54 0)
          (length 3.81)
          (name "Pin_3")
          (number "3"))
        (pin passive line
          (at -5.08 -5.08 0)
          (length 3.81)
          (name "Pin_4")
          (number "4")))
      (embedded_fonts no))
    (symbol "Connector_Generic:Conn_01x30"
      (pin_names
        (offset 1.016)
        (hide yes))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "J"
        (at 0 38.1 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "Conn_01x30"
        (at 0 -40.64 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Generic connector, single row, 01x30, script generated (kicad-library-utils/schlib/autogen/connector/)"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "connector"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "Connector*:*_1x??_*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "Conn_01x30_1_1"
        (rectangle
          (start -1.27 36.83)
          (end 1.27 -39.37)
          (fill
            (type background)))
        (rectangle
          (start -1.27 35.687)
          (end 0 35.433)
          (fill
            (type none)))
        (rectangle
          (start -1.27 33.147)
          (end 0 32.893)
          (fill
            (type none)))
        (rectangle
          (start -1.27 30.607)
          (end 0 30.353)
          (fill
            (type none)))
        (rectangle
          (start -1.27 28.067)
          (end 0 27.813)
          (fill
            (type none)))
        (rectangle
          (start -1.27 25.527)
          (end 0 25.273)
          (fill
            (type none)))
        (rectangle
          (start -1.27 22.987)
          (end 0 22.733)
          (fill
            (type none)))
        (rectangle
          (start -1.27 20.447)
          (end 0 20.193)
          (fill
            (type none)))
        (rectangle
          (start -1.27 17.907)
          (end 0 17.653)
          (fill
            (type none)))
        (rectangle
          (start -1.27 15.367)
          (end 0 15.113)
          (fill
            (type none)))
        (rectangle
          (start -1.27 12.827)
          (end 0 12.573)
          (fill
            (type none)))
        (rectangle
          (start -1.27 10.287)
          (end 0 10.033)
          (fill
            (type none)))
        (rectangle
          (start -1.27 7.747)
          (end 0 7.493)
          (fill
            (type none)))
        (rectangle
          (start -1.27 5.207)
          (end 0 4.953)
          (fill
            (type none)))
        (rectangle
          (start -1.27 2.667)
          (end 0 2.413)
          (fill
            (type none)))
        (rectangle
          (start -1.27 0.127)
          (end 0 -0.127)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -2.413)
          (end 0 -2.667)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -4.953)
          (end 0 -5.207)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -7.493)
          (end 0 -7.747)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -10.033)
          (end 0 -10.287)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -12.573)
          (end 0 -12.827)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -15.113)
          (end 0 -15.367)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -17.653)
          (end 0 -17.907)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -20.193)
          (end 0 -20.447)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -22.733)
          (end 0 -22.987)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -25.273)
          (end 0 -25.527)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -27.813)
          (end 0 -28.067)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -30.353)
          (end 0 -30.607)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -32.893)
          (end 0 -33.147)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -35.433)
          (end 0 -35.687)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -37.973)
          (end 0 -38.227)
          (fill
            (type none)))
        (pin passive line
          (at -5.08 35.56 0)
          (length 3.81)
          (name "Pin_1")
          (number "1"))
        (pin passive line
          (at -5.08 33.02 0)
          (length 3.81)
          (name "Pin_2")
          (number "2"))
        (pin passive line
          (at -5.08 30.48 0)
          (length 3.81)
          (name "Pin_3")
          (number "3"))
        (pin passive line
          (at -5.08 27.94 0)
          (length 3.81)
          (name "Pin_4")
          (number "4"))
        (pin passive line
          (at -5.08 25.4 0)
          (length 3.81)
          (name "Pin_5")
          (number "5"))
        (pin passive line
          (at -5.08 22.86 0)
          (length 3.81)
          (name "Pin_6")
          (number "6"))
        (pin passive line
          (at -5.08 20.32 0)
          (length 3.81)
          (name "Pin_7")
          (number "7"))
        (pin passive line
          (at -5.08 17.78 0)
          (length 3.81)
          (name "Pin_8")
          (number "8"))
        (pin passive line
          (at -5.08 15.24 0)
          (length 3.81)
          (name "Pin_9")
          (number "9"))
        (pin passive line
          (at -5.08 12.7 0)
          (length 3.81)
          (name "Pin_10")
          (number "10"))
        (pin passive line
          (at -5.08 10.16 0)
          (length 3.81)
          (name "Pin_11")
          (number "11"))
        (pin passive line
          (at -5.08 7.62 0)
          (length 3.81)
          (name "Pin_12")
          (number "12"))
        (pin passive line
          (at -5.08 5.08 0)
          (length 3.81)
          (name "Pin_13")
          (number "13"))
        (pin passive line
          (at -5.08 2.54 0)
          (length 3.81)
          (name "Pin_14")
          (number "14"))
        (pin passive line
          (at -5.08 0 0)
          (length 3.81)
          (name "Pin_15")
          (number "15"))
        (pin passive line
          (at -5.08 -2.54 0)
          (length 3.81)
          (name "Pin_16")
          (number "16"))
        (pin passive line
          (at -5.08 -5.08 0)
          (length 3.81)
          (name "Pin_17")
          (number "17"))
        (pin passive line
          (at -5.08 -7.62 0)
          (length 3.81)
          (name "Pin_18")
          (number "18"))
        (pin passive line
          (at -5.08 -10.16 0)
          (length 3.81)
          (name "Pin_19")
          (number "19"))
        (pin passive line
          (at -5.08 -12.7 0)
          (length 3.81)
          (name "Pin_20")
          (number "20"))
        (pin passive line
          (at -5.08 -15.24 0)
          (length 3.81)
          (name "Pin_21")
          (number "21"))
        (pin passive line
          (at -5.08 -17.78 0)
          (length 3.81)
          (name "Pin_22")
          (number "22"))
        (pin passive line
          (at -5.08 -20.32 0)
          (length 3.81)
          (name "Pin_23")
          (number "23"))
        (pin passive line
          (at -5.08 -22.86 0)
          (length 3.81)
          (name "Pin_24")
          (number "24"))
        (pin passive line
          (at -5.08 -25.4 0)
          (length 3.81)
          (name "Pin_25")
          (number "25"))
        (pin passive line
          (at -5.08 -27.94 0)
          (length 3.81)
          (name "Pin_26")
          (number "26"))
        (pin passive line
          (at -5.08 -30.48 0)
          (length 3.81)
          (name "Pin_27")
          (number "27"))
        (pin passive line
          (at -5.08 -33.02 0)
          (length 3.81)
          (name "Pin_28")
          (number "28"))
        (pin passive line
          (at -5.08 -35.56 0)
          (length 3.81)
          (name "Pin_29")
          (number "29"))
        (pin passive line
          (at -5.08 -38.1 0)
          (length 3.81)
          (name "Pin_30")
          (number "30")))
      (embedded_fonts no)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 219.71 48.26 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J11"
      (at 219.71 35.56 0.0))
    (property "Value" "Z1 S1 TOP"
      (at 219.71 38.1 0.0))
    (property "Footprint" "ELFlex:J11_Solder4"
      (at 219.71 48.26 0.0)
      (hide yes))
    (instances
      (project "led-upper-v0.3"
        (path
          (reference "J11")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 214.63 45.72)
      (xy 204.47 45.72)))
  (global_label "ZONE1_24V"
    (shape passive)
    (at 204.47 45.72 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 204.47 45.72 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 214.63 48.26)
      (xy 204.47 48.26)))
  (global_label "ZONE1_W"
    (shape passive)
    (at 204.47 48.26 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 204.47 48.26 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 214.63 50.8)
      (xy 204.47 50.8)))
  (global_label "ZONE1_N"
    (shape passive)
    (at 204.47 50.8 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 204.47 50.8 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 214.63 53.34)
      (xy 204.47 53.34)))
  (global_label "ZONE1_C"
    (shape passive)
    (at 204.47 53.34 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 204.47 53.34 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 318.77 48.26 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J12"
      (at 318.77 35.56 0.0))
    (property "Value" "Z1 S2 TOP"
      (at 318.77 38.1 0.0))
    (property "Footprint" "ELFlex:J12_Solder4"
      (at 318.77 48.26 0.0)
      (hide yes))
    (instances
      (project "led-upper-v0.3"
        (path
          (reference "J12")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 313.69 45.72)
      (xy 302.26 45.72)))
  (global_label "Z1_T23_24V"
    (shape passive)
    (at 302.26 45.72 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 302.26 45.72 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 313.69 48.26)
      (xy 303.53 48.26)))
  (global_label "Z1_T23_W"
    (shape passive)
    (at 303.53 48.26 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 303.53 48.26 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 313.69 50.8)
      (xy 303.53 50.8)))
  (global_label "Z1_T23_N"
    (shape passive)
    (at 303.53 50.8 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 303.53 50.8 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 313.69 53.34)
      (xy 303.53 53.34)))
  (global_label "Z1_T23_C"
    (shape passive)
    (at 303.53 53.34 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 303.53 53.34 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 417.83 48.26 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J13"
      (at 417.83 35.56 0.0))
    (property "Value" "Z1 S3 TOP"
      (at 417.83 38.1 0.0))
    (property "Footprint" "ELFlex:J13_Solder4"
      (at 417.83 48.26 0.0)
      (hide yes))
    (instances
      (project "led-upper-v0.3"
        (path
          (reference "J13")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 412.75 45.72)
      (xy 401.32 45.72)))
  (global_label "Z1_T23_24V"
    (shape passive)
    (at 401.32 45.72 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 401.32 45.72 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 412.75 48.26)
      (xy 402.59 48.26)))
  (global_label "Z1_T23_W"
    (shape passive)
    (at 402.59 48.26 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 402.59 48.26 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 412.75 50.8)
      (xy 402.59 50.8)))
  (global_label "Z1_T23_N"
    (shape passive)
    (at 402.59 50.8 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 402.59 50.8 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 412.75 53.34)
      (xy 402.59 53.34)))
  (global_label "Z1_T23_C"
    (shape passive)
    (at 402.59 53.34 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 402.59 53.34 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 516.89 48.26 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J14"
      (at 516.89 35.56 0.0))
    (property "Value" "Z1 S4 TOP"
      (at 516.89 38.1 0.0))
    (property "Footprint" "ELFlex:J14_Solder4"
      (at 516.89 48.26 0.0)
      (hide yes))
    (instances
      (project "led-upper-v0.3"
        (path
          (reference "J14")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (no_connect
    (at 511.81 45.72))
  (no_connect
    (at 511.81 48.26))
  (no_connect
    (at 511.81 50.8))
  (no_connect
    (at 511.81 53.34))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 219.71 96.52 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J21"
      (at 219.71 83.82 0.0))
    (property "Value" "Z2 S1 TOP"
      (at 219.71 86.36 0.0))
    (property "Footprint" "ELFlex:J21_Solder4"
      (at 219.71 96.52 0.0)
      (hide yes))
    (instances
      (project "led-upper-v0.3"
        (path
          (reference "J21")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 214.63 93.98)
      (xy 204.47 93.98)))
  (global_label "ZONE2_24V"
    (shape passive)
    (at 204.47 93.98 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 204.47 93.98 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 214.63 96.52)
      (xy 204.47 96.52)))
  (global_label "ZONE2_W"
    (shape passive)
    (at 204.47 96.52 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 204.47 96.52 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 214.63 99.06)
      (xy 204.47 99.06)))
  (global_label "ZONE2_N"
    (shape passive)
    (at 204.47 99.06 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 204.47 99.06 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 214.63 101.6)
      (xy 204.47 101.6)))
  (global_label "ZONE2_C"
    (shape passive)
    (at 204.47 101.6 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 204.47 101.6 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 318.77 96.52 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J22"
      (at 318.77 83.82 0.0))
    (property "Value" "Z2 S2 TOP"
      (at 318.77 86.36 0.0))
    (property "Footprint" "ELFlex:J22_Solder4"
      (at 318.77 96.52 0.0)
      (hide yes))
    (instances
      (project "led-upper-v0.3"
        (path
          (reference "J22")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 313.69 93.98)
      (xy 302.26 93.98)))
  (global_label "Z2_T23_24V"
    (shape passive)
    (at 302.26 93.98 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 302.26 93.98 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 313.69 96.52)
      (xy 303.53 96.52)))
  (global_label "Z2_T23_W"
    (shape passive)
    (at 303.53 96.52 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 303.53 96.52 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 313.69 99.06)
      (xy 303.53 99.06)))
  (global_label "Z2_T23_N"
    (shape passive)
    (at 303.53 99.06 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 303.53 99.06 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 313.69 101.6)
      (xy 303.53 101.6)))
  (global_label "Z2_T23_C"
    (shape passive)
    (at 303.53 101.6 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 303.53 101.6 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 417.83 96.52 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J23"
      (at 417.83 83.82 0.0))
    (property "Value" "Z2 S3 TOP"
      (at 417.83 86.36 0.0))
    (property "Footprint" "ELFlex:J23_Solder4"
      (at 417.83 96.52 0.0)
      (hide yes))
    (instances
      (project "led-upper-v0.3"
        (path
          (reference "J23")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 412.75 93.98)
      (xy 401.32 93.98)))
  (global_label "Z2_T23_24V"
    (shape passive)
    (at 401.32 93.98 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 401.32 93.98 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 412.75 96.52)
      (xy 402.59 96.52)))
  (global_label "Z2_T23_W"
    (shape passive)
    (at 402.59 96.52 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 402.59 96.52 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 412.75 99.06)
      (xy 402.59 99.06)))
  (global_label "Z2_T23_N"
    (shape passive)
    (at 402.59 99.06 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 402.59 99.06 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 412.75 101.6)
      (xy 402.59 101.6)))
  (global_label "Z2_T23_C"
    (shape passive)
    (at 402.59 101.6 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 402.59 101.6 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 516.89 96.52 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J24"
      (at 516.89 83.82 0.0))
    (property "Value" "Z2 S4 TOP"
      (at 516.89 86.36 0.0))
    (property "Footprint" "ELFlex:J24_Solder4"
      (at 516.89 96.52 0.0)
      (hide yes))
    (instances
      (project "led-upper-v0.3"
        (path
          (reference "J24")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (no_connect
    (at 511.81 93.98))
  (no_connect
    (at 511.81 96.52))
  (no_connect
    (at 511.81 99.06))
  (no_connect
    (at 511.81 101.6))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 219.71 146.05 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J31"
      (at 219.71 133.35 0.0))
    (property "Value" "Z3 S1 TOP"
      (at 219.71 135.89 0.0))
    (property "Footprint" "ELFlex:J31_Solder4"
      (at 219.71 146.05 0.0)
      (hide yes))
    (instances
      (project "led-upper-v0.3"
        (path
          (reference "J31")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 214.63 143.51)
      (xy 204.47 143.51)))
  (global_label "ZONE3_24V"
    (shape passive)
    (at 204.47 143.51 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 204.47 143.51 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 214.63 146.05)
      (xy 204.47 146.05)))
  (global_label "ZONE3_W"
    (shape passive)
    (at 204.47 146.05 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 204.47 146.05 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 214.63 148.59)
      (xy 204.47 148.59)))
  (global_label "ZONE3_N"
    (shape passive)
    (at 204.47 148.59 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 204.47 148.59 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 214.63 151.13)
      (xy 204.47 151.13)))
  (global_label "ZONE3_C"
    (shape passive)
    (at 204.47 151.13 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 204.47 151.13 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 318.77 146.05 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J32"
      (at 318.77 133.35 0.0))
    (property "Value" "Z3 S2 TOP"
      (at 318.77 135.89 0.0))
    (property "Footprint" "ELFlex:J32_Solder4"
      (at 318.77 146.05 0.0)
      (hide yes))
    (instances
      (project "led-upper-v0.3"
        (path
          (reference "J32")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 313.69 143.51)
      (xy 302.26 143.51)))
  (global_label "Z3_T23_24V"
    (shape passive)
    (at 302.26 143.51 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 302.26 143.51 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 313.69 146.05)
      (xy 303.53 146.05)))
  (global_label "Z3_T23_W"
    (shape passive)
    (at 303.53 146.05 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 303.53 146.05 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 313.69 148.59)
      (xy 303.53 148.59)))
  (global_label "Z3_T23_N"
    (shape passive)
    (at 303.53 148.59 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 303.53 148.59 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 313.69 151.13)
      (xy 303.53 151.13)))
  (global_label "Z3_T23_C"
    (shape passive)
    (at 303.53 151.13 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 303.53 151.13 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 417.83 146.05 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J33"
      (at 417.83 133.35 0.0))
    (property "Value" "Z3 S3 TOP"
      (at 417.83 135.89 0.0))
    (property "Footprint" "ELFlex:J33_Solder4"
      (at 417.83 146.05 0.0)
      (hide yes))
    (instances
      (project "led-upper-v0.3"
        (path
          (reference "J33")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 412.75 143.51)
      (xy 401.32 143.51)))
  (global_label "Z3_T23_24V"
    (shape passive)
    (at 401.32 143.51 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 401.32 143.51 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 412.75 146.05)
      (xy 402.59 146.05)))
  (global_label "Z3_T23_W"
    (shape passive)
    (at 402.59 146.05 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 402.59 146.05 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 412.75 148.59)
      (xy 402.59 148.59)))
  (global_label "Z3_T23_N"
    (shape passive)
    (at 402.59 148.59 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 402.59 148.59 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 412.75 151.13)
      (xy 402.59 151.13)))
  (global_label "Z3_T23_C"
    (shape passive)
    (at 402.59 151.13 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 402.59 151.13 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 516.89 146.05 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J34"
      (at 516.89 133.35 0.0))
    (property "Value" "Z3 S4 TOP"
      (at 516.89 135.89 0.0))
    (property "Footprint" "ELFlex:J34_Solder4"
      (at 516.89 146.05 0.0)
      (hide yes))
    (instances
      (project "led-upper-v0.3"
        (path
          (reference "J34")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (no_connect
    (at 511.81 143.51))
  (no_connect
    (at 511.81 146.05))
  (no_connect
    (at 511.81 148.59))
  (no_connect
    (at 511.81 151.13))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 219.71 195.58 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J41"
      (at 219.71 182.88 0.0))
    (property "Value" "Z4 S1 TOP"
      (at 219.71 185.42 0.0))
    (property "Footprint" "ELFlex:J41_Solder4"
      (at 219.71 195.58 0.0)
      (hide yes))
    (instances
      (project "led-upper-v0.3"
        (path
          (reference "J41")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (no_connect
    (at 214.63 193.04))
  (no_connect
    (at 214.63 195.58))
  (no_connect
    (at 214.63 198.12))
  (no_connect
    (at 214.63 200.66))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 318.77 195.58 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J42"
      (at 318.77 182.88 0.0))
    (property "Value" "Z4 S2 TOP"
      (at 318.77 185.42 0.0))
    (property "Footprint" "ELFlex:J42_Solder4"
      (at 318.77 195.58 0.0)
      (hide yes))
    (instances
      (project "led-upper-v0.3"
        (path
          (reference "J42")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 313.69 193.04)
      (xy 302.26 193.04)))
  (global_label "Z4_T23_24V"
    (shape passive)
    (at 302.26 193.04 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 302.26 193.04 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 313.69 195.58)
      (xy 303.53 195.58)))
  (global_label "Z4_T23_W"
    (shape passive)
    (at 303.53 195.58 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 303.53 195.58 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 313.69 198.12)
      (xy 303.53 198.12)))
  (global_label "Z4_T23_N"
    (shape passive)
    (at 303.53 198.12 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 303.53 198.12 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 313.69 200.66)
      (xy 303.53 200.66)))
  (global_label "Z4_T23_C"
    (shape passive)
    (at 303.53 200.66 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 303.53 200.66 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 417.83 195.58 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J43"
      (at 417.83 182.88 0.0))
    (property "Value" "Z4 S3 TOP"
      (at 417.83 185.42 0.0))
    (property "Footprint" "ELFlex:J43_Solder4"
      (at 417.83 195.58 0.0)
      (hide yes))
    (instances
      (project "led-upper-v0.3"
        (path
          (reference "J43")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 412.75 193.04)
      (xy 401.32 193.04)))
  (global_label "Z4_T23_24V"
    (shape passive)
    (at 401.32 193.04 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 401.32 193.04 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 412.75 195.58)
      (xy 402.59 195.58)))
  (global_label "Z4_T23_W"
    (shape passive)
    (at 402.59 195.58 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 402.59 195.58 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 412.75 198.12)
      (xy 402.59 198.12)))
  (global_label "Z4_T23_N"
    (shape passive)
    (at 402.59 198.12 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 402.59 198.12 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 412.75 200.66)
      (xy 402.59 200.66)))
  (global_label "Z4_T23_C"
    (shape passive)
    (at 402.59 200.66 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 402.59 200.66 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 516.89 195.58 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J44"
      (at 516.89 182.88 0.0))
    (property "Value" "Z4 S4 TOP"
      (at 516.89 185.42 0.0))
    (property "Footprint" "ELFlex:J44_Solder4"
      (at 516.89 195.58 0.0)
      (hide yes))
    (instances
      (project "led-upper-v0.3"
        (path
          (reference "J44")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 511.81 193.04)
      (xy 501.65 193.04)))
  (global_label "ZONE4_24V"
    (shape passive)
    (at 501.65 193.04 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 501.65 193.04 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 511.81 195.58)
      (xy 501.65 195.58)))
  (global_label "ZONE4_W"
    (shape passive)
    (at 501.65 195.58 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 501.65 195.58 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 511.81 198.12)
      (xy 501.65 198.12)))
  (global_label "ZONE4_N"
    (shape passive)
    (at 501.65 198.12 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 501.65 198.12 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 511.81 200.66)
      (xy 501.65 200.66)))
  (global_label "ZONE4_C"
    (shape passive)
    (at 501.65 200.66 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 501.65 200.66 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 219.71 243.84 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J51"
      (at 219.71 231.14 0.0))
    (property "Value" "Z5 S1 TOP"
      (at 219.71 233.68 0.0))
    (property "Footprint" "ELFlex:J51_Solder4"
      (at 219.71 243.84 0.0)
      (hide yes))
    (instances
      (project "led-upper-v0.3"
        (path
          (reference "J51")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (no_connect
    (at 214.63 241.3))
  (no_connect
    (at 214.63 243.84))
  (no_connect
    (at 214.63 246.38))
  (no_connect
    (at 214.63 248.92))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 318.77 243.84 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J52"
      (at 318.77 231.14 0.0))
    (property "Value" "Z5 S2 TOP"
      (at 318.77 233.68 0.0))
    (property "Footprint" "ELFlex:J52_Solder4"
      (at 318.77 243.84 0.0)
      (hide yes))
    (instances
      (project "led-upper-v0.3"
        (path
          (reference "J52")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 313.69 241.3)
      (xy 302.26 241.3)))
  (global_label "Z5_T23_24V"
    (shape passive)
    (at 302.26 241.3 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 302.26 241.3 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 313.69 243.84)
      (xy 303.53 243.84)))
  (global_label "Z5_T23_W"
    (shape passive)
    (at 303.53 243.84 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 303.53 243.84 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 313.69 246.38)
      (xy 303.53 246.38)))
  (global_label "Z5_T23_N"
    (shape passive)
    (at 303.53 246.38 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 303.53 246.38 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 313.69 248.92)
      (xy 303.53 248.92)))
  (global_label "Z5_T23_C"
    (shape passive)
    (at 303.53 248.92 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 303.53 248.92 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 417.83 243.84 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J53"
      (at 417.83 231.14 0.0))
    (property "Value" "Z5 S3 TOP"
      (at 417.83 233.68 0.0))
    (property "Footprint" "ELFlex:J53_Solder4"
      (at 417.83 243.84 0.0)
      (hide yes))
    (instances
      (project "led-upper-v0.3"
        (path
          (reference "J53")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 412.75 241.3)
      (xy 401.32 241.3)))
  (global_label "Z5_T23_24V"
    (shape passive)
    (at 401.32 241.3 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 401.32 241.3 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 412.75 243.84)
      (xy 402.59 243.84)))
  (global_label "Z5_T23_W"
    (shape passive)
    (at 402.59 243.84 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 402.59 243.84 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 412.75 246.38)
      (xy 402.59 246.38)))
  (global_label "Z5_T23_N"
    (shape passive)
    (at 402.59 246.38 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 402.59 246.38 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 412.75 248.92)
      (xy 402.59 248.92)))
  (global_label "Z5_T23_C"
    (shape passive)
    (at 402.59 248.92 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 402.59 248.92 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 516.89 243.84 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J54"
      (at 516.89 231.14 0.0))
    (property "Value" "Z5 S4 TOP"
      (at 516.89 233.68 0.0))
    (property "Footprint" "ELFlex:J54_Solder4"
      (at 516.89 243.84 0.0)
      (hide yes))
    (instances
      (project "led-upper-v0.3"
        (path
          (reference "J54")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 511.81 241.3)
      (xy 501.65 241.3)))
  (global_label "ZONE5_24V"
    (shape passive)
    (at 501.65 241.3 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 501.65 241.3 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 511.81 243.84)
      (xy 501.65 243.84)))
  (global_label "ZONE5_W"
    (shape passive)
    (at 501.65 243.84 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 501.65 243.84 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 511.81 246.38)
      (xy 501.65 246.38)))
  (global_label "ZONE5_N"
    (shape passive)
    (at 501.65 246.38 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 501.65 246.38 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 511.81 248.92)
      (xy 501.65 248.92)))
  (global_label "ZONE5_C"
    (shape passive)
    (at 501.65 248.92 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 501.65 248.92 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 219.71 293.37 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J61"
      (at 219.71 280.67 0.0))
    (property "Value" "Z6 S1 TOP"
      (at 219.71 283.21 0.0))
    (property "Footprint" "ELFlex:J61_Solder4"
      (at 219.71 293.37 0.0)
      (hide yes))
    (instances
      (project "led-upper-v0.3"
        (path
          (reference "J61")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (no_connect
    (at 214.63 290.83))
  (no_connect
    (at 214.63 293.37))
  (no_connect
    (at 214.63 295.91))
  (no_connect
    (at 214.63 298.45))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 318.77 293.37 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J62"
      (at 318.77 280.67 0.0))
    (property "Value" "Z6 S2 TOP"
      (at 318.77 283.21 0.0))
    (property "Footprint" "ELFlex:J62_Solder4"
      (at 318.77 293.37 0.0)
      (hide yes))
    (instances
      (project "led-upper-v0.3"
        (path
          (reference "J62")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 313.69 290.83)
      (xy 302.26 290.83)))
  (global_label "Z6_T23_24V"
    (shape passive)
    (at 302.26 290.83 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 302.26 290.83 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 313.69 293.37)
      (xy 303.53 293.37)))
  (global_label "Z6_T23_W"
    (shape passive)
    (at 303.53 293.37 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 303.53 293.37 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 313.69 295.91)
      (xy 303.53 295.91)))
  (global_label "Z6_T23_N"
    (shape passive)
    (at 303.53 295.91 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 303.53 295.91 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 313.69 298.45)
      (xy 303.53 298.45)))
  (global_label "Z6_T23_C"
    (shape passive)
    (at 303.53 298.45 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 303.53 298.45 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 417.83 293.37 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J63"
      (at 417.83 280.67 0.0))
    (property "Value" "Z6 S3 TOP"
      (at 417.83 283.21 0.0))
    (property "Footprint" "ELFlex:J63_Solder4"
      (at 417.83 293.37 0.0)
      (hide yes))
    (instances
      (project "led-upper-v0.3"
        (path
          (reference "J63")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 412.75 290.83)
      (xy 401.32 290.83)))
  (global_label "Z6_T23_24V"
    (shape passive)
    (at 401.32 290.83 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 401.32 290.83 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 412.75 293.37)
      (xy 402.59 293.37)))
  (global_label "Z6_T23_W"
    (shape passive)
    (at 402.59 293.37 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 402.59 293.37 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 412.75 295.91)
      (xy 402.59 295.91)))
  (global_label "Z6_T23_N"
    (shape passive)
    (at 402.59 295.91 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 402.59 295.91 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 412.75 298.45)
      (xy 402.59 298.45)))
  (global_label "Z6_T23_C"
    (shape passive)
    (at 402.59 298.45 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 402.59 298.45 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 516.89 293.37 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J64"
      (at 516.89 280.67 0.0))
    (property "Value" "Z6 S4 TOP"
      (at 516.89 283.21 0.0))
    (property "Footprint" "ELFlex:J64_Solder4"
      (at 516.89 293.37 0.0)
      (hide yes))
    (instances
      (project "led-upper-v0.3"
        (path
          (reference "J64")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 511.81 290.83)
      (xy 501.65 290.83)))
  (global_label "ZONE6_24V"
    (shape passive)
    (at 501.65 290.83 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 501.65 290.83 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 511.81 293.37)
      (xy 501.65 293.37)))
  (global_label "ZONE6_W"
    (shape passive)
    (at 501.65 293.37 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 501.65 293.37 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 511.81 295.91)
      (xy 501.65 295.91)))
  (global_label "ZONE6_N"
    (shape passive)
    (at 501.65 295.91 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 501.65 295.91 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 511.81 298.45)
      (xy 501.65 298.45)))
  (global_label "ZONE6_C"
    (shape passive)
    (at 501.65 298.45 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 501.65 298.45 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x30")
    (at 90.17 139.7 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom no)
    (on_board yes)
    (dnp no)
    (property "Reference" "J100"
      (at 90.17 93.98 0.0))
    (property "Value" "30-contact FPC tail / Molex 2005280300"
      (at 90.17 96.52 0.0))
    (property "Footprint" "ELFlex:J100_FPC30_BottomContacts"
      (at 90.17 139.7 0.0)
      (hide yes))
    (instances
      (project "led-upper-v0.3"
        (path
          (reference "J100")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "29")
    (pin "30"))
  (wire
    (pts
      (xy 85.09 104.14)
      (xy 74.93 104.14)))
  (global_label "ZONE4_24V"
    (shape passive)
    (at 74.93 104.14 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 104.14 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 106.68)
      (xy 74.93 106.68)))
  (global_label "ZONE4_24V"
    (shape passive)
    (at 74.93 106.68 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 106.68 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 109.22)
      (xy 74.93 109.22)))
  (global_label "ZONE4_W"
    (shape passive)
    (at 74.93 109.22 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 109.22 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 111.76)
      (xy 74.93 111.76)))
  (global_label "ZONE4_N"
    (shape passive)
    (at 74.93 111.76 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 111.76 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 114.3)
      (xy 74.93 114.3)))
  (global_label "ZONE4_C"
    (shape passive)
    (at 74.93 114.3 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 114.3 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 116.84)
      (xy 74.93 116.84)))
  (global_label "ZONE5_24V"
    (shape passive)
    (at 74.93 116.84 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 116.84 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 119.38)
      (xy 74.93 119.38)))
  (global_label "ZONE5_24V"
    (shape passive)
    (at 74.93 119.38 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 119.38 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 121.92)
      (xy 74.93 121.92)))
  (global_label "ZONE5_W"
    (shape passive)
    (at 74.93 121.92 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 121.92 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 124.46)
      (xy 74.93 124.46)))
  (global_label "ZONE5_N"
    (shape passive)
    (at 74.93 124.46 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 124.46 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 127.0)
      (xy 74.93 127.0)))
  (global_label "ZONE5_C"
    (shape passive)
    (at 74.93 127.0 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 127.0 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 129.54)
      (xy 74.93 129.54)))
  (global_label "ZONE6_24V"
    (shape passive)
    (at 74.93 129.54 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 129.54 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 132.08)
      (xy 74.93 132.08)))
  (global_label "ZONE6_24V"
    (shape passive)
    (at 74.93 132.08 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 132.08 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 134.62)
      (xy 74.93 134.62)))
  (global_label "ZONE6_W"
    (shape passive)
    (at 74.93 134.62 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 134.62 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 137.16)
      (xy 74.93 137.16)))
  (global_label "ZONE6_N"
    (shape passive)
    (at 74.93 137.16 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 137.16 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 139.7)
      (xy 74.93 139.7)))
  (global_label "ZONE6_C"
    (shape passive)
    (at 74.93 139.7 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 139.7 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 142.24)
      (xy 74.93 142.24)))
  (global_label "ZONE1_24V"
    (shape passive)
    (at 74.93 142.24 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 142.24 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 144.78)
      (xy 74.93 144.78)))
  (global_label "ZONE1_24V"
    (shape passive)
    (at 74.93 144.78 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 144.78 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 147.32)
      (xy 74.93 147.32)))
  (global_label "ZONE1_W"
    (shape passive)
    (at 74.93 147.32 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 147.32 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 149.86)
      (xy 74.93 149.86)))
  (global_label "ZONE1_N"
    (shape passive)
    (at 74.93 149.86 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 149.86 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 152.4)
      (xy 74.93 152.4)))
  (global_label "ZONE1_C"
    (shape passive)
    (at 74.93 152.4 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 152.4 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 154.94)
      (xy 74.93 154.94)))
  (global_label "ZONE2_24V"
    (shape passive)
    (at 74.93 154.94 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 154.94 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 157.48)
      (xy 74.93 157.48)))
  (global_label "ZONE2_24V"
    (shape passive)
    (at 74.93 157.48 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 157.48 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 160.02)
      (xy 74.93 160.02)))
  (global_label "ZONE2_W"
    (shape passive)
    (at 74.93 160.02 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 160.02 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 162.56)
      (xy 74.93 162.56)))
  (global_label "ZONE2_N"
    (shape passive)
    (at 74.93 162.56 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 162.56 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 165.1)
      (xy 74.93 165.1)))
  (global_label "ZONE2_C"
    (shape passive)
    (at 74.93 165.1 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 165.1 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 167.64)
      (xy 74.93 167.64)))
  (global_label "ZONE3_24V"
    (shape passive)
    (at 74.93 167.64 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 167.64 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 170.18)
      (xy 74.93 170.18)))
  (global_label "ZONE3_24V"
    (shape passive)
    (at 74.93 170.18 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 170.18 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 172.72)
      (xy 74.93 172.72)))
  (global_label "ZONE3_W"
    (shape passive)
    (at 74.93 172.72 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 172.72 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 175.26)
      (xy 74.93 175.26)))
  (global_label "ZONE3_N"
    (shape passive)
    (at 74.93 175.26 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 175.26 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 85.09 177.8)
      (xy 74.93 177.8)))
  (global_label "ZONE3_C"
    (shape passive)
    (at 74.93 177.8 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 74.93 177.8 0.0)
      (hide yes)))
  (text "J100 is fabricated gold fingers, not an assembled connector.\nF-side/stiffener view, tip up: pin 1 LEFT. Gold-face view: pin 1 RIGHT.\nSix groups: Z4, Z5, Z6, Z1, Z2, Z3; each +,+,W,N,C.\nEach positive contact alone is rated for the 0.60 A zone screen.\nNo common positive supply across zones.\nStrip pin 1=+24V, 2=W, 3=N, 4=C.\nUnconnected strip ends receive power through lower flex and strip rails.\nThrough-rail continuity remains a physical test requirement."
    (at 28.0 250.0 0)))
