(kicad_sch
  (version 20250114)
  (generator "engineered-lighting")
  (generator_version "0.2")
  (paper "A3")
  (title_block
    (title "Controller")
    (date "2026-09-06")
    (rev "A draft")
    (company "Engineered Lighting")
    (comment 1 "ENGINEERING DRAFT - see release status before fabrication"))
  (lib_symbols
    (symbol "EL:ESP32-C6-WROOM-1"
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "U"
        (at -25.4 35.56 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "ESP32-C6-WROOM-1"
        (at -25.4 33.02 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" "PCM_Espressif:ESP32-C6-WROOM-1"
        (at 0 -45.085 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-c6-wroom-1_wroom-1u_datasheet_en.pdf"
        (at 0 -48.26 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "ESP32-C6-WROOM-1/U is a module that supports 2.4 GHz Wi-Fi 6 (802.11 ax), Bluetooth® 5 (LE), Zigbee and Thread (802.15.4)"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "esp32-c6 esp32-c6-wroom-1 esp32-c6-wroom-1u"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "ESP32-C6-WROOM-1*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "ESP32-C6-WROOM-1_0_0"
        (text "ESP32-C6-WROOM-1"
          (at 0 -20.955 0)))
      (symbol "ESP32-C6-WROOM-1_0_1"
        (rectangle
          (start -25.4 30.48)
          (end 25.4 -30.48)
          (fill
            (type background))))
      (symbol "ESP32-C6-WROOM-1_1_1"
        (pin power_in line
          (at 0 -33.02 90)
          (length 2.54)
          (name "GND")
          (number "1"))
        (pin power_in line
          (at 0 33.02 270)
          (length 2.54)
          (name "3V3")
          (number "2"))
        (pin input line
          (at -27.94 27.94 0)
          (length 2.54)
          (name "EN/CHIP_PU")
          (number "3"))
        (pin bidirectional line
          (at -27.94 7.62 0)
          (length 2.54)
          (name "MTMS/GPIO4/ADC1_CH4")
          (number "4"))
        (pin bidirectional line
          (at -27.94 5.08 0)
          (length 2.54)
          (name "MTDI/GPIO5/ADC1_CH5")
          (number "5"))
        (pin bidirectional line
          (at -27.94 2.54 0)
          (length 2.54)
          (name "MTCK/GPIO6/ADC1_CH6")
          (number "6"))
        (pin bidirectional line
          (at -27.94 0 0)
          (length 2.54)
          (name "MTDO/GPIO7")
          (number "7"))
        (pin bidirectional line
          (at -27.94 22.86 0)
          (length 2.54)
          (name "GPIO0/ADC1_CH0/XTAL_32K_P")
          (number "8"))
        (pin bidirectional line
          (at -27.94 20.32 0)
          (length 2.54)
          (name "GPIO1/ADC1_CH1/XTAL_32K_N")
          (number "9"))
        (pin bidirectional line
          (at 27.94 7.62 180)
          (length 2.54)
          (name "GPIO8")
          (number "10"))
        (pin bidirectional line
          (at 27.94 2.54 180)
          (length 2.54)
          (name "GPIO10")
          (number "11"))
        (pin bidirectional line
          (at 27.94 0 180)
          (length 2.54)
          (name "GPIO11")
          (number "12"))
        (pin bidirectional line
          (at 27.94 17.78 180)
          (length 2.54)
          (name "GPIO12/USB_D-")
          (number "13"))
        (pin bidirectional line
          (at 27.94 20.32 180)
          (length 2.54)
          (name "GPIO13/USB_D+")
          (number "14"))
        (pin bidirectional line
          (at 27.94 5.08 180)
          (length 2.54)
          (name "GPIO9")
          (number "15"))
        (pin bidirectional line
          (at 27.94 -5.08 180)
          (length 2.54)
          (name "GPIO18")
          (number "16"))
        (pin bidirectional line
          (at 27.94 -7.62 180)
          (length 2.54)
          (name "GPIO19")
          (number "17"))
        (pin bidirectional line
          (at 27.94 -10.16 180)
          (length 2.54)
          (name "GPIO20")
          (number "18"))
        (pin bidirectional line
          (at 27.94 -12.7 180)
          (length 2.54)
          (name "GPIO21")
          (number "19"))
        (pin bidirectional line
          (at 27.94 -15.24 180)
          (length 2.54)
          (name "GPIO22")
          (number "20"))
        (pin bidirectional line
          (at 27.94 -17.78 180)
          (length 2.54)
          (name "GPIO23")
          (number "21"))
        (pin no_connect line
          (at -25.4 -12.7 0)
          (length 2.54)
          (hide yes)
          (name "NC")
          (number "22"))
        (pin bidirectional line
          (at 27.94 -2.54 180)
          (length 2.54)
          (name "GPIO15")
          (number "23"))
        (pin bidirectional line
          (at 27.94 25.4 180)
          (length 2.54)
          (name "U0RXD/GPIO17")
          (number "24"))
        (pin bidirectional line
          (at 27.94 27.94 180)
          (length 2.54)
          (name "U0TXD/GPIO16")
          (number "25"))
        (pin bidirectional line
          (at -27.94 15.24 0)
          (length 2.54)
          (name "GPIO3/ADC1_CH3")
          (number "26"))
        (pin bidirectional line
          (at -27.94 17.78 0)
          (length 2.54)
          (name "GPIO2/ADC1_CH2")
          (number "27"))
        (pin passive line
          (at 0 -33.02 90)
          (length 2.54)
          (hide yes)
          (name "GND")
          (number "28"))
        (pin passive line
          (at 0 -33.02 90)
          (length 2.54)
          (hide yes)
          (name "GND")
          (number "29")))
      (embedded_fonts no))
    (symbol "Device:R"
      (pin_numbers
        (hide yes))
      (pin_names
        (offset 0))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "R"
        (at 2.032 0 90)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "R"
        (at 0 0 90)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" ""
        (at -1.778 0 90)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Resistor"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "R res resistor"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "R_*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "R_0_1"
        (rectangle
          (start -1.016 -2.54)
          (end 1.016 2.54)
          (fill
            (type none))))
      (symbol "R_1_1"
        (pin passive line
          (at 0 3.81 270)
          (length 1.27)
          (name "")
          (number "1"))
        (pin passive line
          (at 0 -3.81 90)
          (length 1.27)
          (name "")
          (number "2")))
      (embedded_fonts no))
    (symbol "Device:C"
      (pin_numbers
        (hide yes))
      (pin_names
        (offset 0.254))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "C"
        (at 0.635 2.54 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "C"
        (at 0.635 -2.54 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" ""
        (at 0.9652 -3.81 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Unpolarized capacitor"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "cap capacitor"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "C_*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762))
          (fill
            (type none)))
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762))
          (fill
            (type none))))
      (symbol "C_1_1"
        (pin passive line
          (at 0 3.81 270)
          (length 2.794)
          (name "")
          (number "1"))
        (pin passive line
          (at 0 -3.81 90)
          (length 2.794)
          (name "")
          (number "2")))
      (embedded_fonts no))
    (symbol "Switch:SW_Push"
      (pin_numbers
        (hide yes))
      (pin_names
        (offset 1.016)
        (hide yes))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "SW"
        (at 1.27 2.54 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "SW_Push"
        (at 0 -1.524 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" ""
        (at 0 5.08 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" ""
        (at 0 5.08 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Push button switch, generic, two pins"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "switch normally-open pushbutton push-button"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "SW_Push_0_1"
        (circle
          (center -2.032 0)
          (radius 0.508)
          (fill
            (type none)))
        (polyline
          (pts
            (xy 0 1.27)
            (xy 0 3.048))
          (fill
            (type none)))
        (circle
          (center 2.032 0)
          (radius 0.508)
          (fill
            (type none)))
        (polyline
          (pts
            (xy 2.54 1.27)
            (xy -2.54 1.27))
          (fill
            (type none)))
        (pin passive line
          (at -5.08 0 0)
          (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line
          (at 5.08 0 180)
          (length 2.54)
          (name "2")
          (number "2")))
      (embedded_fonts no))
    (symbol "Connector_Generic:Conn_01x02"
      (pin_names
        (offset 1.016)
        (hide yes))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "J"
        (at 0 2.54 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "Conn_01x02"
        (at 0 -5.08 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "connector"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "Connector*:*_1x??_*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "Conn_01x02_1_1"
        (rectangle
          (start -1.27 1.27)
          (end 1.27 -3.81)
          (fill
            (type background)))
        (rectangle
          (start -1.27 0.127)
          (end 0 -0.127)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -2.413)
          (end 0 -2.667)
          (fill
            (type none)))
        (pin passive line
          (at -5.08 0 0)
          (length 3.81)
          (name "Pin_1")
          (number "1"))
        (pin passive line
          (at -5.08 -2.54 0)
          (length 3.81)
          (name "Pin_2")
          (number "2")))
      (embedded_fonts no))
    (symbol "Connector_Generic:Conn_01x04"
      (pin_names
        (offset 1.016)
        (hide yes))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "J"
        (at 0 5.08 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "Conn_01x04"
        (at 0 -7.62 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "connector"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "Connector*:*_1x??_*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "Conn_01x04_1_1"
        (rectangle
          (start -1.27 3.81)
          (end 1.27 -6.35)
          (fill
            (type background)))
        (rectangle
          (start -1.27 2.667)
          (end 0 2.413)
          (fill
            (type none)))
        (rectangle
          (start -1.27 0.127)
          (end 0 -0.127)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -2.413)
          (end 0 -2.667)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -4.953)
          (end 0 -5.207)
          (fill
            (type none)))
        (pin passive line
          (at -5.08 2.54 0)
          (length 3.81)
          (name "Pin_1")
          (number "1"))
        (pin passive line
          (at -5.08 0 0)
          (length 3.81)
          (name "Pin_2")
          (number "2"))
        (pin passive line
          (at -5.08 -2.54 0)
          (length 3.81)
          (name "Pin_3")
          (number "3"))
        (pin passive line
          (at -5.08 -5.08 0)
          (length 3.81)
          (name "Pin_4")
          (number "4")))
      (embedded_fonts no))
    (symbol "EL:74HCS08"
      (pin_names
        (offset 0.8))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (property "Reference" "U"
        (at 0 15.239999999999998 0))
      (property "Value" "74HCS08"
        (at 0 -15.239999999999998 0))
      (symbol "74HCS08_0_1"
        (rectangle
          (start -12.7 12.7)
          (end 12.7 -12.7)
          (fill
            (type background))))
      (symbol "74HCS08_1_1"
        (pin input line
          (at -17.78 10.16 0)
          (length 5.08)
          (name "1A")
          (number "1"))
        (pin input line
          (at -17.78 7.62 0)
          (length 5.08)
          (name "1B")
          (number "2"))
        (pin input line
          (at -17.78 5.08 0)
          (length 5.08)
          (name "2A")
          (number "4"))
        (pin input line
          (at -17.78 2.54 0)
          (length 5.08)
          (name "2B")
          (number "5"))
        (pin power_in line
          (at -17.78 0.0 0)
          (length 5.08)
          (name "GND")
          (number "7"))
        (pin input line
          (at -17.78 -2.539999999999999 0)
          (length 5.08)
          (name "3A")
          (number "9"))
        (pin input line
          (at -17.78 -5.08 0)
          (length 5.08)
          (name "3B")
          (number "10"))
        (pin input line
          (at -17.78 -7.620000000000001 0)
          (length 5.08)
          (name "4A")
          (number "12"))
        (pin input line
          (at -17.78 -10.16 0)
          (length 5.08)
          (name "4B")
          (number "13"))
        (pin output line
          (at 17.78 10.16 180)
          (length 5.08)
          (name "1Y")
          (number "3"))
        (pin output line
          (at 17.78 7.62 180)
          (length 5.08)
          (name "2Y")
          (number "6"))
        (pin output line
          (at 17.78 5.08 180)
          (length 5.08)
          (name "3Y")
          (number "8"))
        (pin output line
          (at 17.78 2.54 180)
          (length 5.08)
          (name "4Y")
          (number "11"))
        (pin power_in line
          (at 17.78 0.0 180)
          (length 5.08)
          (name "VCC")
          (number "14"))))
    (symbol "74xGxx:74LVC1G04"
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "U"
        (at 0 7.62 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "74LVC1G04"
        (at 5.08 -7.62 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc1g04.pdf"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Single NOT Gate, Low-Voltage CMOS"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "Single Gate NOT LVC CMOS"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "74LVC1G04_0_1"
        (polyline
          (pts
            (xy -7.62 6.35)
            (xy -7.62 -6.35)
            (xy 5.08 0)
            (xy -7.62 6.35))
          (fill
            (type background))))
      (symbol "74LVC1G04_1_1"
        (pin no_connect line
          (at -7.62 2.54 0)
          (length 2.54)
          (hide yes)
          (name "NC")
          (number "1"))
        (pin input line
          (at -15.24 0 0)
          (length 7.62)
          (name "")
          (number "2"))
        (pin power_in line
          (at -5.08 -10.16 90)
          (length 5.08)
          (name "GND")
          (number "3"))
        (pin output inverted
          (at 12.7 0 180)
          (length 7.62)
          (name "")
          (number "4"))
        (pin power_in line
          (at -5.08 10.16 270)
          (length 5.08)
          (name "VCC")
          (number "5")))
      (embedded_fonts no)))
  (symbol
    (lib_id "EL:ESP32-C6-WROOM-1")
    (at 93.98 104.14 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "U1"
      (at 124.46 63.5 0.0))
    (property "Value" "ESP32-C6-WROOM-1-N8"
      (at 124.46 66.04 0.0))
    (property "Footprint" "EL:ESP32-C6-WROOM-1"
      (at 93.98 104.14 0.0)
      (hide yes))
    (property "MPN" "ESP32-C6-WROOM-1-N8"
      (at 93.98 104.14 0.0)
      (hide yes))
    (property "Manufacturer" "Espressif"
      (at 93.98 104.14 0.0)
      (hide yes))
    (property "Datasheet" "https://documentation.espressif.com/esp32-c6-wroom-1_wroom-1u_datasheet_en.html"
      (at 93.98 104.14 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "U1")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "29"))
  (wire
    (pts
      (xy 93.98 137.16)
      (xy 93.98 144.78)))
  (global_label "GND"
    (shape passive)
    (at 93.98 144.78 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 93.98 144.78 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 93.98 71.12)
      (xy 93.98 63.5)))
  (global_label "+3V3"
    (shape passive)
    (at 93.98 63.5 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 93.98 63.5 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 66.04 76.2)
      (xy 57.15 76.2)))
  (global_label "MCU_EN"
    (shape passive)
    (at 57.15 76.2 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 57.15 76.2 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 66.04 96.52)
      (xy 54.61 96.52)))
  (global_label "GPIO4_STRAP"
    (shape passive)
    (at 54.61 96.52 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 54.61 96.52 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 66.04 99.06)
      (xy 54.61 99.06)))
  (global_label "GPIO5_STRAP"
    (shape passive)
    (at 54.61 99.06 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 54.61 99.06 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 66.04 101.6)
      (xy 57.15 101.6)))
  (global_label "CAN_TX"
    (shape passive)
    (at 57.15 101.6 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 57.15 101.6 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 66.04 104.14)
      (xy 57.15 104.14)))
  (global_label "CAN_RX"
    (shape passive)
    (at 57.15 104.14 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 57.15 104.14 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 66.04 81.28)
      (xy 53.34 81.28)))
  (global_label "LIGHT_ENABLE"
    (shape passive)
    (at 53.34 81.28 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 53.34 81.28 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 66.04 83.82)
      (xy 53.34 83.82)))
  (global_label "USB_PRESENT_N"
    (shape passive)
    (at 53.34 83.82 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 53.34 83.82 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 121.92 96.52)
      (xy 133.35 96.52)))
  (global_label "BOOT_GPIO8"
    (shape passive)
    (at 133.35 96.52 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 133.35 96.52 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 121.92 101.6)
      (xy 132.08 101.6)))
  (global_label "SPOT1_PWM"
    (shape passive)
    (at 132.08 101.6 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 132.08 101.6 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 121.92 104.14)
      (xy 132.08 104.14)))
  (global_label "SPOT2_PWM"
    (shape passive)
    (at 132.08 104.14 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 132.08 104.14 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 121.92 86.36)
      (xy 133.35 86.36)))
  (global_label "USB_DM_MCU"
    (shape passive)
    (at 133.35 86.36 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 133.35 86.36 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 121.92 83.82)
      (xy 133.35 83.82)))
  (global_label "USB_DP_MCU"
    (shape passive)
    (at 133.35 83.82 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 133.35 83.82 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 121.92 99.06)
      (xy 133.35 99.06)))
  (global_label "BOOT_GPIO9"
    (shape passive)
    (at 133.35 99.06 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 133.35 99.06 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 121.92 109.22)
      (xy 132.08 109.22)))
  (global_label "SPOT3_PWM"
    (shape passive)
    (at 132.08 109.22 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 132.08 109.22 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 121.92 111.76)
      (xy 130.81 111.76)))
  (global_label "GPIO19"
    (shape passive)
    (at 130.81 111.76 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 130.81 111.76 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 121.92 114.3)
      (xy 130.81 114.3)))
  (global_label "GPIO20"
    (shape passive)
    (at 130.81 114.3 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 130.81 114.3 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 121.92 116.84)
      (xy 130.81 116.84)))
  (global_label "GPIO21"
    (shape passive)
    (at 130.81 116.84 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 130.81 116.84 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 121.92 119.38)
      (xy 130.81 119.38)))
  (global_label "GPIO22"
    (shape passive)
    (at 130.81 119.38 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 130.81 119.38 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 121.92 121.92)
      (xy 130.81 121.92)))
  (global_label "GPIO23"
    (shape passive)
    (at 130.81 121.92 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 130.81 121.92 0.0)
      (hide yes)))
  (no_connect
    (at 68.58 116.84))
  (wire
    (pts
      (xy 121.92 106.68)
      (xy 134.62 106.68)))
  (global_label "GPIO15_STRAP"
    (shape passive)
    (at 134.62 106.68 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 134.62 106.68 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 121.92 78.74)
      (xy 132.08 78.74)))
  (global_label "UART_RX"
    (shape passive)
    (at 132.08 78.74 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 132.08 78.74 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 121.92 76.2)
      (xy 132.08 76.2)))
  (global_label "UART_TX"
    (shape passive)
    (at 132.08 76.2 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 132.08 76.2 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 66.04 88.9)
      (xy 55.88 88.9)))
  (global_label "I2C_SCL"
    (shape passive)
    (at 55.88 88.9 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 55.88 88.9 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 66.04 86.36)
      (xy 55.88 86.36)))
  (global_label "I2C_SDA"
    (shape passive)
    (at 55.88 86.36 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 55.88 86.36 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 195.58 55.88 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R1"
      (at 200.66 54.61 0.0))
    (property "Value" "10k"
      (at 200.66 57.15 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 195.58 55.88 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-0710KL"
      (at 195.58 55.88 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 195.58 55.88 0.0)
      (hide yes))
    (property "Datasheet" ""
      (at 195.58 55.88 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R1")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 195.58 52.07)
      (xy 195.58 44.45)))
  (global_label "+3V3"
    (shape passive)
    (at 195.58 44.45 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 195.58 44.45 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 195.58 59.69)
      (xy 195.58 68.58)))
  (global_label "MCU_EN"
    (shape passive)
    (at 195.58 68.58 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 195.58 68.58 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:C")
    (at 251.46 55.88 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C1"
      (at 256.54 54.61 0.0))
    (property "Value" "1u"
      (at 256.54 57.15 0.0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
      (at 251.46 55.88 0.0)
      (hide yes))
    (property "MPN" "C1608X7R1E105K080AB"
      (at 251.46 55.88 0.0)
      (hide yes))
    (property "Manufacturer" "TDK"
      (at 251.46 55.88 0.0)
      (hide yes))
    (property "Datasheet" ""
      (at 251.46 55.88 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C1")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 251.46 52.07)
      (xy 251.46 43.18)))
  (global_label "MCU_EN"
    (shape passive)
    (at 251.46 43.18 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 251.46 43.18 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 251.46 59.69)
      (xy 251.46 67.31)))
  (global_label "GND"
    (shape passive)
    (at 251.46 67.31 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 251.46 67.31 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 307.34 55.88 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R2"
      (at 312.42 54.61 0.0))
    (property "Value" "10k"
      (at 312.42 57.15 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 307.34 55.88 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-0710KL"
      (at 307.34 55.88 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 307.34 55.88 0.0)
      (hide yes))
    (property "Datasheet" ""
      (at 307.34 55.88 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R2")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 307.34 52.07)
      (xy 307.34 44.45)))
  (global_label "+3V3"
    (shape passive)
    (at 307.34 44.45 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 307.34 44.45 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 307.34 59.69)
      (xy 307.34 71.12)))
  (global_label "BOOT_GPIO9"
    (shape passive)
    (at 307.34 71.12 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 307.34 71.12 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 363.22 55.88 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R3"
      (at 368.3 54.61 0.0))
    (property "Value" "10k"
      (at 368.3 57.15 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 363.22 55.88 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-0710KL"
      (at 363.22 55.88 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 363.22 55.88 0.0)
      (hide yes))
    (property "Datasheet" ""
      (at 363.22 55.88 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R3")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 363.22 52.07)
      (xy 363.22 44.45)))
  (global_label "+3V3"
    (shape passive)
    (at 363.22 44.45 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 363.22 44.45 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 363.22 59.69)
      (xy 363.22 71.12)))
  (global_label "BOOT_GPIO8"
    (shape passive)
    (at 363.22 71.12 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 363.22 71.12 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 195.58 88.9 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R4"
      (at 200.66 87.63 0.0))
    (property "Value" "10k"
      (at 200.66 90.17 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 195.58 88.9 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-0710KL"
      (at 195.58 88.9 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 195.58 88.9 0.0)
      (hide yes))
    (property "Datasheet" ""
      (at 195.58 88.9 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R4")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 195.58 85.09)
      (xy 195.58 72.39)))
  (global_label "LIGHT_ENABLE"
    (shape passive)
    (at 195.58 72.39 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 195.58 72.39 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 195.58 92.71)
      (xy 195.58 100.33)))
  (global_label "GND"
    (shape passive)
    (at 195.58 100.33 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 195.58 100.33 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 251.46 88.9 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R5"
      (at 256.54 87.63 0.0))
    (property "Value" "10k"
      (at 256.54 90.17 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 251.46 88.9 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-0710KL"
      (at 251.46 88.9 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 251.46 88.9 0.0)
      (hide yes))
    (property "Datasheet" ""
      (at 251.46 88.9 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R5")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 251.46 85.09)
      (xy 251.46 77.47)))
  (global_label "ARM"
    (shape passive)
    (at 251.46 77.47 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 251.46 77.47 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 251.46 92.71)
      (xy 251.46 100.33)))
  (global_label "GND"
    (shape passive)
    (at 251.46 100.33 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 251.46 100.33 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 307.34 88.9 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R6"
      (at 312.42 87.63 0.0))
    (property "Value" "10k"
      (at 312.42 90.17 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 307.34 88.9 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-0710KL"
      (at 307.34 88.9 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 307.34 88.9 0.0)
      (hide yes))
    (property "Datasheet" ""
      (at 307.34 88.9 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R6")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 307.34 85.09)
      (xy 307.34 76.2)))
  (global_label "PCA_OE"
    (shape passive)
    (at 307.34 76.2 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 307.34 76.2 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 307.34 92.71)
      (xy 307.34 100.33)))
  (global_label "+3V3"
    (shape passive)
    (at 307.34 100.33 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 307.34 100.33 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 363.22 88.9 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R7"
      (at 368.3 87.63 0.0))
    (property "Value" "2.2k"
      (at 368.3 90.17 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 363.22 88.9 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-072K2L"
      (at 363.22 88.9 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 363.22 88.9 0.0)
      (hide yes))
    (property "Datasheet" ""
      (at 363.22 88.9 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R7")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 363.22 85.09)
      (xy 363.22 74.93)))
  (global_label "I2C_SDA"
    (shape passive)
    (at 363.22 74.93 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 363.22 74.93 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 363.22 92.71)
      (xy 363.22 100.33)))
  (global_label "+3V3"
    (shape passive)
    (at 363.22 100.33 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 363.22 100.33 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 195.58 121.92 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R8"
      (at 200.66 120.65 0.0))
    (property "Value" "2.2k"
      (at 200.66 123.19 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 195.58 121.92 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-072K2L"
      (at 195.58 121.92 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 195.58 121.92 0.0)
      (hide yes))
    (property "Datasheet" ""
      (at 195.58 121.92 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R8")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 195.58 118.11)
      (xy 195.58 107.95)))
  (global_label "I2C_SCL"
    (shape passive)
    (at 195.58 107.95 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 195.58 107.95 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 195.58 125.73)
      (xy 195.58 133.35)))
  (global_label "+3V3"
    (shape passive)
    (at 195.58 133.35 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 195.58 133.35 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 251.46 121.92 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R9"
      (at 256.54 120.65 0.0))
    (property "Value" "100k"
      (at 256.54 123.19 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 251.46 121.92 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-07100KL"
      (at 251.46 121.92 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 251.46 121.92 0.0)
      (hide yes))
    (property "Datasheet" ""
      (at 251.46 121.92 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R9")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 251.46 118.11)
      (xy 251.46 107.95)))
  (global_label "SPOT1_PWM"
    (shape passive)
    (at 251.46 107.95 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 251.46 107.95 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 251.46 125.73)
      (xy 251.46 133.35)))
  (global_label "GND"
    (shape passive)
    (at 251.46 133.35 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 251.46 133.35 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 307.34 121.92 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R10"
      (at 312.42 120.65 0.0))
    (property "Value" "100k"
      (at 312.42 123.19 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 307.34 121.92 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-07100KL"
      (at 307.34 121.92 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 307.34 121.92 0.0)
      (hide yes))
    (property "Datasheet" ""
      (at 307.34 121.92 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R10")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 307.34 118.11)
      (xy 307.34 107.95)))
  (global_label "SPOT2_PWM"
    (shape passive)
    (at 307.34 107.95 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 307.34 107.95 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 307.34 125.73)
      (xy 307.34 133.35)))
  (global_label "GND"
    (shape passive)
    (at 307.34 133.35 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 307.34 133.35 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 363.22 121.92 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R11"
      (at 368.3 120.65 0.0))
    (property "Value" "100k"
      (at 368.3 123.19 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 363.22 121.92 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-07100KL"
      (at 363.22 121.92 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 363.22 121.92 0.0)
      (hide yes))
    (property "Datasheet" ""
      (at 363.22 121.92 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R11")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 363.22 118.11)
      (xy 363.22 107.95)))
  (global_label "SPOT3_PWM"
    (shape passive)
    (at 363.22 107.95 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 363.22 107.95 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 363.22 125.73)
      (xy 363.22 133.35)))
  (global_label "GND"
    (shape passive)
    (at 363.22 133.35 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 363.22 133.35 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:C")
    (at 195.58 154.94 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C2"
      (at 200.66 153.67 0.0))
    (property "Value" "100n"
      (at 200.66 156.21 0.0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
      (at 195.58 154.94 0.0)
      (hide yes))
    (property "MPN" "GRM188R72A104KA35D"
      (at 195.58 154.94 0.0)
      (hide yes))
    (property "Manufacturer" "Murata"
      (at 195.58 154.94 0.0)
      (hide yes))
    (property "Datasheet" ""
      (at 195.58 154.94 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C2")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 195.58 151.13)
      (xy 195.58 143.51)))
  (global_label "+3V3"
    (shape passive)
    (at 195.58 143.51 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 195.58 143.51 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 195.58 158.75)
      (xy 195.58 166.37)))
  (global_label "GND"
    (shape passive)
    (at 195.58 166.37 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 195.58 166.37 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:C")
    (at 251.46 154.94 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C3"
      (at 256.54 153.67 0.0))
    (property "Value" "22uF 25V X7R"
      (at 256.54 156.21 0.0))
    (property "Footprint" "Capacitor_SMD:C_1210_3225Metric"
      (at 251.46 154.94 0.0)
      (hide yes))
    (property "MPN" "GRM32ER71E226KE15L"
      (at 251.46 154.94 0.0)
      (hide yes))
    (property "Manufacturer" "Murata"
      (at 251.46 154.94 0.0)
      (hide yes))
    (property "Datasheet" "https://www.murata.com/-/media/webrenewal/tool/library/common-pdf/dynamic-model/component-list-d-mlcc-2504.ashx?cvid=20250523010405000000&la=en"
      (at 251.46 154.94 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C3")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 251.46 151.13)
      (xy 251.46 143.51)))
  (global_label "+3V3"
    (shape passive)
    (at 251.46 143.51 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 251.46 143.51 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 251.46 158.75)
      (xy 251.46 166.37)))
  (global_label "GND"
    (shape passive)
    (at 251.46 166.37 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 251.46 166.37 0.0)
      (hide yes)))
  (symbol
    (lib_id "Switch:SW_Push")
    (at 307.34 154.94 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "S1"
      (at 307.34 147.32 0.0))
    (property "Value" "RESET"
      (at 307.34 149.86 0.0))
    (property "Footprint" "Button_Switch_SMD:SW_SPST_TL3305A"
      (at 307.34 154.94 0.0)
      (hide yes))
    (property "MPN" "TL3305AF160QG"
      (at 307.34 154.94 0.0)
      (hide yes))
    (property "Manufacturer" "E-Switch"
      (at 307.34 154.94 0.0)
      (hide yes))
    (property "Datasheet" ""
      (at 307.34 154.94 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "S1")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 302.26 154.94)
      (xy 293.37 154.94)))
  (global_label "MCU_EN"
    (shape passive)
    (at 293.37 154.94 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 293.37 154.94 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 312.42 154.94)
      (xy 320.04 154.94)))
  (global_label "GND"
    (shape passive)
    (at 320.04 154.94 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 320.04 154.94 0.0)
      (hide yes)))
  (symbol
    (lib_id "Switch:SW_Push")
    (at 363.22 154.94 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "S2"
      (at 363.22 147.32 0.0))
    (property "Value" "BOOT"
      (at 363.22 149.86 0.0))
    (property "Footprint" "Button_Switch_SMD:SW_SPST_TL3305A"
      (at 363.22 154.94 0.0)
      (hide yes))
    (property "MPN" "TL3305AF160QG"
      (at 363.22 154.94 0.0)
      (hide yes))
    (property "Manufacturer" "E-Switch"
      (at 363.22 154.94 0.0)
      (hide yes))
    (property "Datasheet" ""
      (at 363.22 154.94 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "S2")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 358.14 154.94)
      (xy 346.71 154.94)))
  (global_label "BOOT_GPIO9"
    (shape passive)
    (at 346.71 154.94 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 346.71 154.94 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 368.3 154.94)
      (xy 375.92 154.94)))
  (global_label "GND"
    (shape passive)
    (at 375.92 154.94 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 375.92 154.94 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x02")
    (at 195.58 187.96 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "J17"
      (at 200.66 186.69 0.0))
    (property "Value" "ARM SWITCH"
      (at 200.66 189.23 0.0))
    (property "Footprint" "ELF:Enclosure_J17"
      (at 195.58 187.96 0.0)
      (hide yes))
    (property "MPN" "B2B-PH-SM4-TB(LF)(SN)"
      (at 195.58 187.96 0.0)
      (hide yes))
    (property "Manufacturer" "JST"
      (at 195.58 187.96 0.0)
      (hide yes))
    (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/ePH.pdf"
      (at 195.58 187.96 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "J17")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 190.5 187.96)
      (xy 182.88 187.96)))
  (global_label "+3V3"
    (shape passive)
    (at 182.88 187.96 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 182.88 187.96 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 190.5 190.5)
      (xy 182.88 190.5)))
  (global_label "ARM"
    (shape passive)
    (at 182.88 190.5 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 182.88 190.5 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x04")
    (at 251.46 187.96 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "J15"
      (at 251.46 175.26 0.0))
    (property "Value" "UART DEBUG"
      (at 251.46 177.8 0.0))
    (property "Footprint" "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
      (at 251.46 187.96 0.0)
      (hide yes))
    (property "MPN" "SM04B-SRSS-TB(LF)(SN)"
      (at 251.46 187.96 0.0)
      (hide yes))
    (property "Manufacturer" "JST"
      (at 251.46 187.96 0.0)
      (hide yes))
    (property "Datasheet" ""
      (at 251.46 187.96 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "J15")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4"))
  (wire
    (pts
      (xy 246.38 185.42)
      (xy 238.76 185.42)))
  (global_label "+3V3"
    (shape passive)
    (at 238.76 185.42 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 238.76 185.42 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 246.38 187.96)
      (xy 238.76 187.96)))
  (global_label "GND"
    (shape passive)
    (at 238.76 187.96 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 238.76 187.96 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 246.38 190.5)
      (xy 236.22 190.5)))
  (global_label "UART_TX"
    (shape passive)
    (at 236.22 190.5 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 236.22 190.5 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 246.38 193.04)
      (xy 236.22 193.04)))
  (global_label "UART_RX"
    (shape passive)
    (at 236.22 193.04 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 236.22 193.04 0.0)
      (hide yes)))
  (symbol
    (lib_id "EL:74HCS08")
    (at 121.92 238.76 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "U5"
      (at 142.24 218.44 0.0))
    (property "Value" "74HCS08PWJ"
      (at 142.24 220.98 0.0))
    (property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
      (at 121.92 238.76 0.0)
      (hide yes))
    (property "MPN" "74HCS08PWJ"
      (at 121.92 238.76 0.0)
      (hide yes))
    (property "Manufacturer" "Nexperia"
      (at 121.92 238.76 0.0)
      (hide yes))
    (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HCS08.pdf"
      (at 121.92 238.76 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "U5")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "4")
    (pin "5")
    (pin "7")
    (pin "9")
    (pin "10")
    (pin "12")
    (pin "13")
    (pin "3")
    (pin "6")
    (pin "8")
    (pin "11")
    (pin "14"))
  (wire
    (pts
      (xy 104.14 228.6)
      (xy 93.98 228.6)))
  (global_label "SPOT1_PWM"
    (shape passive)
    (at 93.98 228.6 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 93.98 228.6 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 104.14 231.14)
      (xy 88.9 231.14)))
  (global_label "LIGHT_ENABLE_SAFE"
    (shape passive)
    (at 88.9 231.14 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 88.9 231.14 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 104.14 233.68)
      (xy 93.98 233.68)))
  (global_label "SPOT2_PWM"
    (shape passive)
    (at 93.98 233.68 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 93.98 233.68 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 104.14 236.22)
      (xy 88.9 236.22)))
  (global_label "LIGHT_ENABLE_SAFE"
    (shape passive)
    (at 88.9 236.22 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 88.9 236.22 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 104.14 238.76)
      (xy 96.52 238.76)))
  (global_label "GND"
    (shape passive)
    (at 96.52 238.76 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 96.52 238.76 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 104.14 241.3)
      (xy 93.98 241.3)))
  (global_label "SPOT3_PWM"
    (shape passive)
    (at 93.98 241.3 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 93.98 241.3 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 104.14 243.84)
      (xy 88.9 243.84)))
  (global_label "LIGHT_ENABLE_SAFE"
    (shape passive)
    (at 88.9 243.84 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 88.9 243.84 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 104.14 246.38)
      (xy 91.44 246.38)))
  (global_label "LIGHT_ENABLE"
    (shape passive)
    (at 91.44 246.38 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 91.44 246.38 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 104.14 248.92)
      (xy 96.52 248.92)))
  (global_label "ARM"
    (shape passive)
    (at 96.52 248.92 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 96.52 248.92 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 139.7 228.6)
      (xy 151.13 228.6)))
  (global_label "SPOT1_CTRL"
    (shape passive)
    (at 151.13 228.6 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 151.13 228.6 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 139.7 231.14)
      (xy 151.13 231.14)))
  (global_label "SPOT2_CTRL"
    (shape passive)
    (at 151.13 231.14 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 151.13 231.14 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 139.7 233.68)
      (xy 151.13 233.68)))
  (global_label "SPOT3_CTRL"
    (shape passive)
    (at 151.13 233.68 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 151.13 233.68 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 139.7 236.22)
      (xy 156.21 236.22)))
  (global_label "LIGHT_REQUEST_ARMED"
    (shape passive)
    (at 156.21 236.22 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 156.21 236.22 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 139.7 238.76)
      (xy 147.32 238.76)))
  (global_label "+3V3"
    (shape passive)
    (at 147.32 238.76 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 147.32 238.76 0.0)
      (hide yes)))
  (symbol
    (lib_id "74xGxx:74LVC1G04")
    (at 241.3 226.06 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "U6"
      (at 257.81 208.28 0.0))
    (property "Value" "SN74LVC1G04DBVR"
      (at 257.81 210.82 0.0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
      (at 241.3 226.06 0.0)
      (hide yes))
    (property "MPN" "SN74LVC1G04DBVR"
      (at 241.3 226.06 0.0)
      (hide yes))
    (property "Manufacturer" "Texas Instruments"
      (at 241.3 226.06 0.0)
      (hide yes))
    (property "Datasheet" ""
      (at 241.3 226.06 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "U6")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5"))
  (no_connect
    (at 233.68 223.52))
  (wire
    (pts
      (xy 226.06 226.06)
      (xy 210.82 226.06)))
  (global_label "LIGHT_ENABLE_SAFE"
    (shape passive)
    (at 210.82 226.06 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 210.82 226.06 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 236.22 236.22)
      (xy 236.22 243.84)))
  (global_label "GND"
    (shape passive)
    (at 236.22 243.84 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 236.22 243.84 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 254.0 226.06)
      (xy 262.89 226.06)))
  (global_label "PCA_OE"
    (shape passive)
    (at 262.89 226.06 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 262.89 226.06 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 236.22 215.9)
      (xy 236.22 208.28)))
  (global_label "+3V3"
    (shape passive)
    (at 236.22 208.28 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 236.22 208.28 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:C")
    (at 45.72 236.22 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C4"
      (at 50.8 234.95 0.0))
    (property "Value" "100n"
      (at 50.8 237.49 0.0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
      (at 45.72 236.22 0.0)
      (hide yes))
    (property "MPN" "GRM188R72A104KA35D"
      (at 45.72 236.22 0.0)
      (hide yes))
    (property "Manufacturer" "Murata"
      (at 45.72 236.22 0.0)
      (hide yes))
    (property "Datasheet" ""
      (at 45.72 236.22 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C4")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 45.72 232.41)
      (xy 45.72 224.79)))
  (global_label "+3V3"
    (shape passive)
    (at 45.72 224.79 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 45.72 224.79 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 45.72 240.03)
      (xy 45.72 247.65)))
  (global_label "GND"
    (shape passive)
    (at 45.72 247.65 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 45.72 247.65 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:C")
    (at 320.04 226.06 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C5"
      (at 325.12 224.79 0.0))
    (property "Value" "100n"
      (at 325.12 227.33 0.0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
      (at 320.04 226.06 0.0)
      (hide yes))
    (property "MPN" "GRM188R72A104KA35D"
      (at 320.04 226.06 0.0)
      (hide yes))
    (property "Manufacturer" "Murata"
      (at 320.04 226.06 0.0)
      (hide yes))
    (property "Datasheet" ""
      (at 320.04 226.06 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C5")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 320.04 222.25)
      (xy 320.04 214.63)))
  (global_label "+3V3"
    (shape passive)
    (at 320.04 214.63 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 320.04 214.63 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 320.04 229.87)
      (xy 320.04 237.49)))
  (global_label "GND"
    (shape passive)
    (at 320.04 237.49 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 320.04 237.49 0.0)
      (hide yes)))
  (text "CONTROLLER"
    (at 20.32 15.24 0))
  (text "GPIO 0 AND physical ARM -> LIGHT_REQUEST_ARMED\nU19 on power_sequence adds READY qualification -> LIGHT_ENABLE_SAFE.\nMCU_EN reset remains here; U18 reaches it through current-limiting R42."
    (at 20.32 180.34 0))
  (embedded_fonts no))