(kicad_sch
  (version 20250114)
  (generator "engineered-lighting")
  (generator_version "0.2")
  (paper "A3")
  (title_block
    (title "Power 1")
    (date "2026-09-06")
    (rev "A draft")
    (company "Engineered Lighting")
    (comment 1 "ENGINEERING DRAFT - see release status before fabrication"))
  (lib_symbols
    (symbol "EL:TPS26630RGER"
      (pin_names
        (offset 0.8))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (property "Reference" "U"
        (at 0 29.21 0))
      (property "Value" "TPS26630RGER"
        (at 0 -29.21 0))
      (symbol "TPS26630RGER_0_1"
        (rectangle
          (start -12.7 26.67)
          (end 12.7 -26.67)
          (fill
            (type background))))
      (symbol "TPS26630RGER_1_1"
        (pin power_in line
          (at -17.78 24.130000000000003 0)
          (length 5.08)
          (name "IN")
          (number "1"))
        (pin power_in line
          (at -17.78 21.590000000000003 0)
          (length 5.08)
          (name "IN")
          (number "2"))
        (pin passive line
          (at -17.78 19.050000000000004 0)
          (length 5.08)
          (name "BGATE")
          (number "3"))
        (pin passive line
          (at -17.78 16.51 0)
          (length 5.08)
          (name "DRV")
          (number "4"))
        (pin power_in line
          (at -17.78 13.970000000000002 0)
          (length 5.08)
          (name "IN_SYS")
          (number "5"))
        (pin input line
          (at -17.78 11.430000000000003 0)
          (length 5.08)
          (name "UVLO")
          (number "6"))
        (pin input line
          (at -17.78 8.890000000000002 0)
          (length 5.08)
          (name "OVP")
          (number "7"))
        (pin power_in line
          (at -17.78 6.350000000000001 0)
          (length 5.08)
          (name "GND")
          (number "8"))
        (pin passive line
          (at -17.78 3.8100000000000023 0)
          (length 5.08)
          (name "dVdt")
          (number "9"))
        (pin passive line
          (at -17.78 1.2700000000000031 0)
          (length 5.08)
          (name "ILIM")
          (number "10"))
        (pin input line
          (at -17.78 -1.269999999999996 0)
          (length 5.08)
          (name "MODE")
          (number "11"))
        (pin passive line
          (at -17.78 -3.8099999999999987 0)
          (length 5.08)
          (name "SHDN_internal_pullup")
          (number "12"))
        (pin passive line
          (at -17.78 -6.349999999999998 0)
          (length 5.08)
          (name "PGTH")
          (number "15"))
        (pin no_connect line
          (at -17.78 -8.89 0)
          (length 5.08)
          (name "DNC")
          (number "19"))
        (pin no_connect line
          (at -17.78 -11.43 0)
          (length 5.08)
          (name "DNC")
          (number "20"))
        (pin no_connect line
          (at -17.78 -13.969999999999999 0)
          (length 5.08)
          (name "DNC")
          (number "21"))
        (pin no_connect line
          (at -17.78 -16.509999999999998 0)
          (length 5.08)
          (name "DNC")
          (number "22"))
        (pin no_connect line
          (at -17.78 -19.049999999999997 0)
          (length 5.08)
          (name "DNC")
          (number "23"))
        (pin no_connect line
          (at -17.78 -21.589999999999996 0)
          (length 5.08)
          (name "DNC")
          (number "24"))
        (pin power_in line
          (at -17.78 -24.129999999999995 0)
          (length 5.08)
          (name "GND_EP")
          (number "25"))
        (pin passive line
          (at 17.78 24.130000000000003 180)
          (length 5.08)
          (name "IMON")
          (number "13"))
        (pin open_collector line
          (at 17.78 21.590000000000003 180)
          (length 5.08)
          (name "FLT")
          (number "14"))
        (pin open_collector line
          (at 17.78 19.050000000000004 180)
          (length 5.08)
          (name "PGOOD")
          (number "16"))
        (pin power_out line
          (at 17.78 16.51 180)
          (length 5.08)
          (name "OUT")
          (number "17"))
        (pin passive line
          (at 17.78 13.970000000000002 180)
          (length 5.08)
          (name "OUT")
          (number "18"))))
    (symbol "EL:CSD19537Q3"
      (pin_names
        (offset 0.8))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (property "Reference" "U"
        (at 0 8.89 0))
      (property "Value" "CSD19537Q3"
        (at 0 -8.89 0))
      (symbol "CSD19537Q3_0_1"
        (rectangle
          (start -12.7 6.35)
          (end 12.7 -6.35)
          (fill
            (type background))))
      (symbol "CSD19537Q3_1_1"
        (pin passive line
          (at -17.78 3.8099999999999996 0)
          (length 5.08)
          (name "S")
          (number "1"))
        (pin passive line
          (at -17.78 1.2699999999999996 0)
          (length 5.08)
          (name "S")
          (number "2"))
        (pin passive line
          (at -17.78 -1.2700000000000005 0)
          (length 5.08)
          (name "S")
          (number "3"))
        (pin input line
          (at -17.78 -3.8100000000000005 0)
          (length 5.08)
          (name "G")
          (number "4"))
        (pin passive line
          (at 17.78 3.8099999999999996 180)
          (length 5.08)
          (name "D")
          (number "5"))))
    (symbol "Transistor_FET:2N7002"
      (pin_names
        (offset 0)
        (hide yes))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (symbol "2N7002_0_1"
        (polyline
          (pts
            (xy 0.254 1.905)
            (xy 0.254 -1.905))
          (fill
            (type none)))
        (polyline
          (pts
            (xy 0.254 0)
            (xy -2.54 0))
          (fill
            (type none)))
        (polyline
          (pts
            (xy 0.762 2.286)
            (xy 0.762 1.27))
          (fill
            (type none)))
        (polyline
          (pts
            (xy 0.762 0.508)
            (xy 0.762 -0.508))
          (fill
            (type none)))
        (polyline
          (pts
            (xy 0.762 -1.27)
            (xy 0.762 -2.286))
          (fill
            (type none)))
        (polyline
          (pts
            (xy 0.762 -1.778)
            (xy 3.302 -1.778)
            (xy 3.302 1.778)
            (xy 0.762 1.778))
          (fill
            (type none)))
        (polyline
          (pts
            (xy 1.016 0)
            (xy 2.032 0.381)
            (xy 2.032 -0.381)
            (xy 1.016 0))
          (fill
            (type outline)))
        (circle
          (center 1.651 0)
          (radius 2.794)
          (fill
            (type none)))
        (polyline
          (pts
            (xy 2.54 2.54)
            (xy 2.54 1.778))
          (fill
            (type none)))
        (circle
          (center 2.54 1.778)
          (radius 0.254)
          (fill
            (type outline)))
        (circle
          (center 2.54 -1.778)
          (radius 0.254)
          (fill
            (type outline)))
        (polyline
          (pts
            (xy 2.54 -2.54)
            (xy 2.54 0)
            (xy 0.762 0))
          (fill
            (type none)))
        (polyline
          (pts
            (xy 2.921 0.381)
            (xy 3.683 0.381))
          (fill
            (type none)))
        (polyline
          (pts
            (xy 3.302 0.381)
            (xy 2.921 -0.254)
            (xy 3.683 -0.254)
            (xy 3.302 0.381))
          (fill
            (type none))))
      (symbol "2N7002_1_1"
        (pin input line
          (at -5.08 0 0)
          (length 2.54)
          (name "G")
          (number "1"))
        (pin passive line
          (at 2.54 -5.08 90)
          (length 2.54)
          (name "S")
          (number "2"))
        (pin passive line
          (at 2.54 5.08 270)
          (length 2.54)
          (name "D")
          (number "3")))
      (embedded_fonts no)
      (property "Reference" "Q"
        (at 5.08 1.905 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "2N7002"
        (at 5.08 0 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" "Package_TO_SOT_SMD:SOT-23"
        (at 5.08 -1.905 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" "https://www.onsemi.com/pub/Collateral/NDS7002A-D.PDF"
        (at 5.08 -3.81 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "0.115A Id, 60V Vds, N-Channel MOSFET, SOT-23"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "N-Channel Switching MOSFET"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "SOT?23*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes)))
    (symbol "Device:D_TVS"
      (pin_numbers
        (hide yes))
      (pin_names
        (offset 1.016)
        (hide yes))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "D"
        (at 0 2.54 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "D_TVS"
        (at 0 -2.54 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Bidirectional transient-voltage-suppression diode"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "diode TVS thyrector"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "TO-???* *_Diode_* *SingleDiode* D_*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "D_TVS_0_1"
        (polyline
          (pts
            (xy -2.54 1.27)
            (xy -2.54 -1.27)
            (xy 2.54 1.27)
            (xy 2.54 -1.27)
            (xy -2.54 1.27))
          (fill
            (type none)))
        (polyline
          (pts
            (xy 0.508 1.27)
            (xy 0 1.27)
            (xy 0 -1.27)
            (xy -0.508 -1.27))
          (fill
            (type none)))
        (polyline
          (pts
            (xy 1.27 0)
            (xy -1.27 0))
          (fill
            (type none))))
      (symbol "D_TVS_1_1"
        (pin passive line
          (at -3.81 0 0)
          (length 2.54)
          (name "A1")
          (number "1"))
        (pin passive line
          (at 3.81 0 180)
          (length 2.54)
          (name "A2")
          (number "2")))
      (embedded_fonts no))
    (symbol "Device:Fuse"
      (pin_numbers
        (hide yes))
      (pin_names
        (offset 0))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "F"
        (at 2.032 0 90)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "Fuse"
        (at -1.905 0 90)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" ""
        (at -1.778 0 90)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Fuse"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "fuse"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "*Fuse*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "Fuse_0_1"
        (rectangle
          (start -0.762 -2.54)
          (end 0.762 2.54)
          (fill
            (type none)))
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0 -2.54))
          (fill
            (type none))))
      (symbol "Fuse_1_1"
        (pin passive line
          (at 0 3.81 270)
          (length 1.27)
          (name "")
          (number "1"))
        (pin passive line
          (at 0 -3.81 90)
          (length 1.27)
          (name "")
          (number "2")))
      (embedded_fonts no))
    (symbol "Device:R"
      (pin_numbers
        (hide yes))
      (pin_names
        (offset 0))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "R"
        (at 2.032 0 90)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "R"
        (at 0 0 90)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" ""
        (at -1.778 0 90)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Resistor"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "R res resistor"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "R_*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "R_0_1"
        (rectangle
          (start -1.016 -2.54)
          (end 1.016 2.54)
          (fill
            (type none))))
      (symbol "R_1_1"
        (pin passive line
          (at 0 3.81 270)
          (length 1.27)
          (name "")
          (number "1"))
        (pin passive line
          (at 0 -3.81 90)
          (length 1.27)
          (name "")
          (number "2")))
      (embedded_fonts no))
    (symbol "Device:C"
      (pin_numbers
        (hide yes))
      (pin_names
        (offset 0.254))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "C"
        (at 0.635 2.54 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "C"
        (at 0.635 -2.54 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" ""
        (at 0.9652 -3.81 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Unpolarized capacitor"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "cap capacitor"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "C_*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762))
          (fill
            (type none)))
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762))
          (fill
            (type none))))
      (symbol "C_1_1"
        (pin passive line
          (at 0 3.81 270)
          (length 2.794)
          (name "")
          (number "1"))
        (pin passive line
          (at 0 -3.81 90)
          (length 2.794)
          (name "")
          (number "2")))
      (embedded_fonts no))
    (symbol "Device:C_Polarized"
      (pin_numbers
        (hide yes))
      (pin_names
        (offset 0.254))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "C"
        (at 0.635 2.54 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "C_Polarized"
        (at 0.635 -2.54 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" ""
        (at 0.9652 -3.81 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Polarized capacitor"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "cap capacitor"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "CP_*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "C_Polarized_0_1"
        (rectangle
          (start -2.286 0.508)
          (end 2.286 1.016)
          (fill
            (type none)))
        (polyline
          (pts
            (xy -1.778 2.286)
            (xy -0.762 2.286))
          (fill
            (type none)))
        (polyline
          (pts
            (xy -1.27 2.794)
            (xy -1.27 1.778))
          (fill
            (type none)))
        (rectangle
          (start 2.286 -0.508)
          (end -2.286 -1.016)
          (fill
            (type outline))))
      (symbol "C_Polarized_1_1"
        (pin passive line
          (at 0 3.81 270)
          (length 2.794)
          (name "")
          (number "1"))
        (pin passive line
          (at 0 -3.81 90)
          (length 2.794)
          (name "")
          (number "2")))
      (embedded_fonts no)))
  (symbol
    (lib_id "EL:TPS26630RGER")
    (at 254.0 82.55 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "U12"
      (at 274.32 48.26 0.0))
    (property "Value" "24V input eFuse / 4.5A nominal"
      (at 274.32 50.8 0.0))
    (property "Footprint" "Package_DFN_QFN:Texas_RGE0024H_VQFN-24-1EP_4x4mm_P0.5mm_EP2.7x2.7mm_ThermalVias"
      (at 254.0 82.55 0.0)
      (hide yes))
    (property "MPN" "TPS26630RGER"
      (at 254.0 82.55 0.0)
      (hide yes))
    (property "Manufacturer" "Texas Instruments"
      (at 254.0 82.55 0.0)
      (hide yes))
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2663.pdf"
      (at 254.0 82.55 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "U12")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "15")
    (pin "19")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "13")
    (pin "14")
    (pin "16")
    (pin "17")
    (pin "18"))
  (wire
    (pts
      (xy 236.22 60.96)
      (xy 226.06 60.96)))
  (global_label "VIN24_RPP"
    (shape passive)
    (at 226.06 60.96 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 226.06 60.96 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 236.22 63.5)
      (xy 224.79 63.5)))
  (global_label "EFUSE_BGATE"
    (shape passive)
    (at 224.79 63.5 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 224.79 63.5 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 236.22 66.04)
      (xy 226.06 66.04)))
  (global_label "EFUSE_DRV"
    (shape passive)
    (at 226.06 66.04 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 226.06 66.04 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 236.22 68.58)
      (xy 224.79 68.58)))
  (global_label "VIN24_FUSED"
    (shape passive)
    (at 224.79 68.58 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 224.79 68.58 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 236.22 71.12)
      (xy 224.79 71.12)))
  (global_label "EFUSE_UVLO"
    (shape passive)
    (at 224.79 71.12 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 224.79 71.12 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 236.22 73.66)
      (xy 226.06 73.66)))
  (global_label "EFUSE_OVP"
    (shape passive)
    (at 226.06 73.66 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 226.06 73.66 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 236.22 76.2)
      (xy 228.6 76.2)))
  (global_label "GND"
    (shape passive)
    (at 228.6 76.2 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 228.6 76.2 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 236.22 78.74)
      (xy 224.79 78.74)))
  (global_label "EFUSE_DVDT"
    (shape passive)
    (at 224.79 78.74 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 224.79 78.74 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 236.22 81.28)
      (xy 224.79 81.28)))
  (global_label "EFUSE_ILIM"
    (shape passive)
    (at 224.79 81.28 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 224.79 81.28 0.0)
      (hide yes)))
  (no_connect
    (at 236.22 83.82))
  (wire
    (pts
      (xy 236.22 86.36)
      (xy 223.52 86.36)))
  (global_label "EFUSE_RESET_N"
    (shape passive)
    (at 223.52 86.36 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 223.52 86.36 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 236.22 88.9)
      (xy 224.79 88.9)))
  (global_label "EFUSE_PGTH"
    (shape passive)
    (at 224.79 88.9 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 224.79 88.9 0.0)
      (hide yes)))
  (no_connect
    (at 236.22 91.44))
  (no_connect
    (at 236.22 93.98))
  (no_connect
    (at 236.22 96.52))
  (no_connect
    (at 236.22 99.06))
  (no_connect
    (at 236.22 101.6))
  (no_connect
    (at 236.22 104.14))
  (wire
    (pts
      (xy 236.22 106.68)
      (xy 228.6 106.68)))
  (global_label "GND"
    (shape passive)
    (at 228.6 106.68 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 228.6 106.68 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 271.78 58.42)
      (xy 283.21 58.42)))
  (global_label "EFUSE_IMON"
    (shape passive)
    (at 283.21 58.42 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 283.21 58.42 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 271.78 60.96)
      (xy 283.21 60.96)))
  (global_label "EFUSE_FLT_N"
    (shape passive)
    (at 283.21 60.96 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 283.21 60.96 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 271.78 63.5)
      (xy 283.21 63.5)))
  (global_label "EFUSE_PGOOD"
    (shape passive)
    (at 283.21 63.5 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 283.21 63.5 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 271.78 68.58)
      (xy 281.94 68.58)))
  (global_label "V24_BUS"
    (shape passive)
    (at 281.94 68.58 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 281.94 68.58 0.0)
      (hide yes)))
  (symbol
    (lib_id "EL:CSD19537Q3")
    (at 106.68 69.85 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "Q500"
      (at 106.68 55.88 0.0))
    (property "Value" "100V reverse blocking MOSFET"
      (at 106.68 58.42 0.0))
    (property "Footprint" "Package_SON:VSON-8_3.3x3.3mm_P0.65mm_NexFET"
      (at 106.68 69.85 0.0)
      (hide yes))
    (property "MPN" "CSD19537Q3"
      (at 106.68 69.85 0.0)
      (hide yes))
    (property "Manufacturer" "Texas Instruments"
      (at 106.68 69.85 0.0)
      (hide yes))
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/csd19537q3.pdf"
      (at 106.68 69.85 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "Q500")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5"))
  (wire
    (pts
      (xy 88.9 68.58)
      (xy 77.47 68.58)))
  (global_label "VIN24_FUSED"
    (shape passive)
    (at 77.47 68.58 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 77.47 68.58 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 88.9 71.12)
      (xy 77.47 71.12)))
  (global_label "VIN24_FUSED"
    (shape passive)
    (at 77.47 71.12 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 77.47 71.12 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 88.9 73.66)
      (xy 77.47 73.66)))
  (global_label "EFUSE_BGATE"
    (shape passive)
    (at 77.47 73.66 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 77.47 73.66 0.0)
      (hide yes)))
  (symbol
    (lib_id "Transistor_FET:2N7002")
    (at 116.84 119.38 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "Q501"
      (at 116.84 106.68 0.0))
    (property "Value" "fast reverse gate pull-down"
      (at 116.84 109.22 0.0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23"
      (at 116.84 119.38 0.0)
      (hide yes))
    (property "MPN" "2N7002BK,215"
      (at 116.84 119.38 0.0)
      (hide yes))
    (property "Manufacturer" "Nexperia"
      (at 116.84 119.38 0.0)
      (hide yes))
    (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/2N7002BK.pdf"
      (at 116.84 119.38 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "Q501")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3"))
  (wire
    (pts
      (xy 111.76 119.38)
      (xy 101.6 119.38)))
  (global_label "EFUSE_DRV"
    (shape passive)
    (at 101.6 119.38 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 101.6 119.38 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 119.38 124.46)
      (xy 119.38 135.89)))
  (global_label "VIN24_FUSED"
    (shape passive)
    (at 119.38 135.89 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 119.38 135.89 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 119.38 114.3)
      (xy 119.38 102.87)))
  (global_label "EFUSE_BGATE"
    (shape passive)
    (at 119.38 102.87 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 119.38 102.87 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:D_TVS")
    (at 30.48 152.4 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "D500"
      (at 30.48 144.78 0.0))
    (property "Value" "SMBJ33CA 33V bidirectional TVS"
      (at 30.48 147.32 0.0))
    (property "Footprint" "Diode_SMD:D_SMB"
      (at 30.48 152.4 0.0)
      (hide yes))
    (property "MPN" "SMBJ33CA"
      (at 30.48 152.4 0.0)
      (hide yes))
    (property "Manufacturer" "Littelfuse"
      (at 30.48 152.4 0.0)
      (hide yes))
    (property "Datasheet" "https://www.littelfuse.com/~/media/electronics/datasheets/tvs_diodes/littelfuse_tvs_diode_smbj_datasheet.pdf.pdf"
      (at 30.48 152.4 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "D500")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 26.67 152.4)
      (xy 15.24 152.4)))
  (global_label "VIN24_FUSED"
    (shape passive)
    (at 15.24 152.4 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 15.24 152.4 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 34.29 152.4)
      (xy 41.91 152.4)))
  (global_label "GND"
    (shape passive)
    (at 41.91 152.4 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 41.91 152.4 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:Fuse")
    (at 35.56 66.04 90)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "F1"
      (at 35.56 57.658 90.0))
    (property "Value" "6.3A backup fuse"
      (at 35.56 60.198 90.0))
    (property "Footprint" "ELF:Enclosure_F1"
      (at 35.56 66.04 0.0)
      (hide yes))
    (property "MPN" "045106.3MRL"
      (at 35.56 66.04 0.0)
      (hide yes))
    (property "Manufacturer" "Littelfuse"
      (at 35.56 66.04 0.0)
      (hide yes))
    (property "Datasheet" "https://www.littelfuse.com/assetdocs/fuse-451-and-453-datasheet?assetguid=533cd5cc-956c-4243-867f-6ab5a62f6ba1"
      (at 35.56 66.04 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "F1")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 31.75 66.04)
      (xy 21.59 66.04)))
  (global_label "VIN24_RAW"
    (shape passive)
    (at 21.59 66.04 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 21.59 66.04 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:Fuse")
    (at 35.56 229.87 90)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "F2"
      (at 35.56 221.488 90.0))
    (property "Value" "1A motor branch fuse"
      (at 35.56 224.028 90.0))
    (property "Footprint" "Fuse:Fuse_Littelfuse-NANO2-451_453"
      (at 35.56 229.87 0.0)
      (hide yes))
    (property "MPN" "0451001.MRL"
      (at 35.56 229.87 0.0)
      (hide yes))
    (property "Manufacturer" "Littelfuse"
      (at 35.56 229.87 0.0)
      (hide yes))
    (property "Datasheet" "https://www.littelfuse.com/assetdocs/fuse-451-and-453-datasheet?assetguid=533cd5cc-956c-4243-867f-6ab5a62f6ba1"
      (at 35.56 229.87 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "F2")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 31.75 229.87)
      (xy 21.59 229.87)))
  (global_label "V24_BUS"
    (shape passive)
    (at 21.59 229.87 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 21.59 229.87 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 39.37 229.87)
      (xy 50.8 229.87)))
  (global_label "V24_MOTOR1"
    (shape passive)
    (at 50.8 229.87 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 50.8 229.87 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:Fuse")
    (at 106.68 229.87 90)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "F3"
      (at 106.68 221.488 90.0))
    (property "Value" "1A motor branch fuse"
      (at 106.68 224.028 90.0))
    (property "Footprint" "Fuse:Fuse_Littelfuse-NANO2-451_453"
      (at 106.68 229.87 0.0)
      (hide yes))
    (property "MPN" "0451001.MRL"
      (at 106.68 229.87 0.0)
      (hide yes))
    (property "Manufacturer" "Littelfuse"
      (at 106.68 229.87 0.0)
      (hide yes))
    (property "Datasheet" "https://www.littelfuse.com/assetdocs/fuse-451-and-453-datasheet?assetguid=533cd5cc-956c-4243-867f-6ab5a62f6ba1"
      (at 106.68 229.87 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "F3")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 102.87 229.87)
      (xy 92.71 229.87)))
  (global_label "V24_BUS"
    (shape passive)
    (at 92.71 229.87 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 92.71 229.87 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 110.49 229.87)
      (xy 121.92 229.87)))
  (global_label "V24_MOTOR2"
    (shape passive)
    (at 121.92 229.87 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 121.92 229.87 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:Fuse")
    (at 177.8 229.87 90)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "F4"
      (at 177.8 221.488 90.0))
    (property "Value" "0.75A ambient zone fuse"
      (at 177.8 224.028 90.0))
    (property "Footprint" "Fuse:Fuse_Littelfuse-NANO2-451_453"
      (at 177.8 229.87 0.0)
      (hide yes))
    (property "MPN" "0451.750MRL"
      (at 177.8 229.87 0.0)
      (hide yes))
    (property "Manufacturer" "Littelfuse"
      (at 177.8 229.87 0.0)
      (hide yes))
    (property "Datasheet" "https://www.littelfuse.com/assetdocs/fuse-451-and-453-datasheet?assetguid=533cd5cc-956c-4243-867f-6ab5a62f6ba1"
      (at 177.8 229.87 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "F4")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 173.99 229.87)
      (xy 163.83 229.87)))
  (global_label "V24_BUS"
    (shape passive)
    (at 163.83 229.87 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 163.83 229.87 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 181.61 229.87)
      (xy 191.77 229.87)))
  (global_label "ZONE1_24V"
    (shape passive)
    (at 191.77 229.87 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 191.77 229.87 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:Fuse")
    (at 248.92 229.87 90)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "F5"
      (at 248.92 221.488 90.0))
    (property "Value" "0.75A ambient zone fuse"
      (at 248.92 224.028 90.0))
    (property "Footprint" "Fuse:Fuse_Littelfuse-NANO2-451_453"
      (at 248.92 229.87 0.0)
      (hide yes))
    (property "MPN" "0451.750MRL"
      (at 248.92 229.87 0.0)
      (hide yes))
    (property "Manufacturer" "Littelfuse"
      (at 248.92 229.87 0.0)
      (hide yes))
    (property "Datasheet" "https://www.littelfuse.com/assetdocs/fuse-451-and-453-datasheet?assetguid=533cd5cc-956c-4243-867f-6ab5a62f6ba1"
      (at 248.92 229.87 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "F5")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 245.11 229.87)
      (xy 234.95 229.87)))
  (global_label "V24_BUS"
    (shape passive)
    (at 234.95 229.87 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 234.95 229.87 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 252.73 229.87)
      (xy 262.89 229.87)))
  (global_label "ZONE2_24V"
    (shape passive)
    (at 262.89 229.87 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 262.89 229.87 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:Fuse")
    (at 320.04 229.87 90)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "F6"
      (at 320.04 221.488 90.0))
    (property "Value" "0.75A ambient zone fuse"
      (at 320.04 224.028 90.0))
    (property "Footprint" "Fuse:Fuse_Littelfuse-NANO2-451_453"
      (at 320.04 229.87 0.0)
      (hide yes))
    (property "MPN" "0451.750MRL"
      (at 320.04 229.87 0.0)
      (hide yes))
    (property "Manufacturer" "Littelfuse"
      (at 320.04 229.87 0.0)
      (hide yes))
    (property "Datasheet" "https://www.littelfuse.com/assetdocs/fuse-451-and-453-datasheet?assetguid=533cd5cc-956c-4243-867f-6ab5a62f6ba1"
      (at 320.04 229.87 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "F6")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 316.23 229.87)
      (xy 306.07 229.87)))
  (global_label "V24_BUS"
    (shape passive)
    (at 306.07 229.87 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 306.07 229.87 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 323.85 229.87)
      (xy 334.01 229.87)))
  (global_label "ZONE3_24V"
    (shape passive)
    (at 334.01 229.87 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 334.01 229.87 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:Fuse")
    (at 35.56 248.92 90)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "F7"
      (at 35.56 240.538 90.0))
    (property "Value" "0.75A ambient zone fuse"
      (at 35.56 243.078 90.0))
    (property "Footprint" "Fuse:Fuse_Littelfuse-NANO2-451_453"
      (at 35.56 248.92 0.0)
      (hide yes))
    (property "MPN" "0451.750MRL"
      (at 35.56 248.92 0.0)
      (hide yes))
    (property "Manufacturer" "Littelfuse"
      (at 35.56 248.92 0.0)
      (hide yes))
    (property "Datasheet" "https://www.littelfuse.com/assetdocs/fuse-451-and-453-datasheet?assetguid=533cd5cc-956c-4243-867f-6ab5a62f6ba1"
      (at 35.56 248.92 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "F7")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 31.75 248.92)
      (xy 21.59 248.92)))
  (global_label "V24_BUS"
    (shape passive)
    (at 21.59 248.92 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 21.59 248.92 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 39.37 248.92)
      (xy 49.53 248.92)))
  (global_label "ZONE4_24V"
    (shape passive)
    (at 49.53 248.92 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 49.53 248.92 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:Fuse")
    (at 106.68 248.92 90)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "F8"
      (at 106.68 240.538 90.0))
    (property "Value" "0.75A ambient zone fuse"
      (at 106.68 243.078 90.0))
    (property "Footprint" "Fuse:Fuse_Littelfuse-NANO2-451_453"
      (at 106.68 248.92 0.0)
      (hide yes))
    (property "MPN" "0451.750MRL"
      (at 106.68 248.92 0.0)
      (hide yes))
    (property "Manufacturer" "Littelfuse"
      (at 106.68 248.92 0.0)
      (hide yes))
    (property "Datasheet" "https://www.littelfuse.com/assetdocs/fuse-451-and-453-datasheet?assetguid=533cd5cc-956c-4243-867f-6ab5a62f6ba1"
      (at 106.68 248.92 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "F8")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 102.87 248.92)
      (xy 92.71 248.92)))
  (global_label "V24_BUS"
    (shape passive)
    (at 92.71 248.92 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 92.71 248.92 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 110.49 248.92)
      (xy 120.65 248.92)))
  (global_label "ZONE5_24V"
    (shape passive)
    (at 120.65 248.92 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 120.65 248.92 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:Fuse")
    (at 177.8 248.92 90)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "F9"
      (at 177.8 240.538 90.0))
    (property "Value" "0.75A ambient zone fuse"
      (at 177.8 243.078 90.0))
    (property "Footprint" "Fuse:Fuse_Littelfuse-NANO2-451_453"
      (at 177.8 248.92 0.0)
      (hide yes))
    (property "MPN" "0451.750MRL"
      (at 177.8 248.92 0.0)
      (hide yes))
    (property "Manufacturer" "Littelfuse"
      (at 177.8 248.92 0.0)
      (hide yes))
    (property "Datasheet" "https://www.littelfuse.com/assetdocs/fuse-451-and-453-datasheet?assetguid=533cd5cc-956c-4243-867f-6ab5a62f6ba1"
      (at 177.8 248.92 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "F9")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 173.99 248.92)
      (xy 163.83 248.92)))
  (global_label "V24_BUS"
    (shape passive)
    (at 163.83 248.92 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 163.83 248.92 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 181.61 248.92)
      (xy 191.77 248.92)))
  (global_label "ZONE6_24V"
    (shape passive)
    (at 191.77 248.92 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 191.77 248.92 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:Fuse")
    (at 248.92 248.92 90)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "F10"
      (at 248.92 240.538 90.0))
    (property "Value" "0.75A ambient zone fuse"
      (at 248.92 243.078 90.0))
    (property "Footprint" "Fuse:Fuse_Littelfuse-NANO2-451_453"
      (at 248.92 248.92 0.0)
      (hide yes))
    (property "MPN" "0451.750MRL"
      (at 248.92 248.92 0.0)
      (hide yes))
    (property "Manufacturer" "Littelfuse"
      (at 248.92 248.92 0.0)
      (hide yes))
    (property "Datasheet" "https://www.littelfuse.com/assetdocs/fuse-451-and-453-datasheet?assetguid=533cd5cc-956c-4243-867f-6ab5a62f6ba1"
      (at 248.92 248.92 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "F10")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 245.11 248.92)
      (xy 234.95 248.92)))
  (global_label "V24_BUS"
    (shape passive)
    (at 234.95 248.92 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 234.95 248.92 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 252.73 248.92)
      (xy 262.89 248.92)))
  (global_label "ZONE7_24V"
    (shape passive)
    (at 262.89 248.92 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 262.89 248.92 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:Fuse")
    (at 320.04 248.92 90)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "F11"
      (at 320.04 240.538 90.0))
    (property "Value" "0.5A logic branch fuse"
      (at 320.04 243.078 90.0))
    (property "Footprint" "Fuse:Fuse_Littelfuse-NANO2-451_453"
      (at 320.04 248.92 0.0)
      (hide yes))
    (property "MPN" "0451.500MRL"
      (at 320.04 248.92 0.0)
      (hide yes))
    (property "Manufacturer" "Littelfuse"
      (at 320.04 248.92 0.0)
      (hide yes))
    (property "Datasheet" "https://www.littelfuse.com/assetdocs/fuse-451-and-453-datasheet?assetguid=533cd5cc-956c-4243-867f-6ab5a62f6ba1"
      (at 320.04 248.92 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "F11")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 316.23 248.92)
      (xy 306.07 248.92)))
  (global_label "V24_BUS"
    (shape passive)
    (at 306.07 248.92 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 306.07 248.92 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 323.85 248.92)
      (xy 334.01 248.92)))
  (global_label "V24_LOGIC"
    (shape passive)
    (at 334.01 248.92 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 334.01 248.92 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 78.74 152.4 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R500"
      (at 83.82 151.13 0.0))
    (property "Value" "4.02k"
      (at 83.82 153.67 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 78.74 152.4 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-074K02L"
      (at 78.74 152.4 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 78.74 152.4 0.0)
      (hide yes))
    (property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
      (at 78.74 152.4 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R500")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 78.74 148.59)
      (xy 78.74 137.16)))
  (global_label "EFUSE_ILIM"
    (shape passive)
    (at 78.74 137.16 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 78.74 137.16 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 78.74 156.21)
      (xy 78.74 163.83)))
  (global_label "GND"
    (shape passive)
    (at 78.74 163.83 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 78.74 163.83 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 127.0 152.4 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R501"
      (at 132.08 151.13 0.0))
    (property "Value" "140k"
      (at 132.08 153.67 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 127.0 152.4 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-07140KL"
      (at 127.0 152.4 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 127.0 152.4 0.0)
      (hide yes))
    (property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
      (at 127.0 152.4 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R501")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 127.0 148.59)
      (xy 127.0 137.16)))
  (global_label "VIN24_FUSED"
    (shape passive)
    (at 127.0 137.16 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 127.0 137.16 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 127.0 156.21)
      (xy 127.0 167.64)))
  (global_label "EFUSE_UVLO"
    (shape passive)
    (at 127.0 167.64 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 127.0 167.64 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 175.26 152.4 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R502"
      (at 180.34 151.13 0.0))
    (property "Value" "10k"
      (at 180.34 153.67 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 175.26 152.4 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-0710KL"
      (at 175.26 152.4 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 175.26 152.4 0.0)
      (hide yes))
    (property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
      (at 175.26 152.4 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R502")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 175.26 148.59)
      (xy 175.26 137.16)))
  (global_label "EFUSE_UVLO"
    (shape passive)
    (at 175.26 137.16 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 175.26 137.16 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 175.26 156.21)
      (xy 175.26 163.83)))
  (global_label "GND"
    (shape passive)
    (at 175.26 163.83 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 175.26 163.83 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 223.52 152.4 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R503"
      (at 228.6 151.13 0.0))
    (property "Value" "210k"
      (at 228.6 153.67 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 223.52 152.4 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-07210KL"
      (at 223.52 152.4 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 223.52 152.4 0.0)
      (hide yes))
    (property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
      (at 223.52 152.4 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R503")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 223.52 148.59)
      (xy 223.52 137.16)))
  (global_label "VIN24_FUSED"
    (shape passive)
    (at 223.52 137.16 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 223.52 137.16 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 223.52 156.21)
      (xy 223.52 166.37)))
  (global_label "EFUSE_OVP"
    (shape passive)
    (at 223.52 166.37 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 223.52 166.37 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 271.78 152.4 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R504"
      (at 276.86 151.13 0.0))
    (property "Value" "10k"
      (at 276.86 153.67 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 271.78 152.4 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-0710KL"
      (at 271.78 152.4 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 271.78 152.4 0.0)
      (hide yes))
    (property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
      (at 271.78 152.4 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R504")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 271.78 148.59)
      (xy 271.78 138.43)))
  (global_label "EFUSE_OVP"
    (shape passive)
    (at 271.78 138.43 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 271.78 138.43 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 271.78 156.21)
      (xy 271.78 163.83)))
  (global_label "GND"
    (shape passive)
    (at 271.78 163.83 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 271.78 163.83 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 320.04 152.4 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R505"
      (at 325.12 151.13 0.0))
    (property "Value" "165k"
      (at 325.12 153.67 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 320.04 152.4 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-07165KL"
      (at 320.04 152.4 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 320.04 152.4 0.0)
      (hide yes))
    (property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
      (at 320.04 152.4 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R505")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 320.04 148.59)
      (xy 320.04 138.43)))
  (global_label "V24_BUS"
    (shape passive)
    (at 320.04 138.43 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 320.04 138.43 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 320.04 156.21)
      (xy 320.04 167.64)))
  (global_label "EFUSE_PGTH"
    (shape passive)
    (at 320.04 167.64 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 320.04 167.64 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 368.3 152.4 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R506"
      (at 373.38 151.13 0.0))
    (property "Value" "10k"
      (at 373.38 153.67 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 368.3 152.4 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-0710KL"
      (at 368.3 152.4 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 368.3 152.4 0.0)
      (hide yes))
    (property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
      (at 368.3 152.4 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R506")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 368.3 148.59)
      (xy 368.3 137.16)))
  (global_label "EFUSE_PGTH"
    (shape passive)
    (at 368.3 137.16 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 368.3 137.16 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 368.3 156.21)
      (xy 368.3 163.83)))
  (global_label "GND"
    (shape passive)
    (at 368.3 163.83 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 368.3 163.83 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 30.48 195.58 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R507"
      (at 35.56 194.31 0.0))
    (property "Value" "10k"
      (at 35.56 196.85 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 30.48 195.58 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-0710KL"
      (at 30.48 195.58 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 30.48 195.58 0.0)
      (hide yes))
    (property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
      (at 30.48 195.58 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R507")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 30.48 191.77)
      (xy 30.48 180.34)))
  (global_label "EFUSE_IMON"
    (shape passive)
    (at 30.48 180.34 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 30.48 180.34 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 30.48 199.39)
      (xy 30.48 207.01)))
  (global_label "GND"
    (shape passive)
    (at 30.48 207.01 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 30.48 207.01 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 78.74 195.58 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R508"
      (at 83.82 194.31 0.0))
    (property "Value" "10k"
      (at 83.82 196.85 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 78.74 195.58 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-0710KL"
      (at 78.74 195.58 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 78.74 195.58 0.0)
      (hide yes))
    (property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
      (at 78.74 195.58 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R508")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 78.74 191.77)
      (xy 78.74 184.15)))
  (global_label "+3V3"
    (shape passive)
    (at 78.74 184.15 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 78.74 184.15 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 78.74 199.39)
      (xy 78.74 210.82)))
  (global_label "EFUSE_FLT_N"
    (shape passive)
    (at 78.74 210.82 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 78.74 210.82 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 127.0 195.58 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R509"
      (at 132.08 194.31 0.0))
    (property "Value" "10k"
      (at 132.08 196.85 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 127.0 195.58 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-0710KL"
      (at 127.0 195.58 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 127.0 195.58 0.0)
      (hide yes))
    (property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
      (at 127.0 195.58 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R509")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 127.0 191.77)
      (xy 127.0 184.15)))
  (global_label "+3V3"
    (shape passive)
    (at 127.0 184.15 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 127.0 184.15 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 127.0 199.39)
      (xy 127.0 210.82)))
  (global_label "EFUSE_PGOOD"
    (shape passive)
    (at 127.0 210.82 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 127.0 210.82 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:C")
    (at 175.26 195.58 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C500"
      (at 180.34 194.31 0.0))
    (property "Value" "100nF 100V X7R"
      (at 180.34 196.85 0.0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
      (at 175.26 195.58 0.0)
      (hide yes))
    (property "MPN" "GRM188R72A104KA35D"
      (at 175.26 195.58 0.0)
      (hide yes))
    (property "Manufacturer" "Murata"
      (at 175.26 195.58 0.0)
      (hide yes))
    (property "Datasheet" "https://www.murata.com/products/productdetail?partno=GRM188R72A104KA35%23"
      (at 175.26 195.58 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C500")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 175.26 191.77)
      (xy 175.26 180.34)))
  (global_label "VIN24_FUSED"
    (shape passive)
    (at 175.26 180.34 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 175.26 180.34 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 175.26 199.39)
      (xy 175.26 207.01)))
  (global_label "GND"
    (shape passive)
    (at 175.26 207.01 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 175.26 207.01 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:C")
    (at 223.52 195.58 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C501"
      (at 228.6 194.31 0.0))
    (property "Value" "1uF 100V X7R"
      (at 228.6 196.85 0.0))
    (property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
      (at 223.52 195.58 0.0)
      (hide yes))
    (property "MPN" "C3216X7R2A105K160AA"
      (at 223.52 195.58 0.0)
      (hide yes))
    (property "Manufacturer" "TDK"
      (at 223.52 195.58 0.0)
      (hide yes))
    (property "Datasheet" "https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C3216X7R2A105K160AA"
      (at 223.52 195.58 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C501")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 223.52 191.77)
      (xy 223.52 180.34)))
  (global_label "VIN24_FUSED"
    (shape passive)
    (at 223.52 180.34 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 223.52 180.34 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 223.52 199.39)
      (xy 223.52 207.01)))
  (global_label "GND"
    (shape passive)
    (at 223.52 207.01 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 223.52 207.01 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:C")
    (at 271.78 195.58 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C502"
      (at 276.86 194.31 0.0))
    (property "Value" "100nF 100V X7R"
      (at 276.86 196.85 0.0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
      (at 271.78 195.58 0.0)
      (hide yes))
    (property "MPN" "GRM188R72A104KA35D"
      (at 271.78 195.58 0.0)
      (hide yes))
    (property "Manufacturer" "Murata"
      (at 271.78 195.58 0.0)
      (hide yes))
    (property "Datasheet" "https://www.murata.com/products/productdetail?partno=GRM188R72A104KA35%23"
      (at 271.78 195.58 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C502")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 271.78 191.77)
      (xy 271.78 181.61)))
  (global_label "VIN24_RPP"
    (shape passive)
    (at 271.78 181.61 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 271.78 181.61 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 271.78 199.39)
      (xy 271.78 207.01)))
  (global_label "GND"
    (shape passive)
    (at 271.78 207.01 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 271.78 207.01 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:C")
    (at 320.04 195.58 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C503"
      (at 325.12 194.31 0.0))
    (property "Value" "100nF 100V X7R"
      (at 325.12 196.85 0.0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
      (at 320.04 195.58 0.0)
      (hide yes))
    (property "MPN" "GRM188R72A104KA35D"
      (at 320.04 195.58 0.0)
      (hide yes))
    (property "Manufacturer" "Murata"
      (at 320.04 195.58 0.0)
      (hide yes))
    (property "Datasheet" "https://www.murata.com/products/productdetail?partno=GRM188R72A104KA35%23"
      (at 320.04 195.58 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C503")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 320.04 191.77)
      (xy 320.04 180.34)))
  (global_label "EFUSE_DVDT"
    (shape passive)
    (at 320.04 180.34 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 320.04 180.34 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 320.04 199.39)
      (xy 320.04 207.01)))
  (global_label "GND"
    (shape passive)
    (at 320.04 207.01 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 320.04 207.01 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:C_Polarized")
    (at 353.06 71.12 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C504"
      (at 358.14 69.85 0.0))
    (property "Value" "1000uF 50V low ESR"
      (at 358.14 72.39 0.0))
    (property "Footprint" "ELF:CP_CDE_AFK_CaseP_D16_H17_Provisional"
      (at 353.06 71.12 0.0)
      (hide yes))
    (property "MPN" "AFK108M50P44T-F"
      (at 353.06 71.12 0.0)
      (hide yes))
    (property "Manufacturer" "Cornell Dubilier / Knowles"
      (at 353.06 71.12 0.0)
      (hide yes))
    (property "Datasheet" "https://www.cde.com/resources/catalogs/AFK.pdf"
      (at 353.06 71.12 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C504")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 353.06 74.93)
      (xy 353.06 82.55)))
  (global_label "GND"
    (shape passive)
    (at 353.06 82.55 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 353.06 82.55 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:C")
    (at 368.3 195.58 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C505"
      (at 373.38 194.31 0.0))
    (property "Value" "100nF 100V X7R"
      (at 373.38 196.85 0.0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
      (at 368.3 195.58 0.0)
      (hide yes))
    (property "MPN" "GRM188R72A104KA35D"
      (at 368.3 195.58 0.0)
      (hide yes))
    (property "Manufacturer" "Murata"
      (at 368.3 195.58 0.0)
      (hide yes))
    (property "Datasheet" "https://www.murata.com/products/productdetail?partno=GRM188R72A104KA35%23"
      (at 368.3 195.58 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C505")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 368.3 191.77)
      (xy 368.3 181.61)))
  (global_label "V24_BUS"
    (shape passive)
    (at 368.3 181.61 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 368.3 181.61 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 368.3 199.39)
      (xy 368.3 207.01)))
  (global_label "GND"
    (shape passive)
    (at 368.3 207.01 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 368.3 207.01 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 39.37 66.04)
      (xy 88.9 66.04)))
  (global_label "VIN24_FUSED"
    (shape passive)
    (at 88.9 66.04 0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 88.9 66.04 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 124.46 66.04)
      (xy 182.88 66.04)))
  (wire
    (pts
      (xy 182.88 66.04)
      (xy 182.88 58.42)))
  (wire
    (pts
      (xy 182.88 58.42)
      (xy 236.22 58.42)))
  (global_label "VIN24_RPP"
    (shape passive)
    (at 182.88 66.04 0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 182.88 66.04 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 271.78 66.04)
      (xy 353.06 66.04)))
  (wire
    (pts
      (xy 353.06 66.04)
      (xy 353.06 67.31)))
  (global_label "V24_BUS"
    (shape passive)
    (at 353.06 66.04 0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 353.06 66.04 0.0)
      (hide yes)))
  (text "POWER 1"
    (at 20.32 15.24 0))
  (text "INPUT / REVERSE PROTECTION / MAIN eFUSE"
    (at 20.32 27.94 0))
  (text "J1 is on power_2. TVS input return is GND.\nU12 nominal current limit 4.5 A; prototype operating target <= 4.0 A."
    (at 20.32 91.44 0))
  (text "Threshold / status / startup components"
    (at 20.32 129.54 0))
  (text "FUSED DISTRIBUTION: motors / ambient zones / logic"
    (at 20.32 217.17 0))
  (embedded_fonts no))