(kicad_sch
  (version 20250114)
  (generator "engineered-lighting")
  (generator_version "0.2")
  (paper "A3")
  (title_block
    (title "Power 2")
    (date "2026-09-06")
    (rev "A draft")
    (company "Engineered Lighting")
    (comment 1 "ENGINEERING DRAFT - see release status before fabrication"))
  (lib_symbols
    (symbol "Regulator_Switching:LMR36510ADDA"
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "U"
        (at 0 11.43 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "LMR36510ADDA"
        (at 0 8.89 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" "Package_SO:Texas_HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.95x4.9mm_Mask2.4x3.1mm_ThermalVias"
        (at 0 -20.32 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmr36510.pdf"
        (at 0 -1.27 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Simple Switcher Synchronous Buck Regulator, Vin=4.2-65V, Iout=1A, F=400kHz, Adjustable output voltage, HSOP-8"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "synchronous buck step-down"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "Texas*HTSOP*1EP*3.9x4.9mm*P1.27mm*EP2.95x4.9mm*Mask2.4x3.1mm*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "LMR36510ADDA_0_1"
        (rectangle
          (start -7.62 7.62)
          (end 7.62 -7.62)
          (fill
            (type background))))
      (symbol "LMR36510ADDA_1_1"
        (pin power_in line
          (at 0 -10.16 90)
          (length 2.54)
          (name "PGND")
          (number "1"))
        (pin power_in line
          (at -10.16 5.08 0)
          (length 2.54)
          (name "VIN")
          (number "2"))
        (pin input line
          (at -10.16 0 0)
          (length 2.54)
          (name "EN")
          (number "3"))
        (pin open_collector line
          (at 10.16 -5.08 180)
          (length 2.54)
          (name "PG")
          (number "4"))
        (pin input line
          (at 10.16 -2.54 180)
          (length 2.54)
          (name "FB")
          (number "5"))
        (pin power_out line
          (at -10.16 -5.08 0)
          (length 2.54)
          (name "VCC")
          (number "6"))
        (pin input line
          (at 10.16 5.08 180)
          (length 2.54)
          (name "BOOT")
          (number "7"))
        (pin output line
          (at 10.16 2.54 180)
          (length 2.54)
          (name "SW")
          (number "8"))
        (pin power_in line
          (at 2.54 -10.16 90)
          (length 2.54)
          (name "PAD")
          (number "9")))
      (embedded_fonts no))
    (symbol "Device:L"
      (pin_numbers
        (hide yes))
      (pin_names
        (offset 1.016)
        (hide yes))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "L"
        (at -1.27 0 90)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "L"
        (at 1.905 0 90)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Inductor"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "inductor choke coil reactor magnetic"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "Choke_* *Coil* Inductor_* L_*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "L_0_1"
        (arc
          (start 0 2.54)
          (mid 0.6323 1.905)
          (end 0 1.27)
          (fill
            (type none)))
        (arc
          (start 0 1.27)
          (mid 0.6323 0.635)
          (end 0 0)
          (fill
            (type none)))
        (arc
          (start 0 0)
          (mid 0.6323 -0.635)
          (end 0 -1.27)
          (fill
            (type none)))
        (arc
          (start 0 -1.27)
          (mid 0.6323 -1.905)
          (end 0 -2.54)
          (fill
            (type none))))
      (symbol "L_1_1"
        (pin passive line
          (at 0 3.81 270)
          (length 1.27)
          (name "1")
          (number "1"))
        (pin passive line
          (at 0 -3.81 90)
          (length 1.27)
          (name "2")
          (number "2")))
      (embedded_fonts no))
    (symbol "Device:C"
      (pin_numbers
        (hide yes))
      (pin_names
        (offset 0.254))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "C"
        (at 0.635 2.54 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "C"
        (at 0.635 -2.54 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" ""
        (at 0.9652 -3.81 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Unpolarized capacitor"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "cap capacitor"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "C_*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762))
          (fill
            (type none)))
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762))
          (fill
            (type none))))
      (symbol "C_1_1"
        (pin passive line
          (at 0 3.81 270)
          (length 2.794)
          (name "")
          (number "1"))
        (pin passive line
          (at 0 -3.81 90)
          (length 2.794)
          (name "")
          (number "2")))
      (embedded_fonts no))
    (symbol "Device:R"
      (pin_numbers
        (hide yes))
      (pin_names
        (offset 0))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "R"
        (at 2.032 0 90)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "R"
        (at 0 0 90)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" ""
        (at -1.778 0 90)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Resistor"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "R res resistor"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "R_*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "R_0_1"
        (rectangle
          (start -1.016 -2.54)
          (end 1.016 2.54)
          (fill
            (type none))))
      (symbol "R_1_1"
        (pin passive line
          (at 0 3.81 270)
          (length 1.27)
          (name "")
          (number "1"))
        (pin passive line
          (at 0 -3.81 90)
          (length 1.27)
          (name "")
          (number "2")))
      (embedded_fonts no))
    (symbol "Regulator_Switching:TPS62162DSG"
      (pin_names
        (offset 0.254))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (symbol "TPS62162DSG_0_1"
        (rectangle
          (start -7.62 10.16)
          (end 7.62 -7.62)
          (fill
            (type background))))
      (symbol "TPS62162DSG_1_1"
        (pin power_in line
          (at 0 -10.16 90)
          (length 2.54)
          (name "PGND")
          (number "1"))
        (pin power_in line
          (at -10.16 7.62 0)
          (length 2.54)
          (name "VIN")
          (number "2"))
        (pin input line
          (at -10.16 5.08 0)
          (length 2.54)
          (name "EN")
          (number "3"))
        (pin power_in line
          (at 2.54 -10.16 90)
          (length 2.54)
          (name "AGND")
          (number "4"))
        (pin input line
          (at 10.16 2.54 180)
          (length 2.54)
          (name "FB")
          (number "5"))
        (pin input line
          (at 10.16 5.08 180)
          (length 2.54)
          (name "VOS")
          (number "6"))
        (pin output line
          (at 10.16 7.62 180)
          (length 2.54)
          (name "SW")
          (number "7"))
        (pin open_collector line
          (at -10.16 -2.54 0)
          (length 2.54)
          (name "PG")
          (number "8"))
        (pin power_in line
          (at -2.54 -10.16 90)
          (length 2.54)
          (name "PAD")
          (number "9")))
      (embedded_fonts no)
      (property "Reference" "U"
        (at -7.62 11.43 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "TPS62162DSG"
        (at -1.27 11.43 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" "Package_SON:WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm_ThermalVias"
        (at 3.81 -8.89 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps62160.pdf"
        (at 0 13.97 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "1A Step-Down Converter with DCS-Control, fixed 3.3V output, 3-17V input voltage, WSON-8"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "step-down dc-dc buck regulator"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "WSON*EP*2x2mm*P0.5mm*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes)))
    (symbol "EL:TPS22919DCKR"
      (pin_names
        (offset 0.8))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (property "Reference" "U"
        (at 0 10.16 0))
      (property "Value" "TPS22919DCKR"
        (at 0 -10.16 0))
      (symbol "TPS22919DCKR_0_1"
        (rectangle
          (start -12.7 7.62)
          (end 12.7 -7.62)
          (fill
            (type background))))
      (symbol "TPS22919DCKR_1_1"
        (pin power_in line
          (at -17.78 5.08 0)
          (length 5.08)
          (name "VIN")
          (number "1"))
        (pin power_in line
          (at -17.78 2.54 0)
          (length 5.08)
          (name "GND")
          (number "2"))
        (pin input line
          (at -17.78 0.0 0)
          (length 5.08)
          (name "ON")
          (number "3"))
        (pin no_connect line
          (at -17.78 -2.54 0)
          (length 5.08)
          (name "NC")
          (number "4"))
        (pin passive line
          (at -17.78 -5.08 0)
          (length 5.08)
          (name "QOD")
          (number "5"))
        (pin power_out line
          (at 17.78 5.08 180)
          (length 5.08)
          (name "VOUT")
          (number "6"))))
    (symbol "Device:D_Schottky"
      (pin_numbers
        (hide yes))
      (pin_names
        (offset 1.016)
        (hide yes))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "D"
        (at 0 2.54 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "D_Schottky"
        (at 0 -2.54 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Schottky diode"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "diode Schottky"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "TO-???* *_Diode_* *SingleDiode* D_*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "D_Schottky_0_1"
        (polyline
          (pts
            (xy -1.905 0.635)
            (xy -1.905 1.27)
            (xy -1.27 1.27)
            (xy -1.27 -1.27)
            (xy -0.635 -1.27)
            (xy -0.635 -0.635))
          (fill
            (type none)))
        (polyline
          (pts
            (xy 1.27 1.27)
            (xy 1.27 -1.27)
            (xy -1.27 0)
            (xy 1.27 1.27))
          (fill
            (type none)))
        (polyline
          (pts
            (xy 1.27 0)
            (xy -1.27 0))
          (fill
            (type none))))
      (symbol "D_Schottky_1_1"
        (pin passive line
          (at -3.81 0 0)
          (length 2.54)
          (name "K")
          (number "1"))
        (pin passive line
          (at 3.81 0 180)
          (length 2.54)
          (name "A")
          (number "2")))
      (embedded_fonts no))
    (symbol "Power_Protection:TVS2700DRV"
      (pin_names
        (offset 0)
        (hide yes))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (symbol "TVS2700DRV_0_0"
        (rectangle
          (start -11.43 2.54)
          (end -5.08 -2.54)
          (fill
            (type none)))
        (polyline
          (pts
            (xy -8.255 2.54)
            (xy -8.255 3.81)
            (xy 0 3.81))
          (fill
            (type none)))
        (polyline
          (pts
            (xy -8.255 -2.54)
            (xy -8.255 -3.81)
            (xy 0 -3.81))
          (fill
            (type none)))
        (polyline
          (pts
            (xy 0 1.27)
            (xy -1.778 1.27))
          (fill
            (type none)))
        (text "Det &"
          (at -8.255 0.635 0))
        (text "Drv"
          (at -8.255 -1.27 0)))
      (symbol "TVS2700DRV_0_1"
        (rectangle
          (start -12.065 5.08)
          (end 2.54 -5.08)
          (fill
            (type background)))
        (polyline
          (pts
            (xy -2.286 1.397)
            (xy -2.286 -1.524))
          (fill
            (type none)))
        (polyline
          (pts
            (xy -2.286 0)
            (xy -5.08 0))
          (fill
            (type none)))
        (polyline
          (pts
            (xy -1.778 1.778)
            (xy -1.778 -1.778))
          (fill
            (type none)))
        (circle
          (center -0.889 0)
          (radius 2.794)
          (fill
            (type none)))
        (polyline
          (pts
            (xy -0.127 -1.27)
            (xy -1.143 -1.651)
            (xy -1.143 -0.889)
            (xy -0.127 -1.27))
          (fill
            (type outline)))
        (polyline
          (pts
            (xy 0 5.08)
            (xy 0 2.54))
          (fill
            (type none)))
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0 1.27))
          (fill
            (type none)))
        (polyline
          (pts
            (xy 0 -2.54)
            (xy 0 -5.08))
          (fill
            (type none)))
        (polyline
          (pts
            (xy 0 -2.54)
            (xy 0 -1.27)
            (xy -1.778 -1.27))
          (fill
            (type none))))
      (symbol "TVS2700DRV_1_1"
        (pin power_in line
          (at 0 -7.62 90)
          (length 2.54)
          (name "GND")
          (number "1"))
        (pin passive line
          (at 0 -7.62 90)
          (length 2.54)
          (hide yes)
          (name "GND")
          (number "2"))
        (pin passive line
          (at 0 -7.62 90)
          (length 2.54)
          (hide yes)
          (name "GND")
          (number "3"))
        (pin passive line
          (at 0 7.62 270)
          (length 2.54)
          (name "IN")
          (number "4"))
        (pin passive line
          (at 0 7.62 270)
          (length 2.54)
          (hide yes)
          (name "IN")
          (number "5"))
        (pin passive line
          (at 0 7.62 270)
          (length 2.54)
          (hide yes)
          (name "IN")
          (number "6"))
        (pin passive line
          (at 0 -7.62 90)
          (length 2.54)
          (hide yes)
          (name "GND")
          (number "7")))
      (embedded_fonts no)
      (property "Reference" "U"
        (at 2.54 1.27 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "TVS2700DRV"
        (at 2.54 -1.27 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
        (at 5.08 -8.89 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" "http://www.ti.com/lit/ds/symlink/tvs2700.pdf"
        (at -2.54 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Flat-Clamp Surge Protection Device. 27Vrwm, WSON-6"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "EMI, ESD, TVS protection transient"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*EP1x1.6mm*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes)))
    (symbol "Connector_Generic:Conn_01x02"
      (pin_names
        (offset 1.016)
        (hide yes))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "J"
        (at 0 2.54 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "Conn_01x02"
        (at 0 -5.08 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "connector"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "Connector*:*_1x??_*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "Conn_01x02_1_1"
        (rectangle
          (start -1.27 1.27)
          (end 1.27 -3.81)
          (fill
            (type background)))
        (rectangle
          (start -1.27 0.127)
          (end 0 -0.127)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -2.413)
          (end 0 -2.667)
          (fill
            (type none)))
        (pin passive line
          (at -5.08 0 0)
          (length 3.81)
          (name "Pin_1")
          (number "1"))
        (pin passive line
          (at -5.08 -2.54 0)
          (length 3.81)
          (name "Pin_2")
          (number "2")))
      (embedded_fonts no)))
  (symbol
    (lib_id "Regulator_Switching:LMR36510ADDA")
    (at 88.9 76.2 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "U10"
      (at 101.6 59.69 0.0))
    (property "Value" "24V to 5V 1A buck"
      (at 101.6 62.23 0.0))
    (property "Footprint" "ELF:TI_DDA0008B_EP2.71x3.4_ThermalVias_125um"
      (at 88.9 76.2 0.0)
      (hide yes))
    (property "MPN" "LMR36510ADDAR"
      (at 88.9 76.2 0.0)
      (hide yes))
    (property "Manufacturer" "Texas Instruments"
      (at 88.9 76.2 0.0)
      (hide yes))
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/lmr36510.pdf"
      (at 88.9 76.2 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "U10")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9"))
  (wire
    (pts
      (xy 88.9 86.36)
      (xy 88.9 93.98)))
  (global_label "GND"
    (shape passive)
    (at 88.9 93.98 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 88.9 93.98 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 78.74 71.12)
      (xy 68.58 71.12)))
  (global_label "V24_LOGIC"
    (shape passive)
    (at 68.58 71.12 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 68.58 71.12 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 78.74 76.2)
      (xy 68.58 76.2)))
  (global_label "V24_LOGIC"
    (shape passive)
    (at 68.58 76.2 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 68.58 76.2 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 99.06 81.28)
      (xy 110.49 81.28)))
  (global_label "BUCK5_PGOOD"
    (shape passive)
    (at 110.49 81.28 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 110.49 81.28 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 99.06 78.74)
      (xy 109.22 78.74)))
  (global_label "BUCK5_FB"
    (shape passive)
    (at 109.22 78.74 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 109.22 78.74 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 78.74 81.28)
      (xy 68.58 81.28)))
  (global_label "BUCK5_VCC"
    (shape passive)
    (at 68.58 81.28 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 68.58 81.28 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 99.06 71.12)
      (xy 110.49 71.12)))
  (global_label "BUCK5_BOOT"
    (shape passive)
    (at 110.49 71.12 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 110.49 71.12 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 91.44 86.36)
      (xy 91.44 93.98)))
  (global_label "GND"
    (shape passive)
    (at 91.44 93.98 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 91.44 93.98 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:L")
    (at 144.78 73.66 90)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "L500"
      (at 144.78 66.04 90.0))
    (property "Value" "22uH 2.5A RMS 5.5A sat"
      (at 144.78 68.58 90.0))
    (property "Footprint" "ELF:L_Bourns_SRP7050TA"
      (at 144.78 73.66 0.0)
      (hide yes))
    (property "MPN" "SRP7050TA-220M"
      (at 144.78 73.66 0.0)
      (hide yes))
    (property "Manufacturer" "Bourns"
      (at 144.78 73.66 0.0)
      (hide yes))
    (property "Datasheet" "https://www.bourns.com/docs/Product-Datasheets/SRP7050TA.pdf"
      (at 144.78 73.66 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "L500")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (symbol
    (lib_id "Device:C")
    (at 35.56 71.12 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C506"
      (at 40.64 69.85 0.0))
    (property "Value" "10uF 50V X7R"
      (at 40.64 72.39 0.0))
    (property "Footprint" "Capacitor_SMD:C_1210_3225Metric"
      (at 35.56 71.12 0.0)
      (hide yes))
    (property "MPN" "GRM32ER71H106KA12L"
      (at 35.56 71.12 0.0)
      (hide yes))
    (property "Manufacturer" "Murata"
      (at 35.56 71.12 0.0)
      (hide yes))
    (property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM32ER71H106KA12-04A.pdf"
      (at 35.56 71.12 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C506")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 35.56 67.31)
      (xy 35.56 57.15)))
  (global_label "V24_LOGIC"
    (shape passive)
    (at 35.56 57.15 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 35.56 57.15 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 35.56 74.93)
      (xy 35.56 82.55)))
  (global_label "GND"
    (shape passive)
    (at 35.56 82.55 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 35.56 82.55 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:C")
    (at 121.92 43.18 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C507"
      (at 127.0 41.91 0.0))
    (property "Value" "220nF 50V X7R"
      (at 127.0 44.45 0.0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
      (at 121.92 43.18 0.0)
      (hide yes))
    (property "MPN" "C2012X7R1H224K125AA"
      (at 121.92 43.18 0.0)
      (hide yes))
    (property "Manufacturer" "TDK"
      (at 121.92 43.18 0.0)
      (hide yes))
    (property "Datasheet" "https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C2012X7R1H224K125AA"
      (at 121.92 43.18 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C507")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 121.92 39.37)
      (xy 121.92 29.21)))
  (global_label "V24_LOGIC"
    (shape passive)
    (at 121.92 29.21 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 121.92 29.21 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 121.92 46.99)
      (xy 121.92 54.61)))
  (global_label "GND"
    (shape passive)
    (at 121.92 54.61 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 121.92 54.61 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:C")
    (at 43.18 111.76 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C508"
      (at 48.26 110.49 0.0))
    (property "Value" "1uF 25V X7R"
      (at 48.26 113.03 0.0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
      (at 43.18 111.76 0.0)
      (hide yes))
    (property "MPN" "C1608X7R1E105K080AB"
      (at 43.18 111.76 0.0)
      (hide yes))
    (property "Manufacturer" "TDK"
      (at 43.18 111.76 0.0)
      (hide yes))
    (property "Datasheet" "https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C1608X7R1E105K080AB"
      (at 43.18 111.76 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C508")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 43.18 107.95)
      (xy 43.18 97.79)))
  (global_label "BUCK5_VCC"
    (shape passive)
    (at 43.18 97.79 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 43.18 97.79 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 43.18 115.57)
      (xy 43.18 123.19)))
  (global_label "GND"
    (shape passive)
    (at 43.18 123.19 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 43.18 123.19 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:C")
    (at 68.58 111.76 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C509"
      (at 73.66 110.49 0.0))
    (property "Value" "100nF 100V X7R"
      (at 73.66 113.03 0.0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
      (at 68.58 111.76 0.0)
      (hide yes))
    (property "MPN" "GRM188R72A104KA35D"
      (at 68.58 111.76 0.0)
      (hide yes))
    (property "Manufacturer" "Murata"
      (at 68.58 111.76 0.0)
      (hide yes))
    (property "Datasheet" "https://www.murata.com/products/productdetail?partno=GRM188R72A104KA35%23"
      (at 68.58 111.76 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C509")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 68.58 107.95)
      (xy 68.58 96.52)))
  (global_label "BUCK5_BOOT"
    (shape passive)
    (at 68.58 96.52 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 68.58 96.52 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 68.58 115.57)
      (xy 68.58 125.73)))
  (global_label "BUCK5_SW"
    (shape passive)
    (at 68.58 125.73 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 68.58 125.73 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:C")
    (at 177.8 96.52 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C510"
      (at 182.88 95.25 0.0))
    (property "Value" "22uF 25V X7R"
      (at 182.88 97.79 0.0))
    (property "Footprint" "Capacitor_SMD:C_1210_3225Metric"
      (at 177.8 96.52 0.0)
      (hide yes))
    (property "MPN" "GRM32ER71E226KE15L"
      (at 177.8 96.52 0.0)
      (hide yes))
    (property "Manufacturer" "Murata"
      (at 177.8 96.52 0.0)
      (hide yes))
    (property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM32ER71E226KE15-01.pdf"
      (at 177.8 96.52 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C510")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 177.8 100.33)
      (xy 177.8 107.95)))
  (global_label "GND"
    (shape passive)
    (at 177.8 107.95 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 177.8 107.95 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:C")
    (at 203.2 96.52 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C511"
      (at 208.28 95.25 0.0))
    (property "Value" "22uF 25V X7R"
      (at 208.28 97.79 0.0))
    (property "Footprint" "Capacitor_SMD:C_1210_3225Metric"
      (at 203.2 96.52 0.0)
      (hide yes))
    (property "MPN" "GRM32ER71E226KE15L"
      (at 203.2 96.52 0.0)
      (hide yes))
    (property "Manufacturer" "Murata"
      (at 203.2 96.52 0.0)
      (hide yes))
    (property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM32ER71E226KE15-01.pdf"
      (at 203.2 96.52 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C511")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 203.2 100.33)
      (xy 203.2 107.95)))
  (global_label "GND"
    (shape passive)
    (at 203.2 107.95 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 203.2 107.95 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 154.94 137.16 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R510"
      (at 160.02 135.89 0.0))
    (property "Value" "100k"
      (at 160.02 138.43 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 154.94 137.16 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-07100KL"
      (at 154.94 137.16 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 154.94 137.16 0.0)
      (hide yes))
    (property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
      (at 154.94 137.16 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R510")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 154.94 133.35)
      (xy 154.94 125.73)))
  (global_label "+5V"
    (shape passive)
    (at 154.94 125.73 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 154.94 125.73 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 154.94 167.64 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R511"
      (at 160.02 166.37 0.0))
    (property "Value" "24.9k"
      (at 160.02 168.91 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 154.94 167.64 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-0724K9L"
      (at 154.94 167.64 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 154.94 167.64 0.0)
      (hide yes))
    (property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
      (at 154.94 167.64 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R511")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 154.94 171.45)
      (xy 154.94 179.07)))
  (global_label "GND"
    (shape passive)
    (at 154.94 179.07 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 154.94 179.07 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 35.56 149.86 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R512"
      (at 40.64 148.59 0.0))
    (property "Value" "10k"
      (at 40.64 151.13 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 35.56 149.86 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-0710KL"
      (at 35.56 149.86 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 35.56 149.86 0.0)
      (hide yes))
    (property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
      (at 35.56 149.86 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R512")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 35.56 146.05)
      (xy 35.56 138.43)))
  (global_label "+3V3"
    (shape passive)
    (at 35.56 138.43 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 35.56 138.43 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 35.56 153.67)
      (xy 35.56 165.1)))
  (global_label "BUCK5_PGOOD"
    (shape passive)
    (at 35.56 165.1 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 35.56 165.1 0.0)
      (hide yes)))
  (symbol
    (lib_id "Regulator_Switching:TPS62162DSG")
    (at 287.02 76.2 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "U11"
      (at 299.72 58.42 0.0))
    (property "Value" "5V to 3.3V 1A fixed buck"
      (at 299.72 60.96 0.0))
    (property "Footprint" "Package_SON:Texas_DSG0008A_WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm_ThermalVias"
      (at 287.02 76.2 0.0)
      (hide yes))
    (property "MPN" "TPS62162DSGR"
      (at 287.02 76.2 0.0)
      (hide yes))
    (property "Manufacturer" "Texas Instruments"
      (at 287.02 76.2 0.0)
      (hide yes))
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps62160.pdf"
      (at 287.02 76.2 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "U11")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9"))
  (wire
    (pts
      (xy 287.02 86.36)
      (xy 287.02 93.98)))
  (global_label "GND"
    (shape passive)
    (at 287.02 93.98 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 287.02 93.98 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 276.86 68.58)
      (xy 269.24 68.58)))
  (global_label "+5V"
    (shape passive)
    (at 269.24 68.58 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 269.24 68.58 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 276.86 71.12)
      (xy 269.24 71.12)))
  (global_label "+5V"
    (shape passive)
    (at 269.24 71.12 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 269.24 71.12 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 289.56 86.36)
      (xy 289.56 93.98)))
  (global_label "GND"
    (shape passive)
    (at 289.56 93.98 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 289.56 93.98 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 297.18 73.66)
      (xy 304.8 73.66)))
  (global_label "GND"
    (shape passive)
    (at 304.8 73.66 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 304.8 73.66 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 297.18 71.12)
      (xy 304.8 71.12)))
  (global_label "+3V3"
    (shape passive)
    (at 304.8 71.12 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 304.8 71.12 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 276.86 78.74)
      (xy 265.43 78.74)))
  (global_label "BUCK3_PGOOD"
    (shape passive)
    (at 265.43 78.74 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 265.43 78.74 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 284.48 86.36)
      (xy 284.48 93.98)))
  (global_label "GND"
    (shape passive)
    (at 284.48 93.98 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 284.48 93.98 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:L")
    (at 342.9 68.58 90)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "L501"
      (at 342.9 60.96 90.0))
    (property "Value" "2.2uH 2.9A RMS 3A sat"
      (at 342.9 63.5 90.0))
    (property "Footprint" "Inductor_SMD:L_Bourns-SRN4018"
      (at 342.9 68.58 0.0)
      (hide yes))
    (property "MPN" "SRN4018-2R2M"
      (at 342.9 68.58 0.0)
      (hide yes))
    (property "Manufacturer" "Bourns"
      (at 342.9 68.58 0.0)
      (hide yes))
    (property "Datasheet" "https://www.bourns.com/docs/product-datasheets/srn4018.pdf"
      (at 342.9 68.58 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "L501")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (symbol
    (lib_id "Device:C")
    (at 236.22 71.12 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C512"
      (at 241.3 69.85 0.0))
    (property "Value" "22uF 25V X7R"
      (at 241.3 72.39 0.0))
    (property "Footprint" "Capacitor_SMD:C_1210_3225Metric"
      (at 236.22 71.12 0.0)
      (hide yes))
    (property "MPN" "GRM32ER71E226KE15L"
      (at 236.22 71.12 0.0)
      (hide yes))
    (property "Manufacturer" "Murata"
      (at 236.22 71.12 0.0)
      (hide yes))
    (property "Datasheet" "https://www.murata.com/-/media/webrenewal/tool/library/common-pdf/dynamic-model/component-list-d-mlcc-2504.ashx?cvid=20250523010405000000&la=en"
      (at 236.22 71.12 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C512")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 236.22 67.31)
      (xy 236.22 59.69)))
  (global_label "+5V"
    (shape passive)
    (at 236.22 59.69 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 236.22 59.69 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 236.22 74.93)
      (xy 236.22 82.55)))
  (global_label "GND"
    (shape passive)
    (at 236.22 82.55 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 236.22 82.55 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:C")
    (at 375.92 99.06 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C513"
      (at 381.0 97.79 0.0))
    (property "Value" "22uF 25V X7R"
      (at 381.0 100.33 0.0))
    (property "Footprint" "Capacitor_SMD:C_1210_3225Metric"
      (at 375.92 99.06 0.0)
      (hide yes))
    (property "MPN" "GRM32ER71E226KE15L"
      (at 375.92 99.06 0.0)
      (hide yes))
    (property "Manufacturer" "Murata"
      (at 375.92 99.06 0.0)
      (hide yes))
    (property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM32ER71E226KE15-01.pdf"
      (at 375.92 99.06 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C513")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 375.92 102.87)
      (xy 375.92 110.49)))
  (global_label "GND"
    (shape passive)
    (at 375.92 110.49 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 375.92 110.49 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 241.3 137.16 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R513"
      (at 246.38 135.89 0.0))
    (property "Value" "10k"
      (at 246.38 138.43 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 241.3 137.16 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-0710KL"
      (at 241.3 137.16 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 241.3 137.16 0.0)
      (hide yes))
    (property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
      (at 241.3 137.16 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R513")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 241.3 133.35)
      (xy 241.3 125.73)))
  (global_label "+3V3"
    (shape passive)
    (at 241.3 125.73 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 241.3 125.73 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 241.3 140.97)
      (xy 241.3 152.4)))
  (global_label "BUCK3_PGOOD"
    (shape passive)
    (at 241.3 152.4 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 241.3 152.4 0.0)
      (hide yes)))
  (symbol
    (lib_id "EL:TPS22919DCKR")
    (at 124.46 218.44 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "U13"
      (at 144.78 203.2 0.0))
    (property "Value" "switched ambient gate bias"
      (at 144.78 205.74 0.0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
      (at 124.46 218.44 0.0)
      (hide yes))
    (property "MPN" "TPS22919DCKR"
      (at 124.46 218.44 0.0)
      (hide yes))
    (property "Manufacturer" "Texas Instruments"
      (at 124.46 218.44 0.0)
      (hide yes))
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps22919.pdf"
      (at 124.46 218.44 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "U13")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6"))
  (wire
    (pts
      (xy 106.68 213.36)
      (xy 99.06 213.36)))
  (global_label "+3V3"
    (shape passive)
    (at 99.06 213.36 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 99.06 213.36 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 106.68 215.9)
      (xy 99.06 215.9)))
  (global_label "GND"
    (shape passive)
    (at 99.06 215.9 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 99.06 215.9 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 106.68 218.44)
      (xy 91.44 218.44)))
  (global_label "LIGHT_ENABLE_SAFE"
    (shape passive)
    (at 91.44 218.44 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 91.44 218.44 0.0)
      (hide yes)))
  (no_connect
    (at 106.68 220.98))
  (wire
    (pts
      (xy 106.68 223.52)
      (xy 96.52 223.52)))
  (global_label "GATE_BIAS"
    (shape passive)
    (at 96.52 223.52 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 96.52 223.52 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 142.24 213.36)
      (xy 152.4 213.36)))
  (global_label "GATE_BIAS"
    (shape passive)
    (at 152.4 213.36 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 152.4 213.36 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 40.64 233.68 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R514"
      (at 45.72 232.41 0.0))
    (property "Value" "4.7k"
      (at 45.72 234.95 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 40.64 233.68 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-074K7L"
      (at 40.64 233.68 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 40.64 233.68 0.0)
      (hide yes))
    (property "Datasheet" "https://yageogroup.com/component-documentation/download/specsheet/RC0603FR-074K7L"
      (at 40.64 233.68 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R514")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 40.64 229.87)
      (xy 40.64 214.63)))
  (global_label "LIGHT_ENABLE_SAFE"
    (shape passive)
    (at 40.64 214.63 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 40.64 214.63 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 40.64 237.49)
      (xy 40.64 245.11)))
  (global_label "GND"
    (shape passive)
    (at 40.64 245.11 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 40.64 245.11 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:C")
    (at 68.58 205.74 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C514"
      (at 73.66 204.47 0.0))
    (property "Value" "100nF 100V X7R"
      (at 73.66 207.01 0.0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
      (at 68.58 205.74 0.0)
      (hide yes))
    (property "MPN" "GRM188R72A104KA35D"
      (at 68.58 205.74 0.0)
      (hide yes))
    (property "Manufacturer" "Murata"
      (at 68.58 205.74 0.0)
      (hide yes))
    (property "Datasheet" "https://www.murata.com/products/productdetail?partno=GRM188R72A104KA35%23"
      (at 68.58 205.74 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C514")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 68.58 201.93)
      (xy 68.58 194.31)))
  (global_label "+3V3"
    (shape passive)
    (at 68.58 194.31 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 68.58 194.31 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 68.58 209.55)
      (xy 68.58 217.17)))
  (global_label "GND"
    (shape passive)
    (at 68.58 217.17 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 68.58 217.17 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:C")
    (at 180.34 205.74 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C515"
      (at 185.42 204.47 0.0))
    (property "Value" "100nF 100V X7R"
      (at 185.42 207.01 0.0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
      (at 180.34 205.74 0.0)
      (hide yes))
    (property "MPN" "GRM188R72A104KA35D"
      (at 180.34 205.74 0.0)
      (hide yes))
    (property "Manufacturer" "Murata"
      (at 180.34 205.74 0.0)
      (hide yes))
    (property "Datasheet" "https://www.murata.com/products/productdetail?partno=GRM188R72A104KA35%23"
      (at 180.34 205.74 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C515")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 180.34 201.93)
      (xy 180.34 191.77)))
  (global_label "GATE_BIAS"
    (shape passive)
    (at 180.34 191.77 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 180.34 191.77 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 180.34 209.55)
      (xy 180.34 217.17)))
  (global_label "GND"
    (shape passive)
    (at 180.34 217.17 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 180.34 217.17 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:D_Schottky")
    (at 246.38 228.6 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "D505"
      (at 246.38 220.98 0.0))
    (property "Value" "60V 5A output negative transient Schottky"
      (at 246.38 223.52 0.0))
    (property "Footprint" "Diode_SMD:D_SMC"
      (at 246.38 228.6 0.0)
      (hide yes))
    (property "MPN" "B560C-13-F"
      (at 246.38 228.6 0.0)
      (hide yes))
    (property "Manufacturer" "Diodes Incorporated"
      (at 246.38 228.6 0.0)
      (hide yes))
    (property "Datasheet" "https://www.diodes.com/datasheet/download/B520C.pdf"
      (at 246.38 228.6 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "D505")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 242.57 228.6)
      (xy 232.41 228.6)))
  (global_label "V24_BUS"
    (shape passive)
    (at 232.41 228.6 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 232.41 228.6 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 250.19 228.6)
      (xy 257.81 228.6)))
  (global_label "GND"
    (shape passive)
    (at 257.81 228.6 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 257.81 228.6 0.0)
      (hide yes)))
  (symbol
    (lib_id "Power_Protection:TVS2700DRV")
    (at 292.1 208.28 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "U501"
      (at 301.9425 193.04 0.0))
    (property "Value" "27V flat-clamp transient protector"
      (at 301.9425 195.58 0.0))
    (property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm_ThermalVias"
      (at 292.1 208.28 0.0)
      (hide yes))
    (property "MPN" "TVS2700DRVR"
      (at 292.1 208.28 0.0)
      (hide yes))
    (property "Manufacturer" "Texas Instruments"
      (at 292.1 208.28 0.0)
      (hide yes))
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/tvs2700.pdf"
      (at 292.1 208.28 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "U501")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7"))
  (wire
    (pts
      (xy 292.1 215.9)
      (xy 292.1 223.52)))
  (global_label "GND"
    (shape passive)
    (at 292.1 223.52 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 292.1 223.52 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 292.1 200.66)
      (xy 292.1 190.5)))
  (global_label "V24_BUS"
    (shape passive)
    (at 292.1 190.5 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 292.1 190.5 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x02")
    (at 335.28 177.8 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "J1"
      (at 340.36 176.53 0.0))
    (property "Value" "24V INPUT"
      (at 340.36 179.07 0.0))
    (property "Footprint" "ELF:Enclosure_J1"
      (at 335.28 177.8 0.0)
      (hide yes))
    (property "MPN" "1771091"
      (at 335.28 177.8 0.0)
      (hide yes))
    (property "Manufacturer" "Phoenix Contact"
      (at 335.28 177.8 0.0)
      (hide yes))
    (property "Datasheet" "https://www.phoenixcontact.com/en-us/products/printed-circuit-board-terminal-ptsm-05-2-25-v-smd-r44-1771091"
      (at 335.28 177.8 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "J1")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 330.2 177.8)
      (xy 320.04 177.8)))
  (global_label "VIN24_RAW"
    (shape passive)
    (at 320.04 177.8 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 320.04 177.8 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 330.2 180.34)
      (xy 322.58 180.34)))
  (global_label "GND"
    (shape passive)
    (at 322.58 180.34 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 322.58 180.34 0.0)
      (hide yes)))
  (symbol
    (lib_id "Connector_Generic:Conn_01x02")
    (at 381.0 223.52 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "J16"
      (at 386.08 222.25 0.0))
    (property "Value" "BRAKE / BUS"
      (at 386.08 224.79 0.0))
    (property "Footprint" "ELF:Enclosure_J16"
      (at 381.0 223.52 0.0)
      (hide yes))
    (property "MPN" "2053380002"
      (at 381.0 223.52 0.0)
      (hide yes))
    (property "Manufacturer" "Molex"
      (at 381.0 223.52 0.0)
      (hide yes))
    (property "Datasheet" ""
      (at 381.0 223.52 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "J16")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 375.92 223.52)
      (xy 365.76 223.52)))
  (global_label "V24_BUS"
    (shape passive)
    (at 365.76 223.52 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 365.76 223.52 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 375.92 226.06)
      (xy 368.3 226.06)))
  (global_label "GND"
    (shape passive)
    (at 368.3 226.06 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 368.3 226.06 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 99.06 73.66)
      (xy 140.97 73.66)))
  (global_label "BUCK5_SW"
    (shape passive)
    (at 140.97 73.66 0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 140.97 73.66 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 297.18 68.58)
      (xy 339.09 68.58)))
  (global_label "BUCK3_SW"
    (shape passive)
    (at 339.09 68.58 0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 339.09 68.58 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 148.59 73.66)
      (xy 177.8 73.66)))
  (wire
    (pts
      (xy 177.8 73.66)
      (xy 177.8 92.71)))
  (global_label "+5V"
    (shape passive)
    (at 177.8 73.66 0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 177.8 73.66 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 148.59 73.66)
      (xy 203.2 73.66)))
  (wire
    (pts
      (xy 203.2 73.66)
      (xy 203.2 92.71)))
  (wire
    (pts
      (xy 346.71 68.58)
      (xy 375.92 68.58)))
  (wire
    (pts
      (xy 375.92 68.58)
      (xy 375.92 95.25)))
  (global_label "+3V3"
    (shape passive)
    (at 375.92 68.58 0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 375.92 68.58 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 154.94 140.97)
      (xy 154.94 163.83)))
  (global_label "BUCK5_FB"
    (shape passive)
    (at 154.94 140.97 0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 154.94 140.97 0.0)
      (hide yes)))
  (text "POWER 2"
    (at 20.32 15.24 0))
  (text "24 V -> 5 V / 1 A"
    (at 25.4 27.94 0))
  (text "5 V -> 3.3 V / 1 A"
    (at 233.68 27.94 0))
  (text "Ambient gate-bias inhibit"
    (at 25.4 182.88 0))
  (text "J1 input continues to F1 on power_1.\nU501 is a local BUS shunt clamp.\nJ16 is the external brake/bus port."
    (at 271.78 137.16 0))
  (embedded_fonts no))