(kicad_sch
  (version 20250114)
  (generator "engineered-lighting")
  (generator_version "0.2")
  (paper "A3")
  (title_block
    (title "Spot 1")
    (date "2026-09-06")
    (rev "A draft")
    (company "Engineered Lighting")
    (comment 1 "ENGINEERING DRAFT - see release status before fabrication"))
  (lib_symbols
    (symbol "EL:TPS26600PWPR"
      (pin_names
        (offset 0.8))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (property "Reference" "U"
        (at 0 20.32 0))
      (property "Value" "TPS26600PWPR"
        (at 0 -20.32 0))
      (symbol "TPS26600PWPR_0_1"
        (rectangle
          (start -12.7 17.78)
          (end 12.7 -17.78)
          (fill
            (type background))))
      (symbol "TPS26600PWPR_1_1"
        (pin power_in line
          (at -17.78 15.240000000000002 0)
          (length 5.08)
          (name "IN")
          (number "1"))
        (pin power_in line
          (at -17.78 12.700000000000003 0)
          (length 5.08)
          (name "IN")
          (number "2"))
        (pin input line
          (at -17.78 10.160000000000002 0)
          (length 5.08)
          (name "UVLO")
          (number "3"))
        (pin no_connect line
          (at -17.78 7.620000000000002 0)
          (length 5.08)
          (name "NC")
          (number "4"))
        (pin input line
          (at -17.78 5.080000000000002 0)
          (length 5.08)
          (name "OVP")
          (number "5"))
        (pin input line
          (at -17.78 2.5400000000000027 0)
          (length 5.08)
          (name "MODE")
          (number "6"))
        (pin input line
          (at -17.78 1.7763568394002505e-15 0)
          (length 5.08)
          (name "SHDN")
          (number "7"))
        (pin power_out line
          (at -17.78 -2.539999999999999 0)
          (length 5.08)
          (name "RTN")
          (number "8"))
        (pin power_in line
          (at -17.78 -5.079999999999998 0)
          (length 5.08)
          (name "GND")
          (number "9"))
        (pin passive line
          (at -17.78 -7.619999999999997 0)
          (length 5.08)
          (name "ILIM")
          (number "11"))
        (pin passive line
          (at -17.78 -10.159999999999997 0)
          (length 5.08)
          (name "dVdt")
          (number "12"))
        (pin no_connect line
          (at -17.78 -12.7 0)
          (length 5.08)
          (name "NC")
          (number "13"))
        (pin power_in line
          (at -17.78 -15.239999999999998 0)
          (length 5.08)
          (name "RTN_EP")
          (number "17"))
        (pin passive line
          (at 17.78 15.240000000000002 180)
          (length 5.08)
          (name "IMON")
          (number "10"))
        (pin open_collector line
          (at 17.78 12.700000000000003 180)
          (length 5.08)
          (name "FLT")
          (number "14"))
        (pin power_out line
          (at 17.78 10.160000000000002 180)
          (length 5.08)
          (name "OUT")
          (number "15"))
        (pin passive line
          (at 17.78 7.620000000000002 180)
          (length 5.08)
          (name "OUT")
          (number "16"))))
    (symbol "Device:R"
      (pin_numbers
        (hide yes))
      (pin_names
        (offset 0))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "R"
        (at 2.032 0 90)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "R"
        (at 0 0 90)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" ""
        (at -1.778 0 90)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Resistor"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "R res resistor"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "R_*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "R_0_1"
        (rectangle
          (start -1.016 -2.54)
          (end 1.016 2.54)
          (fill
            (type none))))
      (symbol "R_1_1"
        (pin passive line
          (at 0 3.81 270)
          (length 1.27)
          (name "")
          (number "1"))
        (pin passive line
          (at 0 -3.81 90)
          (length 1.27)
          (name "")
          (number "2")))
      (embedded_fonts no))
    (symbol "Device:C"
      (pin_numbers
        (hide yes))
      (pin_names
        (offset 0.254))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "C"
        (at 0.635 2.54 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "C"
        (at 0.635 -2.54 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" ""
        (at 0.9652 -3.81 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Unpolarized capacitor"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "cap capacitor"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "C_*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762))
          (fill
            (type none)))
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762))
          (fill
            (type none))))
      (symbol "C_1_1"
        (pin passive line
          (at 0 3.81 270)
          (length 2.794)
          (name "")
          (number "1"))
        (pin passive line
          (at 0 -3.81 90)
          (length 2.794)
          (name "")
          (number "2")))
      (embedded_fonts no))
    (symbol "Device:D_Schottky"
      (pin_numbers
        (hide yes))
      (pin_names
        (offset 1.016)
        (hide yes))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "D"
        (at 0 2.54 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "D_Schottky"
        (at 0 -2.54 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Schottky diode"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "diode Schottky"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "TO-???* *_Diode_* *SingleDiode* D_*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "D_Schottky_0_1"
        (polyline
          (pts
            (xy -1.905 0.635)
            (xy -1.905 1.27)
            (xy -1.27 1.27)
            (xy -1.27 -1.27)
            (xy -0.635 -1.27)
            (xy -0.635 -0.635))
          (fill
            (type none)))
        (polyline
          (pts
            (xy 1.27 1.27)
            (xy 1.27 -1.27)
            (xy -1.27 0)
            (xy 1.27 1.27))
          (fill
            (type none)))
        (polyline
          (pts
            (xy 1.27 0)
            (xy -1.27 0))
          (fill
            (type none))))
      (symbol "D_Schottky_1_1"
        (pin passive line
          (at -3.81 0 0)
          (length 2.54)
          (name "K")
          (number "1"))
        (pin passive line
          (at 3.81 0 180)
          (length 2.54)
          (name "A")
          (number "2")))
      (embedded_fonts no))
    (symbol "Driver_LED:AL8860WT"
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "U"
        (at -6.35 6.35 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "AL8860WT"
        (at 7.62 6.35 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
        (at 0 8.89 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" "https://www.diodes.com/assets/Datasheets/AL8860.pdf"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "40V 1.5A Constant Current Buck LED Driver IC, TSOT-23-5"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "LED Driver Buck Constant Current"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "TSOT?23*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "AL8860WT_0_1"
        (rectangle
          (start -7.62 5.08)
          (end 7.62 -5.08)
          (fill
            (type background))))
      (symbol "AL8860WT_1_1"
        (pin open_collector line
          (at 10.16 -2.54 180)
          (length 2.54)
          (name "SW")
          (number "1"))
        (pin power_in line
          (at 0 -7.62 90)
          (length 2.54)
          (name "GND")
          (number "2"))
        (pin input line
          (at -10.16 2.54 0)
          (length 2.54)
          (name "CTRL")
          (number "3"))
        (pin input line
          (at 10.16 2.54 180)
          (length 2.54)
          (name "SET")
          (number "4"))
        (pin power_in line
          (at 0 7.62 270)
          (length 2.54)
          (name "VIN")
          (number "5")))
      (embedded_fonts no))
    (symbol "Device:L"
      (pin_numbers
        (hide yes))
      (pin_names
        (offset 1.016)
        (hide yes))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "L"
        (at -1.27 0 90)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "L"
        (at 1.905 0 90)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Inductor"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "inductor choke coil reactor magnetic"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "Choke_* *Coil* Inductor_* L_*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "L_0_1"
        (arc
          (start 0 2.54)
          (mid 0.6323 1.905)
          (end 0 1.27)
          (fill
            (type none)))
        (arc
          (start 0 1.27)
          (mid 0.6323 0.635)
          (end 0 0)
          (fill
            (type none)))
        (arc
          (start 0 0)
          (mid 0.6323 -0.635)
          (end 0 -1.27)
          (fill
            (type none)))
        (arc
          (start 0 -1.27)
          (mid 0.6323 -1.905)
          (end 0 -2.54)
          (fill
            (type none))))
      (symbol "L_1_1"
        (pin passive line
          (at 0 3.81 270)
          (length 1.27)
          (name "1")
          (number "1"))
        (pin passive line
          (at 0 -3.81 90)
          (length 1.27)
          (name "2")
          (number "2")))
      (embedded_fonts no)))
  (symbol
    (lib_id "EL:TPS26600PWPR")
    (at 83.82 73.66 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "U14"
      (at 104.14 48.26 0.0))
    (property "Value" "spot branch gated eFuse 0.494A nominal"
      (at 104.14 50.8 0.0))
    (property "Footprint" "ELF:TI_PWP0016A_EP3.3x3.3_6ThermalVias_125um"
      (at 83.82 73.66 0.0)
      (hide yes))
    (property "MPN" "TPS26600PWPR"
      (at 83.82 73.66 0.0)
      (hide yes))
    (property "Manufacturer" "Texas Instruments"
      (at 83.82 73.66 0.0)
      (hide yes))
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2660.pdf"
      (at 83.82 73.66 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "U14")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "17")
    (pin "10")
    (pin "14")
    (pin "15")
    (pin "16"))
  (wire
    (pts
      (xy 66.04 58.42)
      (xy 55.88 58.42)))
  (global_label "V24_BUS"
    (shape passive)
    (at 55.88 58.42 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 55.88 58.42 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 66.04 60.96)
      (xy 55.88 60.96)))
  (global_label "V24_BUS"
    (shape passive)
    (at 55.88 60.96 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 55.88 60.96 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 66.04 63.5)
      (xy 55.88 63.5)))
  (global_label "SPOT_RTN"
    (shape passive)
    (at 55.88 63.5 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 55.88 63.5 0.0)
      (hide yes)))
  (no_connect
    (at 66.04 66.04))
  (wire
    (pts
      (xy 66.04 68.58)
      (xy 52.07 68.58)))
  (global_label "SPOT_EFUSE_OVP"
    (shape passive)
    (at 52.07 68.58 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 52.07 68.58 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 66.04 71.12)
      (xy 52.07 71.12)))
  (global_label "SPOT_EFUSE_MODE"
    (shape passive)
    (at 52.07 71.12 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 52.07 71.12 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 66.04 73.66)
      (xy 50.8 73.66)))
  (global_label "LIGHT_ENABLE_SAFE"
    (shape passive)
    (at 50.8 73.66 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 50.8 73.66 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 66.04 76.2)
      (xy 55.88 76.2)))
  (global_label "SPOT_RTN"
    (shape passive)
    (at 55.88 76.2 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 55.88 76.2 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 66.04 78.74)
      (xy 58.42 78.74)))
  (global_label "GND"
    (shape passive)
    (at 58.42 78.74 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 58.42 78.74 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 66.04 81.28)
      (xy 52.07 81.28)))
  (global_label "SPOT_EFUSE_ILIM"
    (shape passive)
    (at 52.07 81.28 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 52.07 81.28 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 66.04 83.82)
      (xy 52.07 83.82)))
  (global_label "SPOT_EFUSE_DVDT"
    (shape passive)
    (at 52.07 83.82 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 52.07 83.82 0.0)
      (hide yes)))
  (no_connect
    (at 66.04 86.36))
  (wire
    (pts
      (xy 66.04 88.9)
      (xy 55.88 88.9)))
  (global_label "SPOT_RTN"
    (shape passive)
    (at 55.88 88.9 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 55.88 88.9 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 101.6 58.42)
      (xy 115.57 58.42)))
  (global_label "SPOT_EFUSE_IMON"
    (shape passive)
    (at 115.57 58.42 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 115.57 58.42 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 101.6 60.96)
      (xy 115.57 60.96)))
  (global_label "SPOT_EFUSE_FLT_N"
    (shape passive)
    (at 115.57 60.96 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 115.57 60.96 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 101.6 66.04)
      (xy 111.76 66.04)))
  (global_label "V24_SPOT"
    (shape passive)
    (at 111.76 66.04 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 111.76 66.04 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 160.02 50.8 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R515"
      (at 165.1 49.53 0.0))
    (property "Value" "24.3k"
      (at 165.1 52.07 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 160.02 50.8 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-0724K3L"
      (at 160.02 50.8 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 160.02 50.8 0.0)
      (hide yes))
    (property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
      (at 160.02 50.8 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R515")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 160.02 46.99)
      (xy 160.02 33.02)))
  (global_label "SPOT_EFUSE_ILIM"
    (shape passive)
    (at 160.02 33.02 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 160.02 33.02 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 160.02 54.61)
      (xy 160.02 64.77)))
  (global_label "SPOT_RTN"
    (shape passive)
    (at 160.02 64.77 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 160.02 64.77 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 215.9 50.8 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R516"
      (at 220.98 49.53 0.0))
    (property "Value" "402k"
      (at 220.98 52.07 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 215.9 50.8 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-07402KL"
      (at 215.9 50.8 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 215.9 50.8 0.0)
      (hide yes))
    (property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
      (at 215.9 50.8 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R516")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 215.9 46.99)
      (xy 215.9 33.02)))
  (global_label "SPOT_EFUSE_MODE"
    (shape passive)
    (at 215.9 33.02 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 215.9 33.02 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 215.9 54.61)
      (xy 215.9 64.77)))
  (global_label "SPOT_RTN"
    (shape passive)
    (at 215.9 64.77 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 215.9 64.77 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 271.78 50.8 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R517"
      (at 276.86 49.53 0.0))
    (property "Value" "210k"
      (at 276.86 52.07 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 271.78 50.8 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-07210KL"
      (at 271.78 50.8 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 271.78 50.8 0.0)
      (hide yes))
    (property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
      (at 271.78 50.8 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R517")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 271.78 46.99)
      (xy 271.78 36.83)))
  (global_label "V24_BUS"
    (shape passive)
    (at 271.78 36.83 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 271.78 36.83 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 271.78 54.61)
      (xy 271.78 68.58)))
  (global_label "SPOT_EFUSE_OVP"
    (shape passive)
    (at 271.78 68.58 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 271.78 68.58 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 271.78 88.9 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R518"
      (at 276.86 87.63 0.0))
    (property "Value" "10k"
      (at 276.86 90.17 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 271.78 88.9 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-0710KL"
      (at 271.78 88.9 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 271.78 88.9 0.0)
      (hide yes))
    (property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
      (at 271.78 88.9 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R518")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 271.78 85.09)
      (xy 271.78 71.12)))
  (global_label "SPOT_EFUSE_OVP"
    (shape passive)
    (at 271.78 71.12 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 271.78 71.12 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 271.78 92.71)
      (xy 271.78 102.87)))
  (global_label "SPOT_RTN"
    (shape passive)
    (at 271.78 102.87 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 271.78 102.87 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 160.02 116.84 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R519"
      (at 165.1 115.57 0.0))
    (property "Value" "10k"
      (at 165.1 118.11 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 160.02 116.84 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-0710KL"
      (at 160.02 116.84 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 160.02 116.84 0.0)
      (hide yes))
    (property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
      (at 160.02 116.84 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R519")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 160.02 113.03)
      (xy 160.02 99.06)))
  (global_label "SPOT_EFUSE_IMON"
    (shape passive)
    (at 160.02 99.06 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 160.02 99.06 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 160.02 120.65)
      (xy 160.02 130.81)))
  (global_label "SPOT_RTN"
    (shape passive)
    (at 160.02 130.81 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 160.02 130.81 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 215.9 116.84 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R520"
      (at 220.98 115.57 0.0))
    (property "Value" "10k"
      (at 220.98 118.11 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 215.9 116.84 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-0710KL"
      (at 215.9 116.84 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 215.9 116.84 0.0)
      (hide yes))
    (property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
      (at 215.9 116.84 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R520")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 215.9 113.03)
      (xy 215.9 105.41)))
  (global_label "+3V3"
    (shape passive)
    (at 215.9 105.41 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 215.9 105.41 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 215.9 120.65)
      (xy 215.9 134.62)))
  (global_label "SPOT_EFUSE_FLT_N"
    (shape passive)
    (at 215.9 134.62 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 215.9 134.62 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 327.66 116.84 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R521"
      (at 332.74 115.57 0.0))
    (property "Value" "47k"
      (at 332.74 118.11 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 327.66 116.84 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-0747KL"
      (at 327.66 116.84 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 327.66 116.84 0.0)
      (hide yes))
    (property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-0710KL"
      (at 327.66 116.84 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R521")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 327.66 113.03)
      (xy 327.66 102.87)))
  (global_label "V24_SPOT"
    (shape passive)
    (at 327.66 102.87 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 327.66 102.87 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 327.66 120.65)
      (xy 327.66 128.27)))
  (global_label "GND"
    (shape passive)
    (at 327.66 128.27 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 327.66 128.27 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:C")
    (at 160.02 83.82 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C516"
      (at 165.1 82.55 0.0))
    (property "Value" "47nF 50V X7R"
      (at 165.1 85.09 0.0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
      (at 160.02 83.82 0.0)
      (hide yes))
    (property "MPN" "C1608X7R1H473K080AA"
      (at 160.02 83.82 0.0)
      (hide yes))
    (property "Manufacturer" "TDK"
      (at 160.02 83.82 0.0)
      (hide yes))
    (property "Datasheet" "https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C1608X7R1H473K080AA"
      (at 160.02 83.82 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C516")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 160.02 80.01)
      (xy 160.02 66.04)))
  (global_label "SPOT_EFUSE_DVDT"
    (shape passive)
    (at 160.02 66.04 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 160.02 66.04 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 160.02 87.63)
      (xy 160.02 97.79)))
  (global_label "SPOT_RTN"
    (shape passive)
    (at 160.02 97.79 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 160.02 97.79 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:C")
    (at 27.94 111.76 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C517"
      (at 33.02 110.49 0.0))
    (property "Value" "100nF 100V X7R"
      (at 33.02 113.03 0.0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
      (at 27.94 111.76 0.0)
      (hide yes))
    (property "MPN" "GRM188R72A104KA35D"
      (at 27.94 111.76 0.0)
      (hide yes))
    (property "Manufacturer" "Murata"
      (at 27.94 111.76 0.0)
      (hide yes))
    (property "Datasheet" "https://www.murata.com/products/productdetail?partno=GRM188R72A104KA35%23"
      (at 27.94 111.76 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C517")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 27.94 107.95)
      (xy 27.94 97.79)))
  (global_label "V24_BUS"
    (shape passive)
    (at 27.94 97.79 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 27.94 97.79 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 27.94 115.57)
      (xy 27.94 123.19)))
  (global_label "GND"
    (shape passive)
    (at 27.94 123.19 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 27.94 123.19 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:C")
    (at 327.66 83.82 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C518"
      (at 332.74 82.55 0.0))
    (property "Value" "100nF 100V X7R"
      (at 332.74 85.09 0.0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
      (at 327.66 83.82 0.0)
      (hide yes))
    (property "MPN" "GRM188R72A104KA35D"
      (at 327.66 83.82 0.0)
      (hide yes))
    (property "Manufacturer" "Murata"
      (at 327.66 83.82 0.0)
      (hide yes))
    (property "Datasheet" "https://www.murata.com/products/productdetail?partno=GRM188R72A104KA35%23"
      (at 327.66 83.82 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C518")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 327.66 87.63)
      (xy 327.66 95.25)))
  (global_label "GND"
    (shape passive)
    (at 327.66 95.25 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 327.66 95.25 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:D_Schottky")
    (at 381.0 83.82 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "D501"
      (at 381.0 76.2 0.0))
    (property "Value" "60V output negative transient Schottky"
      (at 381.0 78.74 0.0))
    (property "Footprint" "Diode_SMD:D_SMA"
      (at 381.0 83.82 0.0)
      (hide yes))
    (property "MPN" "B160-13-F"
      (at 381.0 83.82 0.0)
      (hide yes))
    (property "Manufacturer" "Diodes Incorporated"
      (at 381.0 83.82 0.0)
      (hide yes))
    (property "Datasheet" "https://www.diodes.com/datasheet/download/B130.pdf"
      (at 381.0 83.82 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "D501")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 377.19 83.82)
      (xy 367.03 83.82)))
  (global_label "V24_SPOT"
    (shape passive)
    (at 367.03 83.82 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 367.03 83.82 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 384.81 83.82)
      (xy 392.43 83.82)))
  (global_label "GND"
    (shape passive)
    (at 392.43 83.82 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 392.43 83.82 0.0)
      (hide yes)))
  (symbol
    (lib_id "Driver_LED:AL8860WT")
    (at 43.18 200.66 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "U7"
      (at 55.88 185.42 0.0))
    (property "Value" "333mA spotlight CC driver"
      (at 55.88 187.96 0.0))
    (property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
      (at 43.18 200.66 0.0)
      (hide yes))
    (property "MPN" "AL8860WT-7"
      (at 43.18 200.66 0.0)
      (hide yes))
    (property "Manufacturer" "Diodes Incorporated"
      (at 43.18 200.66 0.0)
      (hide yes))
    (property "Datasheet" "https://www.diodes.com/datasheet/download/AL8860.pdf"
      (at 43.18 200.66 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "U7")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5"))
  (wire
    (pts
      (xy 43.18 208.28)
      (xy 43.18 215.9)))
  (global_label "GND"
    (shape passive)
    (at 43.18 215.9 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 43.18 215.9 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 33.02 198.12)
      (xy 21.59 198.12)))
  (global_label "SPOT1_CTRL"
    (shape passive)
    (at 21.59 198.12 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 21.59 198.12 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 83.82 170.18 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R523"
      (at 88.9 168.91 0.0))
    (property "Value" "0.300ohm 1% 0.125W"
      (at 88.9 171.45 0.0))
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric"
      (at 83.82 170.18 0.0)
      (hide yes))
    (property "MPN" "ERJ-6RQFR30V"
      (at 83.82 170.18 0.0)
      (hide yes))
    (property "Manufacturer" "Panasonic"
      (at 83.82 170.18 0.0)
      (hide yes))
    (property "Datasheet" "https://industrial.panasonic.com/ww/products/pt/current-sensing-chip-resistors/models/ERJ6RQFR30V"
      (at 83.82 170.18 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R523")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (symbol
    (lib_id "Device:R")
    (at 22.86 229.87 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R526"
      (at 27.94 228.6 0.0))
    (property "Value" "910"
      (at 27.94 231.14 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 22.86 229.87 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-07910RL"
      (at 22.86 229.87 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 22.86 229.87 0.0)
      (hide yes))
    (property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-07910RL"
      (at 22.86 229.87 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R526")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 22.86 226.06)
      (xy 22.86 214.63)))
  (global_label "SPOT1_CTRL"
    (shape passive)
    (at 22.86 214.63 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 22.86 214.63 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 22.86 233.68)
      (xy 22.86 241.3)))
  (global_label "GND"
    (shape passive)
    (at 22.86 241.3 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 22.86 241.3 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:L")
    (at 114.3 224.79 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "L502"
      (at 119.38 223.52 0.0))
    (property "Value" "220uH +/-20%, .6A RMS .7A saturation"
      (at 119.38 226.06 0.0))
    (property "Footprint" "ELF:L_Bourns_SRN6045"
      (at 114.3 224.79 0.0)
      (hide yes))
    (property "MPN" "SRN6045-221M"
      (at 114.3 224.79 0.0)
      (hide yes))
    (property "Manufacturer" "Bourns"
      (at 114.3 224.79 0.0)
      (hide yes))
    (property "Datasheet" "https://www.bourns.com/docs/Product-Datasheets/SRN6045.pdf"
      (at 114.3 224.79 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "L502")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 114.3 220.98)
      (xy 114.3 207.01)))
  (global_label "SPOT1_LED_MINUS"
    (shape passive)
    (at 114.3 207.01 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 114.3 207.01 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:D_Schottky")
    (at 134.62 199.39 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "D502"
      (at 134.62 191.77 0.0))
    (property "Value" "60V 1A flyback Schottky"
      (at 134.62 194.31 0.0))
    (property "Footprint" "Diode_SMD:D_SMA"
      (at 134.62 199.39 0.0)
      (hide yes))
    (property "MPN" "B160-13-F"
      (at 134.62 199.39 0.0)
      (hide yes))
    (property "Manufacturer" "Diodes Incorporated"
      (at 134.62 199.39 0.0)
      (hide yes))
    (property "Datasheet" "https://www.diodes.com/datasheet/download/B130.pdf"
      (at 134.62 199.39 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "D502")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (symbol
    (lib_id "Device:C")
    (at 22.86 175.26 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C519"
      (at 27.94 173.99 0.0))
    (property "Value" "10uF 50V X7R"
      (at 27.94 176.53 0.0))
    (property "Footprint" "Capacitor_SMD:C_1210_3225Metric"
      (at 22.86 175.26 0.0)
      (hide yes))
    (property "MPN" "GRM32ER71H106KA12L"
      (at 22.86 175.26 0.0)
      (hide yes))
    (property "Manufacturer" "Murata"
      (at 22.86 175.26 0.0)
      (hide yes))
    (property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM32ER71H106KA12-04A.pdf"
      (at 22.86 175.26 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C519")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 22.86 171.45)
      (xy 22.86 161.29)))
  (global_label "V24_SPOT"
    (shape passive)
    (at 22.86 161.29 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 22.86 161.29 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 22.86 179.07)
      (xy 22.86 186.69)))
  (global_label "GND"
    (shape passive)
    (at 22.86 186.69 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 22.86 186.69 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:C")
    (at 45.72 175.26 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C520"
      (at 50.8 173.99 0.0))
    (property "Value" "10uF 50V X7R"
      (at 50.8 176.53 0.0))
    (property "Footprint" "Capacitor_SMD:C_1210_3225Metric"
      (at 45.72 175.26 0.0)
      (hide yes))
    (property "MPN" "GRM32ER71H106KA12L"
      (at 45.72 175.26 0.0)
      (hide yes))
    (property "Manufacturer" "Murata"
      (at 45.72 175.26 0.0)
      (hide yes))
    (property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM32ER71H106KA12-04A.pdf"
      (at 45.72 175.26 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C520")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 45.72 171.45)
      (xy 45.72 161.29)))
  (global_label "V24_SPOT"
    (shape passive)
    (at 45.72 161.29 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 45.72 161.29 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 45.72 179.07)
      (xy 45.72 186.69)))
  (global_label "GND"
    (shape passive)
    (at 45.72 186.69 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 45.72 186.69 0.0)
      (hide yes)))
  (symbol
    (lib_id "Driver_LED:AL8860WT")
    (at 172.72 200.66 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "U8"
      (at 185.42 185.42 0.0))
    (property "Value" "333mA spotlight CC driver"
      (at 185.42 187.96 0.0))
    (property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
      (at 172.72 200.66 0.0)
      (hide yes))
    (property "MPN" "AL8860WT-7"
      (at 172.72 200.66 0.0)
      (hide yes))
    (property "Manufacturer" "Diodes Incorporated"
      (at 172.72 200.66 0.0)
      (hide yes))
    (property "Datasheet" "https://www.diodes.com/datasheet/download/AL8860.pdf"
      (at 172.72 200.66 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "U8")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5"))
  (wire
    (pts
      (xy 172.72 208.28)
      (xy 172.72 215.9)))
  (global_label "GND"
    (shape passive)
    (at 172.72 215.9 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 172.72 215.9 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 162.56 198.12)
      (xy 151.13 198.12)))
  (global_label "SPOT2_CTRL"
    (shape passive)
    (at 151.13 198.12 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 151.13 198.12 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 213.36 170.18 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R524"
      (at 218.44 168.91 0.0))
    (property "Value" "0.300ohm 1% 0.125W"
      (at 218.44 171.45 0.0))
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric"
      (at 213.36 170.18 0.0)
      (hide yes))
    (property "MPN" "ERJ-6RQFR30V"
      (at 213.36 170.18 0.0)
      (hide yes))
    (property "Manufacturer" "Panasonic"
      (at 213.36 170.18 0.0)
      (hide yes))
    (property "Datasheet" "https://industrial.panasonic.com/ww/products/pt/current-sensing-chip-resistors/models/ERJ6RQFR30V"
      (at 213.36 170.18 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R524")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (symbol
    (lib_id "Device:R")
    (at 152.4 229.87 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R527"
      (at 157.48 228.6 0.0))
    (property "Value" "910"
      (at 157.48 231.14 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 152.4 229.87 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-07910RL"
      (at 152.4 229.87 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 152.4 229.87 0.0)
      (hide yes))
    (property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-07910RL"
      (at 152.4 229.87 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R527")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 152.4 226.06)
      (xy 152.4 214.63)))
  (global_label "SPOT2_CTRL"
    (shape passive)
    (at 152.4 214.63 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 152.4 214.63 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 152.4 233.68)
      (xy 152.4 241.3)))
  (global_label "GND"
    (shape passive)
    (at 152.4 241.3 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 152.4 241.3 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:L")
    (at 243.84 224.79 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "L503"
      (at 248.92 223.52 0.0))
    (property "Value" "220uH +/-20%, .6A RMS .7A saturation"
      (at 248.92 226.06 0.0))
    (property "Footprint" "ELF:L_Bourns_SRN6045"
      (at 243.84 224.79 0.0)
      (hide yes))
    (property "MPN" "SRN6045-221M"
      (at 243.84 224.79 0.0)
      (hide yes))
    (property "Manufacturer" "Bourns"
      (at 243.84 224.79 0.0)
      (hide yes))
    (property "Datasheet" "https://www.bourns.com/docs/Product-Datasheets/SRN6045.pdf"
      (at 243.84 224.79 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "L503")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 243.84 220.98)
      (xy 243.84 207.01)))
  (global_label "SPOT2_LED_MINUS"
    (shape passive)
    (at 243.84 207.01 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 243.84 207.01 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:D_Schottky")
    (at 264.16 199.39 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "D503"
      (at 264.16 191.77 0.0))
    (property "Value" "60V 1A flyback Schottky"
      (at 264.16 194.31 0.0))
    (property "Footprint" "Diode_SMD:D_SMA"
      (at 264.16 199.39 0.0)
      (hide yes))
    (property "MPN" "B160-13-F"
      (at 264.16 199.39 0.0)
      (hide yes))
    (property "Manufacturer" "Diodes Incorporated"
      (at 264.16 199.39 0.0)
      (hide yes))
    (property "Datasheet" "https://www.diodes.com/datasheet/download/B130.pdf"
      (at 264.16 199.39 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "D503")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (symbol
    (lib_id "Device:C")
    (at 152.4 175.26 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C521"
      (at 157.48 173.99 0.0))
    (property "Value" "10uF 50V X7R"
      (at 157.48 176.53 0.0))
    (property "Footprint" "Capacitor_SMD:C_1210_3225Metric"
      (at 152.4 175.26 0.0)
      (hide yes))
    (property "MPN" "GRM32ER71H106KA12L"
      (at 152.4 175.26 0.0)
      (hide yes))
    (property "Manufacturer" "Murata"
      (at 152.4 175.26 0.0)
      (hide yes))
    (property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM32ER71H106KA12-04A.pdf"
      (at 152.4 175.26 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C521")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 152.4 171.45)
      (xy 152.4 161.29)))
  (global_label "V24_SPOT"
    (shape passive)
    (at 152.4 161.29 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 152.4 161.29 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 152.4 179.07)
      (xy 152.4 186.69)))
  (global_label "GND"
    (shape passive)
    (at 152.4 186.69 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 152.4 186.69 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:C")
    (at 175.26 175.26 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C522"
      (at 180.34 173.99 0.0))
    (property "Value" "10uF 50V X7R"
      (at 180.34 176.53 0.0))
    (property "Footprint" "Capacitor_SMD:C_1210_3225Metric"
      (at 175.26 175.26 0.0)
      (hide yes))
    (property "MPN" "GRM32ER71H106KA12L"
      (at 175.26 175.26 0.0)
      (hide yes))
    (property "Manufacturer" "Murata"
      (at 175.26 175.26 0.0)
      (hide yes))
    (property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM32ER71H106KA12-04A.pdf"
      (at 175.26 175.26 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C522")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 175.26 171.45)
      (xy 175.26 161.29)))
  (global_label "V24_SPOT"
    (shape passive)
    (at 175.26 161.29 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 175.26 161.29 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 175.26 179.07)
      (xy 175.26 186.69)))
  (global_label "GND"
    (shape passive)
    (at 175.26 186.69 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 175.26 186.69 0.0)
      (hide yes)))
  (symbol
    (lib_id "Driver_LED:AL8860WT")
    (at 302.26 200.66 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "U9"
      (at 314.96 185.42 0.0))
    (property "Value" "333mA spotlight CC driver"
      (at 314.96 187.96 0.0))
    (property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
      (at 302.26 200.66 0.0)
      (hide yes))
    (property "MPN" "AL8860WT-7"
      (at 302.26 200.66 0.0)
      (hide yes))
    (property "Manufacturer" "Diodes Incorporated"
      (at 302.26 200.66 0.0)
      (hide yes))
    (property "Datasheet" "https://www.diodes.com/datasheet/download/AL8860.pdf"
      (at 302.26 200.66 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "U9")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5"))
  (wire
    (pts
      (xy 302.26 208.28)
      (xy 302.26 215.9)))
  (global_label "GND"
    (shape passive)
    (at 302.26 215.9 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 302.26 215.9 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 292.1 198.12)
      (xy 280.67 198.12)))
  (global_label "SPOT3_CTRL"
    (shape passive)
    (at 280.67 198.12 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 280.67 198.12 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:R")
    (at 342.9 170.18 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R525"
      (at 347.98 168.91 0.0))
    (property "Value" "0.300ohm 1% 0.125W"
      (at 347.98 171.45 0.0))
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric"
      (at 342.9 170.18 0.0)
      (hide yes))
    (property "MPN" "ERJ-6RQFR30V"
      (at 342.9 170.18 0.0)
      (hide yes))
    (property "Manufacturer" "Panasonic"
      (at 342.9 170.18 0.0)
      (hide yes))
    (property "Datasheet" "https://industrial.panasonic.com/ww/products/pt/current-sensing-chip-resistors/models/ERJ6RQFR30V"
      (at 342.9 170.18 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R525")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (symbol
    (lib_id "Device:R")
    (at 281.94 229.87 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "R528"
      (at 287.02 228.6 0.0))
    (property "Value" "910"
      (at 287.02 231.14 0.0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric"
      (at 281.94 229.87 0.0)
      (hide yes))
    (property "MPN" "RC0603FR-07910RL"
      (at 281.94 229.87 0.0)
      (hide yes))
    (property "Manufacturer" "Yageo"
      (at 281.94 229.87 0.0)
      (hide yes))
    (property "Datasheet" "https://www.yageogroup.com/component-documentation/download/specsheet/RC0603FR-07910RL"
      (at 281.94 229.87 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "R528")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 281.94 226.06)
      (xy 281.94 214.63)))
  (global_label "SPOT3_CTRL"
    (shape passive)
    (at 281.94 214.63 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 281.94 214.63 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 281.94 233.68)
      (xy 281.94 241.3)))
  (global_label "GND"
    (shape passive)
    (at 281.94 241.3 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 281.94 241.3 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:L")
    (at 373.38 224.79 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "L504"
      (at 378.46 223.52 0.0))
    (property "Value" "220uH +/-20%, .6A RMS .7A saturation"
      (at 378.46 226.06 0.0))
    (property "Footprint" "ELF:L_Bourns_SRN6045"
      (at 373.38 224.79 0.0)
      (hide yes))
    (property "MPN" "SRN6045-221M"
      (at 373.38 224.79 0.0)
      (hide yes))
    (property "Manufacturer" "Bourns"
      (at 373.38 224.79 0.0)
      (hide yes))
    (property "Datasheet" "https://www.bourns.com/docs/Product-Datasheets/SRN6045.pdf"
      (at 373.38 224.79 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "L504")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 373.38 220.98)
      (xy 373.38 207.01)))
  (global_label "SPOT3_LED_MINUS"
    (shape passive)
    (at 373.38 207.01 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 373.38 207.01 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 101.6 63.5)
      (xy 327.66 63.5)))
  (wire
    (pts
      (xy 327.66 63.5)
      (xy 327.66 80.01)))
  (global_label "V24_SPOT"
    (shape passive)
    (at 327.66 63.5 0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 327.66 63.5 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 83.82 173.99)
      (xy 83.82 198.12)))
  (wire
    (pts
      (xy 83.82 198.12)
      (xy 53.34 198.12)))
  (global_label "SPOT1_LED_PLUS"
    (shape passive)
    (at 83.82 198.12 0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 83.82 198.12 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 53.34 203.2)
      (xy 53.34 242.57)))
  (wire
    (pts
      (xy 53.34 242.57)
      (xy 114.3 242.57)))
  (wire
    (pts
      (xy 114.3 242.57)
      (xy 114.3 228.6)))
  (global_label "SPOT1_SW"
    (shape passive)
    (at 53.34 242.57 0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 53.34 242.57 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 114.3 242.57)
      (xy 138.43 242.57)))
  (wire
    (pts
      (xy 138.43 242.57)
      (xy 138.43 199.39)))
  (wire
    (pts
      (xy 83.82 166.37)
      (xy 130.81 166.37)))
  (wire
    (pts
      (xy 130.81 166.37)
      (xy 130.81 199.39)))
  (global_label "V24_SPOT"
    (shape passive)
    (at 130.81 166.37 0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 130.81 166.37 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 83.82 166.37)
      (xy 43.18 166.37)))
  (wire
    (pts
      (xy 43.18 166.37)
      (xy 43.18 193.04)))
  (wire
    (pts
      (xy 213.36 173.99)
      (xy 213.36 198.12)))
  (wire
    (pts
      (xy 213.36 198.12)
      (xy 182.88 198.12)))
  (global_label "SPOT2_LED_PLUS"
    (shape passive)
    (at 213.36 198.12 0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 213.36 198.12 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 182.88 203.2)
      (xy 182.88 242.57)))
  (wire
    (pts
      (xy 182.88 242.57)
      (xy 243.84 242.57)))
  (wire
    (pts
      (xy 243.84 242.57)
      (xy 243.84 228.6)))
  (global_label "SPOT2_SW"
    (shape passive)
    (at 182.88 242.57 0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 182.88 242.57 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 243.84 242.57)
      (xy 267.97 242.57)))
  (wire
    (pts
      (xy 267.97 242.57)
      (xy 267.97 199.39)))
  (wire
    (pts
      (xy 213.36 166.37)
      (xy 260.35 166.37)))
  (wire
    (pts
      (xy 260.35 166.37)
      (xy 260.35 199.39)))
  (global_label "V24_SPOT"
    (shape passive)
    (at 260.35 166.37 0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 260.35 166.37 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 213.36 166.37)
      (xy 172.72 166.37)))
  (wire
    (pts
      (xy 172.72 166.37)
      (xy 172.72 193.04)))
  (wire
    (pts
      (xy 342.9 173.99)
      (xy 342.9 198.12)))
  (wire
    (pts
      (xy 342.9 198.12)
      (xy 312.42 198.12)))
  (global_label "SPOT3_LED_PLUS"
    (shape passive)
    (at 342.9 198.12 0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 342.9 198.12 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 312.42 203.2)
      (xy 312.42 242.57)))
  (wire
    (pts
      (xy 312.42 242.57)
      (xy 373.38 242.57)))
  (wire
    (pts
      (xy 373.38 242.57)
      (xy 373.38 228.6)))
  (global_label "SPOT3_SW"
    (shape passive)
    (at 312.42 242.57 0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 312.42 242.57 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 342.9 166.37)
      (xy 302.26 166.37)))
  (wire
    (pts
      (xy 302.26 166.37)
      (xy 302.26 193.04)))
  (global_label "V24_SPOT"
    (shape passive)
    (at 302.26 166.37 0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 302.26 166.37 0.0)
      (hide yes)))
  (junction
    (at 114.3 242.57)
    (diameter 0)
    (color 0 0 0 0))
  (junction
    (at 243.84 242.57)
    (diameter 0)
    (color 0 0 0 0))
  (text "SPOT 1"
    (at 20.32 15.24 0))
  (text "INDEPENDENT SPOT SUPPLY INHIBIT / 0.494 A NOMINAL"
    (at 20.32 27.94 0))
  (text "SPOT_RTN belongs to U14: do not join it to GND. Stored charge remains after inhibition."
    (at 20.32 134.62 0))
  (text "SPOT 1 / 333 mA nominal"
    (at 22.86 149.86 0))
  (text "Paired LED output -> J9 pins 1/2 / spot_2"
    (at 22.86 247.65 0))
  (text "SPOT 2 / 333 mA nominal"
    (at 152.4 149.86 0))
  (text "Paired LED output -> J9 pins 3/4 / spot_2"
    (at 152.4 247.65 0))
  (text "SPOT 3 / 333 mA nominal"
    (at 281.94 149.86 0))
  (text "Paired LED output -> J9 pins 5/6 / spot_2"
    (at 281.94 247.65 0))
  (text "CH3 diode/input capacitors continue on spot_2."
    (at 233.68 139.7 0))
  (embedded_fonts no))
