(kicad_sch
  (version 20250114)
  (generator "engineered-lighting")
  (generator_version "0.2")
  (paper "A3")
  (title_block
    (title "Spot 2")
    (date "2026-09-06")
    (rev "A draft")
    (company "Engineered Lighting")
    (comment 1 "ENGINEERING DRAFT - see release status before fabrication"))
  (lib_symbols
    (symbol "Device:D_Schottky"
      (pin_numbers
        (hide yes))
      (pin_names
        (offset 1.016)
        (hide yes))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "D"
        (at 0 2.54 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "D_Schottky"
        (at 0 -2.54 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Schottky diode"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "diode Schottky"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "TO-???* *_Diode_* *SingleDiode* D_*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "D_Schottky_0_1"
        (polyline
          (pts
            (xy -1.905 0.635)
            (xy -1.905 1.27)
            (xy -1.27 1.27)
            (xy -1.27 -1.27)
            (xy -0.635 -1.27)
            (xy -0.635 -0.635))
          (fill
            (type none)))
        (polyline
          (pts
            (xy 1.27 1.27)
            (xy 1.27 -1.27)
            (xy -1.27 0)
            (xy 1.27 1.27))
          (fill
            (type none)))
        (polyline
          (pts
            (xy 1.27 0)
            (xy -1.27 0))
          (fill
            (type none))))
      (symbol "D_Schottky_1_1"
        (pin passive line
          (at -3.81 0 0)
          (length 2.54)
          (name "K")
          (number "1"))
        (pin passive line
          (at 3.81 0 180)
          (length 2.54)
          (name "A")
          (number "2")))
      (embedded_fonts no))
    (symbol "Device:C"
      (pin_numbers
        (hide yes))
      (pin_names
        (offset 0.254))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "C"
        (at 0.635 2.54 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "C"
        (at 0.635 -2.54 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" ""
        (at 0.9652 -3.81 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Unpolarized capacitor"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "cap capacitor"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "C_*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762))
          (fill
            (type none)))
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762))
          (fill
            (type none))))
      (symbol "C_1_1"
        (pin passive line
          (at 0 3.81 270)
          (length 2.794)
          (name "")
          (number "1"))
        (pin passive line
          (at 0 -3.81 90)
          (length 2.794)
          (name "")
          (number "2")))
      (embedded_fonts no))
    (symbol "Power_Protection:TVS2700DRV"
      (pin_names
        (offset 0)
        (hide yes))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (symbol "TVS2700DRV_0_0"
        (rectangle
          (start -11.43 2.54)
          (end -5.08 -2.54)
          (fill
            (type none)))
        (polyline
          (pts
            (xy -8.255 2.54)
            (xy -8.255 3.81)
            (xy 0 3.81))
          (fill
            (type none)))
        (polyline
          (pts
            (xy -8.255 -2.54)
            (xy -8.255 -3.81)
            (xy 0 -3.81))
          (fill
            (type none)))
        (polyline
          (pts
            (xy 0 1.27)
            (xy -1.778 1.27))
          (fill
            (type none)))
        (text "Det &"
          (at -8.255 0.635 0))
        (text "Drv"
          (at -8.255 -1.27 0)))
      (symbol "TVS2700DRV_0_1"
        (rectangle
          (start -12.065 5.08)
          (end 2.54 -5.08)
          (fill
            (type background)))
        (polyline
          (pts
            (xy -2.286 1.397)
            (xy -2.286 -1.524))
          (fill
            (type none)))
        (polyline
          (pts
            (xy -2.286 0)
            (xy -5.08 0))
          (fill
            (type none)))
        (polyline
          (pts
            (xy -1.778 1.778)
            (xy -1.778 -1.778))
          (fill
            (type none)))
        (circle
          (center -0.889 0)
          (radius 2.794)
          (fill
            (type none)))
        (polyline
          (pts
            (xy -0.127 -1.27)
            (xy -1.143 -1.651)
            (xy -1.143 -0.889)
            (xy -0.127 -1.27))
          (fill
            (type outline)))
        (polyline
          (pts
            (xy 0 5.08)
            (xy 0 2.54))
          (fill
            (type none)))
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0 1.27))
          (fill
            (type none)))
        (polyline
          (pts
            (xy 0 -2.54)
            (xy 0 -5.08))
          (fill
            (type none)))
        (polyline
          (pts
            (xy 0 -2.54)
            (xy 0 -1.27)
            (xy -1.778 -1.27))
          (fill
            (type none))))
      (symbol "TVS2700DRV_1_1"
        (pin power_in line
          (at 0 -7.62 90)
          (length 2.54)
          (name "GND")
          (number "1"))
        (pin passive line
          (at 0 -7.62 90)
          (length 2.54)
          (hide yes)
          (name "GND")
          (number "2"))
        (pin passive line
          (at 0 -7.62 90)
          (length 2.54)
          (hide yes)
          (name "GND")
          (number "3"))
        (pin passive line
          (at 0 7.62 270)
          (length 2.54)
          (name "IN")
          (number "4"))
        (pin passive line
          (at 0 7.62 270)
          (length 2.54)
          (hide yes)
          (name "IN")
          (number "5"))
        (pin passive line
          (at 0 7.62 270)
          (length 2.54)
          (hide yes)
          (name "IN")
          (number "6"))
        (pin passive line
          (at 0 -7.62 90)
          (length 2.54)
          (hide yes)
          (name "GND")
          (number "7")))
      (embedded_fonts no)
      (property "Reference" "U"
        (at 2.54 1.27 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "TVS2700DRV"
        (at 2.54 -1.27 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
        (at 5.08 -8.89 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" "http://www.ti.com/lit/ds/symlink/tvs2700.pdf"
        (at -2.54 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Flat-Clamp Surge Protection Device. 27Vrwm, WSON-6"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "EMI, ESD, TVS protection transient"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*EP1x1.6mm*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes)))
    (symbol "Connector_Generic:Conn_01x02"
      (pin_names
        (offset 1.016)
        (hide yes))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "J"
        (at 0 2.54 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "Conn_01x02"
        (at 0 -5.08 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "connector"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "Connector*:*_1x??_*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "Conn_01x02_1_1"
        (rectangle
          (start -1.27 1.27)
          (end 1.27 -3.81)
          (fill
            (type background)))
        (rectangle
          (start -1.27 0.127)
          (end 0 -0.127)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -2.413)
          (end 0 -2.667)
          (fill
            (type none)))
        (pin passive line
          (at -5.08 0 0)
          (length 3.81)
          (name "Pin_1")
          (number "1"))
        (pin passive line
          (at -5.08 -2.54 0)
          (length 3.81)
          (name "Pin_2")
          (number "2")))
      (embedded_fonts no))
    (symbol "Connector_Generic:Conn_01x06"
      (pin_names
        (offset 1.016)
        (hide yes))
      (exclude_from_sim no)
      (in_bom yes)
      (on_board yes)
      (in_pos_files yes)
      (duplicate_pin_numbers_are_jumpers no)
      (property "Reference" "J"
        (at 0 7.62 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Value" "Conn_01x06"
        (at 0 -10.16 0)
        (show_name no)
        (do_not_autoplace no))
      (property "Footprint" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Datasheet" ""
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "Description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_keywords" "connector"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (property "ki_fp_filters" "Connector*:*_1x??_*"
        (at 0 0 0)
        (show_name no)
        (do_not_autoplace no)
        (hide yes))
      (symbol "Conn_01x06_1_1"
        (rectangle
          (start -1.27 6.35)
          (end 1.27 -8.89)
          (fill
            (type background)))
        (rectangle
          (start -1.27 5.207)
          (end 0 4.953)
          (fill
            (type none)))
        (rectangle
          (start -1.27 2.667)
          (end 0 2.413)
          (fill
            (type none)))
        (rectangle
          (start -1.27 0.127)
          (end 0 -0.127)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -2.413)
          (end 0 -2.667)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -4.953)
          (end 0 -5.207)
          (fill
            (type none)))
        (rectangle
          (start -1.27 -7.493)
          (end 0 -7.747)
          (fill
            (type none)))
        (pin passive line
          (at -5.08 5.08 0)
          (length 3.81)
          (name "Pin_1")
          (number "1"))
        (pin passive line
          (at -5.08 2.54 0)
          (length 3.81)
          (name "Pin_2")
          (number "2"))
        (pin passive line
          (at -5.08 0 0)
          (length 3.81)
          (name "Pin_3")
          (number "3"))
        (pin passive line
          (at -5.08 -2.54 0)
          (length 3.81)
          (name "Pin_4")
          (number "4"))
        (pin passive line
          (at -5.08 -5.08 0)
          (length 3.81)
          (name "Pin_5")
          (number "5"))
        (pin passive line
          (at -5.08 -7.62 0)
          (length 3.81)
          (name "Pin_6")
          (number "6")))
      (embedded_fonts no)))
  (symbol
    (lib_id "Device:D_Schottky")
    (at 175.26 180.34 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "D504"
      (at 175.26 172.72 0.0))
    (property "Value" "60V 1A flyback Schottky"
      (at 175.26 175.26 0.0))
    (property "Footprint" "Diode_SMD:D_SMA"
      (at 175.26 180.34 0.0)
      (hide yes))
    (property "MPN" "B160-13-F"
      (at 175.26 180.34 0.0)
      (hide yes))
    (property "Manufacturer" "Diodes Incorporated"
      (at 175.26 180.34 0.0)
      (hide yes))
    (property "Datasheet" "https://www.diodes.com/datasheet/download/B130.pdf"
      (at 175.26 180.34 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "D504")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 171.45 180.34)
      (xy 161.29 180.34)))
  (global_label "V24_SPOT"
    (shape passive)
    (at 161.29 180.34 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 161.29 180.34 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 179.07 180.34)
      (xy 189.23 180.34)))
  (global_label "SPOT3_SW"
    (shape passive)
    (at 189.23 180.34 180.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 189.23 180.34 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:C")
    (at 43.18 180.34 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C523"
      (at 48.26 179.07 0.0))
    (property "Value" "10uF 50V X7R"
      (at 48.26 181.61 0.0))
    (property "Footprint" "Capacitor_SMD:C_1210_3225Metric"
      (at 43.18 180.34 0.0)
      (hide yes))
    (property "MPN" "GRM32ER71H106KA12L"
      (at 43.18 180.34 0.0)
      (hide yes))
    (property "Manufacturer" "Murata"
      (at 43.18 180.34 0.0)
      (hide yes))
    (property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM32ER71H106KA12-04A.pdf"
      (at 43.18 180.34 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C523")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 43.18 184.15)
      (xy 43.18 191.77)))
  (global_label "GND"
    (shape passive)
    (at 43.18 191.77 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 43.18 191.77 0.0)
      (hide yes)))
  (symbol
    (lib_id "Device:C")
    (at 96.52 180.34 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "C524"
      (at 101.6 179.07 0.0))
    (property "Value" "10uF 50V X7R"
      (at 101.6 181.61 0.0))
    (property "Footprint" "Capacitor_SMD:C_1210_3225Metric"
      (at 96.52 180.34 0.0)
      (hide yes))
    (property "MPN" "GRM32ER71H106KA12L"
      (at 96.52 180.34 0.0)
      (hide yes))
    (property "Manufacturer" "Murata"
      (at 96.52 180.34 0.0)
      (hide yes))
    (property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM32ER71H106KA12-04A.pdf"
      (at 96.52 180.34 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "C524")
          (unit 1))))
    (pin "1")
    (pin "2"))
  (wire
    (pts
      (xy 96.52 184.15)
      (xy 96.52 191.77)))
  (global_label "GND"
    (shape passive)
    (at 96.52 191.77 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 96.52 191.77 0.0)
      (hide yes)))
  (symbol
    (lib_id "Power_Protection:TVS2700DRV")
    (at 292.1 180.34 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "U500"
      (at 301.9425 165.1 0.0))
    (property "Value" "27V flat-clamp transient protector"
      (at 301.9425 167.64 0.0))
    (property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm_ThermalVias"
      (at 292.1 180.34 0.0)
      (hide yes))
    (property "MPN" "TVS2700DRVR"
      (at 292.1 180.34 0.0)
      (hide yes))
    (property "Manufacturer" "Texas Instruments"
      (at 292.1 180.34 0.0)
      (hide yes))
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/tvs2700.pdf"
      (at 292.1 180.34 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "U500")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7"))
  (wire
    (pts
      (xy 292.1 187.96)
      (xy 292.1 195.58)))
  (global_label "GND"
    (shape passive)
    (at 292.1 195.58 90.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 292.1 195.58 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 292.1 172.72)
      (xy 292.1 162.56)))
  (global_label "V24_SPOT"
    (shape passive)
    (at 292.1 162.56 270.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 292.1 162.56 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 43.18 176.53)
      (xy 96.52 176.53)))
  (global_label "V24_SPOT"
    (shape passive)
    (at 96.52 176.53 0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 96.52 176.53 0.0)
      (hide yes)))
  (text "SPOT 2"
    (at 20.32 15.24 0))
  (text "J9: 1/2 = SPOT1 +/-, 3/4 = SPOT2 +/-, 5/6 = SPOT3 +/-.\nAll three LED pairs remain independent; LED- is not GND.\nThe wire service loop reaches the static arm flex; J13 separately carries tilt power and CAN."
    (at 20.32 27.94 0))
  (text "CH3 current loop continuation from U9 on spot_1"
    (at 20.32 132.08 0))
  (text "U500 local spotlight-rail shunt clamp.\nPulse limits do not establish continuous braking."
    (at 241.3 228.6 0))
  (embedded_fonts no)
  (symbol
    (lib_id "Connector_Generic:Conn_01x06")
    (at 76.2 81.28 0)
    (unit 1)
    (exclude_from_sim yes)
    (in_bom yes)
    (on_board yes)
    (dnp no)
    (property "Reference" "J9"
      (at 76.2 66.04 0.0))
    (property "Value" "SPOTLIGHT 3 PAIRS"
      (at 76.2 68.58 0.0))
    (property "Footprint" "EL:JST_GH_BM06B-GHS-TBT_1x06-1MP_P1.25mm_Vertical"
      (at 76.2 81.28 0.0)
      (hide yes))
    (property "MPN" "BM06B-GHS-TBT(LF)(SN)"
      (at 76.2 81.28 0.0)
      (hide yes))
    (property "Manufacturer" "JST"
      (at 76.2 81.28 0.0)
      (hide yes))
    (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eGH.pdf"
      (at 76.2 81.28 0.0)
      (hide yes))
    (instances
      (project "engineered-lighting-rev-a"
        (path
          (reference "J9")
          (unit 1))))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6"))
  (wire
    (pts
      (xy 71.12 76.2)
      (xy 57.15 76.2)))
  (global_label "SPOT1_LED_PLUS"
    (shape passive)
    (at 57.15 76.2 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 57.15 76.2 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 71.12 78.74)
      (xy 57.15 78.74)))
  (global_label "SPOT1_LED_MINUS"
    (shape passive)
    (at 57.15 78.74 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 57.15 78.74 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 71.12 81.28)
      (xy 57.15 81.28)))
  (global_label "SPOT2_LED_PLUS"
    (shape passive)
    (at 57.15 81.28 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 57.15 81.28 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 71.12 83.82)
      (xy 57.15 83.82)))
  (global_label "SPOT2_LED_MINUS"
    (shape passive)
    (at 57.15 83.82 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 57.15 83.82 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 71.12 86.36)
      (xy 57.15 86.36)))
  (global_label "SPOT3_LED_PLUS"
    (shape passive)
    (at 57.15 86.36 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 57.15 86.36 0.0)
      (hide yes)))
  (wire
    (pts
      (xy 71.12 88.9)
      (xy 57.15 88.9)))
  (global_label "SPOT3_LED_MINUS"
    (shape passive)
    (at 57.15 88.9 0.0)
    (property "Intersheetrefs" "${INTERSHEET_REFS}"
      (at 57.15 88.9 0.0)
      (hide yes))))
